#!/bin/sh
# Part of raspi-config https://github.com/RPi-Distro/raspi-config
#
# See LICENSE file for copyright and license details

INTERACTIVE=True
ASK_TO_REBOOT=0
BLACKLIST=/etc/modprobe.d/raspi-blacklist.conf
CONFIG=/boot/config.txt

if ! [[ -f /dev/root ]] && ! [[ -f /etc/.rckeep ]]; then
	cd /dev
	ln -s mmcblk0p2 root
	cd -
	echo "real ugly hack, sorry." > /etc/.rckeep
fi

is_pione() {
   if grep -q "^Revision\s*:\s*00[0-9a-fA-F][0-9a-fA-F]$" /proc/cpuinfo; then
      return 0
   elif  grep -q "^Revision\s*:\s*[ 123][0-9a-fA-F][0-9a-fA-F][0-9a-fA-F]0[0-36][0-9a-fA-F]$" /proc/cpuinfo ; then
      return 0
   else
      return 1
   fi
}

is_pitwo() {
   grep -q "^Revision\s*:\s*[ 123][0-9a-fA-F][0-9a-fA-F][0-9a-fA-F]04[0-9a-fA-F]$" /proc/cpuinfo
   return $?
}

is_pizero() {
   grep -q "^Revision\s*:\s*[ 123][0-9a-fA-F][0-9a-fA-F][0-9a-fA-F]09[0-9a-fA-F]$" /proc/cpuinfo
   return $?
}

get_pi_type() {
   if is_pione; then
      echo 1
   elif is_pitwo; then
      echo 2
   else
      echo 0
   fi
}

get_init_sys() {
  if command -v systemctl > /dev/null && systemctl | grep -q '\-\.mount'; then
    SYSTEMD=1
  elif [ -f /etc/init.d/cron ] && [ ! -h /etc/init.d/cron ]; then
    SYSTEMD=0
  else
    echo "Unrecognised init system"
    return 1
  fi
}

calc_wt_size() {
  # NOTE: it's tempting to redirect stderr to /dev/null, so supress error 
  # output from tput. However in this case, tput detects neither stdout or 
  # stderr is a tty and so only gives default 80, 24 values
  WT_HEIGHT=17
  WT_WIDTH=$(tput cols)

  if [ -z "$WT_WIDTH" ] || [ "$WT_WIDTH" -lt 60 ]; then
    WT_WIDTH=80
  fi
  if [ "$WT_WIDTH" -gt 178 ]; then
    WT_WIDTH=120
  fi
  WT_MENU_HEIGHT=$(($WT_HEIGHT-7))
}

do_about() {
  whiptail --msgbox "\
This tool provides a straight-forward way of doing initial
configuration of the Raspberry Pi. Although it can be run
at any time, some of the options may have difficulties if
you have heavily customised your installation.\
" 20 70 1
}

do_expand_rootfs() {
  get_init_sys
  if [ $SYSTEMD -eq 1 ]; then
    ROOT_PART=$(mount | sed -n 's|^/dev/\(.*\) on / .*|\1|p')
  else
    if ! [ -h /dev/root ]; then
      whiptail --msgbox "/dev/root does not exist or is not a symlink. Don't know how to expand" 20 60 2
      return 0
    fi
    ROOT_PART=$(readlink /dev/root)
  fi

  PART_NUM=${ROOT_PART#mmcblk0p}
  if [ "$PART_NUM" = "$ROOT_PART" ]; then
    whiptail --msgbox "$ROOT_PART is not an SD card. Don't know how to expand" 20 60 2
    return 0
  fi

  # NOTE: the NOOBS partition layout confuses parted. For now, let's only 
  # agree to work with a sufficiently simple partition layout
  if [ "$PART_NUM" -ne 2 ]; then
    whiptail --msgbox "Your partition layout is not currently supported by this tool. You are probably using NOOBS, in which case your root filesystem is already expanded anyway." 20 60 2
    return 0
  fi

  LAST_PART_NUM=$(parted /dev/mmcblk0 -ms unit s p | tail -n 1 | cut -f 1 -d:)
  if [ $LAST_PART_NUM -ne $PART_NUM ]; then
    whiptail --msgbox "$ROOT_PART is not the last partition. Don't know how to expand" 20 60 2
    return 0
  fi

  # Get the starting offset of the root partition
  PART_START=$(parted /dev/mmcblk0 -ms unit s p | grep "^${PART_NUM}" | cut -f 2 -d: | sed 's/[^0-9]//g')
  [ "$PART_START" ] || return 1
  # Return value will likely be error for fdisk as it fails to reload the
  # partition table because the root fs is mounted
  fdisk /dev/mmcblk0 <<EOF
p
d
$PART_NUM
n
p
$PART_NUM
$PART_START

p
w
EOF
  ASK_TO_REBOOT=1

  # now set up an init.d script
cat <<EOF > /etc/init.d/resize2fs_once &&
#!/bin/sh
### BEGIN INIT INFO
# Provides:          resize2fs_once
# Required-Start:
# Required-Stop:
# Default-Start: 3
# Default-Stop:
# Short-Description: Resize the root filesystem to fill partition
# Description:
### END INIT INFO

. /lib/lsb/init-functions

case "\$1" in
  start)
    log_daemon_msg "Starting resize2fs_once" &&
    resize2fs /dev/$ROOT_PART &&
    update-rc.d resize2fs_once remove &&
    rm /etc/init.d/resize2fs_once &&
    log_end_msg \$?
    ;;
  *)
    echo "Usage: \$0 start" >&2
    exit 3
    ;;
esac
EOF
  chmod +x /etc/init.d/resize2fs_once &&
  update-rc.d resize2fs_once defaults
  # sn0wcrash's fix <3
  /bin/ln -s /etc/init.d/resize2fs_once /etc/rc2.d/S01resize2fs_once
  if [ "$INTERACTIVE" = True ]; then
    whiptail --msgbox "Root partition has been resized.\nThe filesystem will be enlarged upon the next reboot" 20 60 2
  fi
}

set_config_var() {
  lua - "$1" "$2" "$3" <<EOF > "$3.bak"
local key=assert(arg[1])
local value=assert(arg[2])
local fn=assert(arg[3])
local file=assert(io.open(fn))
local made_change=false
for line in file:lines() do
  if line:match("^#?%s*"..key.."=.*$") then
    line=key.."="..value
    made_change=true
  end
  print(line)
end

if not made_change then
  print(key.."="..value)
end
EOF
mv "$3.bak" "$3"
}

clear_config_var() {
  lua - "$1" "$2" <<EOF > "$2.bak"
local key=assert(arg[1])
local fn=assert(arg[2])
local file=assert(io.open(fn))
for line in file:lines() do
  if line:match("^%s*"..key.."=.*$") then
    line="#"..line
  end
  print(line)
end
EOF
mv "$2.bak" "$2"
}

get_config_var() {
  lua - "$1" "$2" <<EOF
local key=assert(arg[1])
local fn=assert(arg[2])
local file=assert(io.open(fn))
local found=false
for line in file:lines() do
  local val = line:match("^%s*"..key.."=(.*)$")
  if (val ~= nil) then
    print(val)
    found=true
    break
  end
end
if not found then
   print(0)
end
EOF
}

# $1 is 0 to disable overscan, 1 to disable it
set_overscan() {
  # Stop if /boot is not a mountpoint
  if ! mountpoint -q /boot; then
    return 1
  fi

  [ -e $CONFIG ] || touch $CONFIG

  if [ "$1" -eq 0 ]; then # disable overscan
    sed $CONFIG -i -e "s/^overscan_/#overscan_/"
    set_config_var disable_overscan 1 $CONFIG
  else # enable overscan
    set_config_var disable_overscan 0 $CONFIG
  fi
}

do_overscan() {
  if [ "$INTERACTIVE" = True ]; then
    whiptail --yesno "What would you like to do with overscan" 20 60 2 \
      --yes-button Disable --no-button Enable
    RET=$?
  else
    RET=$1
  fi
  if [ $RET -eq 0 ] || [ $RET -eq 1 ]; then
    ASK_TO_REBOOT=1
    set_overscan $RET;
  else
    return 1
  fi
}

do_change_pass() {
  whiptail --msgbox "You will now be asked to enter a new password for the pi user" 20 60 1
  passwd pi &&
  whiptail --msgbox "Password changed successfully" 20 60 1
}

do_configure_keyboard() {
  dpkg-reconfigure keyboard-configuration &&
  printf "Reloading keymap. This may take a short while\n" &&
  invoke-rc.d keyboard-setup start || return $?
  udevadm trigger --subsystem-match=input --action=change
  return 0
}

do_change_locale() {
  dpkg-reconfigure locales
}

do_change_timezone() {
  dpkg-reconfigure tzdata
}

do_configure_wifi_country() {
  oIFS="$IFS"
  if [ "$INTERACTIVE" = True ]; then
    IFS="/"
    value=$(cat /usr/share/zoneinfo/iso3166.tab | tail -n +26 | tr '\t' '/' | tr '\n' '/')
    COUNTRY=$(whiptail --menu "Select the country in which the Pi is to be used" 20 60 10 ${value} 3>&1 1>&2 2>&3)
  else
    COUNTRY=$1
    true
  fi
  if [ $? -eq 0 ];then
    if [ -e /etc/wpa_supplicant/wpa_supplicant.conf ]; then
        if grep -q "^country=" /etc/wpa_supplicant/wpa_supplicant.conf ; then
            sed -i "s/^country=.*/country=$COUNTRY/g" /etc/wpa_supplicant/wpa_supplicant.conf
        else
            sed -i "1i country=$COUNTRY" /etc/wpa_supplicant/wpa_supplicant.conf
        fi
    else
        echo "country=$COUNTRY" > /etc/wpa_supplicant/wpa_supplicant.conf
    fi
    if [ "$INTERACTIVE" = True ]; then
        whiptail --msgbox "Wi-fi country set to $COUNTRY" 20 60 1
    fi
    ASK_TO_REBOOT=1
  fi
  IFS=$oIFS
}

do_change_hostname() {
  if [ "$INTERACTIVE" = True ]; then
    whiptail --msgbox "\
Please note: RFCs mandate that a hostname's labels \
may contain only the ASCII letters 'a' through 'z' (case-insensitive), 
the digits '0' through '9', and the hyphen.
Hostname labels cannot begin or end with a hyphen. 
No other symbols, punctuation characters, or blank spaces are permitted.\
" 20 70 1
  fi
  CURRENT_HOSTNAME=`cat /etc/hostname | tr -d " \t\n\r"`
  if [ "$INTERACTIVE" = True ]; then
    NEW_HOSTNAME=$(whiptail --inputbox "Please enter a hostname" 20 60 "$CURRENT_HOSTNAME" 3>&1 1>&2 2>&3)
  else
    NEW_HOSTNAME=$1
    true
  fi
  if [ $? -eq 0 ]; then
    echo $NEW_HOSTNAME > /etc/hostname
    sed -i "s/127.0.1.1.*$CURRENT_HOSTNAME/127.0.1.1\t$NEW_HOSTNAME/g" /etc/hosts
    ASK_TO_REBOOT=1
  fi
}

do_memory_split() { # Memory Split
  if [ -e /boot/start_cd.elf ]; then
    # New-style memory split setting
    if ! mountpoint -q /boot; then
      return 1
    fi
    ## get current memory split from /boot/config.txt
    CUR_GPU_MEM=$(get_config_var gpu_mem $CONFIG)
    [ -z "$CUR_GPU_MEM" ] && CUR_GPU_MEM=64
    ## ask users what gpu_mem they want
    if [ "$INTERACTIVE" = True ]; then
      NEW_GPU_MEM=$(whiptail --inputbox "How much memory should the GPU have?  e.g. 16/32/64/128/256" \
        20 70 -- "$CUR_GPU_MEM" 3>&1 1>&2 2>&3)
    else
      NEW_GPU_MEM=$1
      true
    fi
    if [ $? -eq 0 ]; then
      set_config_var gpu_mem "$NEW_GPU_MEM" $CONFIG
      ASK_TO_REBOOT=1
    fi
  else # Old firmware so do start.elf renaming
    get_current_memory_split
    MEMSPLIT=$(whiptail --menu "Set memory split.\n$MEMSPLIT_DESCRIPTION" 20 60 10 \
      "240" "240MiB for ARM, 16MiB for VideoCore" \
      "224" "224MiB for ARM, 32MiB for VideoCore" \
      "192" "192MiB for ARM, 64MiB for VideoCore" \
      "128" "128MiB for ARM, 128MiB for VideoCore" \
      3>&1 1>&2 2>&3)
    if [ $? -eq 0 ]; then
      set_memory_split ${MEMSPLIT}
      ASK_TO_REBOOT=1
    fi
  fi
}

get_current_memory_split() {
  # Stop if /boot is not a mountpoint
  if ! mountpoint -q /boot; then
    return 1
  fi
  AVAILABLE_SPLITS="128 192 224 240"
  MEMSPLIT_DESCRIPTION=""
  for SPLIT in $AVAILABLE_SPLITS;do
    if [ -e /boot/arm${SPLIT}_start.elf ] && cmp /boot/arm${SPLIT}_start.elf /boot/start.elf >/dev/null 2>&1;then
      CURRENT_MEMSPLIT=$SPLIT
      MEMSPLIT_DESCRIPTION="Current: ${CURRENT_MEMSPLIT}MiB for ARM, $((256 - $CURRENT_MEMSPLIT))MiB for VideoCore"
      break
    fi
  done
}

set_memory_split() {
  cp -a /boot/arm${1}_start.elf /boot/start.elf
  sync
}

do_overclock() {
  if ! is_pione && ! is_pitwo; then
    whiptail --msgbox "This Pi cannot be overclocked." 20 60 2
    return 1
  fi
  if [ "$INTERACTIVE" = True ]; then
    whiptail --msgbox "\
Be aware that overclocking may reduce the lifetime of your
Raspberry Pi. If overclocking at a certain level causes
system instability, try a more modest overclock. Hold down
shift during boot to temporarily disable overclock.
See http://elinux.org/RPi_Overclocking for more information.\
" 20 70 1
   if is_pione; then
    OVERCLOCK=$(whiptail --menu "Choose overclock preset" 20 60 10 \
      "None" "700MHz ARM, 250MHz core, 400MHz SDRAM, 0 overvolt" \
      "Modest" "800MHz ARM, 250MHz core, 400MHz SDRAM, 0 overvolt" \
      "Medium" "900MHz ARM, 250MHz core, 450MHz SDRAM, 2 overvolt" \
      "High" "950MHz ARM, 250MHz core, 450MHz SDRAM, 6 overvolt" \
      "Turbo" "1000MHz ARM, 500MHz core, 600MHz SDRAM, 6 overvolt" \
      3>&1 1>&2 2>&3)
   elif is_pitwo; then
    OVERCLOCK=$(whiptail --menu "Choose overclock preset" 20 60 10 \
      "None" "900MHz ARM, 250MHz core, 450MHz SDRAM, 0 overvolt" \
      "High" "1000MHz ARM, 500MHz core, 500MHz SDRAM, 2 overvolt" \
      3>&1 1>&2 2>&3)
   fi
  else
    OVERCLOCK=$1
    true
  fi
  if [ $? -eq 0 ]; then
    case "$OVERCLOCK" in
      None)
        clear_overclock
        ;;
      Modest)
        set_overclock Modest 800 250 400 0
        ;;
      Medium)
        set_overclock Medium 900 250 450 2
        ;;
      High)
        if is_pione; then
          set_overclock High 950 250 450 6
        else
          set_overclock High 1000 500 500 2
        fi
        ;;
      Turbo)
        set_overclock Turbo 1000 500 600 6
        ;;
      *)
        whiptail --msgbox "Programmer error, unrecognised overclock preset" 20 60 2
        return 1
        ;;
    esac
    ASK_TO_REBOOT=1
  fi
}

set_overclock() {
  set_config_var arm_freq $2 $CONFIG &&
  set_config_var core_freq $3 $CONFIG &&
  set_config_var sdram_freq $4 $CONFIG &&
  set_config_var over_voltage $5 $CONFIG &&
  if [ "$INTERACTIVE" = True ]; then
    whiptail --msgbox "Set overclock to preset '$1'" 20 60 2
  fi
}

clear_overclock () {
  clear_config_var arm_freq $CONFIG &&
  clear_config_var core_freq $CONFIG &&
  clear_config_var sdram_freq $CONFIG &&
  clear_config_var over_voltage $CONFIG &&
  if [ "$INTERACTIVE" = True ]; then
    whiptail --msgbox "Set overclock to preset 'None'" 20 60 2
  fi
}

do_ssh() {
  if [ -e /var/log/regen_ssh_keys.log ] && ! grep -q "^finished" /var/log/regen_ssh_keys.log; then
    whiptail --msgbox "Initial ssh key generation still running. Please wait and try again." 20 60 2
    return 1
  fi
  if [ "$INTERACTIVE" = True ]; then
    whiptail --yesno "Would you like the SSH server enabled or disabled?" 20 60 2 \
      --yes-button Enable --no-button Disable
    RET=$?
  else
    RET=$1
  fi
  if [ $RET -eq 0 ]; then
    update-rc.d ssh enable &&
    invoke-rc.d ssh start &&
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "SSH server enabled" 20 60 1
    fi
  elif [ $RET -eq 1 ]; then
    update-rc.d ssh disable &&
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "SSH server disabled" 20 60 1
    fi
  else
    return $RET
  fi
}

do_devicetree() {
  CURRENT_SETTING="enabled" # assume not disabled
  DEFAULT=
  if [ -e $CONFIG ] && grep -q "^device_tree=$" $CONFIG; then
    CURRENT_SETTING="disabled"
    DEFAULT=--defaultno
  fi
  if [ "$INTERACTIVE" = True ]; then
    whiptail --yesno "Would you like the kernel to use Device Tree?" $DEFAULT 20 60 2
    RET=$?
  else
    RET=$1
  fi
  if [ $RET -eq 0 ]; then
    sed $CONFIG -i -e "s/^\(device_tree=\)$/#\1/"
    sed $CONFIG -i -e "s/^#\(device_tree=.\)/\1/"
    SETTING=enabled
  elif [ $RET -eq 1 ]; then
    sed $CONFIG -i -e "s/^#\(device_tree=\)$/\1/"
    sed $CONFIG -i -e "s/^\(device_tree=.\)/#\1/"
    if ! grep -q "^device_tree=$" $CONFIG; then
      printf "device_tree=\n" >> $CONFIG
    fi
    SETTING=disabled
  else
    return 0
  fi
  TENSE=is
  REBOOT=
  if [ $SETTING != $CURRENT_SETTING ]; then
    TENSE="will be"
    REBOOT=" after a reboot"
    ASK_TO_REBOOT=1
  fi
  whiptail --msgbox "Device Tree $TENSE $SETTING$REBOOT" 20 60 1
}

do_spi() {
  DEVICE_TREE="yes" # assume not disabled
  DEFAULT=
  if [ -e $CONFIG ] && grep -q "^device_tree=$" $CONFIG; then
    DEVICE_TREE="no"
  fi

  CURRENT_SETTING="off" # assume disabled
  DEFAULT=--defaultno
  if [ -e $CONFIG ] && grep -q -E "^(device_tree_param|dtparam)=([^,]*,)*spi(=(on|true|yes|1))?(,.*)?$" $CONFIG; then
    CURRENT_SETTING="on"
    DEFAULT=
  fi

  if [ $DEVICE_TREE = "yes" ]; then
    if [ "$INTERACTIVE" = True ]; then
      whiptail --yesno "Would you like the SPI interface to be enabled?" $DEFAULT 20 60 2
      RET=$?
    else
      RET=$1
    fi
    if [ $RET -eq 0 ]; then
      SETTING=on
      STATUS=enabled
    elif [ $RET -eq 1 ]; then
      SETTING=off
      STATUS=disabled
    else
      return 0
    fi
    TENSE=is
    REBOOT=
    if [ $SETTING != $CURRENT_SETTING ]; then
      TENSE="will be"
      REBOOT=" after a reboot"
      ASK_TO_REBOOT=1
    fi
    sed $CONFIG -i -r -e "s/^((device_tree_param|dtparam)=([^,]*,)*spi)(=[^,]*)?/\1=$SETTING/"
    if ! grep -q -E "^(device_tree_param|dtparam)=([^,]*,)*spi=[^,]*" $CONFIG; then
      printf "dtparam=spi=$SETTING\n" >> $CONFIG
    fi
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "The SPI interface $TENSE $STATUS$REBOOT" 20 60 1
    fi
    if [ $SETTING = "off" ]; then
      return 0
    fi
  fi

  CURRENT_STATUS="yes" # assume not blacklisted
  DEFAULT=
  if [ -e $BLACKLIST ] && grep -q "^blacklist[[:space:]]*spi[-_]bcm2708" $BLACKLIST; then
    CURRENT_STATUS="no"
    DEFAULT=--defaultno
  fi

  if ! [ -e $BLACKLIST ]; then
    touch $BLACKLIST
  fi

  if [ "$INTERACTIVE" = True ]; then
    whiptail --yesno "Would you like the SPI kernel module to be loaded by default?" $DEFAULT 20 60 2
    RET=$?
  else
    RET=$1
  fi
  if [ $RET -eq 0 ]; then
    sed $BLACKLIST -i -e "s/^\(blacklist[[:space:]]*spi[-_]bcm2708\)/#\1/"
    modprobe spi-bcm2708
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "SPI kernel module will now be loaded by default" 20 60 1
    fi
  elif [ $RET -eq 1 ]; then
    sed $BLACKLIST -i -e "s/^#\(blacklist[[:space:]]*spi[-_]bcm2708\)/\1/"
    if ! grep -q "^blacklist spi[-_]bcm2708" $BLACKLIST; then
      printf "blacklist spi-bcm2708\n" >> $BLACKLIST
    fi
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "SPI kernel module will no longer be loaded by default" 20 60 1
    fi
  else
    return 0
  fi
}

do_i2c() {
  DEVICE_TREE="yes" # assume not disabled
  DEFAULT=
  if [ -e $CONFIG ] && grep -q "^device_tree=$" $CONFIG; then
    DEVICE_TREE="no"
  fi

  CURRENT_SETTING="off" # assume disabled
  DEFAULT=--defaultno
  if [ -e $CONFIG ] && grep -q -E "^(device_tree_param|dtparam)=([^,]*,)*i2c(_arm)?(=(on|true|yes|1))?(,.*)?$" $CONFIG; then
    CURRENT_SETTING="on"
    DEFAULT=
  fi

  if [ $DEVICE_TREE = "yes" ]; then
    if [ "$INTERACTIVE" = True ]; then
      whiptail --yesno "Would you like the ARM I2C interface to be enabled?" $DEFAULT 20 60 2
      RET=$?
    else
      RET=$1
    fi
    if [ $RET -eq 0 ]; then
      SETTING=on
      STATUS=enabled
    elif [ $RET -eq 1 ]; then
      SETTING=off
      STATUS=disabled
    else
      return 0
    fi
    TENSE=is
    REBOOT=
    if [ $SETTING != $CURRENT_SETTING ]; then
      TENSE="will be"
      REBOOT=" after a reboot"
      ASK_TO_REBOOT=1
    fi
    sed $CONFIG -i -r -e "s/^((device_tree_param|dtparam)=([^,]*,)*i2c(_arm)?)(=[^,]*)?/\1=$SETTING/"
    if ! grep -q -E "^(device_tree_param|dtparam)=([^,]*,)*i2c(_arm)?=[^,]*" $CONFIG; then
      printf "dtparam=i2c_arm=$SETTING\n" >> $CONFIG
    fi
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "The ARM I2C interface $TENSE $STATUS$REBOOT" 20 60 1
    fi
    if [ $SETTING = "off" ]; then
      return 0
    fi
  fi

  CURRENT_STATUS="yes" # assume not blacklisted
  DEFAULT=
  if [ -e $BLACKLIST ] && grep -q "^blacklist[[:space:]]*i2c[-_]bcm2708" $BLACKLIST; then
    CURRENT_STATUS="no"
    DEFAULT=--defaultno
  fi

  if ! [ -e $BLACKLIST ]; then
    touch $BLACKLIST
  fi

  if [ "$INTERACTIVE" = True ]; then
    whiptail --yesno "Would you like the I2C kernel module to be loaded by default?" $DEFAULT 20 60 2
    RET=$?
  else
    RET=$1
  fi
  if [ $RET -eq 0 ]; then
    sed $BLACKLIST -i -e "s/^\(blacklist[[:space:]]*i2c[-_]bcm2708\)/#\1/"
    sed /etc/modules -i -e "s/^#[[:space:]]*\(i2c[-_]dev\)/\1/"
    if ! grep -q "^i2c[-_]dev" /etc/modules; then
      printf "i2c-dev\n" >> /etc/modules
    fi
    modprobe i2c-bcm2708
    modprobe i2c-dev
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "I2C kernel module will now be loaded by default" 20 60 1
    fi
  elif [ $RET -eq 1 ]; then
    sed $BLACKLIST -i -e "s/^#\(blacklist[[:space:]]*i2c[-_]bcm2708\)/\1/"
    if ! grep -q "^blacklist i2c[-_]bcm2708" $BLACKLIST; then
      printf "blacklist i2c-bcm2708\n" >> $BLACKLIST
    fi
    sed /etc/modules -i -e "s/^\(i2c[-_]dev\)/#\1/"
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "I2C kernel module will no longer be loaded by default" 20 60 1
    fi
  else
    return 0
  fi
}

do_serial() {
  DEFAULT=
  if ! grep -q "console=ttyAMA0" /boot/cmdline.txt && ! grep -q "console=serial0" /boot/cmdline.txt ; then
      DEFAULT=--defaultno
  fi

  if [ "$INTERACTIVE" = True ]; then
    whiptail --yesno "Would you like a login shell to be accessible over serial?" $DEFAULT 20 60 2
    RET=$?
  else
    get_init_sys
    RET=$1
  fi
  if [ $RET -eq 1 ]; then
    if [ $SYSTEMD -eq 0 ]; then
      sed -i /etc/inittab -e "s|^.*:.*:respawn:.*ttyAMA0|#&|"
    fi
    sed -i /boot/cmdline.txt -e "s/console=ttyAMA0,[0-9]\+ //"
    sed -i /boot/cmdline.txt -e "s/console=serial0,[0-9]\+ //"
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "Serial is now disabled" 20 60 1
    fi
  elif [ $RET -eq 0 ]; then
    if [ $SYSTEMD -eq 0 ]; then
      sed -i /etc/inittab -e "s|^#\(.*:.*:respawn:.*ttyAMA0\)|\1|"
      if ! grep -q "^T.*:.*:respawn:.*ttyAMA0" /etc/inittab; then
        printf "T0:23:respawn:/sbin/getty -L ttyAMA0 115200 vt100\n" >> /etc/inittab
      fi
    fi
    if grep -q "console=ttyAMA0" /boot/cmdline.txt ; then
      if [ -e /proc/device-tree/aliases/serial0 ]; then
        sed -i /boot/cmdline.txt -e "s/console=ttyAMA0/console=serial0/"
      fi
    elif ! grep -q "console=ttyAMA0" /boot/cmdline.txt && ! grep -q "console=serial0" /boot/cmdline.txt ; then
      if [ -e /proc/device-tree/aliases/serial0 ]; then
        sed -i /boot/cmdline.txt -e "s/root=/console=serial0,115200 root=/"
      else
        sed -i /boot/cmdline.txt -e "s/root=/console=ttyAMA0,115200 root=/"
      fi
    fi
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "Serial is now enabled" 20 60 1
    fi
  else
    return $RET
  fi
  ASK_TO_REBOOT=1
}

disable_raspi_config_at_boot() {
  if [ -e /etc/profile.d/raspi-config.sh ]; then
    rm -f /etc/profile.d/raspi-config.sh
    if [ $SYSTEMD -eq 1 ]; then
      if [ -e /etc/systemd/system/getty@tty1.service.d/raspi-config-override.conf ]; then
        rm /etc/systemd/system/getty@tty1.service.d/raspi-config-override.conf
      fi
    else
      sed -i /etc/inittab \
        -e "s/^#\(.*\)#\s*RPICFG_TO_ENABLE\s*/\1/" \
        -e "/#\s*RPICFG_TO_DISABLE/d"
    fi
    telinit q
  fi
}

do_boot_behaviour_new() {
  if [ "$INTERACTIVE" = True ]; then
    BOOTOPT=$(whiptail --title "Raspberry Pi Software Configuration Tool (raspi-config)" --menu "Boot Options" $WT_HEIGHT $WT_WIDTH $WT_MENU_HEIGHT \
      "B1 Console" "Text console, requiring user to login" \
      "B2 Console Autologin" "Text console, automatically logged in as 'pi' user" \
      "B3 Desktop" "Desktop GUI, requiring user to login" \
      "B4 Desktop Autologin" "Desktop GUI, automatically logged in as 'pi' user" \
      3>&1 1>&2 2>&3)
  else
    get_init_sys
    BOOTOPT=$1
    true
  fi
  if [ $? -eq 0 ]; then
    case "$BOOTOPT" in
      B1*)
        if [ $SYSTEMD -eq 1 ]; then
          systemctl set-default multi-user.target
          ln -fs /lib/systemd/system/getty@.service /etc/systemd/system/getty.target.wants/getty@tty1.service
        else
          [ -e /etc/init.d/lightdm ] && update-rc.d lightdm disable 2
          sed /etc/inittab -i -e "s/1:2345:respawn:\/bin\/login -f pi tty1 <\/dev\/tty1 >\/dev\/tty1 2>&1/1:2345:respawn:\/sbin\/getty --noclear 38400 tty1/"
        fi
        ;;
      B2*)
        if [ $SYSTEMD -eq 1 ]; then
          systemctl set-default multi-user.target
          ln -fs /etc/systemd/system/autologin@.service /etc/systemd/system/getty.target.wants/getty@tty1.service
        else
          [ -e /etc/init.d/lightdm ] && update-rc.d lightdm disable 2
          sed /etc/inittab -i -e "s/1:2345:respawn:\/sbin\/getty --noclear 38400 tty1/1:2345:respawn:\/bin\/login -f pi tty1 <\/dev\/tty1 >\/dev\/tty1 2>&1/"
        fi
        ;;
      B3*)
        if [ -e /etc/init.d/lightdm ]; then
          if [ $SYSTEMD -eq 1 ]; then
            systemctl set-default graphical.target
            ln -fs /lib/systemd/system/getty@.service /etc/systemd/system/getty.target.wants/getty@tty1.service
          else
            update-rc.d lightdm enable 2
          fi
          sed /etc/lightdm/lightdm.conf -i -e "s/^autologin-user=pi/#autologin-user=/"
          disable_raspi_config_at_boot
        else
          whiptail --msgbox "Do sudo apt-get install lightdm to allow configuration of boot to desktop" 20 60 2
          return 1
        fi
        ;;
      B4*)
        if [ -e /etc/init.d/lightdm ]; then
          if id -u pi > /dev/null 2>&1; then
            if [ $SYSTEMD -eq 1 ]; then
              systemctl set-default graphical.target
              ln -fs /etc/systemd/system/autologin@.service /etc/systemd/system/getty.target.wants/getty@tty1.service
            else
              update-rc.d lightdm enable 2
            fi
            sed /etc/lightdm/lightdm.conf -i -e "s/^#autologin-user=.*/autologin-user=pi/"
            disable_raspi_config_at_boot
          else
            whiptail --msgbox "The pi user has been removed, can't set up boot to desktop" 20 60 2
          fi
        else
          whiptail --msgbox "Do sudo apt-get install lightdm to allow configuration of boot to desktop" 20 60 2
          return 1
        fi
        ;;
      *)
        whiptail --msgbox "Programmer error, unrecognised boot option" 20 60 2
        return 1
        ;;
    esac
    ASK_TO_REBOOT=1
  fi
}

do_wait_for_network() {
  get_init_sys
  if [ $SYSTEMD -eq 0 ]; then
    whiptail --msgbox "This option can only be selected when using systemd" 20 60 2
    return 1
  fi
  if [ "$INTERACTIVE" = True ]; then
    RET=$(whiptail --menu "Choose boot option" 20 70 10 \
      "Fast" "Boot without waiting for network connection" \
      "Slow" "Wait for network connection before completing boot" \
      3>&1 1>&2 2>&3)
  else
    get_init_sys
    RET=$1
    true
  fi
  if [ $? -eq 0 ]; then
    case "$RET" in
      Fast)
        rm -f /etc/systemd/system/dhcpcd.service.d/wait.conf
        ;;
      Slow)
        mkdir -p /etc/systemd/system/dhcpcd.service.d/
        cat > /etc/systemd/system/dhcpcd.service.d/wait.conf << EOF
[Service]
ExecStart=
ExecStart=/sbin/dhcpcd -q -w
EOF
        ;;
      *)
        whiptail --msgbox "Programmer error, unrecognised option" 20 60 2
        return 1
        ;;
    esac
  fi
}

do_boot_behaviour() {
  if [ "$INTERACTIVE" = True ]; then
    BOOTOPT=$(whiptail --menu "Choose boot option" 20 60 10 \
      "Console" "Text console, requiring login (default)" \
      "Desktop" "Log in as user 'pi' at the graphical desktop" \
      3>&1 1>&2 2>&3)
  else
    get_init_sys
    BOOTOPT=$1
    true
  fi
  if [ $? -eq 0 ]; then
    case "$BOOTOPT" in
      Console)
        if [ -e /etc/init.d/lightdm ]; then
          if [ $SYSTEMD -eq 1 ]; then
            systemctl set-default multi-user.target
          else
            update-rc.d lightdm disable 2
          fi
        fi
        ;;
      Desktop)
        if [ -e /etc/init.d/lightdm ]; then
          if id -u pi > /dev/null 2>&1; then
            if [ $SYSTEMD -eq 1 ]; then
              systemctl set-default graphical.target
            else
              update-rc.d lightdm enable 2
            fi
            sed /etc/lightdm/lightdm.conf -i -e "s/^#autologin-user=.*/autologin-user=pi/"
            disable_raspi_config_at_boot
          else
            whiptail --msgbox "The pi user has been removed, can't set up boot to desktop" 20 60 2
          fi
        else
          whiptail --msgbox "Do sudo apt-get install lightdm to allow configuration of boot to desktop" 20 60 2
          return 1
        fi
        ;;
      *)
        whiptail --msgbox "Programmer error, unrecognised boot option" 20 60 2
        return 1
        ;;
    esac
    ASK_TO_REBOOT=1
  fi
}

do_rastrack() {
  whiptail --msgbox "\
Rastrack (http://rastrack.co.uk) is a website run by Ryan Walmsley
for tracking where people are using Raspberry Pis around the world.
If you have an internet connection, you can add yourself directly
using this tool. This is just a bit of fun, not any sort of official
registration.\
" 20 70 1
  if [ $? -ne 0 ]; then
    return 0;
  fi
  UNAME=$(whiptail --inputbox "Username / Nickname For Rastrack Addition" 20 70 3>&1 1>&2 2>&3)
  if [ $? -ne 0 ]; then
    return 1;
  fi
  EMAIL=$(whiptail --inputbox "Email Address For Rastrack Addition" 20 70 3>&1 1>&2 2>&3)
  if [ $? -ne 0 ]; then
    return 1;
  fi
  curl --data "name=$UNAME&email=$EMAIL" http://rastrack.co.uk/api.php
  printf "Hit enter to continue\n"
  read TMP
}

# $1 is 0 to disable camera, 1 to enable it
set_camera() {
  # Stop if /boot is not a mountpoint
  if ! mountpoint -q /boot; then
    return 1
  fi

  [ -e $CONFIG ] || touch $CONFIG

  if [ "$1" -eq 0 ]; then # disable camera
    set_config_var start_x 0 $CONFIG
    sed $CONFIG -i -e "s/^startx/#startx/"
    sed $CONFIG -i -e "s/^start_file/#start_file/"
    sed $CONFIG -i -e "s/^fixup_file/#fixup_file/"
  else # enable camera
    set_config_var start_x 1 $CONFIG
    CUR_GPU_MEM=$(get_config_var gpu_mem $CONFIG)
    if [ -z "$CUR_GPU_MEM" ] || [ "$CUR_GPU_MEM" -lt 128 ]; then
      set_config_var gpu_mem 128 $CONFIG
    fi
    sed $CONFIG -i -e "s/^startx/#startx/"
    sed $CONFIG -i -e "s/^fixup_file/#fixup_file/"
  fi
}

do_camera() {
  if [ ! -e /boot/start_x.elf ]; then
    whiptail --msgbox "Your firmware appears to be out of date (no start_x.elf). Please update" 20 60 2
    return 1
  fi
  if [ "$INTERACTIVE" = True ]; then
    whiptail --yesno "Enable support for Raspberry Pi camera?" 20 60 2 \
      --yes-button Disable --no-button Enable
    RET=$?
  else
    RET=$1
  fi
  if [ $RET -eq 0 ] || [ $RET -eq 1 ]; then
    ASK_TO_REBOOT=1
    set_camera $RET;
  else
    return 1
  fi
}

# $1 is 1 to disable interface, 0 to enable it
set_onewire() {
  [ -e $CONFIG ] || touch $CONFIG
  if [ "$1" -eq 1 ]; then # disable driver
    sed $CONFIG -i -e "s/^dtoverlay=w1-gpio/#dtoverlay=w1-gpio/"
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "One-wire interface is disabled" 20 60 1
    fi
  else # enable driver
    sed $CONFIG -i -e "s/^#dtoverlay=w1-gpio/dtoverlay=w1-gpio/"
    if ! grep -q -E "^dtoverlay=w1-gpio" $CONFIG; then
      printf "dtoverlay=w1-gpio\n" >> $CONFIG
    fi
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "One-wire interface is enabled" 20 60 1
    fi
  fi
}

do_onewire() {
  if [ "$INTERACTIVE" = True ]; then
    whiptail --yesno "Enable one-wire interface?" 20 60 2 \
      --yes-button Enable --no-button Disable
    RET=$?
  else
    RET=$1
  fi
  if [ $RET -eq 0 ] || [ $RET -eq 1 ]; then
    ASK_TO_REBOOT=1
    set_onewire $RET;
  else
    return 1
  fi
}

# $1 is 0 to disable driver, 1 to enable it
set_gldriver() {
  [ -e $CONFIG ] || touch $CONFIG

  if [ "$1" -eq 0 ]; then # disable driver
    sed $CONFIG -i -e "s/^dtoverlay=vc4-kms-v3d/#dtoverlay=vc4-kms-v3d/"
    rm /etc/xdg/autostart/xcompmgr.desktop
    mv /usr/share/X11/xorg.conf.d/99-fbturbo.~ /usr/share/X11/xorg.conf.d/99-fbturbo.conf
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "Desktop GL driver is disabled" 20 60 1
    fi
  else # enable driver
    sed $CONFIG -i -e "s/^#dtoverlay=vc4-kms-v3d/dtoverlay=vc4-kms-v3d/"
    if ! grep -q -E "^dtoverlay=vc4-kms-v3d" $CONFIG; then
      printf "dtoverlay=vc4-kms-v3d\n" >> $CONFIG
    fi
    cat <<EOF >/etc/xdg/autostart/xcompmgr.desktop
[Desktop Entry]
Type=Application
Name=xcompmgr
Comment=Start simple compositor
NoDisplay=true
Exec=xcompmgr -a
EOF
    mv /usr/share/X11/xorg.conf.d/99-fbturbo.conf /usr/share/X11/xorg.conf.d/99-fbturbo.~
    sed $CONFIG -i -e "s/^gpu_mem/#gpu_mem/"
    if [ "$INTERACTIVE" = True ]; then
      whiptail --msgbox "Desktop GL driver is enabled" 20 60 1
    fi
  fi
}

do_gldriver() {
  if is_pione || is_pizero; then
    whiptail --msgbox "GL driver cannot be used on Pi 1 or Pi 0" 20 60 2
    return 1
  fi
  if [ ! -e /boot/overlays/vc4-kms-v3d-overlay.dtb ]; then
    whiptail --msgbox "Driver and kernel not present on your system. Please update" 20 60 2
    return 1
  fi
  if [ $(dpkg -l libgl1-mesa-dri | tail -n 1 | cut -d ' ' -f 1) != "ii" ]; then
    whiptail --msgbox "libgl1-mesa-dri not found - please install" 20 60 2
    return 1
  fi
  if [ ! -e /usr/bin/xcompmgr ]; then
    whiptail --msgbox "xcompmgr not found - please install" 20 60 2
    return 1
  fi
  if [ "$INTERACTIVE" = True ]; then
    whiptail --yesno "Enable experimental GL driver for desktop?" 20 60 2 \
      --yes-button Disable --no-button Enable
    RET=$?
  else
    RET=$1
  fi
  if [ $RET -eq 0 ] || [ $RET -eq 1 ]; then
    ASK_TO_REBOOT=1
    set_gldriver $RET;
  else
    return 1
  fi
}

do_update() {
  apt-get update &&
  apt-get install raspi-config &&
  printf "Sleeping 5 seconds before reloading raspi-config\n" &&
  sleep 5 &&
  exec raspi-config
}

do_audio() {
  AUDIO_OUT=$(whiptail --menu "Choose the audio output" 20 60 10 \
    "0" "Auto" \
    "1" "Force 3.5mm ('headphone') jack" \
    "2" "Force HDMI" \
    3>&1 1>&2 2>&3)
  if [ $? -eq 0 ]; then
    amixer cset numid=3 "$AUDIO_OUT"
  fi
}

do_finish() {
  disable_raspi_config_at_boot
  if [ $ASK_TO_REBOOT -eq 1 ]; then
    whiptail --yesno "Would you like to reboot now?" 20 60 2
    if [ $? -eq 0 ]; then # yes
      sync
      reboot
    fi
  fi
  exit 0
}

# $1 = filename, $2 = key name
get_json_string_val() {
  sed -n -e "s/^[[:space:]]*\"$2\"[[:space:]]*:[[:space:]]*\"\(.*\)\"[[:space:]]*,$/\1/p" $1
}

# TODO: This is probably broken
do_apply_os_config() {
  [ -e /boot/os_config.json ] || return 0
  NOOBSFLAVOUR=$(get_json_string_val /boot/os_config.json flavour)
  NOOBSLANGUAGE=$(get_json_string_val /boot/os_config.json language)
  NOOBSKEYBOARD=$(get_json_string_val /boot/os_config.json keyboard)

  if [ -n "$NOOBSFLAVOUR" ]; then
    printf "Setting flavour to %s based on os_config.json from NOOBS. May take a while\n" "$NOOBSFLAVOUR"

    printf "Unrecognised flavour. Ignoring\n"
  fi

  # TODO: currently ignores en_gb settings as we assume we are running in a 
  # first boot context, where UK English settings are default
  case "$NOOBSLANGUAGE" in
    "en")
      if [ "$NOOBSKEYBOARD" = "gb" ]; then
        DEBLANGUAGE="" # UK english is the default, so ignore
      else
        DEBLANGUAGE="en_US.UTF-8"
      fi
      ;;
    "de")
      DEBLANGUAGE="de_DE.UTF-8"
      ;;
    "fi")
      DEBLANGUAGE="fi_FI.UTF-8"
      ;;
    "fr")
      DEBLANGUAGE="fr_FR.UTF-8"
      ;;
    "hu")
      DEBLANGUAGE="hu_HU.UTF-8"
      ;;
    "ja")
      DEBLANGUAGE="ja_JP.UTF-8"
      ;;
    "nl")
      DEBLANGUAGE="nl_NL.UTF-8"
      ;;
    "pt")
      DEBLANGUAGE="pt_PT.UTF-8"
      ;;
    "ru")
      DEBLANGUAGE="ru_RU.UTF-8"
      ;;
    "zh_CN")
      DEBLANGUAGE="zh_CN.UTF-8"
      ;;
    *)
      printf "Language '%s' not handled currently. Run sudo raspi-config to set up" "$NOOBSLANGUAGE"
      ;;
  esac

  if [ -n "$DEBLANGUAGE" ]; then
    printf "Setting language to %s based on os_config.json from NOOBS. May take a while\n" "$DEBLANGUAGE"
    cat << EOF | debconf-set-selections
locales   locales/locales_to_be_generated multiselect     $DEBLANGUAGE UTF-8
EOF
    rm /etc/locale.gen
    dpkg-reconfigure -f noninteractive locales
    update-locale LANG="$DEBLANGUAGE"
    cat << EOF | debconf-set-selections
locales   locales/default_environment_locale select       $DEBLANGUAGE
EOF
  fi

  if [ -n "$NOOBSKEYBOARD" -a "$NOOBSKEYBOARD" != "gb" ]; then
    printf "Setting keyboard layout to %s based on os_config.json from NOOBS. May take a while\n" "$NOOBSKEYBOARD"
    sed -i /etc/default/keyboard -e "s/^XKBLAYOUT.*/XKBLAYOUT=\"$NOOBSKEYBOARD\"/"
    dpkg-reconfigure -f noninteractive keyboard-configuration
    invoke-rc.d keyboard-setup start
  fi
  return 0
}

nonint() {
    $*
}

#
# Command line options for non-interactive use
#
for i in $*
do
  case $i in
  --memory-split)
    OPT_MEMORY_SPLIT=GET
    printf "Not currently supported\n"
    exit 1
    ;;
  --memory-split=*)
    OPT_MEMORY_SPLIT=`echo $i | sed 's/[-a-zA-Z0-9]*=//'`
    printf "Not currently supported\n"
    exit 1
    ;;
  --expand-rootfs)
    INTERACTIVE=False
    do_expand_rootfs
    printf "Please reboot\n"
    exit 0
    ;;
  --apply-os-config)
    INTERACTIVE=False
    do_apply_os_config
    exit $?
    ;;
  nonint)
    INTERACTIVE=False
    $@
    ;;
  *)
    # unknown option
    ;;
  esac
done

#if [ "GET" = "${OPT_MEMORY_SPLIT:-}" ]; then
#  set -u # Fail on unset variables
#  get_current_memory_split
#  echo $CURRENT_MEMSPLIT
#  exit 0
#fi

# Everything else needs to be run as root
if [ $(id -u) -ne 0 ]; then
  printf "Script must be run as root. Try 'sudo raspi-config'\n"
  exit 1
fi

if [ -n "${OPT_MEMORY_SPLIT:-}" ]; then
  set -e # Fail when a command errors
  set_memory_split "${OPT_MEMORY_SPLIT}"
  exit 0
fi

do_internationalisation_menu() {
  FUN=$(whiptail --title "Raspberry Pi Software Configuration Tool (raspi-config)" --menu "Internationalisation Options" $WT_HEIGHT $WT_WIDTH $WT_MENU_HEIGHT --cancel-button Back --ok-button Select \
    "I1 Change Locale" "Set up language and regional settings to match your location" \
    "I2 Change Timezone" "Set up timezone to match your location" \
    "I3 Change Keyboard Layout" "Set the keyboard layout to match your keyboard" \
    "I4 Change Wi-fi Country" "Set the legal channels used in your country" \
    3>&1 1>&2 2>&3)
  RET=$?
  if [ $RET -eq 1 ]; then
    return 0
  elif [ $RET -eq 0 ]; then
    case "$FUN" in
      I1\ *) do_change_locale ;;
      I2\ *) do_change_timezone ;;
      I3\ *) do_configure_keyboard ;;
      I4\ *) do_configure_wifi_country ;;
      *) whiptail --msgbox "Programmer error: unrecognized option" 20 60 1 ;;
    esac || whiptail --msgbox "There was an error running option $FUN" 20 60 1
  fi
}

do_advanced_menu() {
  FUN=$(whiptail --title "Raspberry Pi Software Configuration Tool (raspi-config)" --menu "Advanced Options" $WT_HEIGHT $WT_WIDTH $WT_MENU_HEIGHT --cancel-button Back --ok-button Select \
    "A1 Overscan" "You may need to configure overscan if black bars are present on display" \
    "A2 Hostname" "Set the visible name for this Pi on a network" \
    "A3 Memory Split" "Change the amount of memory made available to the GPU" \
    "A4 SSH" "Enable/Disable remote command line access to your Pi using SSH" \
    "A5 Device Tree" "Enable/Disable the use of Device Tree" \
    "A6 SPI" "Enable/Disable automatic loading of SPI kernel module (needed for e.g. PiFace)" \
    "A7 I2C" "Enable/Disable automatic loading of I2C kernel module" \
    "A8 Serial" "Enable/Disable shell and kernel messages on the serial connection" \
    "A9 Audio" "Force audio out through HDMI or 3.5mm jack" \
    "AA GL Driver" "Enable/Disable experimental desktop GL driver" \
    "AB 1-Wire" "Enable/Disable one-wire interface" \
    "A0 Update" "Update this tool to the latest version" \
    3>&1 1>&2 2>&3)
  RET=$?
  if [ $RET -eq 1 ]; then
    return 0
  elif [ $RET -eq 0 ]; then
    case "$FUN" in
      A1\ *) do_overscan ;;
      A2\ *) do_change_hostname ;;
      A3\ *) do_memory_split ;;
      A4\ *) do_ssh ;;
      A5\ *) do_devicetree ;;
      A6\ *) do_spi ;;
      A7\ *) do_i2c ;;
      A8\ *) do_serial ;;
      A9\ *) do_audio ;;
      AA\ *) do_gldriver ;;
      AB\ *) do_onewire ;;
      A0\ *) do_update ;;
      *) whiptail --msgbox "Programmer error: unrecognized option" 20 60 1 ;;
    esac || whiptail --msgbox "There was an error running option $FUN" 20 60 1
  fi
}


#
# Interactive use loop
#
if [ "$INTERACTIVE" = True ]; then
  get_init_sys
  calc_wt_size
  while true; do
    FUN=$(whiptail --title "Raspberry Pi Software Configuration Tool (raspi-config)" --menu "Setup Options" $WT_HEIGHT $WT_WIDTH $WT_MENU_HEIGHT --cancel-button Finish --ok-button Select \
      "1 Expand Filesystem" "Ensures that all of the SD card storage is available to the OS" \
      "2 Change User Password" "Change password for the default user (pi)" \
      "3 Boot Options" "Choose whether to boot into a desktop environment or the command line" \
      "4 Wait for Network at Boot" "Choose whether to wait for network connection during boot" \
      "5 Internationalisation Options" "Set up language and regional settings to match your location" \
      "6 Enable Camera" "Enable this Pi to work with the Raspberry Pi Camera" \
      "7 Add to Rastrack" "Add this Pi to the online Raspberry Pi Map (Rastrack)" \
      "8 Overclock" "Configure overclocking for your Pi" \
      "9 Advanced Options" "Configure advanced settings" \
      "0 About raspi-config" "Information about this configuration tool" \
      3>&1 1>&2 2>&3)
    RET=$?
    if [ $RET -eq 1 ]; then
      do_finish
    elif [ $RET -eq 0 ]; then
      case "$FUN" in
        1\ *) do_expand_rootfs ;;
        2\ *) do_change_pass ;;
        3\ *) do_boot_behaviour_new ;;
        4\ *) do_wait_for_network ;;
        5\ *) do_internationalisation_menu ;;
        6\ *) do_camera ;;
        7\ *) do_rastrack ;;
        8\ *) do_overclock ;;
        9\ *) do_advanced_menu ;;
        0\ *) do_about ;;
        *) whiptail --msgbox "Programmer error: unrecognized option" 20 60 1 ;;
      esac || whiptail --msgbox "There was an error running option $FUN" 20 60 1
    else
      exit 1
    fi
  done
fi
