
            
(kicad_pcb (version 20171130) (host pcbnew 5.1.6)

  (page A3)
  (title_block
    (title corney_island_wireless)
    (rev 0.2)
    (company ceoloide)
  )

  (general
    (thickness 1.6)
  )

  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

            (net 0 "")
(net 1 "C0")
(net 2 "outer_bottom")
(net 3 "outer_home")
(net 4 "outer_top")
(net 5 "C1")
(net 6 "pinky_bottom")
(net 7 "pinky_home")
(net 8 "pinky_top")
(net 9 "C2")
(net 10 "ring_bottom")
(net 11 "ring_home")
(net 12 "ring_top")
(net 13 "C3")
(net 14 "middle_bottom")
(net 15 "middle_home")
(net 16 "middle_top")
(net 17 "C4")
(net 18 "index_bottom")
(net 19 "index_home")
(net 20 "index_top")
(net 21 "C5")
(net 22 "inner_bottom")
(net 23 "inner_home")
(net 24 "inner_top")
(net 25 "near_home")
(net 26 "mid_home")
(net 27 "far_home")
(net 28 "R2")
(net 29 "R1")
(net 30 "R0")
(net 31 "R3")
(net 32 "RAW")
(net 33 "GND")
(net 34 "RST")
(net 35 "VCC")
(net 36 "P16")
(net 37 "P10")
(net 38 "LED")
(net 39 "DAT")
(net 40 "SDA")
(net 41 "SCL")
(net 42 "CS")
(net 43 "P9")
(net 44 "MCU1_24")
(net 45 "MCU1_1")
(net 46 "MCU1_23")
(net 47 "MCU1_2")
(net 48 "MCU1_22")
(net 49 "MCU1_3")
(net 50 "MCU1_21")
(net 51 "MCU1_4")
(net 52 "MCU1_20")
(net 53 "MCU1_5")
(net 54 "MCU1_19")
(net 55 "MCU1_6")
(net 56 "MCU1_18")
(net 57 "MCU1_7")
(net 58 "MCU1_17")
(net 59 "MCU1_8")
(net 60 "MCU1_16")
(net 61 "MCU1_9")
(net 62 "MCU1_15")
(net 63 "MCU1_10")
(net 64 "MCU1_14")
(net 65 "MCU1_11")
(net 66 "MCU1_13")
(net 67 "MCU1_12")
(net 68 "DISP1_1")
(net 69 "DISP1_2")
(net 70 "DISP1_4")
(net 71 "DISP1_5")
(net 72 "BAT_P")
(net 73 "JST1_1")
(net 74 "JST1_2")
            
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "")
(add_net "C0")
(add_net "outer_bottom")
(add_net "outer_home")
(add_net "outer_top")
(add_net "C1")
(add_net "pinky_bottom")
(add_net "pinky_home")
(add_net "pinky_top")
(add_net "C2")
(add_net "ring_bottom")
(add_net "ring_home")
(add_net "ring_top")
(add_net "C3")
(add_net "middle_bottom")
(add_net "middle_home")
(add_net "middle_top")
(add_net "C4")
(add_net "index_bottom")
(add_net "index_home")
(add_net "index_top")
(add_net "C5")
(add_net "inner_bottom")
(add_net "inner_home")
(add_net "inner_top")
(add_net "near_home")
(add_net "mid_home")
(add_net "far_home")
(add_net "R2")
(add_net "R1")
(add_net "R0")
(add_net "R3")
(add_net "RAW")
(add_net "GND")
(add_net "RST")
(add_net "VCC")
(add_net "P16")
(add_net "P10")
(add_net "LED")
(add_net "DAT")
(add_net "SDA")
(add_net "SCL")
(add_net "CS")
(add_net "P9")
(add_net "MCU1_24")
(add_net "MCU1_1")
(add_net "MCU1_23")
(add_net "MCU1_2")
(add_net "MCU1_22")
(add_net "MCU1_3")
(add_net "MCU1_21")
(add_net "MCU1_4")
(add_net "MCU1_20")
(add_net "MCU1_5")
(add_net "MCU1_19")
(add_net "MCU1_6")
(add_net "MCU1_18")
(add_net "MCU1_7")
(add_net "MCU1_17")
(add_net "MCU1_8")
(add_net "MCU1_16")
(add_net "MCU1_9")
(add_net "MCU1_15")
(add_net "MCU1_10")
(add_net "MCU1_14")
(add_net "MCU1_11")
(add_net "MCU1_13")
(add_net "MCU1_12")
(add_net "DISP1_1")
(add_net "DISP1_2")
(add_net "DISP1_4")
(add_net "DISP1_5")
(add_net "BAT_P")
(add_net "JST1_1")
(add_net "JST1_2")
  )

            
  (module "ceoloide:mounting_hole_npth" (layer F.Cu) (tedit 5F1B9159)
      (at 207.762 100.476 0)
      (fp_text reference "MH1" (at 0 2.55 0) (layer F.SilkS) hide (effects (font (size 1 1) (thickness 0.15))))
      (pad "" np_thru_hole circle (at 0 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  

  (module "ceoloide:mounting_hole_npth" (layer F.Cu) (tedit 5F1B9159)
      (at 222.194 108.995 0)
      (fp_text reference "MH2" (at 0 2.55 0) (layer F.SilkS) hide (effects (font (size 1 1) (thickness 0.15))))
      (pad "" np_thru_hole circle (at 0 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  

  (module "ceoloide:mounting_hole_npth" (layer F.Cu) (tedit 5F1B9159)
      (at 109.5 71.5 0)
      (fp_text reference "MH3" (at 0 2.55 0) (layer F.SilkS) hide (effects (font (size 1 1) (thickness 0.15))))
      (pad "" np_thru_hole circle (at 0 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  

  (module "ceoloide:mounting_hole_npth" (layer F.Cu) (tedit 5F1B9159)
      (at 109.5 90.5 0)
      (fp_text reference "MH4" (at 0 2.55 0) (layer F.SilkS) hide (effects (font (size 1 1) (thickness 0.15))))
      (pad "" np_thru_hole circle (at 0 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  

  (module "ceoloide:mounting_hole_npth" (layer F.Cu) (tedit 5F1B9159)
      (at 185.468 67.986 0)
      (fp_text reference "MH5" (at 0 2.55 0) (layer F.SilkS) hide (effects (font (size 1 1) (thickness 0.15))))
      (pad "" np_thru_hole circle (at 0 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  

  (module "ceoloide:mounting_hole_npth" (layer F.Cu) (tedit 5F1B9159)
      (at 152.657 107.74 0)
      (fp_text reference "MH6" (at 0 2.55 0) (layer F.SilkS) hide (effects (font (size 1 1) (thickness 0.15))))
      (pad "" np_thru_hole circle (at 0 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  

  (module "ceoloide:mounting_hole_npth" (layer F.Cu) (tedit 5F1B9159)
      (at 199.2410516 115.3236576 60)
      (fp_text reference "MH7" (at 0 2.55 60) (layer F.SilkS) hide (effects (font (size 1 1) (thickness 0.15))))
      (pad "" np_thru_hole circle (at 0 0 60) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 100 100 0)

      
      (fp_text reference "S1" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 1 "C0"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 2 "outer_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 1 "C0"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 2 "outer_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 100 81 0)

      
      (fp_text reference "S2" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 1 "C0"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 3 "outer_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 1 "C0"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 3 "outer_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 100 62 0)

      
      (fp_text reference "S3" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 1 "C0"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 4 "outer_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 1 "C0"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 4 "outer_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 119 100 0)

      
      (fp_text reference "S4" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 5 "C1"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 6 "pinky_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 5 "C1"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 6 "pinky_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 119 81 0)

      
      (fp_text reference "S5" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 5 "C1"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 7 "pinky_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 5 "C1"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 7 "pinky_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 119 62 0)

      
      (fp_text reference "S6" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 5 "C1"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 8 "pinky_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 5 "C1"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 8 "pinky_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 138 95.25 0)

      
      (fp_text reference "S7" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 9 "C2"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 10 "ring_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 9 "C2"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 10 "ring_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 138 76.25 0)

      
      (fp_text reference "S8" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 9 "C2"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 11 "ring_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 9 "C2"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 11 "ring_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 138 57.25 0)

      
      (fp_text reference "S9" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 9 "C2"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 12 "ring_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 9 "C2"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 12 "ring_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 157 92.875 0)

      
      (fp_text reference "S10" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 13 "C3"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 14 "middle_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 13 "C3"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 14 "middle_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 157 73.875 0)

      
      (fp_text reference "S11" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 13 "C3"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 15 "middle_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 13 "C3"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 15 "middle_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 157 54.875 0)

      
      (fp_text reference "S12" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 13 "C3"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 16 "middle_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 13 "C3"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 16 "middle_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 176 95.25 0)

      
      (fp_text reference "S13" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 17 "C4"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 18 "index_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 17 "C4"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 18 "index_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 176 76.25 0)

      
      (fp_text reference "S14" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 17 "C4"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 19 "index_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 17 "C4"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 19 "index_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 176 57.25 0)

      
      (fp_text reference "S15" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 17 "C4"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 20 "index_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 17 "C4"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 20 "index_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 195 97.625 0)

      
      (fp_text reference "S16" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 21 "C5"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 22 "inner_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 21 "C5"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 22 "inner_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 195 78.625 0)

      
      (fp_text reference "S17" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 21 "C5"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 23 "inner_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 21 "C5"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 23 "inner_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 195 59.625 0)

      
      (fp_text reference "S18" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 21 "C5"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 24 "inner_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 21 "C5"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 24 "inner_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 166.5 114.875 0)

      
      (fp_text reference "S19" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 13 "C3"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 25 "near_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 13 "C3"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 25 "near_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 187.5 117.625 -15)

      
      (fp_text reference "S20" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 -15) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 17 "C4"))
        (pad 2 smd rect (at 5.842 -5.08 -15) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 26 "mid_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 -15) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 17 "C4"))
        (pad 2 smd rect (at -5.842 -5.08 -15) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 26 "mid_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 209.7468058 121.3891576 60)

      
      (fp_text reference "S21" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 60) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 21 "C5"))
        (pad 2 smd rect (at 5.842 -5.08 60) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 27 "far_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 60) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 21 "C5"))
        (pad 2 smd rect (at -5.842 -5.08 60) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 27 "far_home"))
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 107.4 98.675 90)
            (fp_text reference "D1" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 2 "outer_bottom"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "R2"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 107.4 79.675 90)
            (fp_text reference "D2" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 3 "outer_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "R1"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 107.4 60.675 90)
            (fp_text reference "D3" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 4 "outer_top"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "R0"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 126.4 98.675 90)
            (fp_text reference "D4" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 6 "pinky_bottom"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "R2"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 126.4 79.675 90)
            (fp_text reference "D5" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 7 "pinky_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "R1"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 126.4 60.675 90)
            (fp_text reference "D6" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 8 "pinky_top"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "R0"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 145.4 93.925 90)
            (fp_text reference "D7" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 10 "ring_bottom"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "R2"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 145.4 74.925 90)
            (fp_text reference "D8" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 11 "ring_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "R1"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 145.4 55.925 90)
            (fp_text reference "D9" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 12 "ring_top"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "R0"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 164.4 91.55 90)
            (fp_text reference "D10" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 14 "middle_bottom"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "R2"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 164.4 72.55 90)
            (fp_text reference "D11" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 15 "middle_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "R1"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 164.4 53.55 90)
            (fp_text reference "D12" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 16 "middle_top"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "R0"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 183.4 93.925 90)
            (fp_text reference "D13" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 18 "index_bottom"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "R2"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 183.4 74.925 90)
            (fp_text reference "D14" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 19 "index_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "R1"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 183.4 55.925 90)
            (fp_text reference "D15" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 20 "index_top"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "R0"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 202.4 96.3 90)
            (fp_text reference "D16" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 22 "inner_bottom"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "R2"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 202.4 77.3 90)
            (fp_text reference "D17" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 23 "inner_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "R1"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 202.4 58.3 90)
            (fp_text reference "D18" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 24 "inner_top"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "R0"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 173.9 113.55 90)
            (fp_text reference "D19" (at 0 0 90) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 25 "near_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 31 "R3"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 194.9907863 118.2604092 75)
            (fp_text reference "D20" (at 0 0 75) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 75) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 26 "mid_home"))
            (pad 1 smd rect (at -1.65 0 75) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 31 "R3"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer B.Cu) (tedit 5B24D78E)
            (at 212.2993221 114.3180696 150)
            (fp_text reference "D21" (at 0 0 150) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 150) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 27 "far_home"))
            (pad 1 smd rect (at -1.65 0 150) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 31 "R3"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 92.6 98.675 90)
            (fp_text reference "D22" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "R2"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 2 "outer_bottom"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 92.6 79.675 90)
            (fp_text reference "D23" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "R1"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 3 "outer_home"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 92.6 60.675 90)
            (fp_text reference "D24" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "R0"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 4 "outer_top"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 111.6 98.675 90)
            (fp_text reference "D25" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "R2"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 6 "pinky_bottom"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 111.6 79.675 90)
            (fp_text reference "D26" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "R1"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 7 "pinky_home"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 111.6 60.675 90)
            (fp_text reference "D27" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "R0"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 8 "pinky_top"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 130.6 93.925 90)
            (fp_text reference "D28" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "R2"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 10 "ring_bottom"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 130.6 74.925 90)
            (fp_text reference "D29" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "R1"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 11 "ring_home"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 130.6 55.925 90)
            (fp_text reference "D30" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "R0"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 12 "ring_top"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 149.6 91.55 90)
            (fp_text reference "D31" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "R2"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 14 "middle_bottom"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 149.6 72.55 90)
            (fp_text reference "D32" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "R1"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 15 "middle_home"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 149.6 53.55 90)
            (fp_text reference "D33" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "R0"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 16 "middle_top"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 168.6 93.925 90)
            (fp_text reference "D34" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "R2"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 18 "index_bottom"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 168.6 74.925 90)
            (fp_text reference "D35" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "R1"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 19 "index_home"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 168.6 55.925 90)
            (fp_text reference "D36" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "R0"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 20 "index_top"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 187.6 96.3 90)
            (fp_text reference "D37" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "R2"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 22 "inner_bottom"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 187.6 77.3 90)
            (fp_text reference "D38" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "R1"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 23 "inner_home"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 187.6 58.3 90)
            (fp_text reference "D39" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "R0"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 24 "inner_top"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 159.1 113.55 90)
            (fp_text reference "D40" (at 0 0 90) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 31 "R3"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 25 "near_home"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 180.6950841 114.4298873 75)
            (fp_text reference "D41" (at 0 0 75) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 75) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 31 "R3"))
            (pad 2 smd rect (at 1.65 0 75) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 26 "mid_home"))
        
        )
        

        (module "ceoloide:diode_tht_sod123" (layer F.Cu) (tedit 5B24D78E)
            (at 204.8993221 127.1352456 150)
            (fp_text reference "D42" (at 0 0 150) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 150) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 31 "R3"))
            (pad 2 smd rect (at 1.65 0 150) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 27 "far_home"))
        
        )
        

          
          
        (module "ceoloide:nice_nano" (layer F.Cu) (tedit 6451A4F1)
          (attr virtual)
          (at 214.704 70.87 0)
          (fp_text reference "MCU1" (at 0 -15 0) (layer F.SilkS) hide
            (effects (font (size 1 1) (thickness 0.15)))
          )

          
          (fp_line (start 3.556 -18.034) (end 3.556 -16.51) (layer Dwgs.User) (width 0.15))
          (fp_line (start -3.81 -16.51) (end -3.81 -18.034) (layer Dwgs.User) (width 0.15))
          (fp_line (start -3.81 -18.034) (end 3.556 -18.034) (layer Dwgs.User) (width 0.15))


          
          (fp_line (start -8.89 -16.51) (end 8.89 -16.51) (layer F.Fab) (width 0.12))
          (fp_line (start -8.89 -16.51) (end -8.89 -14) (layer F.Fab) (width 0.12))
          (fp_line (start 8.89 -16.51) (end 8.89 -14) (layer F.Fab) (width 0.12))
          (fp_line (start -8.89 -16.5) (end -8.89 -13.99) (layer B.Fab) (width 0.12))
          (fp_line (start 8.89 -16.51) (end 8.89 -14) (layer B.Fab) (width 0.12))
          (fp_line (start -8.89 -16.51) (end 8.89 -16.51) (layer B.Fab) (width 0.12))

          
          (fp_line (start 6.29 -11.43) (end 8.95 -11.43) (layer F.SilkS) (width 0.12))
          (fp_line (start 6.29 -14.03) (end 8.95 -14.03) (layer F.SilkS) (width 0.12))
          (fp_line (start 6.29 -14.03) (end 6.29 16.57) (layer F.SilkS) (width 0.12))
          (fp_line (start 6.29 16.57) (end 8.95 16.57) (layer F.SilkS) (width 0.12))
          (fp_line (start 8.95 -14.03) (end 8.95 16.57) (layer F.SilkS) (width 0.12))
          (fp_line (start -8.95 -14.03) (end -6.29 -14.03) (layer F.SilkS) (width 0.12))
          (fp_line (start -8.95 -14.03) (end -8.95 16.57) (layer F.SilkS) (width 0.12))
          (fp_line (start -8.95 16.57) (end -6.29 16.57) (layer F.SilkS) (width 0.12))
          (fp_line (start -6.29 -14.03) (end -6.29 16.57) (layer F.SilkS) (width 0.12))
          (fp_line (start -8.95 -11.43) (end -6.29 -11.43) (layer B.SilkS) (width 0.12))
          (fp_line (start -6.29 -14.03) (end -8.95 -14.03) (layer B.SilkS) (width 0.12))
          (fp_line (start -6.29 -14.03) (end -6.29 16.57) (layer B.SilkS) (width 0.12))
          (fp_line (start -6.29 16.57) (end -8.95 16.57) (layer B.SilkS) (width 0.12))
          (fp_line (start -8.95 -14.03) (end -8.95 16.57) (layer B.SilkS) (width 0.12))
          (fp_line (start 8.95 -14.03) (end 6.29 -14.03) (layer B.SilkS) (width 0.12))
          (fp_line (start 8.95 -14.03) (end 8.95 16.57) (layer B.SilkS) (width 0.12))
          (fp_line (start 8.95 16.57) (end 6.29 16.57) (layer B.SilkS) (width 0.12))
          (fp_line (start 6.29 -14.03) (end 6.29 16.57) (layer B.SilkS) (width 0.12))
      
          
        
        (pad 24 thru_hole circle (at -7.62 -12.7 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 44 "MCU1_24"))
        (pad 1 thru_hole circle (at 7.62 -12.7 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 45 "MCU1_1"))
      
        
        (pad 1 thru_hole circle (at 3.4 -12.7 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 32 "RAW"))
        (pad 124 thru_hole circle (at -3.4 -12.7 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 38 "LED"))
      
        
        (pad 24 smd rect (at -5.48 -12.7 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 44 "MCU1_24"))
        (pad 124 smd rect (at -4.58 -12.7 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 38 "LED"))

        
        (pad 1 smd rect (at 4.58 -12.7 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 32 "RAW"))
        (pad 24 smd rect (at 5.48 -12.7 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 45 "MCU1_1"))

        
        (pad 24 smd rect (at -5.48 -12.7 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 44 "MCU1_24"))
        (pad 1 smd rect (at -4.58 -12.7 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 32 "RAW"))

        
        (pad 124 smd rect (at 4.58 -12.7 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 38 "LED"))
        (pad 24 smd rect (at 5.48 -12.7 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 45 "MCU1_1"))
        

            
            (fp_text user LED (at -3 -12.7 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user RAW (at 3 -12.7 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user RAW (at -3 -12.7 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user LED (at 3 -12.7 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user LED (at -3.262 -13.5 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user RAW (at 3.262 -13.5 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user LED (at -3.262 -13.5 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user RAW (at 3.262 -13.5 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
        
        (pad 23 thru_hole circle (at -7.62 -10.16 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 46 "MCU1_23"))
        (pad 2 thru_hole circle (at 7.62 -10.16 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 47 "MCU1_2"))
      
        
        (pad 2 thru_hole circle (at 3.4 -10.16 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 33 "GND"))
        (pad 123 thru_hole circle (at -3.4 -10.16 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 39 "DAT"))
      
        
        (pad 23 smd rect (at -5.48 -10.16 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 46 "MCU1_23"))
        (pad 123 smd rect (at -4.58 -10.16 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 39 "DAT"))

        
        (pad 2 smd rect (at 4.58 -10.16 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 33 "GND"))
        (pad 23 smd rect (at 5.48 -10.16 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 47 "MCU1_2"))

        
        (pad 23 smd rect (at -5.48 -10.16 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 46 "MCU1_23"))
        (pad 2 smd rect (at -4.58 -10.16 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 33 "GND"))

        
        (pad 123 smd rect (at 4.58 -10.16 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 39 "DAT"))
        (pad 23 smd rect (at 5.48 -10.16 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 47 "MCU1_2"))
        

            
            (fp_text user DAT (at -3 -10.16 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user GND (at 3 -10.16 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user GND (at -3 -10.16 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user DAT (at 3 -10.16 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user DAT (at -3.262 -10.96 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user GND (at 3.262 -10.96 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user DAT (at -3.262 -10.96 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user GND (at 3.262 -10.96 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
        
        (pad 22 thru_hole circle (at -7.62 -7.619999999999999 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 48 "MCU1_22"))
        (pad 3 thru_hole circle (at 7.62 -7.619999999999999 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 49 "MCU1_3"))
      
        
        (pad 3 thru_hole circle (at 3.4 -7.619999999999999 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 34 "RST"))
        (pad 122 thru_hole circle (at -3.4 -7.619999999999999 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 33 "GND"))
      
        
        (pad 22 smd rect (at -5.48 -7.619999999999999 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 48 "MCU1_22"))
        (pad 122 smd rect (at -4.58 -7.619999999999999 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 33 "GND"))

        
        (pad 3 smd rect (at 4.58 -7.619999999999999 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 34 "RST"))
        (pad 22 smd rect (at 5.48 -7.619999999999999 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 49 "MCU1_3"))

        
        (pad 22 smd rect (at -5.48 -7.619999999999999 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 48 "MCU1_22"))
        (pad 3 smd rect (at -4.58 -7.619999999999999 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 34 "RST"))

        
        (pad 122 smd rect (at 4.58 -7.619999999999999 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 33 "GND"))
        (pad 22 smd rect (at 5.48 -7.619999999999999 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 49 "MCU1_3"))
        

            
            (fp_text user GND (at -3 -7.619999999999999 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user RST (at 3 -7.619999999999999 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user RST (at -3 -7.619999999999999 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user GND (at 3 -7.619999999999999 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user GND (at -3.262 -8.42 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user RST (at 3.262 -8.42 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user GND (at -3.262 -8.42 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user RST (at 3.262 -8.42 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
        
        (pad 21 thru_hole circle (at -7.62 -5.079999999999999 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 50 "MCU1_21"))
        (pad 4 thru_hole circle (at 7.62 -5.079999999999999 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 51 "MCU1_4"))
      
        
        (pad 4 thru_hole circle (at 3.4 -5.079999999999999 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 35 "VCC"))
        (pad 121 thru_hole circle (at -3.4 -5.079999999999999 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 33 "GND"))
      
        
        (pad 21 smd rect (at -5.48 -5.079999999999999 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 50 "MCU1_21"))
        (pad 121 smd rect (at -4.58 -5.079999999999999 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 33 "GND"))

        
        (pad 4 smd rect (at 4.58 -5.079999999999999 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 35 "VCC"))
        (pad 21 smd rect (at 5.48 -5.079999999999999 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 51 "MCU1_4"))

        
        (pad 21 smd rect (at -5.48 -5.079999999999999 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 50 "MCU1_21"))
        (pad 4 smd rect (at -4.58 -5.079999999999999 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 35 "VCC"))

        
        (pad 121 smd rect (at 4.58 -5.079999999999999 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 33 "GND"))
        (pad 21 smd rect (at 5.48 -5.079999999999999 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 51 "MCU1_4"))
        

            
            (fp_text user GND (at -3 -5.079999999999999 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user VCC (at 3 -5.079999999999999 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user VCC (at -3 -5.079999999999999 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user GND (at 3 -5.079999999999999 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user GND (at -3.262 -5.88 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user VCC (at 3.262 -5.88 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user GND (at -3.262 -5.88 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user VCC (at 3.262 -5.88 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
        
        (pad 20 thru_hole circle (at -7.62 -2.539999999999999 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 52 "MCU1_20"))
        (pad 5 thru_hole circle (at 7.62 -2.539999999999999 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 53 "MCU1_5"))
      
        
        (pad 5 thru_hole circle (at 3.4 -2.539999999999999 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 1 "C0"))
        (pad 120 thru_hole circle (at -3.4 -2.539999999999999 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 40 "SDA"))
      
        
        (pad 20 smd rect (at -5.48 -2.539999999999999 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 52 "MCU1_20"))
        (pad 120 smd rect (at -4.58 -2.539999999999999 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 40 "SDA"))

        
        (pad 5 smd rect (at 4.58 -2.539999999999999 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 1 "C0"))
        (pad 20 smd rect (at 5.48 -2.539999999999999 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 53 "MCU1_5"))

        
        (pad 20 smd rect (at -5.48 -2.539999999999999 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 52 "MCU1_20"))
        (pad 5 smd rect (at -4.58 -2.539999999999999 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 1 "C0"))

        
        (pad 120 smd rect (at 4.58 -2.539999999999999 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 40 "SDA"))
        (pad 20 smd rect (at 5.48 -2.539999999999999 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 53 "MCU1_5"))
        

            
            (fp_text user SDA (at -3 -2.539999999999999 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user C0 (at 3 -2.539999999999999 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user C0 (at -3 -2.539999999999999 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user SDA (at 3 -2.539999999999999 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user SDA (at -3.262 -3.34 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user C0 (at 3.262 -3.34 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user SDA (at -3.262 -3.34 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user C0 (at 3.262 -3.34 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
        
        (pad 19 thru_hole circle (at -7.62 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 54 "MCU1_19"))
        (pad 6 thru_hole circle (at 7.62 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 55 "MCU1_6"))
      
        
        (pad 6 thru_hole circle (at 3.4 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 5 "C1"))
        (pad 119 thru_hole circle (at -3.4 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 41 "SCL"))
      
        
        (pad 19 smd rect (at -5.48 0 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 54 "MCU1_19"))
        (pad 119 smd rect (at -4.58 0 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 41 "SCL"))

        
        (pad 6 smd rect (at 4.58 0 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 5 "C1"))
        (pad 19 smd rect (at 5.48 0 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 55 "MCU1_6"))

        
        (pad 19 smd rect (at -5.48 0 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 54 "MCU1_19"))
        (pad 6 smd rect (at -4.58 0 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 5 "C1"))

        
        (pad 119 smd rect (at 4.58 0 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 41 "SCL"))
        (pad 19 smd rect (at 5.48 0 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 55 "MCU1_6"))
        

            
            (fp_text user SCL (at -3 0 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user C1 (at 3 0 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user C1 (at -3 0 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user SCL (at 3 0 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user SCL (at -3.262 -0.8000000000000007 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user C1 (at 3.262 -0.8000000000000007 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user SCL (at -3.262 -0.8000000000000007 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user C1 (at 3.262 -0.8000000000000007 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
        
        (pad 18 thru_hole circle (at -7.62 2.540000000000001 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 56 "MCU1_18"))
        (pad 7 thru_hole circle (at 7.62 2.540000000000001 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 57 "MCU1_7"))
      
        
        (pad 7 thru_hole circle (at 3.4 2.540000000000001 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 9 "C2"))
        (pad 118 thru_hole circle (at -3.4 2.540000000000001 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 42 "CS"))
      
        
        (pad 18 smd rect (at -5.48 2.540000000000001 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 56 "MCU1_18"))
        (pad 118 smd rect (at -4.58 2.540000000000001 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 42 "CS"))

        
        (pad 7 smd rect (at 4.58 2.540000000000001 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 9 "C2"))
        (pad 18 smd rect (at 5.48 2.540000000000001 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 57 "MCU1_7"))

        
        (pad 18 smd rect (at -5.48 2.540000000000001 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 56 "MCU1_18"))
        (pad 7 smd rect (at -4.58 2.540000000000001 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 9 "C2"))

        
        (pad 118 smd rect (at 4.58 2.540000000000001 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 42 "CS"))
        (pad 18 smd rect (at 5.48 2.540000000000001 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 57 "MCU1_7"))
        

            
            (fp_text user CS (at -3 2.540000000000001 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user C2 (at 3 2.540000000000001 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user C2 (at -3 2.540000000000001 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user CS (at 3 2.540000000000001 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user CS (at -3.262 1.7400000000000002 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user C2 (at 3.262 1.7400000000000002 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user CS (at -3.262 1.7400000000000002 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user C2 (at 3.262 1.7400000000000002 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
        
        (pad 17 thru_hole circle (at -7.62 5.080000000000002 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 58 "MCU1_17"))
        (pad 8 thru_hole circle (at 7.62 5.080000000000002 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 59 "MCU1_8"))
      
        
        (pad 8 thru_hole circle (at 3.4 5.080000000000002 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 13 "C3"))
        (pad 117 thru_hole circle (at -3.4 5.080000000000002 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 30 "R0"))
      
        
        (pad 17 smd rect (at -5.48 5.080000000000002 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 58 "MCU1_17"))
        (pad 117 smd rect (at -4.58 5.080000000000002 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 30 "R0"))

        
        (pad 8 smd rect (at 4.58 5.080000000000002 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 13 "C3"))
        (pad 17 smd rect (at 5.48 5.080000000000002 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 59 "MCU1_8"))

        
        (pad 17 smd rect (at -5.48 5.080000000000002 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 58 "MCU1_17"))
        (pad 8 smd rect (at -4.58 5.080000000000002 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 13 "C3"))

        
        (pad 117 smd rect (at 4.58 5.080000000000002 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 30 "R0"))
        (pad 17 smd rect (at 5.48 5.080000000000002 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 59 "MCU1_8"))
        

            
            (fp_text user R0 (at -3 5.080000000000002 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user C3 (at 3 5.080000000000002 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user C3 (at -3 5.080000000000002 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user R0 (at 3 5.080000000000002 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user R0 (at -3.262 4.280000000000001 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user C3 (at 3.262 4.280000000000001 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user R0 (at -3.262 4.280000000000001 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user C3 (at 3.262 4.280000000000001 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
        
        (pad 16 thru_hole circle (at -7.62 7.620000000000001 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 60 "MCU1_16"))
        (pad 9 thru_hole circle (at 7.62 7.620000000000001 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 61 "MCU1_9"))
      
        
        (pad 9 thru_hole circle (at 3.4 7.620000000000001 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 17 "C4"))
        (pad 116 thru_hole circle (at -3.4 7.620000000000001 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 29 "R1"))
      
        
        (pad 16 smd rect (at -5.48 7.620000000000001 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 60 "MCU1_16"))
        (pad 116 smd rect (at -4.58 7.620000000000001 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 29 "R1"))

        
        (pad 9 smd rect (at 4.58 7.620000000000001 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 17 "C4"))
        (pad 16 smd rect (at 5.48 7.620000000000001 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 61 "MCU1_9"))

        
        (pad 16 smd rect (at -5.48 7.620000000000001 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 60 "MCU1_16"))
        (pad 9 smd rect (at -4.58 7.620000000000001 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 17 "C4"))

        
        (pad 116 smd rect (at 4.58 7.620000000000001 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 29 "R1"))
        (pad 16 smd rect (at 5.48 7.620000000000001 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 61 "MCU1_9"))
        

            
            (fp_text user R1 (at -3 7.620000000000001 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user C4 (at 3 7.620000000000001 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user C4 (at -3 7.620000000000001 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user R1 (at 3 7.620000000000001 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user R1 (at -3.262 6.82 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user C4 (at 3.262 6.82 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user R1 (at -3.262 6.82 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user C4 (at 3.262 6.82 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
        
        (pad 15 thru_hole circle (at -7.62 10.16 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 62 "MCU1_15"))
        (pad 10 thru_hole circle (at 7.62 10.16 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 63 "MCU1_10"))
      
        
        (pad 10 thru_hole circle (at 3.4 10.16 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 21 "C5"))
        (pad 115 thru_hole circle (at -3.4 10.16 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 28 "R2"))
      
        
        (pad 15 smd rect (at -5.48 10.16 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 62 "MCU1_15"))
        (pad 115 smd rect (at -4.58 10.16 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 28 "R2"))

        
        (pad 10 smd rect (at 4.58 10.16 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 21 "C5"))
        (pad 15 smd rect (at 5.48 10.16 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 63 "MCU1_10"))

        
        (pad 15 smd rect (at -5.48 10.16 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 62 "MCU1_15"))
        (pad 10 smd rect (at -4.58 10.16 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 21 "C5"))

        
        (pad 115 smd rect (at 4.58 10.16 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 28 "R2"))
        (pad 15 smd rect (at 5.48 10.16 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 63 "MCU1_10"))
        

            
            (fp_text user R2 (at -3 10.16 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user C5 (at 3 10.16 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user C5 (at -3 10.16 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user R2 (at 3 10.16 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user R2 (at -3.262 9.36 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user C5 (at 3.262 9.36 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user R2 (at -3.262 9.36 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user C5 (at 3.262 9.36 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
        
        (pad 14 thru_hole circle (at -7.62 12.7 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 64 "MCU1_14"))
        (pad 11 thru_hole circle (at 7.62 12.7 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 65 "MCU1_11"))
      
        
        (pad 11 thru_hole circle (at 3.4 12.7 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 36 "P16"))
        (pad 114 thru_hole circle (at -3.4 12.7 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 31 "R3"))
      
        
        (pad 14 smd rect (at -5.48 12.7 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 64 "MCU1_14"))
        (pad 114 smd rect (at -4.58 12.7 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 31 "R3"))

        
        (pad 11 smd rect (at 4.58 12.7 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 36 "P16"))
        (pad 14 smd rect (at 5.48 12.7 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 65 "MCU1_11"))

        
        (pad 14 smd rect (at -5.48 12.7 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 64 "MCU1_14"))
        (pad 11 smd rect (at -4.58 12.7 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 36 "P16"))

        
        (pad 114 smd rect (at 4.58 12.7 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 31 "R3"))
        (pad 14 smd rect (at 5.48 12.7 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 65 "MCU1_11"))
        

            
            (fp_text user R3 (at -3 12.7 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user P16 (at 3 12.7 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user P16 (at -3 12.7 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user R3 (at 3 12.7 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user R3 (at -3.262 11.899999999999999 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user P16 (at 3.262 11.899999999999999 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user R3 (at -3.262 11.899999999999999 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user P16 (at 3.262 11.899999999999999 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
        
        (pad 13 thru_hole circle (at -7.62 15.240000000000002 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 66 "MCU1_13"))
        (pad 12 thru_hole circle (at 7.62 15.240000000000002 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 67 "MCU1_12"))
      
        
        (pad 12 thru_hole circle (at 3.4 15.240000000000002 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 37 "P10"))
        (pad 113 thru_hole circle (at -3.4 15.240000000000002 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 43 "P9"))
      
        
        (pad 13 smd rect (at -5.48 15.240000000000002 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 66 "MCU1_13"))
        (pad 113 smd rect (at -4.58 15.240000000000002 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 43 "P9"))

        
        (pad 12 smd rect (at 4.58 15.240000000000002 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 37 "P10"))
        (pad 13 smd rect (at 5.48 15.240000000000002 0) (size 0.6 1.2) (layers F.Cu F.Mask) (net 67 "MCU1_12"))

        
        (pad 13 smd rect (at -5.48 15.240000000000002 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 66 "MCU1_13"))
        (pad 12 smd rect (at -4.58 15.240000000000002 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 37 "P10"))

        
        (pad 113 smd rect (at 4.58 15.240000000000002 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 43 "P9"))
        (pad 13 smd rect (at 5.48 15.240000000000002 0) (size 0.6 1.2) (layers B.Cu B.Mask) (net 67 "MCU1_12"))
        

            
            (fp_text user P9 (at -3 15.240000000000002 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user P10 (at 3 15.240000000000002 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user P10 (at -3 15.240000000000002 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user P9 (at 3 15.240000000000002 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user P9 (at -3.262 14.440000000000001 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user P10 (at 3.262 14.440000000000001 0) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user P9 (at -3.262 14.440000000000001 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user P10 (at 3.262 14.440000000000001 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
        )

        
        
          (segment (start 219.284 58.170) (end 218.104 58.170) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.124 58.170) (end 211.304 58.170) (width 0.25) (layer F.Cu) (net 13))
          
          (segment (start 207.084 58.170) (end 209.204 58.170) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 58.170) (end 209.204 58.170) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 58.170) (end 222.324 58.170) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 58.170) (end 220.204 58.170) (width 0.25) (layer B.Cu) (net 24))
          
          (segment (start 212.099 58.400) (end 217.874 58.400) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 209.929 58.170) (end 210.279 58.170) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.004 58.895) (end 211.604 58.895) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 210.279 58.170) (end 211.004 58.895) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.604 58.895) (end 212.099 58.400) (width 0.25) (layer "B.Cu") (net 2))

          (segment (start 219.479 58.170) (end 219.129 58.170) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.299 57.950) (end 211.524 57.950) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 219.129 58.170) (end 218.404 57.445) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 218.404 57.445) (end 217.804 57.445) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.804 57.445) (end 217.299 57.950) (width 0.25) (layer "B.Cu") (net 20))
        
          (segment (start 219.284 60.710) (end 218.104 60.710) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.124 60.710) (end 211.304 60.710) (width 0.25) (layer F.Cu) (net 13))
          
          (segment (start 207.084 60.710) (end 209.204 60.710) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 60.710) (end 209.204 60.710) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 60.710) (end 222.324 60.710) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 60.710) (end 220.204 60.710) (width 0.25) (layer B.Cu) (net 24))
          
          (segment (start 212.099 60.940) (end 217.874 60.940) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 209.929 60.710) (end 210.279 60.710) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.004 61.435) (end 211.604 61.435) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 210.279 60.710) (end 211.004 61.435) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.604 61.435) (end 212.099 60.940) (width 0.25) (layer "B.Cu") (net 2))

          (segment (start 219.479 60.710) (end 219.129 60.710) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.299 60.490) (end 211.524 60.490) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 219.129 60.710) (end 218.404 59.985) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 218.404 59.985) (end 217.804 59.985) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.804 59.985) (end 217.299 60.490) (width 0.25) (layer "B.Cu") (net 20))
        
          (segment (start 219.284 63.250) (end 218.104 63.250) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.124 63.250) (end 211.304 63.250) (width 0.25) (layer F.Cu) (net 13))
          
          (segment (start 207.084 63.250) (end 209.204 63.250) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 63.250) (end 209.204 63.250) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 63.250) (end 222.324 63.250) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 63.250) (end 220.204 63.250) (width 0.25) (layer B.Cu) (net 24))
          
          (segment (start 212.099 63.480) (end 217.874 63.480) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 209.929 63.250) (end 210.279 63.250) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.004 63.975) (end 211.604 63.975) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 210.279 63.250) (end 211.004 63.975) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.604 63.975) (end 212.099 63.480) (width 0.25) (layer "B.Cu") (net 2))

          (segment (start 219.479 63.250) (end 219.129 63.250) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.299 63.030) (end 211.524 63.030) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 219.129 63.250) (end 218.404 62.525) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 218.404 62.525) (end 217.804 62.525) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.804 62.525) (end 217.299 63.030) (width 0.25) (layer "B.Cu") (net 20))
        
          (segment (start 219.284 65.790) (end 218.104 65.790) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.124 65.790) (end 211.304 65.790) (width 0.25) (layer F.Cu) (net 13))
          
          (segment (start 207.084 65.790) (end 209.204 65.790) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 65.790) (end 209.204 65.790) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 65.790) (end 222.324 65.790) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 65.790) (end 220.204 65.790) (width 0.25) (layer B.Cu) (net 24))
          
          (segment (start 212.099 66.020) (end 217.874 66.020) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 209.929 65.790) (end 210.279 65.790) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.004 66.515) (end 211.604 66.515) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 210.279 65.790) (end 211.004 66.515) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.604 66.515) (end 212.099 66.020) (width 0.25) (layer "B.Cu") (net 2))

          (segment (start 219.479 65.790) (end 219.129 65.790) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.299 65.570) (end 211.524 65.570) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 219.129 65.790) (end 218.404 65.065) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 218.404 65.065) (end 217.804 65.065) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.804 65.065) (end 217.299 65.570) (width 0.25) (layer "B.Cu") (net 20))
        
          (segment (start 219.284 68.330) (end 218.104 68.330) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.124 68.330) (end 211.304 68.330) (width 0.25) (layer F.Cu) (net 13))
          
          (segment (start 207.084 68.330) (end 209.204 68.330) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 68.330) (end 209.204 68.330) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 68.330) (end 222.324 68.330) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 68.330) (end 220.204 68.330) (width 0.25) (layer B.Cu) (net 24))
          
          (segment (start 212.099 68.560) (end 217.874 68.560) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 209.929 68.330) (end 210.279 68.330) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.004 69.055) (end 211.604 69.055) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 210.279 68.330) (end 211.004 69.055) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.604 69.055) (end 212.099 68.560) (width 0.25) (layer "B.Cu") (net 2))

          (segment (start 219.479 68.330) (end 219.129 68.330) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.299 68.110) (end 211.524 68.110) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 219.129 68.330) (end 218.404 67.605) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 218.404 67.605) (end 217.804 67.605) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.804 67.605) (end 217.299 68.110) (width 0.25) (layer "B.Cu") (net 20))
        
          (segment (start 219.284 70.870) (end 218.104 70.870) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.124 70.870) (end 211.304 70.870) (width 0.25) (layer F.Cu) (net 13))
          
          (segment (start 207.084 70.870) (end 209.204 70.870) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 70.870) (end 209.204 70.870) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 70.870) (end 222.324 70.870) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 70.870) (end 220.204 70.870) (width 0.25) (layer B.Cu) (net 24))
          
          (segment (start 212.099 71.100) (end 217.874 71.100) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 209.929 70.870) (end 210.279 70.870) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.004 71.595) (end 211.604 71.595) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 210.279 70.870) (end 211.004 71.595) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.604 71.595) (end 212.099 71.100) (width 0.25) (layer "B.Cu") (net 2))

          (segment (start 219.479 70.870) (end 219.129 70.870) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.299 70.650) (end 211.524 70.650) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 219.129 70.870) (end 218.404 70.145) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 218.404 70.145) (end 217.804 70.145) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.804 70.145) (end 217.299 70.650) (width 0.25) (layer "B.Cu") (net 20))
        
          (segment (start 219.284 73.410) (end 218.104 73.410) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.124 73.410) (end 211.304 73.410) (width 0.25) (layer F.Cu) (net 13))
          
          (segment (start 207.084 73.410) (end 209.204 73.410) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 73.410) (end 209.204 73.410) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 73.410) (end 222.324 73.410) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 73.410) (end 220.204 73.410) (width 0.25) (layer B.Cu) (net 24))
          
          (segment (start 212.099 73.640) (end 217.874 73.640) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 209.929 73.410) (end 210.279 73.410) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.004 74.135) (end 211.604 74.135) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 210.279 73.410) (end 211.004 74.135) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.604 74.135) (end 212.099 73.640) (width 0.25) (layer "B.Cu") (net 2))

          (segment (start 219.479 73.410) (end 219.129 73.410) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.299 73.190) (end 211.524 73.190) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 219.129 73.410) (end 218.404 72.685) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 218.404 72.685) (end 217.804 72.685) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.804 72.685) (end 217.299 73.190) (width 0.25) (layer "B.Cu") (net 20))
        
          (segment (start 219.284 75.950) (end 218.104 75.950) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.124 75.950) (end 211.304 75.950) (width 0.25) (layer F.Cu) (net 13))
          
          (segment (start 207.084 75.950) (end 209.204 75.950) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 75.950) (end 209.204 75.950) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 75.950) (end 222.324 75.950) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 75.950) (end 220.204 75.950) (width 0.25) (layer B.Cu) (net 24))
          
          (segment (start 212.099 76.180) (end 217.874 76.180) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 209.929 75.950) (end 210.279 75.950) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.004 76.675) (end 211.604 76.675) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 210.279 75.950) (end 211.004 76.675) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.604 76.675) (end 212.099 76.180) (width 0.25) (layer "B.Cu") (net 2))

          (segment (start 219.479 75.950) (end 219.129 75.950) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.299 75.730) (end 211.524 75.730) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 219.129 75.950) (end 218.404 75.225) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 218.404 75.225) (end 217.804 75.225) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.804 75.225) (end 217.299 75.730) (width 0.25) (layer "B.Cu") (net 20))
        
          (segment (start 219.284 78.490) (end 218.104 78.490) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.124 78.490) (end 211.304 78.490) (width 0.25) (layer F.Cu) (net 13))
          
          (segment (start 207.084 78.490) (end 209.204 78.490) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 78.490) (end 209.204 78.490) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 78.490) (end 222.324 78.490) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 78.490) (end 220.204 78.490) (width 0.25) (layer B.Cu) (net 24))
          
          (segment (start 212.099 78.720) (end 217.874 78.720) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 209.929 78.490) (end 210.279 78.490) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.004 79.215) (end 211.604 79.215) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 210.279 78.490) (end 211.004 79.215) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.604 79.215) (end 212.099 78.720) (width 0.25) (layer "B.Cu") (net 2))

          (segment (start 219.479 78.490) (end 219.129 78.490) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.299 78.270) (end 211.524 78.270) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 219.129 78.490) (end 218.404 77.765) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 218.404 77.765) (end 217.804 77.765) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.804 77.765) (end 217.299 78.270) (width 0.25) (layer "B.Cu") (net 20))
        
          (segment (start 219.284 81.030) (end 218.104 81.030) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.124 81.030) (end 211.304 81.030) (width 0.25) (layer F.Cu) (net 13))
          
          (segment (start 207.084 81.030) (end 209.204 81.030) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 81.030) (end 209.204 81.030) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 81.030) (end 222.324 81.030) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 81.030) (end 220.204 81.030) (width 0.25) (layer B.Cu) (net 24))
          
          (segment (start 212.099 81.260) (end 217.874 81.260) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 209.929 81.030) (end 210.279 81.030) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.004 81.755) (end 211.604 81.755) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 210.279 81.030) (end 211.004 81.755) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.604 81.755) (end 212.099 81.260) (width 0.25) (layer "B.Cu") (net 2))

          (segment (start 219.479 81.030) (end 219.129 81.030) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.299 80.810) (end 211.524 80.810) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 219.129 81.030) (end 218.404 80.305) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 218.404 80.305) (end 217.804 80.305) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.804 80.305) (end 217.299 80.810) (width 0.25) (layer "B.Cu") (net 20))
        
          (segment (start 219.284 83.570) (end 218.104 83.570) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.124 83.570) (end 211.304 83.570) (width 0.25) (layer F.Cu) (net 13))
          
          (segment (start 207.084 83.570) (end 209.204 83.570) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 83.570) (end 209.204 83.570) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 83.570) (end 222.324 83.570) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 83.570) (end 220.204 83.570) (width 0.25) (layer B.Cu) (net 24))
          
          (segment (start 212.099 83.800) (end 217.874 83.800) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 209.929 83.570) (end 210.279 83.570) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.004 84.295) (end 211.604 84.295) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 210.279 83.570) (end 211.004 84.295) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.604 84.295) (end 212.099 83.800) (width 0.25) (layer "B.Cu") (net 2))

          (segment (start 219.479 83.570) (end 219.129 83.570) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.299 83.350) (end 211.524 83.350) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 219.129 83.570) (end 218.404 82.845) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 218.404 82.845) (end 217.804 82.845) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.804 82.845) (end 217.299 83.350) (width 0.25) (layer "B.Cu") (net 20))
        
          (segment (start 219.284 86.110) (end 218.104 86.110) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.124 86.110) (end 211.304 86.110) (width 0.25) (layer F.Cu) (net 13))
          
          (segment (start 207.084 86.110) (end 209.204 86.110) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 86.110) (end 209.204 86.110) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 86.110) (end 222.324 86.110) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 86.110) (end 220.204 86.110) (width 0.25) (layer B.Cu) (net 24))
          
          (segment (start 212.099 86.340) (end 217.874 86.340) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 209.929 86.110) (end 210.279 86.110) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.004 86.835) (end 211.604 86.835) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 210.279 86.110) (end 211.004 86.835) (width 0.25) (layer "B.Cu") (net 2))
          (segment (start 211.604 86.835) (end 212.099 86.340) (width 0.25) (layer "B.Cu") (net 2))

          (segment (start 219.479 86.110) (end 219.129 86.110) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.299 85.890) (end 211.524 85.890) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 219.129 86.110) (end 218.404 85.385) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 218.404 85.385) (end 217.804 85.385) (width 0.25) (layer "B.Cu") (net 20))
          (segment (start 217.804 85.385) (end 217.299 85.890) (width 0.25) (layer "B.Cu") (net 20))
        
    

      (gr_text "JLCJLCJLCJLC" (at 138 107.6 0) (layer F.SilkS)
        (effects (font (size 1 1) (thickness 0.15))
        )
      )
      
      (gr_text "JLCJLCJLCJLC" (at 138 107.6 0) (layer B.SilkS)
        (effects (font (size 1 1) (thickness 0.15))
         (justify mirror))
      )
      

      (module "ceoloide:nice_view" (layer F.Cu) (tedit 6448AF5B)
        (at 214.647 73.25 0)
        (attr virtual)
        (fp_text reference "DISP1" (at 0 20 0) (layer F.SilkS) hide
          (effects (font (size 1 1) (thickness 0.15)))
        )
        (fp_text user %R (at 0 20 0) (layer F.Fab)
          (effects (font (size 1 1) (thickness 0.15)))
        )
        
        (fp_line (start -6.5 -18) (end 6.5 -18) (layer F.Fab) (width 0.15))
        (fp_line (start 6.5 18) (end -6.5 18) (layer F.Fab) (width 0.15))
        (fp_line (start -7 17.5) (end -7 -17.5) (layer F.Fab) (width 0.15))
        (fp_line (start 7 17.5) (end 7 -17.5) (layer F.Fab) (width 0.15))
        (fp_arc (start -6.5 17.5) (end -7 17.5) (angle -90) (layer F.Fab) (width 0.15))
        (fp_arc (start 6.5 17.5) (end 6.5 18) (angle -90) (layer F.Fab) (width 0.15))
        (fp_arc (start 6.5 -17.5) (end 6.5 -18) (angle 90) (layer F.Fab) (width 0.15))
        (fp_arc (start -6.5 -17.5) (end -6.5 -18) (angle -90) (layer F.Fab) (width 0.15))
        (fp_line (start -6.41 15.37) (end -6.41 18.03) (layer F.SilkS) (width 0.12))
        (fp_line (start 6.41 18.03) (end -6.41 18.03) (layer F.SilkS) (width 0.12))
        (fp_line (start 6.41 15.37) (end 6.41 18.03) (layer F.SilkS) (width 0.12))
        (fp_line (start 6.41 15.37) (end -6.41 15.37) (layer F.SilkS) (width 0.12))
        (fp_line (start 6.88 14.9) (end 6.88 18.45) (layer F.CrtYd) (width 0.15))
        (fp_line (start 6.88 18.45) (end -6.82 18.45) (layer F.CrtYd) (width 0.15))
        (fp_line (start -6.82 18.45) (end -6.82 14.9) (layer F.CrtYd) (width 0.15))
        (fp_line (start -6.82 14.9) (end 6.88 14.9) (layer F.CrtYd) (width 0.15))
    
        (fp_line (start 6.41 15.37) (end 6.41 18.03) (layer B.SilkS) (width 0.12))
        (fp_line (start 6.41 15.37) (end -6.41 15.37) (layer B.SilkS) (width 0.12))
        (fp_line (start 6.41 18.03) (end -6.41 18.03) (layer B.SilkS) (width 0.12))
        (fp_line (start 6.88 14.9) (end 6.88 18.45) (layer B.CrtYd) (width 0.15))
        (fp_line (start 6.88 18.45) (end -6.82 18.45) (layer B.CrtYd) (width 0.15))
        (fp_line (start -6.82 18.45) (end -6.82 14.9) (layer B.CrtYd) (width 0.15))
        (fp_line (start -6.82 14.9) (end 6.88 14.9) (layer B.CrtYd) (width 0.15))
        (fp_line (start -6.41 15.37) (end -6.41 18.03) (layer B.SilkS) (width 0.12))
        (fp_line (start -6.5 18) (end 6.5 18) (layer B.Fab) (width 0.15))
        (fp_line (start 7 -17.5) (end 7 17.5) (layer B.Fab) (width 0.15))
        (fp_line (start 6.5 -18) (end -6.5 -18) (layer B.Fab) (width 0.15))
        (fp_line (start -7 -17.5) (end -7 17.5) (layer B.Fab) (width 0.15))
        (fp_arc (start -6.5 -17.5) (end -7 -17.5) (angle 90) (layer B.Fab) (width 0.15))
        (fp_arc (start 6.5 -17.5) (end 6.5 -18) (angle 90) (layer B.Fab) (width 0.15))
        (fp_arc (start 6.5 17.5) (end 6.5 18) (angle -90) (layer B.Fab) (width 0.15))
        (fp_arc (start -6.5 17.5) (end -6.5 18) (angle 90) (layer B.Fab) (width 0.15))
    
        (fp_line (start 5.93 17.9) (end 5.93 19.9) (layer F.Fab) (width 0.15))
        (fp_line (start -5.93 19.9) (end -5.93 17.9) (layer F.Fab) (width 0.15))
        (fp_line (start -5.93 17.9) (end -4.23 17.9) (layer F.Fab) (width 0.15))
        (fp_line (start -4.23 19.9) (end -5.93 19.9) (layer F.Fab) (width 0.15))
        (fp_line (start -4.23 17.9) (end -4.23 19.9) (layer F.Fab) (width 0.15))
        (fp_line (start -3.39 19.9) (end -3.39 17.9) (layer F.Fab) (width 0.15))
        (fp_line (start -3.39 17.9) (end -1.69 17.9) (layer F.Fab) (width 0.15))
        (fp_line (start -1.69 19.9) (end -3.39 19.9) (layer F.Fab) (width 0.15))
        (fp_line (start -1.69 17.9) (end -1.69 19.9) (layer F.Fab) (width 0.15))
        (fp_line (start 3.39 17.9) (end 3.39 19.9) (layer F.Fab) (width 0.15))
        (fp_line (start 3.39 19.9) (end 1.69 19.9) (layer F.Fab) (width 0.15))
        (fp_line (start 1.69 19.9) (end 1.69 17.9) (layer F.Fab) (width 0.15))
        (fp_line (start 1.69 17.9) (end 3.39 17.9) (layer F.Fab) (width 0.15))
        (fp_line (start 5.93 19.9) (end 4.23 19.9) (layer F.Fab) (width 0.15))
        (fp_line (start 4.23 19.9) (end 4.23 17.9) (layer F.Fab) (width 0.15))
        (fp_line (start 4.23 17.9) (end 5.93 17.9) (layer F.Fab) (width 0.15))

        (pad 14 smd rect (at -5.08 18.450000000000003 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 68 "DISP1_1"))
        (pad 15 smd rect (at -2.54 18.450000000000003 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 69 "DISP1_2"))
        (pad 16 smd rect (at 2.54 18.450000000000003 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 70 "DISP1_4"))
        (pad 17 smd rect (at 5.08 18.450000000000003 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 71 "DISP1_5"))

        (pad 10 smd rect (at -5.08 19.35 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 42 "CS"))
        (pad 11 smd rect (at -2.54 19.35 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 33 "GND"))
        (pad 12 smd rect (at 2.54 19.35 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 41 "SCL"))
        (pad 13 smd rect (at 5.08 19.35 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 40 "SDA"))
    
        (fp_line (start -5.93 17.9) (end -5.93 19.9) (layer B.Fab) (width 0.15))
        (fp_line (start -5.93 19.9) (end -4.23 19.9) (layer B.Fab) (width 0.15))
        (fp_line (start -4.23 17.9) (end -5.93 17.9) (layer B.Fab) (width 0.15))
        (fp_line (start -4.23 19.9) (end -4.23 17.9) (layer B.Fab) (width 0.15))
        (fp_line (start -3.39 19.9) (end -1.69 19.9) (layer B.Fab) (width 0.15))
        (fp_line (start -1.69 17.9) (end -3.39 17.9) (layer B.Fab) (width 0.15))
        (fp_line (start 4.23 19.9) (end 5.93 19.9) (layer B.Fab) (width 0.15))
        (fp_line (start 5.93 19.9) (end 5.93 17.9) (layer B.Fab) (width 0.15))
        (fp_line (start 3.39 17.9) (end 1.69 17.9) (layer B.Fab) (width 0.15))
        (fp_line (start -1.69 19.9) (end -1.69 17.9) (layer B.Fab) (width 0.15))
        (fp_line (start -3.39 17.9) (end -3.39 19.9) (layer B.Fab) (width 0.15))
        (fp_line (start 1.69 17.9) (end 1.69 19.9) (layer B.Fab) (width 0.15))
        (fp_line (start 1.69 19.9) (end 3.39 19.9) (layer B.Fab) (width 0.15))
        (fp_line (start 3.39 19.9) (end 3.39 17.9) (layer B.Fab) (width 0.15))
        (fp_line (start 5.93 17.9) (end 4.23 17.9) (layer B.Fab) (width 0.15))
        (fp_line (start 4.23 17.9) (end 4.23 19.9) (layer B.Fab) (width 0.15))

        (pad 24 smd rect (at 5.08 18.450000000000003 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 71 "DISP1_5"))
        (pad 25 smd rect (at 2.54 18.450000000000003 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 70 "DISP1_4"))
        (pad 26 smd rect (at -2.54 18.450000000000003 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 69 "DISP1_2"))
        (pad 27 smd rect (at -5.08 18.450000000000003 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 68 "DISP1_1"))

        (pad 20 smd rect (at 5.08 19.35 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 42 "CS"))
        (pad 21 smd rect (at 2.54 19.35 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 33 "GND"))
        (pad 22 smd rect (at -2.54 19.35 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 41 "SCL"))
        (pad 23 smd rect (at -5.08 19.35 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 40 "SDA"))
    
      (pad 1 thru_hole oval (at -5.08 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 68 "DISP1_1"))
      (pad 2 thru_hole oval (at -2.54 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 69 "DISP1_2"))
      (pad 3 thru_hole oval (at 0 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 35 "VCC"))
      (pad 4 thru_hole oval (at 2.54 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 70 "DISP1_4"))
      (pad 5 thru_hole circle (at 5.08 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 71 "DISP1_5"))

      (fp_line (start 5.4 13.4) (end 5.4 -11.9) (layer Dwgs.User) (width 0.15))
      (fp_line (start -5.4 13.4) (end -5.4 -11.9) (layer Dwgs.User) (width 0.15))
      (fp_line (start 5.4 -11.9) (end -5.4 -11.9) (layer Dwgs.User) (width 0.15))
      (fp_line (start -5.4 13.4) (end 5.4 13.4) (layer Dwgs.User) (width 0.15))
    )
    
    (segment (start 209.567 89.950) (end 209.567 91.700) (width 0.25) (layer "F.Cu") (net 42))
    (segment (start 212.107 89.950) (end 212.107 91.700) (width 0.25) (layer "F.Cu") (net 33))
    (segment (start 217.187 89.950) (end 217.187 91.700) (width 0.25) (layer "F.Cu") (net 41))
    (segment (start 219.727 89.950) (end 219.727 91.700) (width 0.25) (layer "F.Cu") (net 40))
    (segment (start 209.567 89.950) (end 209.567 91.700) (width 0.25) (layer "B.Cu") (net 42))
    (segment (start 212.107 89.950) (end 212.107 91.700) (width 0.25) (layer "B.Cu") (net 33))
    (segment (start 217.187 89.950) (end 217.187 91.700) (width 0.25) (layer "B.Cu") (net 41))
    (segment (start 219.727 89.950) (end 219.727 91.700) (width 0.25) (layer "B.Cu") (net 40))
    

      (module "ceoloide:power_switch_smd_side" (layer F.Cu) (tedit 64473C6F)
        (at 223 99 0)
        (attr smd)
        (fp_text value "power_switch" (at 0 2.5 0) (layer F.Fab)
          (effects (font (size 1 1) (thickness 0.15)))
        )
    
        (fp_line (start -1.305 -3.35) (end -1.305 3.35) (layer F.Fab) (width 0.1))
        (fp_line (start 1.295 -3.35) (end -1.305 -3.35) (layer F.Fab) (width 0.1))
        (fp_line (start 1.295 3.35) (end 1.295 -3.35) (layer F.Fab) (width 0.1))
        (fp_line (start -1.305 3.35) (end 1.295 3.35) (layer F.Fab) (width 0.1))
        (fp_line (start 2.595 0.1) (end 1.295 0.1) (layer F.Fab) (width 0.1))
        (fp_line (start 2.645 0.15) (end 2.595 0.1) (layer F.Fab) (width 0.1))
        (fp_line (start 2.845 0.35) (end 2.645 0.15) (layer F.Fab) (width 0.1))
        (fp_line (start 2.845 1.2) (end 2.845 0.35) (layer F.Fab) (width 0.1))
        (fp_line (start 2.645 1.4) (end 2.845 1.2) (layer F.Fab) (width 0.1))
        (fp_line (start 1.345 1.4) (end 2.645 1.4) (layer F.Fab) (width 0.1))
        (pad "" smd rect (at 1.125 -3.65 90) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
        (pad "" smd rect (at -1.085 -3.65 90) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
        (pad "" smd rect (at -1.085 3.65 90) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
        (pad "" smd rect (at 1.125 3.65 90) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
        (pad 1 smd rect (at -1.735 2.25 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask) )
        (pad 2 smd rect (at -1.735 -0.75 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask) (net 32 "RAW"))
        (pad 3 smd rect (at -1.735 -2.25 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask) (net 72 "BAT_P"))

    
        (fp_text reference "PWR1" (at -3.6 0 -90) (layer F.SilkS) hide
          (effects (font (size 1 1) (thickness 0.15)))
        )
        (fp_text user "ON" (at 0 -4.5 0) (layer "F.SilkS")
          (effects (font (size 1 1) (thickness 0.15)) (justify bottom))
        )
        (fp_text user "OFF" (at 0 4.5 0) (layer "F.SilkS")
          (effects (font (size 1 1) (thickness 0.15)) (justify top))
        )
        (fp_line (start 0.415 -3.45) (end -0.375 -3.45) (layer F.SilkS) (width 0.12))
        (fp_line (start -0.375 3.45) (end 0.415 3.45) (layer F.SilkS) (width 0.12))
        (fp_line (start -1.425 1.6) (end -1.425 -0.1) (layer F.SilkS) (width 0.12))
        (fp_line (start 1.425 2.85) (end 1.425 -2.85) (layer F.SilkS) (width 0.12))
        (fp_line (start -1.425 -1.4) (end -1.425 -1.6) (layer F.SilkS) (width 0.12))
    
        (fp_line (start 2.595 -0.1) (end 1.295 -0.1) (layer B.Fab) (width 0.1))
        (fp_line (start -1.305 3.35) (end -1.305 -3.35) (layer B.Fab) (width 0.1))
        (fp_line (start 2.645 -0.15) (end 2.595 -0.1) (layer B.Fab) (width 0.1))
        (fp_line (start 2.845 -1.2) (end 2.845 -0.35) (layer B.Fab) (width 0.1))
        (fp_line (start 1.345 -1.4) (end 2.645 -1.4) (layer B.Fab) (width 0.1))
        (fp_line (start 2.845 -0.35) (end 2.645 -0.15) (layer B.Fab) (width 0.1))
        (fp_line (start 2.645 -1.4) (end 2.845 -1.2) (layer B.Fab) (width 0.1))
        (fp_line (start 1.295 -3.35) (end 1.295 3.35) (layer B.Fab) (width 0.1))
        (fp_line (start 1.295 3.35) (end -1.305 3.35) (layer B.Fab) (width 0.1))
        (fp_line (start -1.305 -3.35) (end 1.295 -3.35) (layer B.Fab) (width 0.1))
        (pad "" smd rect (at -1.085 -3.65 270) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
        (pad "" smd rect (at 1.125 -3.65 270) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
        (pad "" smd rect (at -1.085 3.65 270) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
        (pad "" smd rect (at 1.125 3.65 270) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
        (pad 1 smd rect (at -1.735 -2.25 270) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask) (net 72 "BAT_P"))
        (pad 2 smd rect (at -1.735 0.75 270) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask) (net 32 "RAW"))
        (pad 3 smd rect (at -1.735 2.25 270) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask) )
      
        (fp_text user "PWR1" (at -3.5 0 90) (layer B.SilkS) hide
          (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
        )
        (fp_text user "ON" (at 0 -4.5 0) (layer "B.SilkS")
          (effects (font (size 1 1) (thickness 0.15)) (justify bottom mirror))
        )
        (fp_text user "OFF" (at 0 4.5 0) (layer "B.SilkS")
          (effects (font (size 1 1) (thickness 0.15)) (justify top mirror))
        )
        (fp_line (start -1.425 1.4) (end -1.425 1.6) (layer B.SilkS) (width 0.12))
        (fp_line (start 0.415 3.45) (end -0.375 3.45) (layer B.SilkS) (width 0.12))
        (fp_line (start -0.375 -3.45) (end 0.415 -3.45) (layer B.SilkS) (width 0.12))
        (fp_line (start -1.425 -1.6) (end -1.425 0.1) (layer B.SilkS) (width 0.12))
        (fp_line (start 1.425 -2.85) (end 1.425 2.85) (layer B.SilkS) (width 0.12))
    
      (pad "" np_thru_hole circle (at 0.025 -1.5 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at 0.025 1.5 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    )
    

        (module "ceoloide:reset_button_smd_side" (layer F.Cu) (tedit 64473C6F)
          (at 214.704 55.165 0)
          (attr smd)
          (fp_text value "reset_button_smd_side" (at 0 2.5 0) (layer F.Fab)
            (effects (font (size 1 1) (thickness 0.15)))
          )
          (fp_line (start -2.35 -1.75) (end -2.35 1.75) (width 0.1) (layer "Dwgs.User"))
          (fp_line (start -2.35 -1.75) (end 2.35 -1.75) (width 0.1) (layer "Dwgs.User"))
          (fp_line (start -2.35 1.75) (end 2.35 1.75) (width 0.1) (layer "Dwgs.User"))
          (fp_line (start -1.3 -2.75) (end -1.3 -1.75) (width 0.1) (layer "Dwgs.User"))
          (fp_line (start -1.3 -2.75) (end 1.3 -2.75) (width 0.1) (layer "Dwgs.User"))
          (fp_line (start 1.3 -2.75) (end 1.3 -1.75) (width 0.1) (layer "Dwgs.User"))
          (fp_line (start 2.35 -1.75) (end 2.35 1.75) (width 0.1) (layer "Dwgs.User"))
      
        (pad "" np_thru_hole circle (at 0 -1.375 180) (size 0.75 0.75) (drill 0.75) (layers "*.Cu" "*.Mask"))
        (pad "" np_thru_hole circle (at 0 1.375 180) (size 0.75 0.75) (drill 0.75) (layers "*.Cu" "*.Mask"))
      
        (pad "1" smd rect (at 2.625 -0.85 180) (size 1.55 1) (layers "F.Cu" "F.Paste" "F.Mask") (net 33 "GND"))
        (pad "2" smd rect (at 2.625 0.85 180) (size 1.55 1) (layers "F.Cu" "F.Paste" "F.Mask") (net 34 "RST"))
        (pad "3" smd rect (at -2.625 -0.85 180) (size 1.55 1) (layers "F.Cu" "F.Paste" "F.Mask") (net 33 "GND"))
        (pad "4" smd rect (at -2.625 0.85 180) (size 1.55 1) (layers "F.Cu" "F.Paste" "F.Mask") (net 34 "RST"))
      
        (fp_text reference "RST1" (at 0 0 0) (layer F.SilkS) hide
          (effects (font (size 1 1) (thickness 0.15)))
        )
        (fp_line (start -2.35 -1.5) (end -2.35 -1.75) (width 0.1) (layer "F.SilkS"))
        (fp_line (start -2.35 1.5) (end -2.35 1.75) (width 0.1) (layer "F.SilkS"))
        (fp_line (start -2.1 -1.75) (end -2.35 -1.75) (width 0.1) (layer "F.SilkS"))
        (fp_line (start -2.1 1.75) (end -2.35 1.75) (width 0.1) (layer "F.SilkS"))
        (fp_line (start 2.1 -1.75) (end 2.35 -1.75) (width 0.1) (layer "F.SilkS"))
        (fp_line (start 2.1 1.75) (end 2.35 1.75) (width 0.1) (layer "F.SilkS"))
        (fp_line (start 2.35 -1.5) (end 2.35 -1.75) (width 0.1) (layer "F.SilkS"))
        (fp_line (start 2.35 1.5) (end 2.35 1.75) (width 0.1) (layer "F.SilkS"))
      
        (pad "1" smd rect (at -2.625 -0.85 180) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask") (net 33 "GND"))
        (pad "2" smd rect (at -2.625 0.85 180) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask") (net 34 "RST"))
        (pad "3" smd rect (at 2.625 -0.85 180) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask") (net 33 "GND"))
        (pad "4" smd rect (at 2.625 0.85 180) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask") (net 34 "RST"))
      
        (fp_text reference "RST1" (at 0 0 0) (layer B.SilkS) hide
          (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
        )
        (fp_line (start -2.35 -1.5) (end -2.35 -1.75) (width 0.1) (layer "B.SilkS"))
        (fp_line (start -2.35 1.5) (end -2.35 1.75) (width 0.1) (layer "B.SilkS"))
        (fp_line (start -2.1 -1.75) (end -2.35 -1.75) (width 0.1) (layer "B.SilkS"))
        (fp_line (start -2.1 1.75) (end -2.35 1.75) (width 0.1) (layer "B.SilkS"))
        (fp_line (start 2.1 -1.75) (end 2.35 -1.75) (width 0.1) (layer "B.SilkS"))
        (fp_line (start 2.1 1.75) (end 2.35 1.75) (width 0.1) (layer "B.SilkS"))
        (fp_line (start 2.35 -1.5) (end 2.35 -1.75) (width 0.1) (layer "B.SilkS"))
        (fp_line (start 2.35 1.5) (end 2.35 1.75) (width 0.1) (layer "B.SilkS"))
      
      )
      

            (module "ceoloide/battery_connector_jst_ph_2" (layer F.Cu) (tedit 6135B927)
                (at 211.75 97.75 90)

                (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)")
                (fp_text reference "JST1" (at 0 4.8 90) (layer "F.SilkS") hide
                    (effects (font (size 1 1) (thickness 0.15)))
                )
            
                (fp_line (start -2.95 -1.35) (end -2.95 6.25) (width 0.1) (layer "F.Fab"))
                (fp_line (start -2.95 6.25) (end 2.95 6.25) (width 0.1) (layer "F.Fab"))
                (fp_line (start -2.25 -1.35) (end -2.95 -1.35) (width 0.1) (layer "F.Fab"))
                (fp_line (start -2.25 0.25) (end -2.25 -1.35) (width 0.1) (layer "F.Fab"))
                (fp_line (start 2.25 -1.35) (end 2.25 0.25) (width 0.1) (layer "F.Fab"))
                (fp_line (start 2.25 0.25) (end -2.25 0.25) (width 0.1) (layer "F.Fab"))
                (fp_line (start 2.95 -1.35) (end 2.25 -1.35) (width 0.1) (layer "F.Fab"))
                (fp_line (start 2.95 6.25) (end 2.95 -1.35) (width 0.1) (layer "F.Fab"))
        
                (fp_line (start -1.5 7.40) (end -0.5 7.40) (width 0.1) (layer "F.SilkS"))
                (fp_line (start 1.5 7.40) (end 0.5 7.40) (width 0.1) (layer "F.SilkS"))
                (fp_line (start 1 6.90) (end 1 7.90) (width 0.1) (layer "F.SilkS"))
                (fp_line (start -2.06 -1.46) (end -3.06 -1.46) (width 0.12) (layer "F.SilkS"))
                (fp_line (start -3.06 -1.46) (end -3.06 -0.46) (width 0.12) (layer "F.SilkS"))
                (fp_line (start 2.14 -1.46) (end 3.06 -1.46) (width 0.12) (layer "F.SilkS"))
                (fp_line (start 3.06 -1.46) (end 3.06 -0.46) (width 0.12) (layer "F.SilkS"))
                (fp_line (start -2.14 6.36) (end -3.06 6.36) (width 0.12) (layer "F.SilkS"))
                (fp_line (start -3.06 6.36) (end -3.06 5.36) (width 0.12) (layer "F.SilkS"))
                (fp_line (start 2.14 6.36) (end 3.06 6.36) (width 0.12) (layer "F.SilkS"))
                (fp_line (start 3.06 6.36) (end 3.06 5.36) (width 0.12) (layer "F.SilkS"))
        
                (fp_line (start -2.95 -1.35) (end -2.25 -1.35) (width 0.1) (layer "B.Fab"))
                (fp_line (start -2.95 6.25) (end -2.95 -1.35) (width 0.1) (layer "B.Fab"))
                (fp_line (start -2.25 -1.35) (end -2.25 0.25) (width 0.1) (layer "B.Fab"))
                (fp_line (start -2.25 0.25) (end 2.25 0.25) (width 0.1) (layer "B.Fab"))
                (fp_line (start 2.25 -1.35) (end 2.95 -1.35) (width 0.1) (layer "B.Fab"))
                (fp_line (start 2.25 0.25) (end 2.25 -1.35) (width 0.1) (layer "B.Fab"))
                (fp_line (start 2.95 -1.35) (end 2.95 6.25) (width 0.1) (layer "B.Fab"))
                (fp_line (start 2.95 6.25) (end -2.95 6.25) (width 0.1) (layer "B.Fab"))
        
                (fp_line (start 1.5 7.40) (end 0.5 7.40) (width 0.1) (layer "B.SilkS"))
                (fp_line (start -1.5 7.40) (end -0.5 7.40) (width 0.1) (layer "B.SilkS"))
                (fp_line (start -1 6.90) (end -1 7.90) (width 0.1) (layer "B.SilkS"))
                (fp_line (start -2.06 -1.46) (end -3.06 -1.46) (width 0.12) (layer "B.SilkS"))
                (fp_line (start -3.06 -1.46) (end -3.06 -0.46) (width 0.12) (layer "B.SilkS"))
                (fp_line (start 2.14 -1.46) (end 3.06 -1.46) (width 0.12) (layer "B.SilkS"))
                (fp_line (start 3.06 -1.46) (end 3.06 -0.46) (width 0.12) (layer "B.SilkS"))
                (fp_line (start -2.14 6.36) (end -3.06 6.36) (width 0.12) (layer "B.SilkS"))
                (fp_line (start -3.06 6.36) (end -3.06 5.36) (width 0.12) (layer "B.SilkS"))
                (fp_line (start 2.14 6.36) (end 3.06 6.36) (width 0.12) (layer "B.SilkS"))
                (fp_line (start 3.06 6.36) (end 3.06 5.36) (width 0.12) (layer "B.SilkS"))
        
                (pad 11 thru_hole oval (at -1 0 90) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask") (net 73 "JST1_1"))
                (pad 12 thru_hole oval (at 1 0 90) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask") (net 74 "JST1_2"))
                (pad 21 smd custom (at -1 1.8 270) (size 0.1 0.1) (layers "F.Cu" "F.Mask")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0.4)
                        (xy -0.6 0.4)
                        (xy -0.6 0.2)
                        (xy 0 -0.4)
                        (xy 0.6 0.2)
                        )   
                        (width 0))
                    )
                    (net 73 "JST1_1"))
                (pad 31 smd custom (at -1 1.8 270) (size 0.1 0.1) (layers "B.Cu" "B.Mask")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0.4)
                        (xy -0.6 0.4)
                        (xy -0.6 0.2)
                        (xy 0 -0.4)
                        (xy 0.6 0.2)
                        )
                        (width 0))
                    )
                    (net 73 "JST1_1"))
                (pad 22 smd custom (at 1 1.8 270) (size 0.1 0.1) (layers "F.Cu" "F.Mask")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0.4)
                        (xy -0.6 0.4)
                        (xy -0.6 0.2)
                        (xy 0 -0.4)
                        (xy 0.6 0.2)
                        )
                        (width 0))
                    )
                    (net 74 "JST1_2"))
                (pad 32 smd custom (at 1 1.8 270) (size 0.1 0.1) (layers "B.Cu" "B.Mask")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0.4)
                        (xy -0.6 0.4)
                        (xy -0.6 0.2)
                        (xy 0 -0.4)
                        (xy 0.6 0.2)
                        )
                        (width 0))
                    )
                    (net 74 "JST1_2"))
                (pad 1 smd custom (at -1 2.816 270) (size 1.2 0.5) (layers "F.Cu" "F.Mask") (net 72 "BAT_P")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0)
                        (xy -0.6 0)
                        (xy -0.6 1)
                        (xy 0 0.4)
                        (xy 0.6 1)
                        )
                        (width 0))
                    ) )
                (pad 1 smd custom (at 1 2.816 270) (size 1.2 0.5) (layers "B.Cu" "B.Mask") (net 72 "BAT_P")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0)
                        (xy -0.6 0)
                        (xy -0.6 1)
                        (xy 0 0.4)
                        (xy 0.6 1)
                        )
                        (width 0))
                    ) )
                (pad 2 smd custom (at -1 2.816 270) (size 1.2 0.5) (layers "B.Cu" "B.Mask") (net 33 "GND")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0)
                        (xy -0.6 0)
                        (xy -0.6 1)
                        (xy 0 0.4)
                        (xy 0.6 1)
                        )
                        (width 0))
                    ) )
                (pad 2 smd custom (at 1 2.816 270) (size 1.2 0.5) (layers "F.Cu" "F.Mask") (net 33 "GND")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0)
                        (xy -0.6 0)
                        (xy -0.6 1)
                        (xy 0 0.4)
                        (xy 0.6 1)
                        )
                        (width 0))
                    ) )
            
            )
         
        (segment (start 213.550 98.750) (end 211.750 98.750) (width 0.25) (layer "F.Cu") (net 73))
        (segment (start 213.550 98.750) (end 211.750 98.750) (width 0.25) (layer "B.Cu") (net 73))
        (segment (start 213.550 96.750) (end 211.750 96.750) (width 0.25) (layer "F.Cu") (net 74))
        (segment (start 213.550 96.750) (end 211.750 96.750) (width 0.25) (layer "B.Cu") (net 74))
        
            (gr_line (start 91.08198222285509 108.74001780012622) (end 91.08001777794281 53.49000464193523) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 91.58000462794281 52.98998684198348) (end 128.58001314999998 52.98901315754868) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 129.08 52.48901315754736) (end 129.08 48.74) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 129.58 48.24) (end 147.58 48.24) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 148.08 47.74) (end 148.08 46.488) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 148.58 45.988) (end 165.582 45.988) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 166.082 46.488) (end 166.082 47.74) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 166.582 48.24) (end 184.582 48.24) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 185.082 48.74) (end 185.082 50.238) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 185.582 50.738) (end 203.58222192628773 50.738) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 204.08222192628773 51.23777800000971) (end 204.08277807371226 52.49022199999308) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 224.518 113.996596) (end 210.97353193043912 137.45836746290388) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 210.29050971794075 137.64139668455357) (end 195.12364206223265 128.884801539137) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 194.9382670622326 128.82200823913698) (end 157.77296812333506 123.97775897688982) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 157.43351034067848 123.77643070068846) (end 146.98977558129695 109.44552227620129) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 146.5856927986404 109.24) (end 91.58198222285512 109.24) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 204.58277807371226 52.99) (end 224.333 52.99) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 224.833 53.49) (end 224.833 113.31702540612952) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 224.76601270000006 113.5670254061294) (end 224.518 113.996596) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 91.58001777794281 53.48998684156686) (end 91.58000457794282 52.98998684156686) (angle -90.00053289295953) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 128.58 52.48901315754736) (end 128.5800131 52.98901315754736) (angle -89.99849312100235) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 129.58 48.74) (end 129.58 48.24) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 147.58 47.74) (end 147.58 48.24) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 148.58 46.488) (end 148.58 45.988) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 165.582 46.488) (end 166.082 46.488) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 166.582 47.74) (end 166.082 47.74) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 184.582 48.74) (end 185.082 48.74) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 185.582 50.238) (end 185.082 50.238) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 203.58222192628773 51.238) (end 204.08222192628773 51.237778) (angle -89.97456067668081) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 204.58277807371226 52.48999999999069) (end 204.08277807371226 52.49022199999069) (angle -89.97456067529339) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 224.333 53.49) (end 224.833 53.49) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 224.333 113.31702540612952) (end 224.7660127 113.56702540612952) (angle -30.000000108401252) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 210.54050971794078 137.20838398455356) (end 210.29050971794078 137.64139668455357) (angle -90.00218462143252) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 194.87364206223262 129.31781423913696) (end 195.12364206223262 128.88480153913696) (angle -22.57374496727097) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 157.83759312333507 123.48195297688983) (end 157.43351032333507 123.77643067688983) (angle -46.490828368152734) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 146.5856927986404 109.73999999999998) (end 146.9897755986404 109.44552229999998) (angle -53.917083509298145) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 91.58198222285512 108.74) (end 91.08198222285512 108.74001779999999) (angle -89.99796025578533) (layer Edge.Cuts) (width 0.15))
            
)

        