
            
(kicad_pcb (version 20171130) (host pcbnew 5.1.6)

  (page A3)
  (title_block
    (title corney_island_wireless)
    (rev 0.1)
    (company ceoloide)
  )

  (general
    (thickness 1.6)
  )

  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

            (net 0 "")
(net 1 "C0")
(net 2 "outer_bottom")
(net 3 "outer_home")
(net 4 "outer_top")
(net 5 "C1")
(net 6 "pinky_bottom")
(net 7 "pinky_home")
(net 8 "pinky_top")
(net 9 "C2")
(net 10 "ring_bottom")
(net 11 "ring_home")
(net 12 "ring_top")
(net 13 "C3")
(net 14 "middle_bottom")
(net 15 "middle_home")
(net 16 "middle_top")
(net 17 "C4")
(net 18 "index_bottom")
(net 19 "index_home")
(net 20 "index_top")
(net 21 "C5")
(net 22 "inner_bottom")
(net 23 "inner_home")
(net 24 "inner_top")
(net 25 "near_home")
(net 26 "mid_home")
(net 27 "far_home")
(net 28 "R2")
(net 29 "R1")
(net 30 "R0")
(net 31 "R3")
(net 32 "RAW")
(net 33 "GND")
(net 34 "RST")
(net 35 "VCC")
(net 36 "P16")
(net 37 "P10")
(net 38 "LED")
(net 39 "DAT")
(net 40 "SDA")
(net 41 "SCL")
(net 42 "CS")
(net 43 "P9")
(net 44 "MCU1_24")
(net 45 "MCU1_1")
(net 46 "MCU1_23")
(net 47 "MCU1_2")
(net 48 "MCU1_22")
(net 49 "MCU1_3")
(net 50 "MCU1_21")
(net 51 "MCU1_4")
(net 52 "MCU1_20")
(net 53 "MCU1_5")
(net 54 "MCU1_19")
(net 55 "MCU1_6")
(net 56 "MCU1_18")
(net 57 "MCU1_7")
(net 58 "MCU1_17")
(net 59 "MCU1_8")
(net 60 "MCU1_16")
(net 61 "MCU1_9")
(net 62 "MCU1_15")
(net 63 "MCU1_10")
(net 64 "MCU1_14")
(net 65 "MCU1_11")
(net 66 "MCU1_13")
(net 67 "MCU1_12")
(net 68 "DISP1_1")
(net 69 "DISP1_2")
(net 70 "DISP1_4")
(net 71 "DISP1_5")
(net 72 "BAT_P")
(net 73 "JST1_1")
(net 74 "JST1_2")
            
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "")
(add_net "C0")
(add_net "outer_bottom")
(add_net "outer_home")
(add_net "outer_top")
(add_net "C1")
(add_net "pinky_bottom")
(add_net "pinky_home")
(add_net "pinky_top")
(add_net "C2")
(add_net "ring_bottom")
(add_net "ring_home")
(add_net "ring_top")
(add_net "C3")
(add_net "middle_bottom")
(add_net "middle_home")
(add_net "middle_top")
(add_net "C4")
(add_net "index_bottom")
(add_net "index_home")
(add_net "index_top")
(add_net "C5")
(add_net "inner_bottom")
(add_net "inner_home")
(add_net "inner_top")
(add_net "near_home")
(add_net "mid_home")
(add_net "far_home")
(add_net "R2")
(add_net "R1")
(add_net "R0")
(add_net "R3")
(add_net "RAW")
(add_net "GND")
(add_net "RST")
(add_net "VCC")
(add_net "P16")
(add_net "P10")
(add_net "LED")
(add_net "DAT")
(add_net "SDA")
(add_net "SCL")
(add_net "CS")
(add_net "P9")
(add_net "MCU1_24")
(add_net "MCU1_1")
(add_net "MCU1_23")
(add_net "MCU1_2")
(add_net "MCU1_22")
(add_net "MCU1_3")
(add_net "MCU1_21")
(add_net "MCU1_4")
(add_net "MCU1_20")
(add_net "MCU1_5")
(add_net "MCU1_19")
(add_net "MCU1_6")
(add_net "MCU1_18")
(add_net "MCU1_7")
(add_net "MCU1_17")
(add_net "MCU1_8")
(add_net "MCU1_16")
(add_net "MCU1_9")
(add_net "MCU1_15")
(add_net "MCU1_10")
(add_net "MCU1_14")
(add_net "MCU1_11")
(add_net "MCU1_13")
(add_net "MCU1_12")
(add_net "DISP1_1")
(add_net "DISP1_2")
(add_net "DISP1_4")
(add_net "DISP1_5")
(add_net "BAT_P")
(add_net "JST1_1")
(add_net "JST1_2")
  )

            
        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 100 100 0)

      
      (fp_text reference "S1" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 1 "C0"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 2 "outer_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 1 "C0"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 2 "outer_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 100 81 0)

      
      (fp_text reference "S2" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 1 "C0"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 3 "outer_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 1 "C0"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 3 "outer_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 100 62 0)

      
      (fp_text reference "S3" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 1 "C0"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 4 "outer_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 1 "C0"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 4 "outer_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 119 100 0)

      
      (fp_text reference "S4" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 5 "C1"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 6 "pinky_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 5 "C1"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 6 "pinky_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 119 81 0)

      
      (fp_text reference "S5" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 5 "C1"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 7 "pinky_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 5 "C1"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 7 "pinky_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 119 62 0)

      
      (fp_text reference "S6" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 5 "C1"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 8 "pinky_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 5 "C1"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 8 "pinky_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 138 95.25 0)

      
      (fp_text reference "S7" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 9 "C2"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 10 "ring_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 9 "C2"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 10 "ring_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 138 76.25 0)

      
      (fp_text reference "S8" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 9 "C2"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 11 "ring_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 9 "C2"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 11 "ring_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 138 57.25 0)

      
      (fp_text reference "S9" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 9 "C2"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 12 "ring_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 9 "C2"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 12 "ring_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 157 92.875 0)

      
      (fp_text reference "S10" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 13 "C3"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 14 "middle_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 13 "C3"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 14 "middle_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 157 73.875 0)

      
      (fp_text reference "S11" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 13 "C3"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 15 "middle_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 13 "C3"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 15 "middle_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 157 54.875 0)

      
      (fp_text reference "S12" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 13 "C3"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 16 "middle_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 13 "C3"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 16 "middle_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 176 95.25 0)

      
      (fp_text reference "S13" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 17 "C4"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 18 "index_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 17 "C4"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 18 "index_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 176 76.25 0)

      
      (fp_text reference "S14" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 17 "C4"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 19 "index_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 17 "C4"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 19 "index_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 176 57.25 0)

      
      (fp_text reference "S15" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 17 "C4"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 20 "index_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 17 "C4"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 20 "index_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 195 97.625 0)

      
      (fp_text reference "S16" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 21 "C5"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 22 "inner_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 21 "C5"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 22 "inner_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 195 78.625 0)

      
      (fp_text reference "S17" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 21 "C5"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 23 "inner_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 21 "C5"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 23 "inner_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 195 59.625 0)

      
      (fp_text reference "S18" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 21 "C5"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 24 "inner_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 21 "C5"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 24 "inner_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 166.5 114.875 0)

      
      (fp_text reference "S19" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 13 "C3"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 25 "near_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 13 "C3"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 25 "near_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 187.5 117.625 -15)

      
      (fp_text reference "S20" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 -15) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 17 "C4"))
        (pad 2 smd rect (at 5.842 -5.08 -15) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 26 "mid_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 -15) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 17 "C4"))
        (pad 2 smd rect (at -5.842 -5.08 -15) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 26 "mid_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 209.7468058 121.3891576 60)

      
      (fp_text reference "S21" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 60) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 21 "C5"))
        (pad 2 smd rect (at 5.842 -5.08 60) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 27 "far_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 60) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 21 "C5"))
        (pad 2 smd rect (at -5.842 -5.08 60) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 27 "far_home"))
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 107 98.675 90)
            (fp_text reference "D1" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 2 "outer_bottom"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "R2"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 107 79.675 90)
            (fp_text reference "D2" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 3 "outer_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "R1"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 107 60.675 90)
            (fp_text reference "D3" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 4 "outer_top"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "R0"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 126 98.675 90)
            (fp_text reference "D4" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 6 "pinky_bottom"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "R2"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 126 79.675 90)
            (fp_text reference "D5" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 7 "pinky_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "R1"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 126 60.675 90)
            (fp_text reference "D6" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 8 "pinky_top"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "R0"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 145 93.925 90)
            (fp_text reference "D7" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 10 "ring_bottom"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "R2"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 145 74.925 90)
            (fp_text reference "D8" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 11 "ring_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "R1"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 145 55.925 90)
            (fp_text reference "D9" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 12 "ring_top"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "R0"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 164 91.55 90)
            (fp_text reference "D10" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 14 "middle_bottom"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "R2"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 164 72.55 90)
            (fp_text reference "D11" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 15 "middle_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "R1"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 164 53.55 90)
            (fp_text reference "D12" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 16 "middle_top"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "R0"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 183 93.925 90)
            (fp_text reference "D13" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 18 "index_bottom"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "R2"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 183 74.925 90)
            (fp_text reference "D14" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 19 "index_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "R1"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 183 55.925 90)
            (fp_text reference "D15" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 20 "index_top"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "R0"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 202 96.3 90)
            (fp_text reference "D16" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 22 "inner_bottom"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "R2"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 202 77.3 90)
            (fp_text reference "D17" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 23 "inner_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "R1"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 202 58.3 90)
            (fp_text reference "D18" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 24 "inner_top"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "R0"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 173.5 113.55 90)
            (fp_text reference "D19" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 25 "near_home"))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 31 "R3"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 194.604416 118.1568816 75)
            (fp_text reference "D20" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 75) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 26 "mid_home"))
            (pad 1 smd rect (at -1.65 0 75) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 31 "R3"))
        
        )
        

        (module ComboDiode (layer B.Cu) (tedit 5B24D78E)
            (at 212.0993221 114.66447980000001 150)
            (fp_text reference "D21" (at 0 0) (layer B.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))
            (pad 2 smd rect (at 1.65 0 150) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 27 "far_home"))
            (pad 1 smd rect (at -1.65 0 150) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 31 "R3"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 93 98.675 90)
            (fp_text reference "D22" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "R2"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 2 "outer_bottom"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 93 79.675 90)
            (fp_text reference "D23" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "R1"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 3 "outer_home"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 93 60.675 90)
            (fp_text reference "D24" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "R0"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 4 "outer_top"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 112 98.675 90)
            (fp_text reference "D25" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "R2"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 6 "pinky_bottom"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 112 79.675 90)
            (fp_text reference "D26" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "R1"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 7 "pinky_home"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 112 60.675 90)
            (fp_text reference "D27" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "R0"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 8 "pinky_top"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 131 93.925 90)
            (fp_text reference "D28" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "R2"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 10 "ring_bottom"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 131 74.925 90)
            (fp_text reference "D29" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "R1"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 11 "ring_home"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 131 55.925 90)
            (fp_text reference "D30" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "R0"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 12 "ring_top"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 150 91.55 90)
            (fp_text reference "D31" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "R2"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 14 "middle_bottom"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 150 72.55 90)
            (fp_text reference "D32" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "R1"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 15 "middle_home"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 150 53.55 90)
            (fp_text reference "D33" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "R0"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 16 "middle_top"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 169 93.925 90)
            (fp_text reference "D34" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "R2"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 18 "index_bottom"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 169 74.925 90)
            (fp_text reference "D35" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "R1"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 19 "index_home"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 169 55.925 90)
            (fp_text reference "D36" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "R0"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 20 "index_top"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 188 96.3 90)
            (fp_text reference "D37" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "R2"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 22 "inner_bottom"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 188 77.3 90)
            (fp_text reference "D38" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "R1"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 23 "inner_home"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 188 58.3 90)
            (fp_text reference "D39" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "R0"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 24 "inner_top"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 159.5 113.55 90)
            (fp_text reference "D40" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 31 "R3"))
            (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 25 "near_home"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 181.0814545 114.533415 75)
            (fp_text reference "D41" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 75) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 31 "R3"))
            (pad 2 smd rect (at 1.65 0 75) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 26 "mid_home"))
        
        )
        

        (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
            (at 205.0993221 126.78883540000001 150)
            (fp_text reference "D42" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
            (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
            (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
            (pad 1 smd rect (at -1.65 0 150) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 31 "R3"))
            (pad 2 smd rect (at 1.65 0 150) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 27 "far_home"))
        
        )
        

          
          
        (module nice_nano (layer F.Cu) (tedit 6451A4F1)
          (attr virtual)
          (at 214.704 70.87 0)
          (fp_text reference "MCU1" (at 0 -15) (layer F.SilkS) hide
            (effects (font (size 1 1) (thickness 0.15)))
          )

          
          (fp_line (start 3.556 -18.034) (end 3.556 -16.51) (layer Dwgs.User) (width 0.15))
          (fp_line (start -3.81 -16.51) (end -3.81 -18.034) (layer Dwgs.User) (width 0.15))
          (fp_line (start -3.81 -18.034) (end 3.556 -18.034) (layer Dwgs.User) (width 0.15))


          
          (fp_line (start -8.89 -16.51) (end 8.89 -16.51) (layer F.Fab) (width 0.12))
          (fp_line (start -8.89 -16.51) (end -8.89 -14) (layer F.Fab) (width 0.12))
          (fp_line (start 8.89 -16.51) (end 8.89 -14) (layer F.Fab) (width 0.12))
          (fp_line (start -8.89 -16.5) (end -8.89 -13.99) (layer B.Fab) (width 0.12))
          (fp_line (start 8.89 -16.51) (end 8.89 -14) (layer B.Fab) (width 0.12))
          (fp_line (start -8.89 -16.51) (end 8.89 -16.51) (layer B.Fab) (width 0.12))

          
          (fp_line (start 6.29 -11.43) (end 8.95 -11.43) (layer F.SilkS) (width 0.12))
          (fp_line (start 6.29 -14.03) (end 8.95 -14.03) (layer F.SilkS) (width 0.12))
          (fp_line (start 6.29 -14.03) (end 6.29 16.57) (layer F.SilkS) (width 0.12))
          (fp_line (start 6.29 16.57) (end 8.95 16.57) (layer F.SilkS) (width 0.12))
          (fp_line (start 8.95 -14.03) (end 8.95 16.57) (layer F.SilkS) (width 0.12))
          (fp_line (start -8.95 -14.03) (end -6.29 -14.03) (layer F.SilkS) (width 0.12))
          (fp_line (start -8.95 -14.03) (end -8.95 16.57) (layer F.SilkS) (width 0.12))
          (fp_line (start -8.95 16.57) (end -6.29 16.57) (layer F.SilkS) (width 0.12))
          (fp_line (start -6.29 -14.03) (end -6.29 16.57) (layer F.SilkS) (width 0.12))
          (fp_line (start -8.95 -11.43) (end -6.29 -11.43) (layer B.SilkS) (width 0.12))
          (fp_line (start -6.29 -14.03) (end -8.95 -14.03) (layer B.SilkS) (width 0.12))
          (fp_line (start -6.29 -14.03) (end -6.29 16.57) (layer B.SilkS) (width 0.12))
          (fp_line (start -6.29 16.57) (end -8.95 16.57) (layer B.SilkS) (width 0.12))
          (fp_line (start -8.95 -14.03) (end -8.95 16.57) (layer B.SilkS) (width 0.12))
          (fp_line (start 8.95 -14.03) (end 6.29 -14.03) (layer B.SilkS) (width 0.12))
          (fp_line (start 8.95 -14.03) (end 8.95 16.57) (layer B.SilkS) (width 0.12))
          (fp_line (start 8.95 16.57) (end 6.29 16.57) (layer B.SilkS) (width 0.12))
          (fp_line (start 6.29 -14.03) (end 6.29 16.57) (layer B.SilkS) (width 0.12))
      
          
          
          (pad 24 thru_hole circle (at -7.62 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 44 "MCU1_24"))
          (pad 1 thru_hole circle (at 7.62 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 45 "MCU1_1"))

          
          (pad 124 thru_hole circle (at -3.262 -12.7) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 38 "LED"))
          (pad 1 thru_hole circle (at 3.262 -12.7) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 32 "RAW"))

          
          (pad 24 smd custom (at -5.5 -12.7) (size 0.2 0.2) (layers F.Cu F.Mask) (net 44 "MCU1_24")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))
          (pad 124 smd custom (at -4.775 -12.7) (size 0.2 0.2) (layers F.Cu F.Mask) (net 38 "LED")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 1 smd custom (at 4.775 -12.7 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 32 "RAW")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 1 smd custom (at 5.5 -12.7 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 45 "MCU1_1")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))

          
          (pad 24 smd custom (at -5.5 -12.7) (size 0.2 0.2) (layers B.Cu B.Mask) (net 44 "MCU1_24")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))

          (pad 1 smd custom (at -4.775 -12.7) (size 0.2 0.2) (layers B.Cu B.Mask) (net 32 "RAW")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 124 smd custom (at 4.775 -12.7 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 38 "LED")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 1 smd custom (at 5.5 -12.7 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 45 "MCU1_1")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))
        

            
            (fp_text user RAW (at -3 -12.7) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user LED (at 3 -12.7) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user LED (at -3 -12.7 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user RAW (at 3 -12.7 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user LED (at -3.262 -13.5) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user RAW (at 3.262 -13.5) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user LED (at -3.262 -13.5 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user RAW (at 3.262 -13.5 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
          (pad 23 thru_hole circle (at -7.62 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 46 "MCU1_23"))
          (pad 2 thru_hole circle (at 7.62 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 47 "MCU1_2"))

          
          (pad 123 thru_hole circle (at -3.262 -10.16) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 39 "DAT"))
          (pad 2 thru_hole circle (at 3.262 -10.16) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 33 "GND"))

          
          (pad 23 smd custom (at -5.5 -10.16) (size 0.2 0.2) (layers F.Cu F.Mask) (net 46 "MCU1_23")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))
          (pad 123 smd custom (at -4.775 -10.16) (size 0.2 0.2) (layers F.Cu F.Mask) (net 39 "DAT")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 2 smd custom (at 4.775 -10.16 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 33 "GND")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 2 smd custom (at 5.5 -10.16 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 47 "MCU1_2")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))

          
          (pad 23 smd custom (at -5.5 -10.16) (size 0.2 0.2) (layers B.Cu B.Mask) (net 46 "MCU1_23")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))

          (pad 2 smd custom (at -4.775 -10.16) (size 0.2 0.2) (layers B.Cu B.Mask) (net 33 "GND")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 123 smd custom (at 4.775 -10.16 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 39 "DAT")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 2 smd custom (at 5.5 -10.16 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 47 "MCU1_2")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))
        

            
            (fp_text user GND (at -3 -10.16) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user DAT (at 3 -10.16) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user DAT (at -3 -10.16 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user GND (at 3 -10.16 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user DAT (at -3.262 -10.96) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user GND (at 3.262 -10.96) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user DAT (at -3.262 -10.96 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user GND (at 3.262 -10.96 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
          (pad 22 thru_hole circle (at -7.62 -7.619999999999999) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 48 "MCU1_22"))
          (pad 3 thru_hole circle (at 7.62 -7.619999999999999) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 49 "MCU1_3"))

          
          (pad 122 thru_hole circle (at -3.262 -7.619999999999999) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 33 "GND"))
          (pad 3 thru_hole circle (at 3.262 -7.619999999999999) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 34 "RST"))

          
          (pad 22 smd custom (at -5.5 -7.619999999999999) (size 0.2 0.2) (layers F.Cu F.Mask) (net 48 "MCU1_22")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))
          (pad 122 smd custom (at -4.775 -7.619999999999999) (size 0.2 0.2) (layers F.Cu F.Mask) (net 33 "GND")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 3 smd custom (at 4.775 -7.619999999999999 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 34 "RST")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 3 smd custom (at 5.5 -7.619999999999999 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 49 "MCU1_3")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))

          
          (pad 22 smd custom (at -5.5 -7.619999999999999) (size 0.2 0.2) (layers B.Cu B.Mask) (net 48 "MCU1_22")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))

          (pad 3 smd custom (at -4.775 -7.619999999999999) (size 0.2 0.2) (layers B.Cu B.Mask) (net 34 "RST")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 122 smd custom (at 4.775 -7.619999999999999 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 33 "GND")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 3 smd custom (at 5.5 -7.619999999999999 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 49 "MCU1_3")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))
        

            
            (fp_text user RST (at -3 -7.619999999999999) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user GND (at 3 -7.619999999999999) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user GND (at -3 -7.619999999999999 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user RST (at 3 -7.619999999999999 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user GND (at -3.262 -8.42) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user RST (at 3.262 -8.42) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user GND (at -3.262 -8.42 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user RST (at 3.262 -8.42 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
          (pad 21 thru_hole circle (at -7.62 -5.079999999999999) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 50 "MCU1_21"))
          (pad 4 thru_hole circle (at 7.62 -5.079999999999999) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 51 "MCU1_4"))

          
          (pad 121 thru_hole circle (at -3.262 -5.079999999999999) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 33 "GND"))
          (pad 4 thru_hole circle (at 3.262 -5.079999999999999) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 35 "VCC"))

          
          (pad 21 smd custom (at -5.5 -5.079999999999999) (size 0.2 0.2) (layers F.Cu F.Mask) (net 50 "MCU1_21")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))
          (pad 121 smd custom (at -4.775 -5.079999999999999) (size 0.2 0.2) (layers F.Cu F.Mask) (net 33 "GND")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 4 smd custom (at 4.775 -5.079999999999999 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 35 "VCC")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 4 smd custom (at 5.5 -5.079999999999999 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 51 "MCU1_4")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))

          
          (pad 21 smd custom (at -5.5 -5.079999999999999) (size 0.2 0.2) (layers B.Cu B.Mask) (net 50 "MCU1_21")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))

          (pad 4 smd custom (at -4.775 -5.079999999999999) (size 0.2 0.2) (layers B.Cu B.Mask) (net 35 "VCC")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 121 smd custom (at 4.775 -5.079999999999999 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 33 "GND")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 4 smd custom (at 5.5 -5.079999999999999 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 51 "MCU1_4")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))
        

            
            (fp_text user VCC (at -3 -5.079999999999999) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user GND (at 3 -5.079999999999999) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user GND (at -3 -5.079999999999999 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user VCC (at 3 -5.079999999999999 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user GND (at -3.262 -5.88) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user VCC (at 3.262 -5.88) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user GND (at -3.262 -5.88 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user VCC (at 3.262 -5.88 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
          (pad 20 thru_hole circle (at -7.62 -2.539999999999999) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 52 "MCU1_20"))
          (pad 5 thru_hole circle (at 7.62 -2.539999999999999) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 53 "MCU1_5"))

          
          (pad 120 thru_hole circle (at -3.262 -2.539999999999999) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 40 "SDA"))
          (pad 5 thru_hole circle (at 3.262 -2.539999999999999) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 1 "C0"))

          
          (pad 20 smd custom (at -5.5 -2.539999999999999) (size 0.2 0.2) (layers F.Cu F.Mask) (net 52 "MCU1_20")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))
          (pad 120 smd custom (at -4.775 -2.539999999999999) (size 0.2 0.2) (layers F.Cu F.Mask) (net 40 "SDA")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 5 smd custom (at 4.775 -2.539999999999999 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 1 "C0")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 5 smd custom (at 5.5 -2.539999999999999 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 53 "MCU1_5")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))

          
          (pad 20 smd custom (at -5.5 -2.539999999999999) (size 0.2 0.2) (layers B.Cu B.Mask) (net 52 "MCU1_20")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))

          (pad 5 smd custom (at -4.775 -2.539999999999999) (size 0.2 0.2) (layers B.Cu B.Mask) (net 1 "C0")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 120 smd custom (at 4.775 -2.539999999999999 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 40 "SDA")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 5 smd custom (at 5.5 -2.539999999999999 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 53 "MCU1_5")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))
        

            
            (fp_text user C0 (at -3 -2.539999999999999) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user SDA (at 3 -2.539999999999999) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user SDA (at -3 -2.539999999999999 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user C0 (at 3 -2.539999999999999 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user SDA (at -3.262 -3.34) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user C0 (at 3.262 -3.34) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user SDA (at -3.262 -3.34 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user C0 (at 3.262 -3.34 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
          (pad 19 thru_hole circle (at -7.62 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 54 "MCU1_19"))
          (pad 6 thru_hole circle (at 7.62 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 55 "MCU1_6"))

          
          (pad 119 thru_hole circle (at -3.262 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 41 "SCL"))
          (pad 6 thru_hole circle (at 3.262 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 5 "C1"))

          
          (pad 19 smd custom (at -5.5 0) (size 0.2 0.2) (layers F.Cu F.Mask) (net 54 "MCU1_19")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))
          (pad 119 smd custom (at -4.775 0) (size 0.2 0.2) (layers F.Cu F.Mask) (net 41 "SCL")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 6 smd custom (at 4.775 0 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 5 "C1")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 6 smd custom (at 5.5 0 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 55 "MCU1_6")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))

          
          (pad 19 smd custom (at -5.5 0) (size 0.2 0.2) (layers B.Cu B.Mask) (net 54 "MCU1_19")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))

          (pad 6 smd custom (at -4.775 0) (size 0.2 0.2) (layers B.Cu B.Mask) (net 5 "C1")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 119 smd custom (at 4.775 0 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 41 "SCL")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 6 smd custom (at 5.5 0 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 55 "MCU1_6")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))
        

            
            (fp_text user C1 (at -3 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user SCL (at 3 0) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user SCL (at -3 0 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user C1 (at 3 0 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user SCL (at -3.262 -0.8000000000000007) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user C1 (at 3.262 -0.8000000000000007) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user SCL (at -3.262 -0.8000000000000007 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user C1 (at 3.262 -0.8000000000000007 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
          (pad 18 thru_hole circle (at -7.62 2.540000000000001) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 56 "MCU1_18"))
          (pad 7 thru_hole circle (at 7.62 2.540000000000001) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 57 "MCU1_7"))

          
          (pad 118 thru_hole circle (at -3.262 2.540000000000001) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 42 "CS"))
          (pad 7 thru_hole circle (at 3.262 2.540000000000001) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 9 "C2"))

          
          (pad 18 smd custom (at -5.5 2.540000000000001) (size 0.2 0.2) (layers F.Cu F.Mask) (net 56 "MCU1_18")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))
          (pad 118 smd custom (at -4.775 2.540000000000001) (size 0.2 0.2) (layers F.Cu F.Mask) (net 42 "CS")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 7 smd custom (at 4.775 2.540000000000001 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 9 "C2")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 7 smd custom (at 5.5 2.540000000000001 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 57 "MCU1_7")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))

          
          (pad 18 smd custom (at -5.5 2.540000000000001) (size 0.2 0.2) (layers B.Cu B.Mask) (net 56 "MCU1_18")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))

          (pad 7 smd custom (at -4.775 2.540000000000001) (size 0.2 0.2) (layers B.Cu B.Mask) (net 9 "C2")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 118 smd custom (at 4.775 2.540000000000001 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 42 "CS")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 7 smd custom (at 5.5 2.540000000000001 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 57 "MCU1_7")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))
        

            
            (fp_text user C2 (at -3 2.540000000000001) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user CS (at 3 2.540000000000001) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user CS (at -3 2.540000000000001 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user C2 (at 3 2.540000000000001 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user CS (at -3.262 1.7400000000000002) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user C2 (at 3.262 1.7400000000000002) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user CS (at -3.262 1.7400000000000002 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user C2 (at 3.262 1.7400000000000002 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
          (pad 17 thru_hole circle (at -7.62 5.080000000000002) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 58 "MCU1_17"))
          (pad 8 thru_hole circle (at 7.62 5.080000000000002) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 59 "MCU1_8"))

          
          (pad 117 thru_hole circle (at -3.262 5.080000000000002) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 30 "R0"))
          (pad 8 thru_hole circle (at 3.262 5.080000000000002) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 13 "C3"))

          
          (pad 17 smd custom (at -5.5 5.080000000000002) (size 0.2 0.2) (layers F.Cu F.Mask) (net 58 "MCU1_17")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))
          (pad 117 smd custom (at -4.775 5.080000000000002) (size 0.2 0.2) (layers F.Cu F.Mask) (net 30 "R0")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 8 smd custom (at 4.775 5.080000000000002 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 13 "C3")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 8 smd custom (at 5.5 5.080000000000002 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 59 "MCU1_8")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))

          
          (pad 17 smd custom (at -5.5 5.080000000000002) (size 0.2 0.2) (layers B.Cu B.Mask) (net 58 "MCU1_17")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))

          (pad 8 smd custom (at -4.775 5.080000000000002) (size 0.2 0.2) (layers B.Cu B.Mask) (net 13 "C3")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 117 smd custom (at 4.775 5.080000000000002 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 30 "R0")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 8 smd custom (at 5.5 5.080000000000002 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 59 "MCU1_8")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))
        

            
            (fp_text user C3 (at -3 5.080000000000002) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user R0 (at 3 5.080000000000002) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user R0 (at -3 5.080000000000002 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user C3 (at 3 5.080000000000002 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user R0 (at -3.262 4.280000000000001) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user C3 (at 3.262 4.280000000000001) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user R0 (at -3.262 4.280000000000001 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user C3 (at 3.262 4.280000000000001 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
          (pad 16 thru_hole circle (at -7.62 7.620000000000001) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 60 "MCU1_16"))
          (pad 9 thru_hole circle (at 7.62 7.620000000000001) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 61 "MCU1_9"))

          
          (pad 116 thru_hole circle (at -3.262 7.620000000000001) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 29 "R1"))
          (pad 9 thru_hole circle (at 3.262 7.620000000000001) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 17 "C4"))

          
          (pad 16 smd custom (at -5.5 7.620000000000001) (size 0.2 0.2) (layers F.Cu F.Mask) (net 60 "MCU1_16")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))
          (pad 116 smd custom (at -4.775 7.620000000000001) (size 0.2 0.2) (layers F.Cu F.Mask) (net 29 "R1")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 9 smd custom (at 4.775 7.620000000000001 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 17 "C4")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 9 smd custom (at 5.5 7.620000000000001 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 61 "MCU1_9")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))

          
          (pad 16 smd custom (at -5.5 7.620000000000001) (size 0.2 0.2) (layers B.Cu B.Mask) (net 60 "MCU1_16")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))

          (pad 9 smd custom (at -4.775 7.620000000000001) (size 0.2 0.2) (layers B.Cu B.Mask) (net 17 "C4")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 116 smd custom (at 4.775 7.620000000000001 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 29 "R1")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 9 smd custom (at 5.5 7.620000000000001 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 61 "MCU1_9")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))
        

            
            (fp_text user C4 (at -3 7.620000000000001) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user R1 (at 3 7.620000000000001) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user R1 (at -3 7.620000000000001 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user C4 (at 3 7.620000000000001 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user R1 (at -3.262 6.82) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user C4 (at 3.262 6.82) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user R1 (at -3.262 6.82 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user C4 (at 3.262 6.82 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
          (pad 15 thru_hole circle (at -7.62 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 62 "MCU1_15"))
          (pad 10 thru_hole circle (at 7.62 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 63 "MCU1_10"))

          
          (pad 115 thru_hole circle (at -3.262 10.16) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 28 "R2"))
          (pad 10 thru_hole circle (at 3.262 10.16) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 21 "C5"))

          
          (pad 15 smd custom (at -5.5 10.16) (size 0.2 0.2) (layers F.Cu F.Mask) (net 62 "MCU1_15")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))
          (pad 115 smd custom (at -4.775 10.16) (size 0.2 0.2) (layers F.Cu F.Mask) (net 28 "R2")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 10 smd custom (at 4.775 10.16 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 21 "C5")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 10 smd custom (at 5.5 10.16 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 63 "MCU1_10")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))

          
          (pad 15 smd custom (at -5.5 10.16) (size 0.2 0.2) (layers B.Cu B.Mask) (net 62 "MCU1_15")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))

          (pad 10 smd custom (at -4.775 10.16) (size 0.2 0.2) (layers B.Cu B.Mask) (net 21 "C5")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 115 smd custom (at 4.775 10.16 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 28 "R2")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 10 smd custom (at 5.5 10.16 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 63 "MCU1_10")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))
        

            
            (fp_text user C5 (at -3 10.16) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user R2 (at 3 10.16) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user R2 (at -3 10.16 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user C5 (at 3 10.16 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user R2 (at -3.262 9.36) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user C5 (at 3.262 9.36) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user R2 (at -3.262 9.36 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user C5 (at 3.262 9.36 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
          (pad 14 thru_hole circle (at -7.62 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 64 "MCU1_14"))
          (pad 11 thru_hole circle (at 7.62 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 65 "MCU1_11"))

          
          (pad 114 thru_hole circle (at -3.262 12.7) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 31 "R3"))
          (pad 11 thru_hole circle (at 3.262 12.7) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 36 "P16"))

          
          (pad 14 smd custom (at -5.5 12.7) (size 0.2 0.2) (layers F.Cu F.Mask) (net 64 "MCU1_14")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))
          (pad 114 smd custom (at -4.775 12.7) (size 0.2 0.2) (layers F.Cu F.Mask) (net 31 "R3")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 11 smd custom (at 4.775 12.7 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 36 "P16")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 11 smd custom (at 5.5 12.7 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 65 "MCU1_11")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))

          
          (pad 14 smd custom (at -5.5 12.7) (size 0.2 0.2) (layers B.Cu B.Mask) (net 64 "MCU1_14")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))

          (pad 11 smd custom (at -4.775 12.7) (size 0.2 0.2) (layers B.Cu B.Mask) (net 36 "P16")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 114 smd custom (at 4.775 12.7 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 31 "R3")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 11 smd custom (at 5.5 12.7 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 65 "MCU1_11")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))
        

            
            (fp_text user P16 (at -3 12.7) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user R3 (at 3 12.7) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user R3 (at -3 12.7 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user P16 (at 3 12.7 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user R3 (at -3.262 11.899999999999999) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user P16 (at 3.262 11.899999999999999) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user R3 (at -3.262 11.899999999999999 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user P16 (at 3.262 11.899999999999999 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
          (pad 13 thru_hole circle (at -7.62 15.240000000000002) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 66 "MCU1_13"))
          (pad 12 thru_hole circle (at 7.62 15.240000000000002) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 67 "MCU1_12"))

          
          (pad 113 thru_hole circle (at -3.262 15.240000000000002) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 43 "P9"))
          (pad 12 thru_hole circle (at 3.262 15.240000000000002) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask) (net 37 "P10"))

          
          (pad 13 smd custom (at -5.5 15.240000000000002) (size 0.2 0.2) (layers F.Cu F.Mask) (net 66 "MCU1_13")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))
          (pad 113 smd custom (at -4.775 15.240000000000002) (size 0.2 0.2) (layers F.Cu F.Mask) (net 43 "P9")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 12 smd custom (at 4.775 15.240000000000002 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 37 "P10")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 -0.625) (xy 0.5 -0.625) (xy 0.5 0.625) (xy -0.65 0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 12 smd custom (at 5.5 15.240000000000002 180) (size 0.2 0.2) (layers F.Cu F.Mask) (net 67 "MCU1_12")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 -0.625) (xy -0.25 -0.625) (xy 0.25 0) (xy -0.25 0.625) (xy -0.5 0.625)
            ) (width 0))
          ))

          
          (pad 13 smd custom (at -5.5 15.240000000000002) (size 0.2 0.2) (layers B.Cu B.Mask) (net 66 "MCU1_13")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))

          (pad 12 smd custom (at -4.775 15.240000000000002) (size 0.2 0.2) (layers B.Cu B.Mask) (net 37 "P10")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))

          
          (pad 113 smd custom (at 4.775 15.240000000000002 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 43 "P9")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.65 0.625) (xy 0.5 0.625) (xy 0.5 -0.625) (xy -0.65 -0.625) (xy -0.15 0)
            ) (width 0))
          ))
          (pad 12 smd custom (at 5.5 15.240000000000002 180) (size 0.2 0.2) (layers B.Cu B.Mask) (net 67 "MCU1_12")
            (zone_connect 2)
            (options (clearance outline) (anchor rect))
            (primitives
              (gr_poly (pts
                (xy -0.5 0.625) (xy -0.25 0.625) (xy 0.25 0) (xy -0.25 -0.625) (xy -0.5 -0.625)
            ) (width 0))
          ))
        

            
            (fp_text user P10 (at -3 15.240000000000002) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left))
            )
            (fp_text user P9 (at 3 15.240000000000002) (layer F.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right))
            )

            
            (fp_text user P9 (at -3 15.240000000000002 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
            )
            (fp_text user P10 (at 3 15.240000000000002 180) (layer B.SilkS)
              (effects (font (size 1 1) (thickness 0.15)) (justify left mirror))
            )
          
            
            (fp_text user P9 (at -3.262 14.440000000000001) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )
            (fp_text user P10 (at 3.262 14.440000000000001) (layer F.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)))
            )

            
            (fp_text user P9 (at -3.262 14.440000000000001 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
            (fp_text user P10 (at 3.262 14.440000000000001 180) (layer B.Fab)
              (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
            )
          
          
        )

        
        
          (segment (start 219.479 58.170) (end 217.966 58.170) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.369 58.170) (end 211.094 58.895) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 58.170) (end 210.369 58.170) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.094 58.895) (end 211.790 58.895) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 58.518) (end 212.167 58.507) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.790 58.895) (end 212.167 58.518) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 58.507) (end 212.254 58.420) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 217.716 58.420) (end 217.966 58.170) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.254 58.420) (end 217.716 58.420) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 58.170) (end 211.442 58.170) (width 0.25) (layer F.Cu) (net 13))
          (segment (start 218.314 57.445) (end 217.618 57.445) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.039 58.170) (end 218.314 57.445) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.479 58.170) (end 219.039 58.170) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.618 57.445) (end 217.143 57.920) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 211.692 57.920) (end 211.442 58.170) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.143 57.920) (end 211.692 57.920) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 207.084 58.170) (end 209.204 58.170) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 58.170) (end 209.204 58.170) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 58.170) (end 222.324 58.170) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 58.170) (end 220.204 58.170) (width 0.25) (layer B.Cu) (net 24))
        
          (segment (start 219.479 60.710) (end 217.966 60.710) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.369 60.710) (end 211.094 61.435) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 60.710) (end 210.369 60.710) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.094 61.435) (end 211.790 61.435) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 61.058) (end 212.167 61.047) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.790 61.435) (end 212.167 61.058) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 61.047) (end 212.254 60.960) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 217.716 60.960) (end 217.966 60.710) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.254 60.960) (end 217.716 60.960) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 60.710) (end 211.442 60.710) (width 0.25) (layer F.Cu) (net 13))
          (segment (start 218.314 59.985) (end 217.618 59.985) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.039 60.710) (end 218.314 59.985) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.479 60.710) (end 219.039 60.710) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.618 59.985) (end 217.143 60.460) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 211.692 60.460) (end 211.442 60.710) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.143 60.460) (end 211.692 60.460) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 207.084 60.710) (end 209.204 60.710) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 60.710) (end 209.204 60.710) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 60.710) (end 222.324 60.710) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 60.710) (end 220.204 60.710) (width 0.25) (layer B.Cu) (net 24))
        
          (segment (start 219.479 63.250) (end 217.966 63.250) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.369 63.250) (end 211.094 63.975) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 63.250) (end 210.369 63.250) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.094 63.975) (end 211.790 63.975) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 63.598) (end 212.167 63.587) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.790 63.975) (end 212.167 63.598) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 63.587) (end 212.254 63.500) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 217.716 63.500) (end 217.966 63.250) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.254 63.500) (end 217.716 63.500) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 63.250) (end 211.442 63.250) (width 0.25) (layer F.Cu) (net 13))
          (segment (start 218.314 62.525) (end 217.618 62.525) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.039 63.250) (end 218.314 62.525) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.479 63.250) (end 219.039 63.250) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.618 62.525) (end 217.143 63.000) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 211.692 63.000) (end 211.442 63.250) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.143 63.000) (end 211.692 63.000) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 207.084 63.250) (end 209.204 63.250) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 63.250) (end 209.204 63.250) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 63.250) (end 222.324 63.250) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 63.250) (end 220.204 63.250) (width 0.25) (layer B.Cu) (net 24))
        
          (segment (start 219.479 65.790) (end 217.966 65.790) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.369 65.790) (end 211.094 66.515) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 65.790) (end 210.369 65.790) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.094 66.515) (end 211.790 66.515) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 66.138) (end 212.167 66.127) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.790 66.515) (end 212.167 66.138) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 66.127) (end 212.254 66.040) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 217.716 66.040) (end 217.966 65.790) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.254 66.040) (end 217.716 66.040) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 65.790) (end 211.442 65.790) (width 0.25) (layer F.Cu) (net 13))
          (segment (start 218.314 65.065) (end 217.618 65.065) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.039 65.790) (end 218.314 65.065) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.479 65.790) (end 219.039 65.790) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.618 65.065) (end 217.143 65.540) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 211.692 65.540) (end 211.442 65.790) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.143 65.540) (end 211.692 65.540) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 207.084 65.790) (end 209.204 65.790) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 65.790) (end 209.204 65.790) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 65.790) (end 222.324 65.790) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 65.790) (end 220.204 65.790) (width 0.25) (layer B.Cu) (net 24))
        
          (segment (start 219.479 68.330) (end 217.966 68.330) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.369 68.330) (end 211.094 69.055) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 68.330) (end 210.369 68.330) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.094 69.055) (end 211.790 69.055) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 68.678) (end 212.167 68.667) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.790 69.055) (end 212.167 68.678) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 68.667) (end 212.254 68.580) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 217.716 68.580) (end 217.966 68.330) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.254 68.580) (end 217.716 68.580) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 68.330) (end 211.442 68.330) (width 0.25) (layer F.Cu) (net 13))
          (segment (start 218.314 67.605) (end 217.618 67.605) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.039 68.330) (end 218.314 67.605) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.479 68.330) (end 219.039 68.330) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.618 67.605) (end 217.143 68.080) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 211.692 68.080) (end 211.442 68.330) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.143 68.080) (end 211.692 68.080) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 207.084 68.330) (end 209.204 68.330) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 68.330) (end 209.204 68.330) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 68.330) (end 222.324 68.330) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 68.330) (end 220.204 68.330) (width 0.25) (layer B.Cu) (net 24))
        
          (segment (start 219.479 70.870) (end 217.966 70.870) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.369 70.870) (end 211.094 71.595) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 70.870) (end 210.369 70.870) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.094 71.595) (end 211.790 71.595) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 71.218) (end 212.167 71.207) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.790 71.595) (end 212.167 71.218) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 71.207) (end 212.254 71.120) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 217.716 71.120) (end 217.966 70.870) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.254 71.120) (end 217.716 71.120) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 70.870) (end 211.442 70.870) (width 0.25) (layer F.Cu) (net 13))
          (segment (start 218.314 70.145) (end 217.618 70.145) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.039 70.870) (end 218.314 70.145) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.479 70.870) (end 219.039 70.870) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.618 70.145) (end 217.143 70.620) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 211.692 70.620) (end 211.442 70.870) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.143 70.620) (end 211.692 70.620) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 207.084 70.870) (end 209.204 70.870) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 70.870) (end 209.204 70.870) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 70.870) (end 222.324 70.870) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 70.870) (end 220.204 70.870) (width 0.25) (layer B.Cu) (net 24))
        
          (segment (start 219.479 73.410) (end 217.966 73.410) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.369 73.410) (end 211.094 74.135) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 73.410) (end 210.369 73.410) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.094 74.135) (end 211.790 74.135) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 73.758) (end 212.167 73.747) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.790 74.135) (end 212.167 73.758) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 73.747) (end 212.254 73.660) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 217.716 73.660) (end 217.966 73.410) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.254 73.660) (end 217.716 73.660) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 73.410) (end 211.442 73.410) (width 0.25) (layer F.Cu) (net 13))
          (segment (start 218.314 72.685) (end 217.618 72.685) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.039 73.410) (end 218.314 72.685) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.479 73.410) (end 219.039 73.410) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.618 72.685) (end 217.143 73.160) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 211.692 73.160) (end 211.442 73.410) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.143 73.160) (end 211.692 73.160) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 207.084 73.410) (end 209.204 73.410) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 73.410) (end 209.204 73.410) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 73.410) (end 222.324 73.410) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 73.410) (end 220.204 73.410) (width 0.25) (layer B.Cu) (net 24))
        
          (segment (start 219.479 75.950) (end 217.966 75.950) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.369 75.950) (end 211.094 76.675) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 75.950) (end 210.369 75.950) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.094 76.675) (end 211.790 76.675) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 76.298) (end 212.167 76.287) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.790 76.675) (end 212.167 76.298) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 76.287) (end 212.254 76.200) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 217.716 76.200) (end 217.966 75.950) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.254 76.200) (end 217.716 76.200) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 75.950) (end 211.442 75.950) (width 0.25) (layer F.Cu) (net 13))
          (segment (start 218.314 75.225) (end 217.618 75.225) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.039 75.950) (end 218.314 75.225) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.479 75.950) (end 219.039 75.950) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.618 75.225) (end 217.143 75.700) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 211.692 75.700) (end 211.442 75.950) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.143 75.700) (end 211.692 75.700) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 207.084 75.950) (end 209.204 75.950) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 75.950) (end 209.204 75.950) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 75.950) (end 222.324 75.950) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 75.950) (end 220.204 75.950) (width 0.25) (layer B.Cu) (net 24))
        
          (segment (start 219.479 78.490) (end 217.966 78.490) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.369 78.490) (end 211.094 79.215) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 78.490) (end 210.369 78.490) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.094 79.215) (end 211.790 79.215) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 78.838) (end 212.167 78.827) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.790 79.215) (end 212.167 78.838) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 78.827) (end 212.254 78.740) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 217.716 78.740) (end 217.966 78.490) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.254 78.740) (end 217.716 78.740) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 78.490) (end 211.442 78.490) (width 0.25) (layer F.Cu) (net 13))
          (segment (start 218.314 77.765) (end 217.618 77.765) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.039 78.490) (end 218.314 77.765) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.479 78.490) (end 219.039 78.490) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.618 77.765) (end 217.143 78.240) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 211.692 78.240) (end 211.442 78.490) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.143 78.240) (end 211.692 78.240) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 207.084 78.490) (end 209.204 78.490) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 78.490) (end 209.204 78.490) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 78.490) (end 222.324 78.490) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 78.490) (end 220.204 78.490) (width 0.25) (layer B.Cu) (net 24))
        
          (segment (start 219.479 81.030) (end 217.966 81.030) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.369 81.030) (end 211.094 81.755) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 81.030) (end 210.369 81.030) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.094 81.755) (end 211.790 81.755) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 81.378) (end 212.167 81.367) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.790 81.755) (end 212.167 81.378) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 81.367) (end 212.254 81.280) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 217.716 81.280) (end 217.966 81.030) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.254 81.280) (end 217.716 81.280) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 81.030) (end 211.442 81.030) (width 0.25) (layer F.Cu) (net 13))
          (segment (start 218.314 80.305) (end 217.618 80.305) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.039 81.030) (end 218.314 80.305) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.479 81.030) (end 219.039 81.030) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.618 80.305) (end 217.143 80.780) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 211.692 80.780) (end 211.442 81.030) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.143 80.780) (end 211.692 80.780) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 207.084 81.030) (end 209.204 81.030) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 81.030) (end 209.204 81.030) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 81.030) (end 222.324 81.030) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 81.030) (end 220.204 81.030) (width 0.25) (layer B.Cu) (net 24))
        
          (segment (start 219.479 83.570) (end 217.966 83.570) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.369 83.570) (end 211.094 84.295) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 83.570) (end 210.369 83.570) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.094 84.295) (end 211.790 84.295) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 83.918) (end 212.167 83.907) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.790 84.295) (end 212.167 83.918) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 83.907) (end 212.254 83.820) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 217.716 83.820) (end 217.966 83.570) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.254 83.820) (end 217.716 83.820) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 83.570) (end 211.442 83.570) (width 0.25) (layer F.Cu) (net 13))
          (segment (start 218.314 82.845) (end 217.618 82.845) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.039 83.570) (end 218.314 82.845) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.479 83.570) (end 219.039 83.570) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.618 82.845) (end 217.143 83.320) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 211.692 83.320) (end 211.442 83.570) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.143 83.320) (end 211.692 83.320) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 207.084 83.570) (end 209.204 83.570) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 83.570) (end 209.204 83.570) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 83.570) (end 222.324 83.570) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 83.570) (end 220.204 83.570) (width 0.25) (layer B.Cu) (net 24))
        
          (segment (start 219.479 86.110) (end 217.966 86.110) (width 0.25) (layer F.Cu) (net 1))
          (segment (start 210.369 86.110) (end 211.094 86.835) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 86.110) (end 210.369 86.110) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.094 86.835) (end 211.790 86.835) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 86.458) (end 212.167 86.447) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 211.790 86.835) (end 212.167 86.458) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.167 86.447) (end 212.254 86.360) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 217.716 86.360) (end 217.966 86.110) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 212.254 86.360) (end 217.716 86.360) (width 0.25) (layer B.Cu) (net 1))
          (segment (start 209.929 86.110) (end 211.442 86.110) (width 0.25) (layer F.Cu) (net 13))
          (segment (start 218.314 85.385) (end 217.618 85.385) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.039 86.110) (end 218.314 85.385) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 219.479 86.110) (end 219.039 86.110) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.618 85.385) (end 217.143 85.860) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 211.692 85.860) (end 211.442 86.110) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 217.143 85.860) (end 211.692 85.860) (width 0.25) (layer B.Cu) (net 13))
          (segment (start 207.084 86.110) (end 209.204 86.110) (width 0.25) (layer F.Cu) (net 23))
          (segment (start 207.084 86.110) (end 209.204 86.110) (width 0.25) (layer B.Cu) (net 23))
          (segment (start 220.204 86.110) (end 222.324 86.110) (width 0.25) (layer F.Cu) (net 24))
          (segment (start 222.324 86.110) (end 220.204 86.110) (width 0.25) (layer B.Cu) (net 24))
        
    

      (gr_text "JLCJLCJLCJLC" (at 138 107.6 0) (layer F.SilkS)
        (effects (font (size 1 1) (thickness 0.15)))
      )
    

      (module nice!view (layer F.Cu) (tedit 6448AF5B)
        (at 214.647 73.75 0)
        (attr virtual)
        (fp_text reference "DISP1" (at 0 20 0) (layer F.SilkS) hide
          (effects (font (size 1 1) (thickness 0.15)))
        )
        (fp_text user %R (at 0 20 0) (layer F.Fab)
          (effects (font (size 1 1) (thickness 0.15)))
        )
        
        (fp_line (start -6.5 -18) (end 6.5 -18) (layer F.Fab) (width 0.15))
        (fp_line (start 6.5 18) (end -6.5 18) (layer F.Fab) (width 0.15))
        (fp_line (start -7 17.5) (end -7 -17.5) (layer F.Fab) (width 0.15))
        (fp_line (start 7 17.5) (end 7 -17.5) (layer F.Fab) (width 0.15))
        (fp_arc (start -6.5 17.5) (end -7 17.5) (angle -90) (layer F.Fab) (width 0.15))
        (fp_arc (start 6.5 17.5) (end 6.5 18) (angle -90) (layer F.Fab) (width 0.15))
        (fp_arc (start 6.5 -17.5) (end 6.5 -18) (angle 90) (layer F.Fab) (width 0.15))
        (fp_arc (start -6.5 -17.5) (end -6.5 -18) (angle -90) (layer F.Fab) (width 0.15))
        (fp_line (start -6.41 15.37) (end -6.41 18.03) (layer F.SilkS) (width 0.12))
        (fp_line (start 6.41 18.03) (end -6.41 18.03) (layer F.SilkS) (width 0.12))
        (fp_line (start 6.41 15.37) (end 6.41 18.03) (layer F.SilkS) (width 0.12))
        (fp_line (start 6.41 15.37) (end -6.41 15.37) (layer F.SilkS) (width 0.12))
        (fp_line (start 6.88 14.9) (end 6.88 18.45) (layer F.CrtYd) (width 0.15))
        (fp_line (start 6.88 18.45) (end -6.82 18.45) (layer F.CrtYd) (width 0.15))
        (fp_line (start -6.82 18.45) (end -6.82 14.9) (layer F.CrtYd) (width 0.15))
        (fp_line (start -6.82 14.9) (end 6.88 14.9) (layer F.CrtYd) (width 0.15))
    
        (fp_line (start 6.41 15.37) (end 6.41 18.03) (layer B.SilkS) (width 0.12))
        (fp_line (start 6.41 15.37) (end -6.41 15.37) (layer B.SilkS) (width 0.12))
        (fp_line (start 6.41 18.03) (end -6.41 18.03) (layer B.SilkS) (width 0.12))
        (fp_line (start 6.88 14.9) (end 6.88 18.45) (layer B.CrtYd) (width 0.15))
        (fp_line (start 6.88 18.45) (end -6.82 18.45) (layer B.CrtYd) (width 0.15))
        (fp_line (start -6.82 18.45) (end -6.82 14.9) (layer B.CrtYd) (width 0.15))
        (fp_line (start -6.82 14.9) (end 6.88 14.9) (layer B.CrtYd) (width 0.15))
        (fp_line (start -6.41 15.37) (end -6.41 18.03) (layer B.SilkS) (width 0.12))
        (fp_line (start -6.5 18) (end 6.5 18) (layer B.Fab) (width 0.15))
        (fp_line (start 7 -17.5) (end 7 17.5) (layer B.Fab) (width 0.15))
        (fp_line (start 6.5 -18) (end -6.5 -18) (layer B.Fab) (width 0.15))
        (fp_line (start -7 -17.5) (end -7 17.5) (layer B.Fab) (width 0.15))
        (fp_arc (start -6.5 -17.5) (end -7 -17.5) (angle 90) (layer B.Fab) (width 0.15))
        (fp_arc (start 6.5 -17.5) (end 6.5 -18) (angle 90) (layer B.Fab) (width 0.15))
        (fp_arc (start 6.5 17.5) (end 6.5 18) (angle -90) (layer B.Fab) (width 0.15))
        (fp_arc (start -6.5 17.5) (end -6.5 18) (angle 90) (layer B.Fab) (width 0.15))
    
        (fp_line (start 5.93 18.6) (end 5.93 20.6) (layer F.Fab) (width 0.15))
        (fp_line (start -5.93 20.6) (end -5.93 18.6) (layer F.Fab) (width 0.15))
        (fp_line (start -5.93 18.6) (end -4.23 18.6) (layer F.Fab) (width 0.15))
        (fp_line (start -4.23 20.6) (end -5.93 20.6) (layer F.Fab) (width 0.15))
        (fp_line (start -4.23 18.6) (end -4.23 20.6) (layer F.Fab) (width 0.15))
        (fp_line (start -3.39 20.6) (end -3.39 18.6) (layer F.Fab) (width 0.15))
        (fp_line (start -3.39 18.6) (end -1.69 18.6) (layer F.Fab) (width 0.15))
        (fp_line (start -1.69 20.6) (end -3.39 20.6) (layer F.Fab) (width 0.15))
        (fp_line (start -1.69 18.6) (end -1.69 20.6) (layer F.Fab) (width 0.15))
        (fp_line (start 3.39 18.6) (end 3.39 20.6) (layer F.Fab) (width 0.15))
        (fp_line (start 3.39 20.6) (end 1.69 20.6) (layer F.Fab) (width 0.15))
        (fp_line (start 1.69 20.6) (end 1.69 18.6) (layer F.Fab) (width 0.15))
        (fp_line (start 1.69 18.6) (end 3.39 18.6) (layer F.Fab) (width 0.15))
        (fp_line (start 5.93 20.6) (end 4.23 20.6) (layer F.Fab) (width 0.15))
        (fp_line (start 4.23 20.6) (end 4.23 18.6) (layer F.Fab) (width 0.15))
        (fp_line (start 4.23 18.6) (end 5.93 18.6) (layer F.Fab) (width 0.15))

        (pad 14 smd rect (at -5.08 19.15 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 68 "DISP1_1"))
        (pad 15 smd rect (at -2.54 19.15 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 69 "DISP1_2"))
        (pad 16 smd rect (at 2.54 19.15 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 70 "DISP1_4"))
        (pad 17 smd rect (at 5.08 19.15 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 71 "DISP1_5"))

        (pad 10 smd rect (at -5.08 20.05 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 42 "CS"))
        (pad 11 smd rect (at -2.54 20.05 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 33 "GND"))
        (pad 12 smd rect (at 2.54 20.05 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 41 "SCL"))
        (pad 13 smd rect (at 5.08 20.05 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 40 "SDA"))
    
        (fp_line (start -5.93 18.6) (end -5.93 20.6) (layer B.Fab) (width 0.15))
        (fp_line (start -5.93 20.6) (end -4.23 20.6) (layer B.Fab) (width 0.15))
        (fp_line (start -4.23 18.6) (end -5.93 18.6) (layer B.Fab) (width 0.15))
        (fp_line (start -4.23 20.6) (end -4.23 18.6) (layer B.Fab) (width 0.15))
        (fp_line (start -3.39 20.6) (end -1.69 20.6) (layer B.Fab) (width 0.15))
        (fp_line (start -1.69 18.6) (end -3.39 18.6) (layer B.Fab) (width 0.15))
        (fp_line (start 4.23 20.6) (end 5.93 20.6) (layer B.Fab) (width 0.15))
        (fp_line (start 5.93 20.6) (end 5.93 18.6) (layer B.Fab) (width 0.15))
        (fp_line (start 3.39 18.6) (end 1.69 18.6) (layer B.Fab) (width 0.15))
        (fp_line (start -1.69 20.6) (end -1.69 18.6) (layer B.Fab) (width 0.15))
        (fp_line (start -3.39 18.6) (end -3.39 20.6) (layer B.Fab) (width 0.15))
        (fp_line (start 1.69 18.6) (end 1.69 20.6) (layer B.Fab) (width 0.15))
        (fp_line (start 1.69 20.6) (end 3.39 20.6) (layer B.Fab) (width 0.15))
        (fp_line (start 3.39 20.6) (end 3.39 18.6) (layer B.Fab) (width 0.15))
        (fp_line (start 5.93 18.6) (end 4.23 18.6) (layer B.Fab) (width 0.15))
        (fp_line (start 4.23 18.6) (end 4.23 20.6) (layer B.Fab) (width 0.15))

        (pad 24 smd rect (at 5.08 19.15 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 71 "DISP1_5"))
        (pad 25 smd rect (at 2.54 19.15 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 70 "DISP1_4"))
        (pad 26 smd rect (at -2.54 19.15 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 69 "DISP1_2"))
        (pad 27 smd rect (at -5.08 19.15 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 68 "DISP1_1"))

        (pad 20 smd rect (at 5.08 20.05 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 42 "CS"))
        (pad 21 smd rect (at 2.54 20.05 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 33 "GND"))
        (pad 22 smd rect (at -2.54 20.05 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 41 "SCL"))
        (pad 23 smd rect (at -5.08 20.05 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 40 "SDA"))
    
      (pad 1 thru_hole oval (at -5.08 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 68 "DISP1_1"))
      (pad 2 thru_hole oval (at -2.54 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 69 "DISP1_2"))
      (pad 3 thru_hole oval (at 0 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 35 "VCC"))
      (pad 4 thru_hole oval (at 2.54 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 70 "DISP1_4"))
      (pad 5 thru_hole circle (at 5.08 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 71 "DISP1_5"))

      (fp_line (start 5.4 13.4) (end 5.4 -11.9) (layer Dwgs.User) (width 0.15))
      (fp_line (start -5.4 13.4) (end -5.4 -11.9) (layer Dwgs.User) (width 0.15))
      (fp_line (start 5.4 -11.9) (end -5.4 -11.9) (layer Dwgs.User) (width 0.15))
      (fp_line (start -5.4 13.4) (end 5.4 13.4) (layer Dwgs.User) (width 0.15))
    )
    
    (segment (start 209.567 90.450) (end 209.567 92.900) (width 0.15) (layer "F.Cu") (net 42))
    (segment (start 212.107 90.450) (end 212.107 92.900) (width 0.25) (layer "F.Cu") (net 33))
    (segment (start 217.187 90.450) (end 217.187 92.900) (width 0.15) (layer "F.Cu") (net 41))
    (segment (start 219.727 90.450) (end 219.727 92.900) (width 0.15) (layer "F.Cu") (net 40))
    (segment (start 209.567 90.450) (end 209.567 92.900) (width 0.15) (layer "B.Cu") (net 42))
    (segment (start 212.107 90.450) (end 212.107 92.900) (width 0.15) (layer "B.Cu") (net 33))
    (segment (start 217.187 90.450) (end 217.187 92.900) (width 0.25) (layer "B.Cu") (net 41))
    (segment (start 219.727 90.450) (end 219.727 92.900) (width 0.15) (layer "B.Cu") (net 40))
    

        (module power_switch (layer F.Cu) (tedit 644556E6)
          (at 214.5 54.97 90)
          (attr smd)

      
          (fp_text reference "SW1" (at -3.6 0 0) (layer F.SilkS) hide
            (effects (font (size 1 1) (thickness 0.15)))
          )

          (fp_line (start 0.415 -3.45) (end -0.375 -3.45) (layer F.SilkS) (width 0.12))
          (fp_line (start -0.375 3.45) (end 0.415 3.45) (layer F.SilkS) (width 0.12))
          (fp_line (start -1.425 1.6) (end -1.425 -0.1) (layer F.SilkS) (width 0.12))
          (fp_line (start 1.425 2.85) (end 1.425 -2.85) (layer F.SilkS) (width 0.12))
          (fp_line (start 1.795 4.4) (end -2.755 4.4) (layer F.CrtYd) (width 0.05))
          (fp_line (start 1.795 1.65) (end 1.795 4.4) (layer F.CrtYd) (width 0.05))
          (fp_line (start 3.095 1.65) (end 1.795 1.65) (layer F.CrtYd) (width 0.05))
          (fp_line (start 3.095 -1.65) (end 3.095 1.65) (layer F.CrtYd) (width 0.05))
          (fp_line (start 1.795 -1.65) (end 3.095 -1.65) (layer F.CrtYd) (width 0.05))
          (fp_line (start 1.795 -4.4) (end 1.795 -1.65) (layer F.CrtYd) (width 0.05))
          (fp_line (start -2.755 -4.4) (end 1.795 -4.4) (layer F.CrtYd) (width 0.05))
          (fp_line (start -2.755 4.4) (end -2.755 -4.4) (layer F.CrtYd) (width 0.05))
          (fp_line (start -1.425 -1.4) (end -1.425 -1.6) (layer F.SilkS) (width 0.12))
          (fp_line (start -1.305 -3.35) (end -1.305 3.35) (layer F.Fab) (width 0.1))
          (fp_line (start 1.295 -3.35) (end -1.305 -3.35) (layer F.Fab) (width 0.1))
          (fp_line (start 1.295 3.35) (end 1.295 -3.35) (layer F.Fab) (width 0.1))
          (fp_line (start -1.305 3.35) (end 1.295 3.35) (layer F.Fab) (width 0.1))
          (fp_line (start 2.595 0.1) (end 1.295 0.1) (layer F.Fab) (width 0.1))
          (fp_line (start 2.645 0.15) (end 2.595 0.1) (layer F.Fab) (width 0.1))
          (fp_line (start 2.845 0.35) (end 2.645 0.15) (layer F.Fab) (width 0.1))
          (fp_line (start 2.845 1.2) (end 2.845 0.35) (layer F.Fab) (width 0.1))
          (fp_line (start 2.645 1.4) (end 2.845 1.2) (layer F.Fab) (width 0.1))
          (fp_line (start 1.345 1.4) (end 2.645 1.4) (layer F.Fab) (width 0.1))

          (pad "" smd rect (at 1.125 -3.65 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
          (pad "" smd rect (at -1.085 -3.65 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
          (pad "" smd rect (at -1.085 3.65 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
          (pad 1 smd rect (at -1.735 2.25 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
          (pad 2 smd rect (at -1.735 -0.75 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask) (net 72 "BAT_P"))
          (pad 3 smd rect (at -1.735 -2.25 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask) (net 32 "RAW"))
          (pad "" smd rect (at 1.125 3.65 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask))

      
        
        (fp_text user "SW1" (at -3.5 0 180) (layer B.SilkS) hide
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
        )
        (fp_line (start 2.595 -0.1) (end 1.295 -0.1) (layer B.Fab) (width 0.1))
        (fp_line (start -1.305 3.35) (end -1.305 -3.35) (layer B.Fab) (width 0.1))
        (fp_line (start 2.645 -0.15) (end 2.595 -0.1) (layer B.Fab) (width 0.1))
        (fp_line (start -1.425 1.4) (end -1.425 1.6) (layer B.SilkS) (width 0.12))
        (fp_line (start 0.415 3.45) (end -0.375 3.45) (layer B.SilkS) (width 0.12))
        (fp_line (start -0.375 -3.45) (end 0.415 -3.45) (layer B.SilkS) (width 0.12))
        (fp_line (start -1.425 -1.6) (end -1.425 0.1) (layer B.SilkS) (width 0.12))
        (fp_line (start 1.425 -2.85) (end 1.425 2.85) (layer B.SilkS) (width 0.12))
        (fp_line (start 1.795 4.4) (end 1.795 1.65) (layer B.CrtYd) (width 0.05))
        (fp_line (start -2.755 4.4) (end 1.795 4.4) (layer B.CrtYd) (width 0.05))
        (fp_line (start 2.845 -1.2) (end 2.845 -0.35) (layer B.Fab) (width 0.1))
        (fp_line (start 1.345 -1.4) (end 2.645 -1.4) (layer B.Fab) (width 0.1))
        (fp_line (start 1.795 -4.4) (end -2.755 -4.4) (layer B.CrtYd) (width 0.05))
        (fp_line (start 1.795 -1.65) (end 1.795 -4.4) (layer B.CrtYd) (width 0.05))
        (fp_line (start 3.095 -1.65) (end 1.795 -1.65) (layer B.CrtYd) (width 0.05))
        (fp_line (start 2.845 -0.35) (end 2.645 -0.15) (layer B.Fab) (width 0.1))
        (fp_line (start 2.645 -1.4) (end 2.845 -1.2) (layer B.Fab) (width 0.1))
        (fp_line (start 1.295 -3.35) (end 1.295 3.35) (layer B.Fab) (width 0.1))
        (fp_line (start 1.295 3.35) (end -1.305 3.35) (layer B.Fab) (width 0.1))
        (fp_line (start -1.305 -3.35) (end 1.295 -3.35) (layer B.Fab) (width 0.1))
        (fp_line (start -2.755 -4.4) (end -2.755 4.4) (layer B.CrtYd) (width 0.05))
        (fp_line (start 3.095 1.65) (end 3.095 -1.65) (layer B.CrtYd) (width 0.05))
        (fp_line (start 1.795 1.65) (end 3.095 1.65) (layer B.CrtYd) (width 0.05))
        (pad "" smd rect (at -1.085 -3.65 360) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
        (pad "" smd rect (at 1.125 -3.65 360) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
        (pad 4 smd rect (at -1.735 2.25 360) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask))
        (pad "" smd rect (at -1.085 3.65 360) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
        (pad 5 smd rect (at -1.735 0.75 360) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask) (net 72 "BAT_P"))
        (pad 6 smd rect (at -1.735 -2.25 360) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask) (net 32 "RAW"))
        (pad "" smd rect (at 1.125 3.65 360) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
        
          (pad "" np_thru_hole circle (at 0.025 -1.5 180) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
          (pad "" np_thru_hole circle (at 0.025 1.5 180) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
        )
        

        (module sw_reset_side (layer F.Cu) (tedit 64473C6F)
          (at 206.65 55.065 90)
          (attr smd)

          (fp_text reference "SW2" (at 0 3.5 90) (layer F.SilkS) hide
            (effects (font (size 1 1) (thickness 0.15)))
          )
      
          (fp_line (start 1.7 2.75) (end -1.7 2.75) (layer F.CrtYd) (width 0.05))
          (fp_line (start -1.7 2.75) (end -1.7 -2.75) (layer F.CrtYd) (width 0.05))
          (fp_line (start 2.1 0.85) (end 2.1 -0.85) (layer F.Fab) (width 0.1))
          (fp_line (start 1.7 -1.1) (end 2.35 -1.1) (layer F.CrtYd) (width 0.05))
          (fp_line (start -1.7 -2.75) (end 1.7 -2.75) (layer F.CrtYd) (width 0.05))
          (fp_line (start 1.45 -1.75) (end 1.45 1.75) (layer F.Fab) (width 0.1))
          (fp_line (start 1.7 1.1) (end 1.7 2.75) (layer F.CrtYd) (width 0.05))
          (fp_line (start 2.35 1.1) (end 1.7 1.1) (layer F.CrtYd) (width 0.05))
          (fp_line (start 1.7 -2.75) (end 1.7 -1.1) (layer F.CrtYd) (width 0.05))
          (fp_line (start 1.55 -1.75) (end 1.55 1.75) (layer F.SilkS) (width 0.12))
          (fp_line (start 2.1 -0.85) (end 1.45 -0.85) (layer F.Fab) (width 0.1))
          (fp_line (start 2.35 -1.1) (end 2.35 1.1) (layer F.CrtYd) (width 0.05))
          (fp_line (start 2.1 0.85) (end 1.45 0.85) (layer F.Fab) (width 0.1))
          (fp_line (start -1.55 1.75) (end -1.55 -1.75) (layer F.SilkS) (width 0.12))
          (fp_line (start 1.45 1.75) (end -1.4 1.75) (layer F.Fab) (width 0.1))
          (fp_line (start -1.45 1.75) (end -1.45 -1.75) (layer F.Fab) (width 0.1))
          (fp_line (start -1.45 -1.75) (end 1.45 -1.75) (layer F.Fab) (width 0.1))

          (pad 1 smd rect (at -0.72 -1.8 180) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask) (net 33 "GND"))

          (pad 1 smd rect (at -0.72 1.8 180) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask) (net 33 "GND"))
          (pad 2 smd rect (at 0.72 -1.8 180) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask) (net 34 "RST"))
          (pad 2 smd rect (at 0.72 1.8 180) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask) (net 34 "RST"))
      
      (fp_line (start -1.45 1.75) (end 1.45 1.75) (layer B.Fab) (width 0.1))
      (fp_line (start 1.45 1.75) (end 1.45 -1.75) (layer B.Fab) (width 0.1))
      (fp_line (start 1.7 -1.1) (end 1.7 -2.75) (layer B.CrtYd) (width 0.05))
      (fp_line (start 2.35 -1.1) (end 1.7 -1.1) (layer B.CrtYd) (width 0.05))
      (fp_line (start 1.7 2.75) (end 1.7 1.1) (layer B.CrtYd) (width 0.05))
      (fp_line (start 1.55 1.75) (end 1.55 -1.75) (layer B.SilkS) (width 0.12))
      (fp_line (start 2.1 0.85) (end 1.45 0.85) (layer B.Fab) (width 0.1))
      (fp_line (start 2.35 1.1) (end 2.35 -1.1) (layer B.CrtYd) (width 0.05))
      (fp_line (start 2.1 -0.85) (end 1.45 -0.85) (layer B.Fab) (width 0.1))
      (fp_line (start -1.55 -1.75) (end -1.55 1.75) (layer B.SilkS) (width 0.12))
      (fp_line (start 1.45 -1.75) (end -1.4 -1.75) (layer B.Fab) (width 0.1))
      (fp_line (start -1.45 -1.75) (end -1.45 1.75) (layer B.Fab) (width 0.1))
      (fp_line (start 1.7 -2.75) (end -1.7 -2.75) (layer B.CrtYd) (width 0.05))
      (fp_line (start -1.7 -2.75) (end -1.7 2.75) (layer B.CrtYd) (width 0.05))
      (fp_line (start 2.1 -0.85) (end 2.1 0.85) (layer B.Fab) (width 0.1))
      (fp_line (start 1.7 1.1) (end 2.35 1.1) (layer B.CrtYd) (width 0.05))
      (fp_line (start -1.7 2.75) (end 1.7 2.75) (layer B.CrtYd) (width 0.05))
      (pad 1 smd rect (at -0.72 -1.8 360) (size 1.4 1.05) (layers B.Cu B.Paste B.Mask) (net 33 "GND"))
      (pad 2 smd rect (at 0.72 1.8 360) (size 1.4 1.05) (layers B.Cu B.Paste B.Mask) (net 34 "RST"))
      (pad 2 smd rect (at 0.72 -1.8 360) (size 1.4 1.05) (layers B.Cu B.Paste B.Mask) (net 34 "RST"))
      (pad 1 smd rect (at -0.72 1.8 360) (size 1.4 1.05) (layers B.Cu B.Paste B.Mask) (net 33 "GND"))
      (fp_text user SW2 (at 0 3.5 90) (layer B.SilkS) hide
        (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      )
      
        )
      

            (module "JST_PH_S2B-PH-K" (layer F.Cu) (tedit 6135B927)
                (at 221.5 98.75 -90)

                (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)")
                (fp_text reference "JST1" (at 1 -2.55 -90) (layer "F.SilkS") hide
                    (effects (font (size 1 1) (thickness 0.15)))
                )
            
                (fp_line (start -2.95 -1.35) (end -2.95 6.25) (width 0.1) (layer "F.Fab"))
                (fp_line (start -2.95 6.25) (end 2.95 6.25) (width 0.1) (layer "F.Fab"))
                (fp_line (start -2.25 -1.35) (end -2.95 -1.35) (width 0.1) (layer "F.Fab"))
                (fp_line (start -2.25 0.25) (end -2.25 -1.35) (width 0.1) (layer "F.Fab"))
                (fp_line (start 2.25 -1.35) (end 2.25 0.25) (width 0.1) (layer "F.Fab"))
                (fp_line (start 2.25 0.25) (end -2.25 0.25) (width 0.1) (layer "F.Fab"))
                (fp_line (start 2.95 -1.35) (end 2.25 -1.35) (width 0.1) (layer "F.Fab"))
                (fp_line (start 2.95 6.25) (end 2.95 -1.35) (width 0.1) (layer "F.Fab"))
        
                (fp_line (start -3.45 -1.85) (end -3.45 8.5) (width 0.05) (layer "F.CrtYd"))
                (fp_line (start -3.45 8.5) (end 3.45 8.5) (width 0.05) (layer "F.CrtYd"))
                (fp_line (start 3.45 -1.85) (end -3.45 -1.85) (width 0.05) (layer "F.CrtYd"))
                (fp_line (start 3.45 8.5) (end 3.45 -1.85) (width 0.05) (layer "F.CrtYd"))
        
                (fp_line (start 1.5 4.375) (end 0.5 4.375) (width 0.1) (layer "F.SilkS"))
                (fp_line (start -1.5 4.375) (end -0.5 4.375) (width 0.1) (layer "F.SilkS"))
                (fp_line (start -1 3.875) (end -1 4.875) (width 0.1) (layer "F.SilkS"))
                (fp_line (start -2.06 -1.46) (end -3.06 -1.46) (width 0.12) (layer "F.SilkS"))
                (fp_line (start -3.06 -1.46) (end -3.06 -0.46) (width 0.12) (layer "F.SilkS"))
                (fp_line (start 2.14 -1.46) (end 3.06 -1.46) (width 0.12) (layer "F.SilkS"))
                (fp_line (start 3.06 -1.46) (end 3.06 -0.46) (width 0.12) (layer "F.SilkS"))
                (fp_line (start -2.14 6.36) (end -3.06 6.36) (width 0.12) (layer "F.SilkS"))
                (fp_line (start -3.06 6.36) (end -3.06 5.36) (width 0.12) (layer "F.SilkS"))
                (fp_line (start 2.14 6.36) (end 3.06 6.36) (width 0.12) (layer "F.SilkS"))
                (fp_line (start 3.06 6.36) (end 3.06 5.36) (width 0.12) (layer "F.SilkS"))
        
                (fp_line (start -2.95 -1.35) (end -2.25 -1.35) (width 0.1) (layer "B.Fab"))
                (fp_line (start -2.95 6.25) (end -2.95 -1.35) (width 0.1) (layer "B.Fab"))
                (fp_line (start -2.25 -1.35) (end -2.25 0.25) (width 0.1) (layer "B.Fab"))
                (fp_line (start -2.25 0.25) (end 2.25 0.25) (width 0.1) (layer "B.Fab"))
                (fp_line (start 2.25 -1.35) (end 2.95 -1.35) (width 0.1) (layer "B.Fab"))
                (fp_line (start 2.25 0.25) (end 2.25 -1.35) (width 0.1) (layer "B.Fab"))
                (fp_line (start 2.95 -1.35) (end 2.95 6.25) (width 0.1) (layer "B.Fab"))
                (fp_line (start 2.95 6.25) (end -2.95 6.25) (width 0.1) (layer "B.Fab"))
        
                (fp_line (start -3.45 -1.85) (end -3.45 8.5) (width 0.05) (layer "B.CrtYd"))
                (fp_line (start -3.45 8.5) (end 3.45 8.5) (width 0.05) (layer "B.CrtYd"))
                (fp_line (start 3.45 -1.85) (end -3.45 -1.85) (width 0.05) (layer "B.CrtYd"))
                (fp_line (start 3.45 8.5) (end 3.45 -1.85) (width 0.05) (layer "B.CrtYd"))
        
                (fp_line (start -1.5 4.375) (end -0.5 4.375) (width 0.1) (layer "B.SilkS"))
                (fp_line (start 1.5 4.375) (end 0.5 4.375) (width 0.1) (layer "B.SilkS"))
                (fp_line (start 1 3.875) (end 1 4.875) (width 0.1) (layer "B.SilkS"))
                (fp_line (start -2.06 -1.46) (end -3.06 -1.46) (width 0.12) (layer "B.SilkS"))
                (fp_line (start -3.06 -1.46) (end -3.06 -0.46) (width 0.12) (layer "B.SilkS"))
                (fp_line (start 2.14 -1.46) (end 3.06 -1.46) (width 0.12) (layer "B.SilkS"))
                (fp_line (start 3.06 -1.46) (end 3.06 -0.46) (width 0.12) (layer "B.SilkS"))
                (fp_line (start -2.14 6.36) (end -3.06 6.36) (width 0.12) (layer "B.SilkS"))
                (fp_line (start -3.06 6.36) (end -3.06 5.36) (width 0.12) (layer "B.SilkS"))
                (fp_line (start 2.14 6.36) (end 3.06 6.36) (width 0.12) (layer "B.SilkS"))
                (fp_line (start 3.06 6.36) (end 3.06 5.36) (width 0.12) (layer "B.SilkS"))
        
                (pad 11 thru_hole oval (at -1 0 -90) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask") (net 73 "JST1_1"))
                (pad 12 thru_hole oval (at 1 0 -90) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask") (net 74 "JST1_2"))
                (pad 21 smd custom (at -1 1.8 90) (size 0.1 0.1) (layers "F.Cu" "F.Mask")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0.4)
                        (xy -0.6 0.4)
                        (xy -0.6 0.2)
                        (xy 0 -0.4)
                        (xy 0.6 0.2)
                        )   
                        (width 0))
                    )
                    (net 73 "JST1_1"))
                (pad 31 smd custom (at -1 1.8 90) (size 0.1 0.1) (layers "B.Cu" "B.Mask")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0.4)
                        (xy -0.6 0.4)
                        (xy -0.6 0.2)
                        (xy 0 -0.4)
                        (xy 0.6 0.2)
                        )
                        (width 0))
                    )
                    (net 73 "JST1_1"))
                (pad 22 smd custom (at 1 1.8 90) (size 0.1 0.1) (layers "F.Cu" "F.Mask")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0.4)
                        (xy -0.6 0.4)
                        (xy -0.6 0.2)
                        (xy 0 -0.4)
                        (xy 0.6 0.2)
                        )
                        (width 0))
                    )
                    (net 74 "JST1_2"))
                (pad 32 smd custom (at 1 1.8 90) (size 0.1 0.1) (layers "B.Cu" "B.Mask")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0.4)
                        (xy -0.6 0.4)
                        (xy -0.6 0.2)
                        (xy 0 -0.4)
                        (xy 0.6 0.2)
                        )
                        (width 0))
                    )
                    (net 74 "JST1_2"))
                (pad 1 smd custom (at -1 2.816 90) (size 1.2 0.5) (layers "F.Cu" "F.Mask") (net 33 "GND")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0)
                        (xy -0.6 0)
                        (xy -0.6 1)
                        (xy 0 0.4)
                        (xy 0.6 1)
                        )
                        (width 0))
                    ) )
                (pad 1 smd custom (at 1 2.816 90) (size 1.2 0.5) (layers "B.Cu" "B.Mask") (net 33 "GND")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0)
                        (xy -0.6 0)
                        (xy -0.6 1)
                        (xy 0 0.4)
                        (xy 0.6 1)
                        )
                        (width 0))
                    ) )
                (pad 2 smd custom (at -1 2.816 90) (size 1.2 0.5) (layers "B.Cu" "B.Mask") (net 72 "BAT_P")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0)
                        (xy -0.6 0)
                        (xy -0.6 1)
                        (xy 0 0.4)
                        (xy 0.6 1)
                        )
                        (width 0))
                    ) )
                (pad 2 smd custom (at 1 2.816 90) (size 1.2 0.5) (layers "F.Cu" "F.Mask") (net 72 "BAT_P")
                    (clearance 0.1) (zone_connect 0)
                    (options (clearance outline) (anchor rect))
                    (primitives
                    (gr_poly
                        (pts
                        (xy 0.6 0)
                        (xy -0.6 0)
                        (xy -0.6 1)
                        (xy 0 0.4)
                        (xy 0.6 1)
                        )
                        (width 0))
                    ) )
            
            )
         
        (segment (start 219.700 97.750) (end 221.500 97.750) (width 0.25) (layer "F.Cu") (net 73))
        (segment (start 219.700 97.750) (end 221.500 97.750) (width 0.25) (layer "B.Cu") (net 73))
        (segment (start 219.700 99.750) (end 221.500 99.750) (width 0.25) (layer "F.Cu") (net 74))
        (segment (start 219.700 99.750) (end 221.500 99.750) (width 0.25) (layer "B.Cu") (net 74))
        
            (gr_line (start 91.08198222285509 108.74001780012622) (end 91.08001777794281 53.49000464193523) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 91.58000462794281 52.98998684198348) (end 128.58001314999998 52.98901315754868) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 129.08 52.48901315754736) (end 129.08 48.74) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 129.58 48.24) (end 147.58 48.24) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 148.08 47.74) (end 148.08 46.488) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 148.58 45.988) (end 165.582 45.988) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 166.082 46.488) (end 166.082 47.74) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 166.582 48.24) (end 184.582 48.24) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 185.082 48.74) (end 185.082 50.238) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 185.582 50.738) (end 203.58222192628773 50.738) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 204.08222192628773 51.23777800000971) (end 204.08277807371226 52.49022199999308) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 224.518 113.996596) (end 210.97353193043912 137.45836746290388) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 210.29050971794075 137.64139668455357) (end 195.12364206223265 128.884801539137) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 194.9382670622326 128.82200823913698) (end 157.77296812333506 123.97775897688982) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 157.43351034067848 123.77643070068846) (end 146.98977558129695 109.44552227620129) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 146.5856927986404 109.24) (end 91.58198222285512 109.24) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 204.58277807371226 52.99) (end 224.333 52.99) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 224.833 53.49) (end 224.833 113.31702540612952) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 224.76601270000006 113.5670254061294) (end 224.518 113.996596) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 91.58001777794281 53.48998684156686) (end 91.58000457794282 52.98998684156686) (angle -90.00053289295953) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 128.58 52.48901315754736) (end 128.5800131 52.98901315754736) (angle -89.99849312100235) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 129.58 48.74) (end 129.58 48.24) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 147.58 47.74) (end 147.58 48.24) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 148.58 46.488) (end 148.58 45.988) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 165.582 46.488) (end 166.082 46.488) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 166.582 47.74) (end 166.082 47.74) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 184.582 48.74) (end 185.082 48.74) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 185.582 50.238) (end 185.082 50.238) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 203.58222192628773 51.238) (end 204.08222192628773 51.237778) (angle -89.97456067668081) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 204.58277807371226 52.48999999999069) (end 204.08277807371226 52.49022199999069) (angle -89.97456067529339) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 224.333 53.49) (end 224.833 53.49) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 224.333 113.31702540612952) (end 224.7660127 113.56702540612952) (angle -30.000000108401252) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 210.54050971794078 137.20838398455356) (end 210.29050971794078 137.64139668455357) (angle -90.00218462143252) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 194.87364206223262 129.31781423913696) (end 195.12364206223262 128.88480153913696) (angle -22.57374496727097) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 157.83759312333507 123.48195297688983) (end 157.43351032333507 123.77643067688983) (angle -46.490828368152734) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 146.5856927986404 109.73999999999998) (end 146.9897755986404 109.44552229999998) (angle -53.917083509298145) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 91.58198222285512 108.74) (end 91.08198222285512 108.74001779999999) (angle -89.99796025578533) (layer Edge.Cuts) (width 0.15))
(gr_line (start 93 109) (end 107 109) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 109 107) (end 109 93) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 107 91) (end 93 91) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 91 93) (end 91 107) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 93 90) (end 107 90) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 109 88) (end 109 74) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 107 72) (end 93 72) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 91 74) (end 91 88) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 93 71) (end 107 71) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 109 69) (end 109 55) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 107 53) (end 93 53) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 91 55) (end 91 69) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 112 109) (end 126 109) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 128 107) (end 128 93) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 126 91) (end 112 91) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 110 93) (end 110 107) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 112 90) (end 126 90) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 128 88) (end 128 74) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 126 72) (end 112 72) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 110 74) (end 110 88) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 112 71) (end 126 71) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 128 69) (end 128 55) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 126 53) (end 112 53) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 110 55) (end 110 69) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 131 104.25) (end 145 104.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 147 102.25) (end 147 88.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 145 86.25) (end 131 86.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 129 88.25) (end 129 102.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 131 85.25) (end 145 85.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 147 83.25) (end 147 69.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 145 67.25) (end 131 67.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 129 69.25) (end 129 83.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 131 66.25) (end 145 66.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 147 64.25) (end 147 50.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 145 48.25) (end 131 48.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 129 50.25) (end 129 64.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 150 101.875) (end 164 101.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 166 99.875) (end 166 85.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 164 83.875) (end 150 83.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 148 85.875) (end 148 99.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 150 82.875) (end 164 82.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 166 80.875) (end 166 66.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 164 64.875) (end 150 64.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 148 66.875) (end 148 80.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 150 63.875) (end 164 63.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 166 61.875) (end 166 47.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 164 45.875) (end 150 45.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 148 47.875) (end 148 61.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 169 104.25) (end 183 104.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 185 102.25) (end 185 88.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 183 86.25) (end 169 86.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 167 88.25) (end 167 102.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 169 85.25) (end 183 85.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 185 83.25) (end 185 69.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 183 67.25) (end 169 67.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 167 69.25) (end 167 83.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 169 66.25) (end 183 66.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 185 64.25) (end 185 50.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 183 48.25) (end 169 48.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 167 50.25) (end 167 64.25) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 188 106.625) (end 202 106.625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 204 104.625) (end 204 90.625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 202 88.625) (end 188 88.625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 186 90.625) (end 186 104.625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 188 87.625) (end 202 87.625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 204 85.625) (end 204 71.625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 202 69.625) (end 188 69.625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 186 71.625) (end 186 85.625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 188 68.625) (end 202 68.625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 204 66.625) (end 204 52.625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 202 50.625) (end 188 50.625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 186 52.625) (end 186 66.625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 159.5 123.875) (end 173.5 123.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 175.5 121.875) (end 175.5 107.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 173.5 105.875) (end 159.5 105.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 157.5 107.875) (end 157.5 121.875) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 178.40914797087967 124.50659912276711) (end 191.9321093727671 128.1300657157229) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 194.38159912276706 126.71585202912047) (end 198.00506571572294 113.19289062723283) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 196.59085202912036 110.7434008772329) (end 183.06789062723294 107.11993428427706) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 180.61840087723292 108.53414797087953) (end 176.99493428427706 122.05710937276717) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 107 107) (end 107 109) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 107 93) (end 109 93) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 93 93) (end 93 91) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 93 107) (end 91 107) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 107 88) (end 107 90) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 107 74) (end 109 74) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 93 74) (end 93 72) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 93 88) (end 91 88) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 107 69) (end 107 71) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 107 55) (end 109 55) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 93 55) (end 93 53) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 93 69) (end 91 69) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 126 107) (end 126 109) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 126 93) (end 128 93) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 112 93) (end 112 91) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 112 107) (end 110 107) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 126 88) (end 126 90) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 126 74) (end 128 74) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 112 74) (end 112 72) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 112 88) (end 110 88) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 126 69) (end 126 71) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 126 55) (end 128 55) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 112 55) (end 112 53) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 112 69) (end 110 69) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 145 102.25) (end 145 104.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 145 88.25) (end 147 88.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 131 88.25) (end 131 86.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 131 102.25) (end 129 102.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 145 83.25) (end 145 85.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 145 69.25) (end 147 69.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 131 69.25) (end 131 67.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 131 83.25) (end 129 83.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 145 64.25) (end 145 66.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 145 50.25) (end 147 50.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 131 50.25) (end 131 48.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 131 64.25) (end 129 64.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 164 99.875) (end 164 101.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 164 85.875) (end 166 85.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 150 85.875) (end 150 83.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 150 99.875) (end 148 99.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 164 80.875) (end 164 82.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 164 66.875) (end 166 66.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 150 66.875) (end 150 64.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 150 80.875) (end 148 80.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 164 61.875) (end 164 63.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 164 47.875) (end 166 47.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 150 47.875) (end 150 45.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 150 61.875) (end 148 61.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 183 102.25) (end 183 104.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 183 88.25) (end 185 88.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 169 88.25) (end 169 86.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 169 102.25) (end 167 102.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 183 83.25) (end 183 85.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 183 69.25) (end 185 69.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 169 69.25) (end 169 67.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 169 83.25) (end 167 83.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 183 64.25) (end 183 66.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 183 50.25) (end 185 50.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 169 50.25) (end 169 48.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 169 64.25) (end 167 64.25) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 202 104.625) (end 202 106.625) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 202 90.625) (end 204 90.625) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 188 90.625) (end 188 88.625) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 188 104.625) (end 186 104.625) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 202 85.625) (end 202 87.625) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 202 71.625) (end 204 71.625) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 188 71.625) (end 188 69.625) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 188 85.625) (end 186 85.625) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 202 66.625) (end 202 68.625) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 202 52.625) (end 204 52.625) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 188 52.625) (end 188 50.625) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 188 66.625) (end 186 66.625) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 173.5 121.875) (end 173.5 123.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 173.5 107.875) (end 175.5 107.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 159.5 107.875) (end 159.5 105.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 159.5 121.875) (end 157.5 121.875) (angle -90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 192.4497474044658 126.19821399742165) (end 191.9321094044658 128.13006569742166) (angle -89.99999999999687) (layer Dwgs.User) (width 0.15))
(gr_arc (start 196.07321399742165 112.67525259553406) (end 198.00506569742166 113.19289059553407) (angle -90.00000000000067) (layer Dwgs.User) (width 0.15))
(gr_arc (start 182.5502525955342 109.05178600257834) (end 183.0678905955342 107.11993430257834) (angle -89.99999999999815) (layer Dwgs.User) (width 0.15))
(gr_arc (start 178.92678600257835 122.57474740446582) (end 176.99493430257834 122.05710940446582) (angle -89.99999999999926) (layer Dwgs.User) (width 0.15))
(gr_line (start 211.79103439358497 135.84844979629634) (end 223.29103440641504 115.92986540370367) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 222.55898360641504 113.19781460370372) (end 210.43462800641498 106.1978146037037) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 207.70257720641504 106.92986540370367) (end 196.202577193585 126.84844979629628) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_line (start 196.934627993585 129.5805005962963) (end 209.05898359358497 136.58050059629625) (angle 90) (layer Dwgs.User) (width 0.15))
(gr_arc (start 221.558983606415 114.92986540370373) (end 223.291034406415 115.92986540370373) (angle -89.99999999999768) (layer Dwgs.User) (width 0.15))
(gr_arc (start 209.434628006415 107.9298654037037) (end 210.434628006415 106.1978146037037) (angle -89.99999999999822) (layer Dwgs.User) (width 0.15))
(gr_arc (start 197.93462799358502 127.84844979629622) (end 196.20257719358503 126.84844979629622) (angle -89.99999999999872) (layer Dwgs.User) (width 0.15))
(gr_arc (start 210.05898359358497 134.84844979629628) (end 209.05898359358497 136.58050059629628) (angle -89.99999999999903) (layer Dwgs.User) (width 0.15))
(gr_circle (center 109.5 71.5) (end 111.65 71.5) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 109.5 90.5) (end 111.65 90.5) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 185.468 67.986) (end 187.618 67.986) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 152.657 107.74) (end 154.80700000000002 107.74) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 199.2410516 115.3236576) (end 201.3910516 115.3236576) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 207.762 100.476) (end 208.862 100.476) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 222.194 108.995) (end 223.29399999999998 108.995) (layer Edge.Cuts) (width 0.15))
            
)

        