
            
(kicad_pcb (version 20171130) (host pcbnew 5.1.6)

  (page A3)
  (title_block
    (title right)
    (rev v1.0.0)
    (company Unknown)
  )

  (general
    (thickness 1.6)
  )

  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

            (net 0 "")
(net 1 "mirror_q_bottom")
(net 2 "C1")
(net 3 "mirror_q_home")
(net 4 "mirror_q_top")
(net 5 "mirror_q_num")
(net 6 "mirror_q_f")
(net 7 "mirror_w_bottom")
(net 8 "C2")
(net 9 "mirror_w_home")
(net 10 "mirror_w_top")
(net 11 "mirror_w_num")
(net 12 "mirror_w_f")
(net 13 "mirror_e_bottom")
(net 14 "C3")
(net 15 "mirror_e_home")
(net 16 "mirror_e_top")
(net 17 "mirror_e_num")
(net 18 "mirror_e_f")
(net 19 "mirror_r_bottom")
(net 20 "C4")
(net 21 "mirror_r_home")
(net 22 "mirror_r_top")
(net 23 "mirror_r_num")
(net 24 "mirror_r_f")
(net 25 "mirror_t_bottom")
(net 26 "C5")
(net 27 "mirror_t_home")
(net 28 "mirror_t_top")
(net 29 "mirror_t_num")
(net 30 "mirror_t_f")
(net 31 "mirror_one_down")
(net 32 "C0")
(net 33 "mirror_one_up")
(net 34 "mirror_two_down")
(net 35 "mirror_two_up")
(net 36 "mirror_three_down")
(net 37 "mirror_three_up")
(net 38 "mirror_one_f")
(net 39 "C6")
(net 40 "mirror_alt_space")
(net 41 "mirror_space_space")
(net 42 "mirror_sym_bottom")
(net 43 "mirror_sym_home")
(net 44 "mirror_sym_top")
(net 45 "mirror_sym_num")
(net 46 "mirror_sym_f")
(net 47 "mirror_sym_ctl_down")
(net 48 "C7")
(net 49 "mirror_sym_ctl_up")
(net 50 "mirror_one_enter")
(net 51 "mirror_one_back")
(net 52 "R4")
(net 53 "R3")
(net 54 "R2")
(net 55 "R1")
(net 56 "R0")
(net 57 "R7")
(net 58 "R6")
(net 59 "R5")
(net 60 "BAT_P")
(net 61 "GND")
(net 62 "RST")
(net 63 "VCC")
(net 64 "DPC")
(net 65 "DPD")
(net 66 "DPE")
(net 67 "DISP1_1")
(net 68 "DISP1_2")
(net 69 "DISP1_4")
(net 70 "DISP1_5")
            
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "")
(add_net "mirror_q_bottom")
(add_net "C1")
(add_net "mirror_q_home")
(add_net "mirror_q_top")
(add_net "mirror_q_num")
(add_net "mirror_q_f")
(add_net "mirror_w_bottom")
(add_net "C2")
(add_net "mirror_w_home")
(add_net "mirror_w_top")
(add_net "mirror_w_num")
(add_net "mirror_w_f")
(add_net "mirror_e_bottom")
(add_net "C3")
(add_net "mirror_e_home")
(add_net "mirror_e_top")
(add_net "mirror_e_num")
(add_net "mirror_e_f")
(add_net "mirror_r_bottom")
(add_net "C4")
(add_net "mirror_r_home")
(add_net "mirror_r_top")
(add_net "mirror_r_num")
(add_net "mirror_r_f")
(add_net "mirror_t_bottom")
(add_net "C5")
(add_net "mirror_t_home")
(add_net "mirror_t_top")
(add_net "mirror_t_num")
(add_net "mirror_t_f")
(add_net "mirror_one_down")
(add_net "C0")
(add_net "mirror_one_up")
(add_net "mirror_two_down")
(add_net "mirror_two_up")
(add_net "mirror_three_down")
(add_net "mirror_three_up")
(add_net "mirror_one_f")
(add_net "C6")
(add_net "mirror_alt_space")
(add_net "mirror_space_space")
(add_net "mirror_sym_bottom")
(add_net "mirror_sym_home")
(add_net "mirror_sym_top")
(add_net "mirror_sym_num")
(add_net "mirror_sym_f")
(add_net "mirror_sym_ctl_down")
(add_net "C7")
(add_net "mirror_sym_ctl_up")
(add_net "mirror_one_enter")
(add_net "mirror_one_back")
(add_net "R4")
(add_net "R3")
(add_net "R2")
(add_net "R1")
(add_net "R0")
(add_net "R7")
(add_net "R6")
(add_net "R5")
(add_net "BAT_P")
(add_net "GND")
(add_net "RST")
(add_net "VCC")
(add_net "DPC")
(add_net "DPD")
(add_net "DPE")
(add_net "DISP1_1")
(add_net "DISP1_2")
(add_net "DISP1_4")
(add_net "DISP1_5")
  )

            
          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 346.5 100 0) 

                
        (fp_text reference "S1" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 1 "mirror_q_bottom") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 2 "C1") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 346.5 83 0) 

                
        (fp_text reference "S2" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 3 "mirror_q_home") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 2 "C1") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 346.5 66 0) 

                
        (fp_text reference "S3" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 4 "mirror_q_top") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 2 "C1") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 346.5 49 0) 

                
        (fp_text reference "S4" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 5 "mirror_q_num") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 2 "C1") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 346.5 32 0) 

                
        (fp_text reference "S5" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 6 "mirror_q_f") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 2 "C1") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 328.5 100 0) 

                
        (fp_text reference "S6" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 7 "mirror_w_bottom") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 8 "C2") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 328.5 83 0) 

                
        (fp_text reference "S7" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 9 "mirror_w_home") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 8 "C2") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 328.5 66 0) 

                
        (fp_text reference "S8" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 10 "mirror_w_top") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 8 "C2") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 328.5 49 0) 

                
        (fp_text reference "S9" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 11 "mirror_w_num") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 8 "C2") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 328.5 32 0) 

                
        (fp_text reference "S10" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 12 "mirror_w_f") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 8 "C2") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 310.5 100 0) 

                
        (fp_text reference "S11" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 13 "mirror_e_bottom") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 14 "C3") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 310.5 83 0) 

                
        (fp_text reference "S12" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 15 "mirror_e_home") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 14 "C3") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 310.5 66 0) 

                
        (fp_text reference "S13" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 16 "mirror_e_top") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 14 "C3") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 310.5 49 0) 

                
        (fp_text reference "S14" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 17 "mirror_e_num") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 14 "C3") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 310.5 32 0) 

                
        (fp_text reference "S15" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 18 "mirror_e_f") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 14 "C3") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 292.5 100 0) 

                
        (fp_text reference "S16" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 19 "mirror_r_bottom") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 20 "C4") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 292.5 83 0) 

                
        (fp_text reference "S17" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 21 "mirror_r_home") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 20 "C4") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 292.5 66 0) 

                
        (fp_text reference "S18" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 22 "mirror_r_top") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 20 "C4") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 292.5 49 0) 

                
        (fp_text reference "S19" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 23 "mirror_r_num") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 20 "C4") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 292.5 32 0) 

                
        (fp_text reference "S20" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 24 "mirror_r_f") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 20 "C4") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 274.5 100 0) 

                
        (fp_text reference "S21" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 25 "mirror_t_bottom") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 26 "C5") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 274.5 83 0) 

                
        (fp_text reference "S22" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 27 "mirror_t_home") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 26 "C5") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 274.5 66 0) 

                
        (fp_text reference "S23" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 28 "mirror_t_top") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 26 "C5") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 274.5 49 0) 

                
        (fp_text reference "S24" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 29 "mirror_t_num") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 26 "C5") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 274.5 32 0) 

                
        (fp_text reference "S25" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 30 "mirror_t_f") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 26 "C5") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 364.5 134 0) 

                
        (fp_text reference "S26" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 31 "mirror_one_down") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 32 "C0") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 364.5 117 0) 

                
        (fp_text reference "S27" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 33 "mirror_one_up") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 32 "C0") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 346.5 134 0) 

                
        (fp_text reference "S28" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 34 "mirror_two_down") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 2 "C1") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 346.5 117 0) 

                
        (fp_text reference "S29" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 35 "mirror_two_up") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 2 "C1") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 328.5 134 0) 

                
        (fp_text reference "S30" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 36 "mirror_three_down") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 8 "C2") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 328.5 117 0) 

                
        (fp_text reference "S31" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 37 "mirror_three_up") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 8 "C2") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 252 32 0) 

                
        (fp_text reference "S32" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 38 "mirror_one_f") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 39 "C6") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 310.5 117 0) 

                
        (fp_text reference "S33" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 40 "mirror_alt_space") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 14 "C3") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 270 117 0) 

                
        (fp_text reference "S34" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 41 "mirror_space_space") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 20 "C4") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 364.5 100 0) 

                
        (fp_text reference "S35" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 42 "mirror_sym_bottom") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 32 "C0") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 364.5 83 0) 

                
        (fp_text reference "S36" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 43 "mirror_sym_home") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 32 "C0") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 364.5 66 0) 

                
        (fp_text reference "S37" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 44 "mirror_sym_top") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 32 "C0") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 364.5 49 0) 

                
        (fp_text reference "S38" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 45 "mirror_sym_num") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 32 "C0") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 364.5 32 0) 

                
        (fp_text reference "S39" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 46 "mirror_sym_f") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 32 "C0") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 387 134 0) 

                
        (fp_text reference "S40" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 47 "mirror_sym_ctl_down") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 48 "C7") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 387 117 0) 

                
        (fp_text reference "S41" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 49 "mirror_sym_ctl_up") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 48 "C7") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 387 100 0) 

                
        (fp_text reference "S42" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 42 "mirror_sym_bottom") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 48 "C7") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 387 83 0) 

                
        (fp_text reference "S43" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 43 "mirror_sym_home") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 48 "C7") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 387 66 0) 

                
        (fp_text reference "S44" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 44 "mirror_sym_top") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 48 "C7") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 387 49 0) 

                
        (fp_text reference "S45" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 45 "mirror_sym_num") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 48 "C7") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 387 32 0) 

                
        (fp_text reference "S46" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 46 "mirror_sym_f") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 48 "C7") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 252 91.5 -270) 

                
        (fp_text reference "S47" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 50 "mirror_one_enter") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 39 "C6") (clearance 0.2))
			  )
          

          
        (module lib:Kailh_PG1232 (layer F.Cu) (tedit 5E1ADAC2)
        (at 252 57.5 -270) 

                
        (fp_text reference "S48" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value Kailh_PG1232 (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_line (start -7.25 -6.75) (end -6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 -6.75) (end -7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start -7.25 6.75) (end -6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start -7.25 6.75) (end -7.25 5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 -6.75) (end 6.25 -6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 -6.75) (end 7.25 -5.75) (layer Dwgs.User) (width 0.15))

        (fp_line (start 7.25 6.75) (end 6.25 6.75) (layer Dwgs.User) (width 0.15))
        (fp_line (start 7.25 6.75) (end 7.25 5.75) (layer Dwgs.User) (width 0.15))


        (fp_line (start 2.8 -5.35) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end 2.8 -3.2) (layer Dwgs.User) (width 0.15))
        (fp_line (start 2.8 -3.2) (end 2.8 -5.35) (layer Dwgs.User) (width 0.15))
        (fp_line (start -2.8 -3.2) (end -2.8 -5.35) (layer Dwgs.User) (width 0.15))
        
                	 
        (fp_line (start 2.25 2.6) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 2.25 3.6) (end 2.25 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 3.6) (end 2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -2.25 2.6) (end -2.25 3.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 2.6) (end -5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        (fp_line (start 5.8 -2.95) (end 5.8 2.6) (layer Edge.Cuts) (width 0.12))
        (fp_line (start -5.8 -2.95) (end 5.8 -2.95) (layer Edge.Cuts) (width 0.12))
        
            
        (pad 3 thru_hole circle (at 5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
        (pad 4 thru_hole circle (at -5.3 -4.75) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (clearance 0.2))
      
          
        
        (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.15))
        (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.15))
        
          
        
        (pad 1 thru_hole circle (at -4.58 5.1) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 51 "mirror_one_back") (clearance 0.2))
        (pad 2 thru_hole circle (at 2 5.4) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (net 39 "C6") (clearance 0.2))
			  )
          

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 354.5 100 -90)
        (attr virtual)

        
        (fp_text reference "D1" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 1 "mirror_q_bottom"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 1 "mirror_q_bottom"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 52 "R4"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 1 "mirror_q_bottom"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 354.5 83 -90)
        (attr virtual)

        
        (fp_text reference "D2" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 3 "mirror_q_home"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 3 "mirror_q_home"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 53 "R3"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 3 "mirror_q_home"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 354.5 66 -90)
        (attr virtual)

        
        (fp_text reference "D3" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 4 "mirror_q_top"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 4 "mirror_q_top"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 54 "R2"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 4 "mirror_q_top"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 354.5 49 -90)
        (attr virtual)

        
        (fp_text reference "D4" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 5 "mirror_q_num"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 5 "mirror_q_num"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 55 "R1"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 5 "mirror_q_num"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 354.5 32 -90)
        (attr virtual)

        
        (fp_text reference "D5" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 6 "mirror_q_f"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 6 "mirror_q_f"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 56 "R0"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 6 "mirror_q_f"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 336.5 100 -90)
        (attr virtual)

        
        (fp_text reference "D6" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 7 "mirror_w_bottom"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 7 "mirror_w_bottom"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 52 "R4"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 7 "mirror_w_bottom"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 336.5 83 -90)
        (attr virtual)

        
        (fp_text reference "D7" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 9 "mirror_w_home"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 9 "mirror_w_home"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 53 "R3"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 9 "mirror_w_home"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 336.5 66 -90)
        (attr virtual)

        
        (fp_text reference "D8" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 10 "mirror_w_top"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 10 "mirror_w_top"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 54 "R2"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 10 "mirror_w_top"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 336.5 49 -90)
        (attr virtual)

        
        (fp_text reference "D9" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 11 "mirror_w_num"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 11 "mirror_w_num"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 55 "R1"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 11 "mirror_w_num"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 336.5 32 -90)
        (attr virtual)

        
        (fp_text reference "D10" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 12 "mirror_w_f"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 12 "mirror_w_f"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 56 "R0"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 12 "mirror_w_f"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 318.5 100 -90)
        (attr virtual)

        
        (fp_text reference "D11" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 13 "mirror_e_bottom"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 13 "mirror_e_bottom"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 52 "R4"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 13 "mirror_e_bottom"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 318.5 83 -90)
        (attr virtual)

        
        (fp_text reference "D12" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 15 "mirror_e_home"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 15 "mirror_e_home"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 53 "R3"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 15 "mirror_e_home"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 318.5 66 -90)
        (attr virtual)

        
        (fp_text reference "D13" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 16 "mirror_e_top"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 16 "mirror_e_top"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 54 "R2"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 16 "mirror_e_top"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 318.5 49 -90)
        (attr virtual)

        
        (fp_text reference "D14" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 17 "mirror_e_num"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 17 "mirror_e_num"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 55 "R1"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 17 "mirror_e_num"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 318.5 32 -90)
        (attr virtual)

        
        (fp_text reference "D15" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 18 "mirror_e_f"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 18 "mirror_e_f"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 56 "R0"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 18 "mirror_e_f"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 300.5 100 -90)
        (attr virtual)

        
        (fp_text reference "D16" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 19 "mirror_r_bottom"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 19 "mirror_r_bottom"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 52 "R4"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 19 "mirror_r_bottom"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 300.5 83 -90)
        (attr virtual)

        
        (fp_text reference "D17" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 21 "mirror_r_home"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 21 "mirror_r_home"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 53 "R3"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 21 "mirror_r_home"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 300.5 66 -90)
        (attr virtual)

        
        (fp_text reference "D18" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 22 "mirror_r_top"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 22 "mirror_r_top"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 54 "R2"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 22 "mirror_r_top"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 300.5 49 -90)
        (attr virtual)

        
        (fp_text reference "D19" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 23 "mirror_r_num"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 23 "mirror_r_num"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 55 "R1"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 23 "mirror_r_num"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 300.5 32 -90)
        (attr virtual)

        
        (fp_text reference "D20" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 24 "mirror_r_f"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 24 "mirror_r_f"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 56 "R0"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 24 "mirror_r_f"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 282.5 100 -90)
        (attr virtual)

        
        (fp_text reference "D21" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 25 "mirror_t_bottom"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 25 "mirror_t_bottom"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 52 "R4"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 25 "mirror_t_bottom"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 282.5 83 -90)
        (attr virtual)

        
        (fp_text reference "D22" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 27 "mirror_t_home"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 27 "mirror_t_home"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 53 "R3"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 27 "mirror_t_home"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 282.5 66 -90)
        (attr virtual)

        
        (fp_text reference "D23" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 28 "mirror_t_top"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 28 "mirror_t_top"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 54 "R2"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 28 "mirror_t_top"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 282.5 49 -90)
        (attr virtual)

        
        (fp_text reference "D24" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 29 "mirror_t_num"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 29 "mirror_t_num"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 55 "R1"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 29 "mirror_t_num"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 282.5 32 -90)
        (attr virtual)

        
        (fp_text reference "D25" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 30 "mirror_t_f"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 30 "mirror_t_f"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 56 "R0"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 30 "mirror_t_f"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 372.5 134 -90)
        (attr virtual)

        
        (fp_text reference "D26" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 57 "R7"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 31 "mirror_one_down"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 57 "R7"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 31 "mirror_one_down"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 57 "R7"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 31 "mirror_one_down"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 372.5 117 -90)
        (attr virtual)

        
        (fp_text reference "D27" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 57 "R7"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 33 "mirror_one_up"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 57 "R7"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 33 "mirror_one_up"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 57 "R7"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 33 "mirror_one_up"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 354.5 134 -90)
        (attr virtual)

        
        (fp_text reference "D28" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 57 "R7"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 34 "mirror_two_down"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 57 "R7"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 34 "mirror_two_down"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 57 "R7"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 34 "mirror_two_down"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 354.5 117 -90)
        (attr virtual)

        
        (fp_text reference "D29" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 57 "R7"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 35 "mirror_two_up"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 57 "R7"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 35 "mirror_two_up"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 57 "R7"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 35 "mirror_two_up"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 336.5 134 -90)
        (attr virtual)

        
        (fp_text reference "D30" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 57 "R7"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 36 "mirror_three_down"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 57 "R7"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 36 "mirror_three_down"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 57 "R7"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 36 "mirror_three_down"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 336.5 117 -90)
        (attr virtual)

        
        (fp_text reference "D31" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 57 "R7"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 37 "mirror_three_up"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 57 "R7"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 37 "mirror_three_up"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 57 "R7"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 37 "mirror_three_up"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 260 91.5 -90)
        (attr virtual)

        
        (fp_text reference "D32" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 50 "mirror_one_enter"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 50 "mirror_one_enter"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 54 "R2"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 50 "mirror_one_enter"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 260 57.5 -90)
        (attr virtual)

        
        (fp_text reference "D33" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 51 "mirror_one_back"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 51 "mirror_one_back"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 55 "R1"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 51 "mirror_one_back"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 260 32 -90)
        (attr virtual)

        
        (fp_text reference "D34" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 38 "mirror_one_f"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 38 "mirror_one_f"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 56 "R0"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 38 "mirror_one_f"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 318.5 117 -90)
        (attr virtual)

        
        (fp_text reference "D35" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 58 "R6"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 40 "mirror_alt_space"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 58 "R6"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 40 "mirror_alt_space"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 58 "R6"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 40 "mirror_alt_space"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 278 117 -90)
        (attr virtual)

        
        (fp_text reference "D36" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 58 "R6"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 41 "mirror_space_space"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 58 "R6"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 41 "mirror_space_space"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 58 "R6"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 41 "mirror_space_space"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 372.5 100 -90)
        (attr virtual)

        
        (fp_text reference "D37" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 42 "mirror_sym_bottom"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 42 "mirror_sym_bottom"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 52 "R4"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 42 "mirror_sym_bottom"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 372.5 83 -90)
        (attr virtual)

        
        (fp_text reference "D38" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 43 "mirror_sym_home"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 43 "mirror_sym_home"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 53 "R3"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 43 "mirror_sym_home"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 372.5 66 -90)
        (attr virtual)

        
        (fp_text reference "D39" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 44 "mirror_sym_top"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 44 "mirror_sym_top"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 54 "R2"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 44 "mirror_sym_top"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 372.5 49 -90)
        (attr virtual)

        
        (fp_text reference "D40" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 45 "mirror_sym_num"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 45 "mirror_sym_num"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 55 "R1"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 45 "mirror_sym_num"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 372.5 32 -90)
        (attr virtual)

        
        (fp_text reference "D41" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 46 "mirror_sym_f"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 46 "mirror_sym_f"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 56 "R0"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 46 "mirror_sym_f"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 395 134 -90)
        (attr virtual)

        
        (fp_text reference "D42" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 58 "R6"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 47 "mirror_sym_ctl_down"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 58 "R6"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 47 "mirror_sym_ctl_down"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 58 "R6"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 47 "mirror_sym_ctl_down"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 395 117 -90)
        (attr virtual)

        
        (fp_text reference "D43" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 59 "R5"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 49 "mirror_sym_ctl_up"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 59 "R5"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 49 "mirror_sym_ctl_up"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 59 "R5"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 49 "mirror_sym_ctl_up"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 395 100 -90)
        (attr virtual)

        
        (fp_text reference "D44" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 42 "mirror_sym_bottom"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 52 "R4"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 42 "mirror_sym_bottom"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 52 "R4"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 42 "mirror_sym_bottom"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 395 83 -90)
        (attr virtual)

        
        (fp_text reference "D45" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 43 "mirror_sym_home"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 53 "R3"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 43 "mirror_sym_home"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 53 "R3"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 43 "mirror_sym_home"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 395 66 -90)
        (attr virtual)

        
        (fp_text reference "D46" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 44 "mirror_sym_top"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 54 "R2"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 44 "mirror_sym_top"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 54 "R2"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 44 "mirror_sym_top"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 395 49 -90)
        (attr virtual)

        
        (fp_text reference "D47" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 45 "mirror_sym_num"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 55 "R1"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 45 "mirror_sym_num"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 55 "R1"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 45 "mirror_sym_num"))
        
    )
    

    (module ComboDiode (layer F.Cu) (tedit 5B24D78E)
        (at 395 32 -90)
        (attr virtual)

        
        (fp_text reference "D48" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        
        (fp_line (start 0.25 0) (end 0.75 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer F.SilkS) (width 0.1))
        (fp_line (start 0.25 0) (end 0.75 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 0.4) (end -0.35 0) (layer B.SilkS) (width 0.1))
        (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end 0.25 -0.4) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.SilkS) (width 0.1))
        (fp_line (start -0.75 0) (end -0.35 0) (layer B.SilkS) (width 0.1))

        
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 46 "mirror_sym_f"))
        (pad 1 smd rect (at -1.65 0 -90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask) (net 56 "R0"))
        (pad 2 smd rect (at 1.65 0 -90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask) (net 46 "mirror_sym_f"))

        
        
        (pad 1 thru_hole rect (at -3.81 0 -90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask) (net 56 "R0"))
        (pad 2 thru_hole circle (at 3.81 0 -90) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask) (net 46 "mirror_sym_f"))
        
    )
    

        
      (module ProMicro (layer F.Cu) (tedit 5B307E4C)
      (at 228.25 43.53 -90)

      
      (fp_text reference "MCU1" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
    
      
      (fp_line (start -19.304 -3.81) (end -14.224 -3.81) (layer Dwgs.User) (width 0.15))
      (fp_line (start -19.304 3.81) (end -19.304 -3.81) (layer Dwgs.User) (width 0.15))
      (fp_line (start -14.224 3.81) (end -19.304 3.81) (layer Dwgs.User) (width 0.15))
      (fp_line (start -14.224 -3.81) (end -14.224 3.81) (layer Dwgs.User) (width 0.15))
    
      
      (fp_line (start -17.78 8.89) (end 15.24 8.89) (layer F.SilkS) (width 0.15))
      (fp_line (start 15.24 8.89) (end 15.24 -8.89) (layer F.SilkS) (width 0.15))
      (fp_line (start 15.24 -8.89) (end -17.78 -8.89) (layer F.SilkS) (width 0.15))
      (fp_line (start -17.78 -8.89) (end -17.78 8.89) (layer F.SilkS) (width 0.15))
      
        
        
        (fp_line (start -15.24 6.35) (end -12.7 6.35) (layer F.SilkS) (width 0.15))
        (fp_line (start -15.24 6.35) (end -15.24 8.89) (layer F.SilkS) (width 0.15))
        (fp_line (start -12.7 6.35) (end -12.7 8.89) (layer F.SilkS) (width 0.15))
      
        
        (fp_text user RAW (at -13.97 4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user GND (at -11.43 4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user RST (at -8.89 4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user VCC (at -6.35 4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P21 (at -3.81 4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P20 (at -1.27 4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P19 (at 1.27 4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P18 (at 3.81 4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P15 (at 6.35 4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P14 (at 8.89 4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P16 (at 11.43 4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P10 (at 13.97 4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
      
        (fp_text user P01 (at -13.97 -4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P00 (at -11.43 -4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user GND (at -8.89 -4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user GND (at -6.35 -4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P02 (at -3.81 -4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P03 (at -1.27 -4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P04 (at 1.27 -4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P05 (at 3.81 -4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P06 (at 6.35 -4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P07 (at 8.89 -4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P08 (at 11.43 -4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
        (fp_text user P09 (at 13.97 -4.8 0) (layer F.SilkS) (effects (font (size 0.8 0.8) (thickness 0.15))))
      
        
        (pad 1 thru_hole rect (at -13.97 7.62 -90) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 60 "BAT_P"))
        (pad 2 thru_hole circle (at -11.43 7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 61 "GND"))
        (pad 3 thru_hole circle (at -8.89 7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 62 "RST"))
        (pad 4 thru_hole circle (at -6.35 7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 63 "VCC"))
        (pad 5 thru_hole circle (at -3.81 7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 32 "C0"))
        (pad 6 thru_hole circle (at -1.27 7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 2 "C1"))
        (pad 7 thru_hole circle (at 1.27 7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 8 "C2"))
        (pad 8 thru_hole circle (at 3.81 7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 14 "C3"))
        (pad 9 thru_hole circle (at 6.35 7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 20 "C4"))
        (pad 10 thru_hole circle (at 8.89 7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 26 "C5"))
        (pad 11 thru_hole circle (at 11.43 7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 39 "C6"))
        (pad 12 thru_hole circle (at 13.97 7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 48 "C7"))
        
        (pad 13 thru_hole circle (at -13.97 -7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 64 "DPC"))
        (pad 14 thru_hole circle (at -11.43 -7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 65 "DPD"))
        (pad 15 thru_hole circle (at -8.89 -7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 61 "GND"))
        (pad 16 thru_hole circle (at -6.35 -7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 61 "GND"))
        (pad 17 thru_hole circle (at -3.81 -7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 66 "DPE"))
        (pad 18 thru_hole circle (at -1.27 -7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 55 "R1"))
        (pad 19 thru_hole circle (at 1.27 -7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 54 "R2"))
        (pad 20 thru_hole circle (at 3.81 -7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 53 "R3"))
        (pad 21 thru_hole circle (at 6.35 -7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 52 "R4"))
        (pad 22 thru_hole circle (at 8.89 -7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 59 "R5"))
        (pad 23 thru_hole circle (at 11.43 -7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 58 "R6"))
        (pad 24 thru_hole circle (at 13.97 -7.62 0) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask) (net 57 "R7"))
      )
        

      (module nice!view (layer F.Cu) (tedit 6448AF5B)
        (at 228.25 44.53 0)
        (attr virtual)
        (fp_text reference "DISP1" (at 0 20 0) (layer F.SilkS) hide
          (effects (font (size 1 1) (thickness 0.15)))
        )
        
        (fp_line (start -6.5 -18) (end 6.5 -18) (layer F.Fab) (width 0.15))
        (fp_line (start 6.5 18) (end -6.5 18) (layer F.Fab) (width 0.15))
        (fp_line (start -7 17.5) (end -7 -17.5) (layer F.Fab) (width 0.15))
        (fp_line (start 7 17.5) (end 7 -17.5) (layer F.Fab) (width 0.15))
        (fp_line (start -6.41 15.37) (end -6.41 18.03) (layer F.SilkS) (width 0.12))
        (fp_line (start 6.41 18.03) (end -6.41 18.03) (layer F.SilkS) (width 0.12))
        (fp_line (start 6.88 14.9) (end 6.88 18.45) (layer F.CrtYd) (width 0.15))
        (fp_line (start 6.88 18.45) (end -6.82 18.45) (layer F.CrtYd) (width 0.15))
        (fp_line (start -6.82 18.45) (end -6.82 14.9) (layer F.CrtYd) (width 0.15))
        (fp_line (start -6.82 14.9) (end 6.88 14.9) (layer F.CrtYd) (width 0.15))
        (fp_line (start 6.41 15.37) (end 6.41 18.03) (layer F.SilkS) (width 0.12))
        (fp_line (start 6.41 15.37) (end -6.41 15.37) (layer F.SilkS) (width 0.12))
        (fp_arc (start -6.5 17.5) (end -7 17.5) (angle -90) (layer F.Fab) (width 0.15))
        (fp_arc (start 6.5 17.5) (end 6.5 18) (angle -90) (layer F.Fab) (width 0.15))
        (fp_arc (start 6.5 -17.5) (end 6.5 -18) (angle 90) (layer F.Fab) (width 0.15))
        (fp_arc (start -6.5 -17.5) (end -6.5 -18) (angle -90) (layer F.Fab) (width 0.15))
        (fp_text user %R (at 0 20 0) (layer F.Fab)
          (effects (font (size 1 1) (thickness 0.15)))
        )

    
        (fp_line (start 6.41 15.37) (end 6.41 18.03) (layer B.SilkS) (width 0.12))
        (fp_line (start 6.41 15.37) (end -6.41 15.37) (layer B.SilkS) (width 0.12))
        (fp_line (start 6.41 18.03) (end -6.41 18.03) (layer B.SilkS) (width 0.12))
        (fp_line (start 6.88 14.9) (end 6.88 18.45) (layer B.CrtYd) (width 0.15))
        (fp_line (start 6.88 18.45) (end -6.82 18.45) (layer B.CrtYd) (width 0.15))
        (fp_line (start -6.82 18.45) (end -6.82 14.9) (layer B.CrtYd) (width 0.15))
        (fp_line (start -6.82 14.9) (end 6.88 14.9) (layer B.CrtYd) (width 0.15))
        (fp_line (start -6.41 15.37) (end -6.41 18.03) (layer B.SilkS) (width 0.12))
        (fp_line (start -6.5 18) (end 6.5 18) (layer B.Fab) (width 0.15))
        (fp_line (start 7 -17.5) (end 7 17.5) (layer B.Fab) (width 0.15))
        (fp_line (start 6.5 -18) (end -6.5 -18) (layer B.Fab) (width 0.15))
        (fp_line (start -7 -17.5) (end -7 17.5) (layer B.Fab) (width 0.15))
        (fp_arc (start -6.5 -17.5) (end -7 -17.5) (angle 90) (layer B.Fab) (width 0.15))
        (fp_arc (start 6.5 -17.5) (end 6.5 -18) (angle 90) (layer B.Fab) (width 0.15))
        (fp_arc (start 6.5 17.5) (end 6.5 18) (angle -90) (layer B.Fab) (width 0.15))
        (fp_arc (start -6.5 17.5) (end -6.5 18) (angle 90) (layer B.Fab) (width 0.15))
    
        (fp_line (start 5.93 12.9) (end 5.93 14.9) (layer F.Fab) (width 0.15))
        (fp_line (start -5.93 14.9) (end -5.93 12.9) (layer F.Fab) (width 0.15))
        (fp_line (start -5.93 12.9) (end -4.23 12.9) (layer F.Fab) (width 0.15))
        (fp_line (start -4.23 14.9) (end -5.93 14.9) (layer F.Fab) (width 0.15))
        (fp_line (start -4.23 12.9) (end -4.23 14.9) (layer F.Fab) (width 0.15))
        (fp_line (start -3.39 14.9) (end -3.39 12.9) (layer F.Fab) (width 0.15))
        (fp_line (start -3.39 12.9) (end -1.69 12.9) (layer F.Fab) (width 0.15))
        (fp_line (start -1.69 14.9) (end -3.39 14.9) (layer F.Fab) (width 0.15))
        (fp_line (start -1.69 12.9) (end -1.69 14.9) (layer F.Fab) (width 0.15))
        (fp_line (start 3.39 12.9) (end 3.39 14.9) (layer F.Fab) (width 0.15))
        (fp_line (start 3.39 14.9) (end 1.69 14.9) (layer F.Fab) (width 0.15))
        (fp_line (start 1.69 14.9) (end 1.69 12.9) (layer F.Fab) (width 0.15))
        (fp_line (start 1.69 12.9) (end 3.39 12.9) (layer F.Fab) (width 0.15))
        (fp_line (start 5.93 14.9) (end 4.23 14.9) (layer F.Fab) (width 0.15))
        (fp_line (start 4.23 14.9) (end 4.23 12.9) (layer F.Fab) (width 0.15))
        (fp_line (start 4.23 12.9) (end 5.93 12.9) (layer F.Fab) (width 0.15))

        (pad 14 smd rect (at -5.08 13.45 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 65 "DPD"))
        (pad 15 smd rect (at -2.54 13.45 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 64 "DPC"))
        (pad 16 smd rect (at 2.54 13.45 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 61 "GND"))
        (pad 17 smd rect (at 5.08 13.45 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 66 "DPE"))

        (pad 10 smd rect (at -5.08 14.35 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 67 "DISP1_1"))
        (pad 11 smd rect (at -2.54 14.35 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 68 "DISP1_2"))
        (pad 12 smd rect (at 2.54 14.35 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 69 "DISP1_4"))
        (pad 13 smd rect (at 5.08 14.35 90) (size 0.6 1.2) (layers F.Cu F.Mask) (net 70 "DISP1_5"))
    
        (fp_line (start -5.93 12.9) (end -5.93 14.9) (layer B.Fab) (width 0.15))
        (fp_line (start -5.93 14.9) (end -4.23 14.9) (layer B.Fab) (width 0.15))
        (fp_line (start -4.23 12.9) (end -5.93 12.9) (layer B.Fab) (width 0.15))
        (fp_line (start -4.23 14.9) (end -4.23 12.9) (layer B.Fab) (width 0.15))
        (fp_line (start -3.39 14.9) (end -1.69 14.9) (layer B.Fab) (width 0.15))
        (fp_line (start -1.69 12.9) (end -3.39 12.9) (layer B.Fab) (width 0.15))
        (fp_line (start 4.23 14.9) (end 5.93 14.9) (layer B.Fab) (width 0.15))
        (fp_line (start 5.93 14.9) (end 5.93 12.9) (layer B.Fab) (width 0.15))
        (fp_line (start 3.39 12.9) (end 1.69 12.9) (layer B.Fab) (width 0.15))
        (fp_line (start -1.69 14.9) (end -1.69 12.9) (layer B.Fab) (width 0.15))
        (fp_line (start -3.39 12.9) (end -3.39 14.9) (layer B.Fab) (width 0.15))
        (fp_line (start 1.69 12.9) (end 1.69 14.9) (layer B.Fab) (width 0.15))
        (fp_line (start 1.69 14.9) (end 3.39 14.9) (layer B.Fab) (width 0.15))
        (fp_line (start 3.39 14.9) (end 3.39 12.9) (layer B.Fab) (width 0.15))
        (fp_line (start 5.93 12.9) (end 4.23 12.9) (layer B.Fab) (width 0.15))
        (fp_line (start 4.23 12.9) (end 4.23 14.9) (layer B.Fab) (width 0.15))

        (pad 24 smd rect (at 5.08 13.45 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 65 "DPD"))
        (pad 25 smd rect (at 2.54 13.45 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 64 "DPC"))
        (pad 26 smd rect (at -2.54 13.45 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 61 "GND"))
        (pad 27 smd rect (at -5.08 13.45 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 66 "DPE"))

        (pad 20 smd rect (at 5.08 14.35 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 70 "DISP1_5"))
        (pad 21 smd rect (at 2.54 14.35 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 69 "DISP1_4"))
        (pad 22 smd rect (at -2.54 14.35 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 68 "DISP1_2"))
        (pad 23 smd rect (at -5.08 14.35 270) (size 0.6 1.2) (layers B.Cu B.Mask) (net 67 "DISP1_1"))
    
      (pad 1 thru_hole oval (at -5.08 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 67 "DISP1_1"))
      (pad 2 thru_hole oval (at -2.54 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 68 "DISP1_2"))
      (pad 3 thru_hole oval (at 0 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 63 "VCC"))
      (pad 4 thru_hole oval (at 2.54 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 69 "DISP1_4"))
      (pad 5 thru_hole circle (at 5.08 16.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (net 70 "DISP1_5"))

      (fp_line (start 5.4 13.4) (end 5.4 -11.9) (layer Dwgs.User) (width 0.15))
      (fp_line (start -5.4 13.4) (end -5.4 -11.9) (layer Dwgs.User) (width 0.15))
      (fp_line (start 5.4 -11.9) (end -5.4 -11.9) (layer Dwgs.User) (width 0.15))
      (fp_line (start -5.4 13.4) (end 5.4 13.4) (layer Dwgs.User) (width 0.15))
    )
    

    
    (module JST_PH_S2B-PH-K_02x2.00mm_Angled (layer F.Cu) (tedit 58D3FE32)

        (descr "JST PH series connector, S2B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
        (tags "connector jst ph")

        (at 232.55 65.04 0)

        
        (fp_text reference "JST1" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

        (fp_line (start -2.25 0.25) (end -2.25 -1.35) (layer F.SilkS) (width 0.15))
        (fp_line (start -2.25 -1.35) (end -2.95 -1.35) (layer F.SilkS) (width 0.15))
        (fp_line (start -2.95 -1.35) (end -2.95 6.25) (layer F.SilkS) (width 0.15))
        (fp_line (start -2.95 6.25) (end 2.95 6.25) (layer F.SilkS) (width 0.15))
        (fp_line (start 2.95 6.25) (end 2.95 -1.35) (layer F.SilkS) (width 0.15))
        (fp_line (start 2.95 -1.35) (end 2.25 -1.35) (layer F.SilkS) (width 0.15))
        (fp_line (start 2.25 -1.35) (end 2.25 0.25) (layer F.SilkS) (width 0.15))
        (fp_line (start 2.25 0.25) (end -2.25 0.25) (layer F.SilkS) (width 0.15))

        (fp_line (start -1 1.5) (end -1 2.0) (layer F.SilkS) (width 0.15))
        (fp_line (start -1.25 1.75) (end -0.75 1.75) (layer F.SilkS) (width 0.15))

        (pad 1 thru_hole rect (at -1 0 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask) (net 60 "BAT_P"))
        (pad 2 thru_hole oval (at 1 0 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask) (net 61 "GND"))
            
    )
    
    

    
    (module E73:SW_TACT_ALPS_SKQGABE010 (layer F.Cu) (tstamp 5BF2CC94)

        (descr "Low-profile SMD Tactile Switch, https://www.e-switch.com/product-catalog/tact/product-lines/tl3342-series-low-profile-smt-tact-switch")
        (tags "SPST Tactile Switch")

        (at 223.95 68.04 0)
        
        (fp_text reference "B1" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        
        
        (fp_line (start 2.75 1.25) (end 1.25 2.75) (layer F.SilkS) (width 0.15))
        (fp_line (start 2.75 -1.25) (end 1.25 -2.75) (layer F.SilkS) (width 0.15))
        (fp_line (start 2.75 -1.25) (end 2.75 1.25) (layer F.SilkS) (width 0.15))
        (fp_line (start -1.25 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.15))
        (fp_line (start -1.25 -2.75) (end 1.25 -2.75) (layer F.SilkS) (width 0.15))
        (fp_line (start -2.75 1.25) (end -1.25 2.75) (layer F.SilkS) (width 0.15))
        (fp_line (start -2.75 -1.25) (end -1.25 -2.75) (layer F.SilkS) (width 0.15))
        (fp_line (start -2.75 -1.25) (end -2.75 1.25) (layer F.SilkS) (width 0.15))
        
        
        (pad 1 smd rect (at -3.1 -1.85 0) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask) (net 61 "GND"))
        (pad 1 smd rect (at 3.1 -1.85 0) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask) (net 61 "GND"))
        (pad 2 smd rect (at -3.1 1.85 0) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask) (net 62 "RST"))
        (pad 2 smd rect (at 3.1 1.85 0) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask) (net 62 "RST"))
    )
    
    
            (gr_line (start 400.5 140.5) (end 400.5 25.5) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 220 23.5) (end 398.5 23.5) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 220 125.5) (end 313 125.5) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 315 127.5) (end 315 140.5) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 317 142.5) (end 398.5 142.5) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 398.5 25.5) (end 400.5 25.5) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 313 127.5) (end 315 127.5) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 317 140.5) (end 315 140.5) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 398.5 140.5) (end 398.5 142.5) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 218 25.5) (end 218 123.5) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 220 25.5) (end 220 23.5) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 220 123.5) (end 218 123.5) (angle -90) (layer Edge.Cuts) (width 0.15))
            
)

        