
            
(kicad_pcb (version 20171130) (host pcbnew 5.1.6)

  (page A3)
  (title_block
    (title corney_island)
    (rev v1.0.0)
    (company Unknown)
  )

  (general
    (thickness 1.6)
  )

  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

            (net 0 "")
(net 1 "C0")
(net 2 "outer_bottom")
(net 3 "outer_home")
(net 4 "outer_top")
(net 5 "C1")
(net 6 "pinky_bottom")
(net 7 "pinky_home")
(net 8 "pinky_top")
(net 9 "C2")
(net 10 "ring_bottom")
(net 11 "ring_home")
(net 12 "ring_top")
(net 13 "C3")
(net 14 "middle_bottom")
(net 15 "middle_home")
(net 16 "middle_top")
(net 17 "C4")
(net 18 "index_bottom")
(net 19 "index_home")
(net 20 "index_top")
(net 21 "C5")
(net 22 "inner_bottom")
(net 23 "inner_home")
(net 24 "inner_top")
(net 25 "near_home")
(net 26 "far_home")
(net 27 "R0")
(net 28 "R1")
(net 29 "R2")
(net 30 "R3")
(net 31 "RAW")
(net 32 "GND")
(net 33 "RST")
(net 34 "VCC")
(net 35 "P16")
(net 36 "P10")
(net 37 "P1")
(net 38 "data")
(net 39 "SDA")
(net 40 "SCL")
(net 41 "P8")
(net 42 "P9")
(net 43 "J1-PadA")
            
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "")
(add_net "C0")
(add_net "outer_bottom")
(add_net "outer_home")
(add_net "outer_top")
(add_net "C1")
(add_net "pinky_bottom")
(add_net "pinky_home")
(add_net "pinky_top")
(add_net "C2")
(add_net "ring_bottom")
(add_net "ring_home")
(add_net "ring_top")
(add_net "C3")
(add_net "middle_bottom")
(add_net "middle_home")
(add_net "middle_top")
(add_net "C4")
(add_net "index_bottom")
(add_net "index_home")
(add_net "index_top")
(add_net "C5")
(add_net "inner_bottom")
(add_net "inner_home")
(add_net "inner_top")
(add_net "near_home")
(add_net "far_home")
(add_net "R0")
(add_net "R1")
(add_net "R2")
(add_net "R3")
(add_net "RAW")
(add_net "GND")
(add_net "RST")
(add_net "VCC")
(add_net "P16")
(add_net "P10")
(add_net "P1")
(add_net "data")
(add_net "SDA")
(add_net "SCL")
(add_net "P8")
(add_net "P9")
(add_net "J1-PadA")
  )

            
        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 100 100 0)

      
      (fp_text reference "S1" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 1 "C0"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 2 "outer_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 1 "C0"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 2 "outer_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 100 81 0)

      
      (fp_text reference "S2" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 1 "C0"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 3 "outer_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 1 "C0"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 3 "outer_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 100 62 0)

      
      (fp_text reference "S3" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 1 "C0"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 4 "outer_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 1 "C0"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 4 "outer_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 119 100 0)

      
      (fp_text reference "S4" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 5 "C1"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 6 "pinky_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 5 "C1"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 6 "pinky_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 119 81 0)

      
      (fp_text reference "S5" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 5 "C1"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 7 "pinky_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 5 "C1"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 7 "pinky_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 119 62 0)

      
      (fp_text reference "S6" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 5 "C1"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 8 "pinky_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 5 "C1"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 8 "pinky_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 138 95.25 0)

      
      (fp_text reference "S7" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 9 "C2"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 10 "ring_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 9 "C2"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 10 "ring_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 138 76.25 0)

      
      (fp_text reference "S8" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 9 "C2"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 11 "ring_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 9 "C2"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 11 "ring_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 138 57.25 0)

      
      (fp_text reference "S9" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 9 "C2"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 12 "ring_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 9 "C2"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 12 "ring_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 157 92.875 0)

      
      (fp_text reference "S10" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 13 "C3"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 14 "middle_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 13 "C3"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 14 "middle_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 157 73.875 0)

      
      (fp_text reference "S11" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 13 "C3"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 15 "middle_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 13 "C3"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 15 "middle_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 157 54.875 0)

      
      (fp_text reference "S12" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 13 "C3"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 16 "middle_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 13 "C3"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 16 "middle_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 176 95.25 0)

      
      (fp_text reference "S13" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 17 "C4"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 18 "index_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 17 "C4"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 18 "index_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 176 76.25 0)

      
      (fp_text reference "S14" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 17 "C4"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 19 "index_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 17 "C4"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 19 "index_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 176 57.25 0)

      
      (fp_text reference "S15" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 17 "C4"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 20 "index_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 17 "C4"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 20 "index_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 195 97.625 0)

      
      (fp_text reference "S16" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 21 "C5"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 22 "inner_bottom"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 21 "C5"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 22 "inner_bottom"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 195 78.625 0)

      
      (fp_text reference "S17" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 21 "C5"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 23 "inner_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 21 "C5"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 23 "inner_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 195 59.625 0)

      
      (fp_text reference "S18" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 21 "C5"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 24 "inner_top"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 21 "C5"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 24 "inner_top"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 166.5 114.75 0)

      
      (fp_text reference "S19" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 13 "C3"))
        (pad 2 smd rect (at 5.842 -5.08 0) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 25 "near_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 13 "C3"))
        (pad 2 smd rect (at -5.842 -5.08 0) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 25 "near_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 187.6350763 117.5324856 -15)

      
      (fp_text reference "S20" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 -15) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 17 "C4"))
        (pad 2 smd rect (at 5.842 -5.08 -15) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 15 "middle_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 -15) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 17 "C4"))
        (pad 2 smd rect (at -5.842 -5.08 -15) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 15 "middle_home"))
        )
        

        
      (module MX (layer F.Cu) (tedit 5DD4F656)
      (at 209.45706199999998 121.2027878 60)

      
      (fp_text reference "S21" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
      (fp_text value "" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))

      
      (fp_line (start -7 -6) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -6 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -6 -7) (end -7 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start -7 7) (end -7 6) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 6) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 6 -7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 6 7) (end 7 7) (layer Dwgs.User) (width 0.15))
      (fp_line (start 7 -7) (end 7 -6) (layer Dwgs.User) (width 0.15))
    
      
      (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))

      
      (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
      
        
        
        
        (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at -7.085 -2.54 60) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 21 "C5"))
        (pad 2 smd rect (at 5.842 -5.08 60) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask) (net 26 "far_home"))
        
        
        
        (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
        
        
        (pad 1 smd rect (at 7.085 -2.54 60) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 21 "C5"))
        (pad 2 smd rect (at -5.842 -5.08 60) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask) (net 26 "far_home"))
        )
        

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 107.5 103.5 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D1" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 27 "R0"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 2 "outer_bottom"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 107.5 84.5 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D2" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 28 "R1"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 3 "outer_home"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 107.5 65.5 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D3" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 29 "R2"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 4 "outer_top"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 126.5 103.5 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D4" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 27 "R0"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 6 "pinky_bottom"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 126.5 84.5 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D5" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 28 "R1"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 7 "pinky_home"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 126.5 65.5 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D6" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 29 "R2"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 8 "pinky_top"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 145.5 98.75 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D7" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 27 "R0"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 10 "ring_bottom"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 145.5 79.75 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D8" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 28 "R1"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 11 "ring_home"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 145.5 60.75 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D9" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 29 "R2"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 12 "ring_top"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 164.5 96.375 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D10" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 27 "R0"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 14 "middle_bottom"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 164.5 77.375 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D11" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 28 "R1"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 15 "middle_home"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 164.5 58.375 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D12" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 29 "R2"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 16 "middle_top"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 183.5 98.75 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D13" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 27 "R0"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 18 "index_bottom"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 183.5 79.75 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D14" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 28 "R1"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 19 "index_home"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 183.5 60.75 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D15" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 29 "R2"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 20 "index_top"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 202.5 101.125 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D16" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 27 "R0"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 22 "inner_bottom"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 202.5 82.125 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D17" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 28 "R1"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 23 "inner_home"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 202.5 63.125 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D18" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 29 "R2"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 24 "inner_top"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 174 118.25 90)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D19" (at 0 -2 90) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 90) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 30 "R3"))
            (pad "2" thru_hole rect (at 1.4 0 90) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 25 "near_home"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 193.9736533 122.8543688 75)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D20" (at 0 -2 75) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 75) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 75) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 30 "R3"))
            (pad "2" thru_hole rect (at 1.4 0 75) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 15 "middle_home"))
        )
    

        (footprint "Diode_SMD:Nexperia_CFP3_SOD-123W"
            (at 216.2381509 116.4575973 150)
            (descr "Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf")
            (tags "CFP3 SOD-123W")
            (attr smd)
            (fp_text reference "D21" (at 0 -2 150) (layer "F.SilkS") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_text value "Nexperia_CFP3_SOD-123W" (at 0 2 150) (layer "F.Fab") hide
                (effects (font (size 1 1) (thickness 0.15)))
            )
            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "F.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "F.Fab"))

            (fp_line (start -2.26 -0.95) (end -2.26 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 -0.95) (end 1.4 -0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.26 0.95) (end 1.4 0.95) (stroke (width 0.12) (type solid)) (layer "B.SilkS"))
            (fp_line (start -2.25 -1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -2.25 -1.1) (end 2.25 -1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 -1.1) (end 2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start 2.25 1.1) (end -2.25 1.1) (stroke (width 0.05) (type solid)) (layer "B.CrtYd"))
            (fp_line (start -1.3 -0.85) (end 1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -1.3 0.85) (end -1.3 -0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.75 0) (end -0.35 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 -0.55) (end -0.35 0.55) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 -0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start -0.35 0) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.25 -0.4) (end 0.25 0.4) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 0.75 0) (end 0.25 0) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 -0.85) (end 1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (fp_line (start 1.3 0.85) (end -1.3 0.85) (stroke (width 0.1) (type solid)) (layer "B.Fab"))
            (pad "1" thru_hole rect (at -1.4 0 150) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 30 "R3"))
            (pad "2" thru_hole rect (at 1.4 0 150) (size 1.2 1.2) (drill 0.3) (layers *.Cu *.Mask) (zone_connect 2) (net 26 "far_home"))
        )
    

            (module ProMicro (layer F.Cu) (tedit 6135B927)
            (at 214.7 71.8 -90)

            
            (descr "Solder-jumper reversible Pro Micro footprint")
            (tags "promicro ProMicro reversible solder jumper")
            (fp_text reference "MCU1" (at -16.256 -0.254 0) (layer F.SilkS) hide
            (effects (font (size 1 1) (thickness 0.15)))
            )

            
            (fp_line (start -15.24 6.35) (end -12.7 6.35) (layer F.SilkS) (width 0.15))
            (fp_line (start -15.24 6.35) (end -15.24 8.89) (layer F.SilkS) (width 0.15))
            (fp_line (start -12.7 6.35) (end -12.7 8.89) (layer F.SilkS) (width 0.15))
            (fp_line (start -12.7 8.89) (end -15.24 8.89) (layer F.SilkS) (width 0.15))
            (fp_line (start -15.24 -6.35) (end -12.7 -6.35) (layer B.SilkS) (width 0.15))
            (fp_line (start -15.24 -6.35) (end -15.24 -8.89) (layer B.SilkS) (width 0.15))
            (fp_line (start -12.7 -6.35) (end -12.7 -8.89) (layer B.SilkS) (width 0.15))
            (fp_line (start -12.7 -8.89) (end -15.24 -8.89) (layer B.SilkS) (width 0.15))

            
            (fp_line (start -19.304 -3.81) (end -14.224 -3.81) (layer Dwgs.User) (width 0.15))
            (fp_line (start -19.304 3.81) (end -19.304 -3.81) (layer Dwgs.User) (width 0.15))
            (fp_line (start -14.224 3.81) (end -19.304 3.81) (layer Dwgs.User) (width 0.15))
            (fp_line (start -14.224 -3.81) (end -14.224 3.81) (layer Dwgs.User) (width 0.15))

            (fp_circle (center 13.97 0.762) (end 14.095 0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center 13.97 0.762) (end 14.095 0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center 13.97 -0.762) (end 14.095 -0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center 13.97 -0.762) (end 14.095 -0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center 11.43 0.762) (end 11.555 0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center 11.43 0.762) (end 11.555 0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center 11.43 -0.762) (end 11.555 -0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center 11.43 -0.762) (end 11.555 -0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center 8.89 0.762) (end 9.015 0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center 8.89 0.762) (end 9.015 0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center 8.89 -0.762) (end 9.015 -0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center 8.89 -0.762) (end 9.015 -0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center 6.35 0.762) (end 6.475 0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center 6.35 0.762) (end 6.475 0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center 6.35 -0.762) (end 6.475 -0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center 6.35 -0.762) (end 6.475 -0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center 3.81 0.762) (end 3.935 0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center 3.81 0.762) (end 3.935 0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center 3.81 -0.762) (end 3.935 -0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center 3.81 -0.762) (end 3.935 -0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center 1.27 0.762) (end 1.395 0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center 1.27 0.762) (end 1.395 0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center 1.27 -0.762) (end 1.395 -0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center 1.27 -0.762) (end 1.395 -0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center -1.27 0.762) (end -1.145 0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center -1.27 0.762) (end -1.145 0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center -1.27 -0.762) (end -1.145 -0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center -1.27 -0.762) (end -1.145 -0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center -3.81 0.762) (end -3.685 0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center -3.81 0.762) (end -3.685 0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center -3.81 -0.762) (end -3.685 -0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center -3.81 -0.762) (end -3.685 -0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center -6.35 0.762) (end -6.225 0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center -6.35 0.762) (end -6.225 0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center -6.35 -0.762) (end -6.225 -0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center -6.35 -0.762) (end -6.225 -0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center -8.89 0.762) (end -8.765 0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center -8.89 0.762) (end -8.765 0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center -8.89 -0.762) (end -8.765 -0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center -8.89 -0.762) (end -8.765 -0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center -11.43 -0.762) (end -11.305 -0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center -11.43 -0.762) (end -11.305 -0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center -11.43 0.762) (end -11.305 0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center -11.43 0.762) (end -11.305 0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center -13.97 0.762) (end -13.845 0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center -13.97 0.762) (end -13.845 0.762) (layer F.Mask) (width 0.25))
            (fp_circle (center -13.97 -0.762) (end -13.845 -0.762) (layer B.Mask) (width 0.25))
            (fp_circle (center -13.97 -0.762) (end -13.845 -0.762) (layer F.Mask) (width 0.25))
            (fp_poly (pts (xy 14.478 -5.08) (xy 13.462 -5.08) (xy 13.462 -6.096) (xy 14.478 -6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy 11.938 -5.08) (xy 10.922 -5.08) (xy 10.922 -6.096) (xy 11.938 -6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy 9.398 -5.08) (xy 8.382 -5.08) (xy 8.382 -6.096) (xy 9.398 -6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy 6.858 -5.08) (xy 5.842 -5.08) (xy 5.842 -6.096) (xy 6.858 -6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy 4.318 -5.08) (xy 3.302 -5.08) (xy 3.302 -6.096) (xy 4.318 -6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy 1.778 -5.08) (xy 0.762 -5.08) (xy 0.762 -6.096) (xy 1.778 -6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -0.762 -5.08) (xy -1.778 -5.08) (xy -1.778 -6.096) (xy -0.762 -6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -3.302 -5.08) (xy -4.318 -5.08) (xy -4.318 -6.096) (xy -3.302 -6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -5.842 -5.08) (xy -6.858 -5.08) (xy -6.858 -6.096) (xy -5.842 -6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -8.382 -5.08) (xy -9.398 -5.08) (xy -9.398 -6.096) (xy -8.382 -6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -10.922 -5.08) (xy -11.938 -5.08) (xy -11.938 -6.096) (xy -10.922 -6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -13.462 -5.08) (xy -14.478 -5.08) (xy -14.478 -6.096) (xy -13.462 -6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy 13.462 5.08) (xy 14.478 5.08) (xy 14.478 6.096) (xy 13.462 6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy 10.922 5.08) (xy 11.938 5.08) (xy 11.938 6.096) (xy 10.922 6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy 8.382 5.08) (xy 9.398 5.08) (xy 9.398 6.096) (xy 8.382 6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy 5.842 5.08) (xy 6.858 5.08) (xy 6.858 6.096) (xy 5.842 6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy 3.302 5.08) (xy 4.318 5.08) (xy 4.318 6.096) (xy 3.302 6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy 0.762 5.08) (xy 1.778 5.08) (xy 1.778 6.096) (xy 0.762 6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -1.778 5.08) (xy -0.762 5.08) (xy -0.762 6.096) (xy -1.778 6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -4.318 5.08) (xy -3.302 5.08) (xy -3.302 6.096) (xy -4.318 6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -6.858 5.08) (xy -5.842 5.08) (xy -5.842 6.096) (xy -6.858 6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -9.398 5.08) (xy -8.382 5.08) (xy -8.382 6.096) (xy -9.398 6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -11.938 5.08) (xy -10.922 5.08) (xy -10.922 6.096) (xy -11.938 6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -14.478 5.08) (xy -13.462 5.08) (xy -13.462 6.096) (xy -14.478 6.096)) (layer B.Mask) (width 0.1))
            (fp_poly (pts (xy -13.462 -5.08) (xy -14.478 -5.08) (xy -14.478 -6.096) (xy -13.462 -6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy 1.778 -5.08) (xy 0.762 -5.08) (xy 0.762 -6.096) (xy 1.778 -6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy -10.922 -5.08) (xy -11.938 -5.08) (xy -11.938 -6.096) (xy -10.922 -6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy -8.382 -5.08) (xy -9.398 -5.08) (xy -9.398 -6.096) (xy -8.382 -6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy -3.302 -5.08) (xy -4.318 -5.08) (xy -4.318 -6.096) (xy -3.302 -6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy -0.762 -5.08) (xy -1.778 -5.08) (xy -1.778 -6.096) (xy -0.762 -6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy 6.858 -5.08) (xy 5.842 -5.08) (xy 5.842 -6.096) (xy 6.858 -6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy 11.938 -5.08) (xy 10.922 -5.08) (xy 10.922 -6.096) (xy 11.938 -6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy -5.842 -5.08) (xy -6.858 -5.08) (xy -6.858 -6.096) (xy -5.842 -6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy 4.318 -5.08) (xy 3.302 -5.08) (xy 3.302 -6.096) (xy 4.318 -6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy 9.398 -5.08) (xy 8.382 -5.08) (xy 8.382 -6.096) (xy 9.398 -6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy 14.478 -5.08) (xy 13.462 -5.08) (xy 13.462 -6.096) (xy 14.478 -6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy 13.462 5.08) (xy 14.478 5.08) (xy 14.478 6.096) (xy 13.462 6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy 10.922 5.08) (xy 11.938 5.08) (xy 11.938 6.096) (xy 10.922 6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy 8.382 5.08) (xy 9.398 5.08) (xy 9.398 6.096) (xy 8.382 6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy 5.842 5.08) (xy 6.858 5.08) (xy 6.858 6.096) (xy 5.842 6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy 3.302 5.08) (xy 4.318 5.08) (xy 4.318 6.096) (xy 3.302 6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy 0.762 5.08) (xy 1.778 5.08) (xy 1.778 6.096) (xy 0.762 6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy -1.778 5.08) (xy -0.762 5.08) (xy -0.762 6.096) (xy -1.778 6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy -4.318 5.08) (xy -3.302 5.08) (xy -3.302 6.096) (xy -4.318 6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy -6.858 5.08) (xy -5.842 5.08) (xy -5.842 6.096) (xy -6.858 6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy -9.398 5.08) (xy -8.382 5.08) (xy -8.382 6.096) (xy -9.398 6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy -11.938 5.08) (xy -10.922 5.08) (xy -10.922 6.096) (xy -11.938 6.096)) (layer F.Mask) (width 0.1))
            (fp_poly (pts (xy -14.478 5.08) (xy -13.462 5.08) (xy -13.462 6.096) (xy -14.478 6.096)) (layer F.Mask) (width 0.1))
            (pad "" thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
            (zone_connect 0))
            (pad "" thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
            (pad "" smd custom (at -13.97 5.842 90) (size 0.1 0.1) (layers F.Cu F.Mask)
            (clearance 0.1) (zone_connect 0)
            (options (clearance outline) (anchor rect))
            (primitives
                (gr_poly (pts
                (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 24 smd custom (at -13.97 4.826 90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 37 "P1")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -13.97 6.35 90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" thru_hole rect (at -13.97 7.62 -90) (size 1.6 1.6) (drill 1.1) (layers F.Cu F.Mask)
                (zone_connect 0))
                (pad "" thru_hole rect (at -13.97 -7.62 -90) (size 1.6 1.6) (drill 1.1) (layers B.Cu B.Mask)
                (zone_connect 0))
                (pad "" smd custom (at -11.43 6.35 90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -11.43 5.842 90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 23 smd custom (at -11.43 4.826 90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 38 "data")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -8.89 6.35 90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -8.89 5.842 90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 22 smd custom (at -8.89 4.826 90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 32 "GND")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -6.35 6.35 90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -6.35 5.842 90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 21 smd custom (at -6.35 4.826 90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 32 "GND")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -3.81 6.35 90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -3.81 5.842 90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 20 smd custom (at -3.81 4.826 90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 39 "SDA")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -1.27 6.35 90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -1.27 5.842 90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 19 smd custom (at -1.27 4.826 90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 40 "SCL")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 1.27 6.35 90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 1.27 5.842 90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 18 smd custom (at 1.27 4.826 90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 27 "R0")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 3.81 6.35 90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 3.81 5.842 90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 17 smd custom (at 3.81 4.826 90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 28 "R1")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 6.35 6.35 90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 6.35 5.842 90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 16 smd custom (at 6.35 4.826 90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 29 "R2")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 8.89 6.35 90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 8.89 5.842 90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 15 smd custom (at 8.89 4.826 90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 30 "R3")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 11.43 6.35 90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 11.43 5.842 90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 14 smd custom (at 11.43 4.826 90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 41 "P8")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 13.97 6.35 90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 13.97 5.842 90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 13 smd custom (at 13.97 4.826 90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 42 "P9")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad 1 smd custom (at -13.97 -4.826 -90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 31 "RAW")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad 3 smd custom (at -8.89 -4.826 -90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 33 "RST")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -8.89 -6.35 -90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -8.89 -5.842 -90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad "" smd custom (at -13.97 -5.842 -90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad "" smd custom (at -11.43 -6.35 -90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad 2 smd custom (at -11.43 -4.826 -90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 32 "GND")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -13.97 -6.35 -90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad 4 smd custom (at -6.35 -4.826 -90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 34 "VCC")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -11.43 -5.842 -90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad "" smd custom (at -6.35 -5.842 -90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 6 smd custom (at -1.27 -4.826 -90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 5 "C1")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad 7 smd custom (at 1.27 -4.826 -90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 9 "C2")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 13.97 -6.35 -90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 1.27 -5.842 -90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad "" smd custom (at 8.89 -6.35 -90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad 8 smd custom (at 3.81 -4.826 -90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 13 "C3")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 1.27 -6.35 -90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad 12 smd custom (at 13.97 -4.826 -90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 36 "P10")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 3.81 -5.842 -90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad "" smd custom (at 6.35 -6.35 -90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 13.97 -5.842 -90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad "" smd custom (at -3.81 -6.35 -90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 3.81 -6.35 -90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -1.27 -6.35 -90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad 9 smd custom (at 6.35 -4.826 -90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 17 "C4")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -6.35 -6.35 -90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -3.81 -5.842 -90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad "" smd custom (at -1.27 -5.842 -90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad "" smd custom (at 6.35 -5.842 -90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 10 smd custom (at 8.89 -4.826 -90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 21 "C5")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 8.89 -5.842 -90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad "" smd custom (at 11.43 -5.842 -90) (size 0.1 0.1) (layers F.Cu F.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 11 smd custom (at 11.43 -4.826 -90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 35 "P16")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 11.43 -6.35 -90) (size 0.25 1) (layers F.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad 5 smd custom (at -3.81 -4.826 -90) (size 1.2 0.5) (layers F.Cu F.Mask) (net 1 "C0")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -13.97 6.35 90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad 1 smd custom (at -13.97 4.826 90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 31 "RAW")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -13.97 5.842 90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad "" smd custom (at -11.43 6.35 90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -11.43 5.842 90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 2 smd custom (at -11.43 4.826 90) (size 1.2 0.5) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -8.89 6.35 90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -8.89 5.842 90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 3 smd custom (at -8.89 4.826 90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 33 "RST")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -6.35 6.35 90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -6.35 5.842 90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 4 smd custom (at -6.35 4.826 90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 34 "VCC")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -3.81 6.35 90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -3.81 5.842 90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 5 smd custom (at -3.81 4.826 90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 1 "C0")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -1.27 6.35 90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -1.27 5.842 90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 6 smd custom (at -1.27 4.826 90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 5 "C1")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 1.27 6.35 90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 1.27 5.842 90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 7 smd custom (at 1.27 4.826 90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 9 "C2")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 3.81 6.35 90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 3.81 5.842 90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 8 smd custom (at 3.81 4.826 90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 13 "C3")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 6.35 6.35 90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 6.35 5.842 90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 9 smd custom (at 6.35 4.826 90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 17 "C4")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 8.89 6.35 90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 8.89 5.842 90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 10 smd custom (at 8.89 4.826 90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 21 "C5")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 11.43 6.35 90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 11.43 5.842 90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 11 smd custom (at 11.43 4.826 90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 35 "P16")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 13.97 6.35 90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 13.97 5.842 90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 12 smd custom (at 13.97 4.826 90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 36 "P10")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -13.97 -6.35 -90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -13.97 -5.842 -90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 24 smd custom (at -13.97 -4.826 -90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 37 "P1")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad 23 smd custom (at -11.43 -4.826 -90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 38 "data")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -11.43 -6.35 -90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -11.43 -5.842 -90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 22 smd custom (at -8.89 -4.826 -90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 32 "GND")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -8.89 -6.35 -90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -8.89 -5.842 -90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 21 smd custom (at -6.35 -4.826 -90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 32 "GND")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -6.35 -6.35 -90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -6.35 -5.842 -90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 20 smd custom (at -3.81 -4.826 -90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 39 "SDA")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -3.81 -6.35 -90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -3.81 -5.842 -90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 19 smd custom (at -1.27 -4.826 -90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 40 "SCL")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at -1.27 -6.35 -90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at -1.27 -5.842 -90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 18 smd custom (at 1.27 -4.826 -90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 27 "R0")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 1.27 -6.35 -90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 1.27 -5.842 -90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 17 smd custom (at 3.81 -4.826 -90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 28 "R1")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 3.81 -6.35 -90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 3.81 -5.842 -90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 16 smd custom (at 6.35 -4.826 -90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 29 "R2")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 6.35 -6.35 -90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 6.35 -5.842 -90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 15 smd custom (at 8.89 -4.826 -90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 30 "R3")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 8.89 -6.35 -90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 8.89 -5.842 -90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 14 smd custom (at 11.43 -4.826 -90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 41 "P8")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 11.43 -6.35 -90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 11.43 -5.842 -90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
                (pad 13 smd custom (at 13.97 -4.826 -90) (size 1.2 0.5) (layers B.Cu B.Mask) (net 42 "P9")
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 0) (xy -0.6 0) (xy -0.6 -1) (xy 0 -0.4) (xy 0.6 -1)
            ) (width 0))
                ))
                (pad "" smd custom (at 13.97 -6.35 -90) (size 0.25 1) (layers B.Cu)
                (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                ))
                (pad "" smd custom (at 13.97 -5.842 -90) (size 0.1 0.1) (layers B.Cu B.Mask)
                (clearance 0.1) (zone_connect 0)
                (options (clearance outline) (anchor rect))
                (primitives
                    (gr_poly (pts
                    (xy 0.6 -0.4) (xy -0.6 -0.4) (xy -0.6 -0.2) (xy 0 0.4) (xy 0.6 -0.2)
            ) (width 0))
                ))
            )
            (segment (start 216.22799999999998 66.216) (end 218.76 66.216) (width 0.25) (layer "F.Cu"))
            (segment (start 218.76 66.216) (end 219.52599999999998 65.45) (width 0.25) (layer "F.Cu"))
            (segment (start 215.462 65.45) (end 216.22799999999998 66.216) (width 0.25) (layer "F.Cu"))
            (segment (start 215.462 65.45) (end 214.696 64.684) (width 0.25) (layer "B.Cu"))
            (segment (start 214.696 64.684) (end 210.64 64.684) (width 0.25) (layer "B.Cu"))
            (segment (start 210.64 64.684) (end 209.874 65.45) (width 0.25) (layer "B.Cu"))
            (segment (start 215.462 60.37) (end 216.22799999999998 61.135999999999996) (width 0.25) (layer "F.Cu"))
            (segment (start 210.634099 62.156220999999995) (end 209.868099 62.92222099999999) (width 0.25) (layer "F.Cu"))
            (segment (start 216.22799999999998 61.135999999999996) (end 218.76 61.135999999999996) (width 0.25) (layer "F.Cu"))
            (segment (start 213.166099 62.156220999999995) (end 210.634099 62.156220999999995) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 65.462221) (end 213.166099 64.696221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 62.92222099999999) (end 213.166099 62.156220999999995) (width 0.25) (layer "F.Cu"))
            (segment (start 210.634099 64.696221) (end 209.868099 65.462221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.166099 64.696221) (end 210.634099 64.696221) (width 0.25) (layer "F.Cu"))
            (segment (start 218.76 61.135999999999996) (end 219.52599999999998 60.37) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 65.462221) (end 214.69809899999998 66.22822099999999) (width 0.25) (layer "B.Cu"))
            (segment (start 218.754099 63.688221) (end 219.520099 62.92222099999999) (width 0.25) (layer "B.Cu"))
            (segment (start 214.69809899999998 63.688221) (end 218.754099 63.688221) (width 0.25) (layer "B.Cu"))
            (segment (start 213.932099 62.92222099999999) (end 214.69809899999998 63.688221) (width 0.25) (layer "B.Cu"))
            (segment (start 214.69809899999998 66.22822099999999) (end 218.754099 66.22822099999999) (width 0.25) (layer "B.Cu"))
            (segment (start 215.462 60.37) (end 214.696 59.604) (width 0.25) (layer "B.Cu"))
            (segment (start 210.64 59.604) (end 209.874 60.37) (width 0.25) (layer "B.Cu"))
            (segment (start 214.696 59.604) (end 210.64 59.604) (width 0.25) (layer "B.Cu"))
            (segment (start 218.754099 66.22822099999999) (end 219.520099 65.462221) (width 0.25) (layer "B.Cu"))
            (segment (start 213.932099 85.78222099999999) (end 213.166099 85.016221) (width 0.25) (layer "F.Cu"))
            (segment (start 210.634099 85.016221) (end 209.868099 85.78222099999999) (width 0.25) (layer "F.Cu"))
            (segment (start 213.166099 85.016221) (end 210.634099 85.016221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 85.78222099999999) (end 214.69809899999998 86.548221) (width 0.25) (layer "B.Cu"))
            (segment (start 214.69809899999998 86.548221) (end 218.754099 86.548221) (width 0.25) (layer "B.Cu"))
            (segment (start 218.754099 86.548221) (end 219.520099 85.78222099999999) (width 0.25) (layer "B.Cu"))
            (segment (start 210.634099 67.236221) (end 209.868099 68.00222099999999) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 68.00222099999999) (end 213.166099 67.236221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.166099 67.236221) (end 210.634099 67.236221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 68.00222099999999) (end 214.69809899999998 68.768221) (width 0.25) (layer "B.Cu"))
            (segment (start 214.69809899999998 68.768221) (end 218.754099 68.768221) (width 0.25) (layer "B.Cu"))
            (segment (start 218.754099 68.768221) (end 219.520099 68.00222099999999) (width 0.25) (layer "B.Cu"))
            (segment (start 210.634099 59.616220999999996) (end 209.868099 60.382221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.166099 59.616220999999996) (end 210.634099 59.616220999999996) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 60.382221) (end 213.166099 59.616220999999996) (width 0.25) (layer "F.Cu"))
            (segment (start 214.69809899999998 61.148221) (end 218.754099 61.148221) (width 0.25) (layer "B.Cu"))
            (segment (start 213.932099 60.382221) (end 214.69809899999998 61.148221) (width 0.25) (layer "B.Cu"))
            (segment (start 218.754099 61.148221) (end 219.520099 60.382221) (width 0.25) (layer "B.Cu"))
            (segment (start 213.166099 57.076221) (end 210.634099 57.076221) (width 0.25) (layer "F.Cu"))
            (segment (start 210.634099 57.076221) (end 209.868099 57.842220999999995) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 57.842220999999995) (end 213.166099 57.076221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 57.842220999999995) (end 214.69809899999998 58.608221) (width 0.25) (layer "B.Cu"))
            (segment (start 214.69809899999998 58.608221) (end 218.754099 58.608221) (width 0.25) (layer "B.Cu"))
            (segment (start 218.754099 58.608221) (end 219.520099 57.842220999999995) (width 0.25) (layer "B.Cu"))
            (segment (start 213.166099 82.476221) (end 210.634099 82.476221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 83.242221) (end 213.166099 82.476221) (width 0.25) (layer "F.Cu"))
            (segment (start 210.634099 82.476221) (end 209.868099 83.242221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 83.242221) (end 214.69809899999998 84.00822099999999) (width 0.25) (layer "B.Cu"))
            (segment (start 218.754099 84.00822099999999) (end 219.520099 83.242221) (width 0.25) (layer "B.Cu"))
            (segment (start 214.69809899999998 84.00822099999999) (end 218.754099 84.00822099999999) (width 0.25) (layer "B.Cu"))
            (segment (start 210.634099 79.936221) (end 209.868099 80.702221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 80.702221) (end 213.166099 79.936221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.166099 79.936221) (end 210.634099 79.936221) (width 0.25) (layer "F.Cu"))
            (segment (start 218.754099 81.468221) (end 219.520099 80.702221) (width 0.25) (layer "B.Cu"))
            (segment (start 213.932099 80.702221) (end 214.69809899999998 81.468221) (width 0.25) (layer "B.Cu"))
            (segment (start 214.69809899999998 81.468221) (end 218.754099 81.468221) (width 0.25) (layer "B.Cu"))
            (segment (start 213.166099 77.396221) (end 210.634099 77.396221) (width 0.25) (layer "F.Cu"))
            (segment (start 210.634099 77.396221) (end 209.868099 78.162221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 78.162221) (end 213.166099 77.396221) (width 0.25) (layer "F.Cu"))
            (segment (start 218.754099 78.928221) (end 219.520099 78.162221) (width 0.25) (layer "B.Cu"))
            (segment (start 214.69809899999998 78.928221) (end 218.754099 78.928221) (width 0.25) (layer "B.Cu"))
            (segment (start 213.932099 78.162221) (end 214.69809899999998 78.928221) (width 0.25) (layer "B.Cu"))
            (segment (start 210.634099 74.85622099999999) (end 209.868099 75.622221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 75.622221) (end 213.166099 74.85622099999999) (width 0.25) (layer "F.Cu"))
            (segment (start 213.166099 74.85622099999999) (end 210.634099 74.85622099999999) (width 0.25) (layer "F.Cu"))
            (segment (start 218.754099 76.388221) (end 219.520099 75.622221) (width 0.25) (layer "B.Cu"))
            (segment (start 214.69809899999998 76.388221) (end 218.754099 76.388221) (width 0.25) (layer "B.Cu"))
            (segment (start 213.932099 75.622221) (end 214.69809899999998 76.388221) (width 0.25) (layer "B.Cu"))
            (segment (start 210.634099 72.316221) (end 209.868099 73.082221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.166099 72.316221) (end 210.634099 72.316221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 73.082221) (end 213.166099 72.316221) (width 0.25) (layer "F.Cu"))
            (segment (start 218.754099 73.848221) (end 219.520099 73.082221) (width 0.25) (layer "B.Cu"))
            (segment (start 214.69809899999998 73.848221) (end 218.754099 73.848221) (width 0.25) (layer "B.Cu"))
            (segment (start 213.932099 73.082221) (end 214.69809899999998 73.848221) (width 0.25) (layer "B.Cu"))
            (segment (start 210.634099 69.77622099999999) (end 209.868099 70.542221) (width 0.25) (layer "F.Cu"))
            (segment (start 213.932099 70.542221) (end 213.166099 69.77622099999999) (width 0.25) (layer "F.Cu"))
            (segment (start 213.166099 69.77622099999999) (end 210.634099 69.77622099999999) (width 0.25) (layer "F.Cu"))
            (segment (start 214.69809899999998 71.308221) (end 218.754099 71.308221) (width 0.25) (layer "B.Cu"))
            (segment (start 218.754099 71.308221) (end 219.520099 70.542221) (width 0.25) (layer "B.Cu"))
            (segment (start 213.932099 70.542221) (end 214.69809899999998 71.308221) (width 0.25) (layer "B.Cu"))
            (segment (start 218.76 58.596) (end 219.52599999999998 57.83) (width 0.25) (layer "F.Cu"))
            (segment (start 216.22799999999998 58.596) (end 218.76 58.596) (width 0.25) (layer "F.Cu"))
            (segment (start 215.462 57.83) (end 216.22799999999998 58.596) (width 0.25) (layer "F.Cu"))
            (segment (start 214.696 57.06399999999999) (end 210.64 57.06399999999999) (width 0.25) (layer "B.Cu"))
            (segment (start 210.64 57.06399999999999) (end 209.874 57.83) (width 0.25) (layer "B.Cu"))
            (segment (start 215.462 57.83) (end 214.696 57.06399999999999) (width 0.25) (layer "B.Cu"))
            (segment (start 215.462 62.91) (end 216.22799999999998 63.675999999999995) (width 0.25) (layer "F.Cu"))
            (segment (start 218.76 63.675999999999995) (end 219.52599999999998 62.91) (width 0.25) (layer "F.Cu"))
            (segment (start 216.22799999999998 63.675999999999995) (end 218.76 63.675999999999995) (width 0.25) (layer "F.Cu"))
            (segment (start 214.696 62.144) (end 210.64 62.144) (width 0.25) (layer "B.Cu"))
            (segment (start 215.462 62.91) (end 214.696 62.144) (width 0.25) (layer "B.Cu"))
            (segment (start 210.64 62.144) (end 209.874 62.91) (width 0.25) (layer "B.Cu"))
            (segment (start 218.76 68.756) (end 219.52599999999998 67.99) (width 0.25) (layer "F.Cu"))
            (segment (start 215.462 67.99) (end 216.22799999999998 68.756) (width 0.25) (layer "F.Cu"))
            (segment (start 216.22799999999998 68.756) (end 218.76 68.756) (width 0.25) (layer "F.Cu"))
            (segment (start 214.696 67.224) (end 210.64 67.224) (width 0.25) (layer "B.Cu"))
            (segment (start 215.462 67.99) (end 214.696 67.224) (width 0.25) (layer "B.Cu"))
            (segment (start 210.64 67.224) (end 209.874 67.99) (width 0.25) (layer "B.Cu"))
            (segment (start 215.462 70.53) (end 216.22799999999998 71.29599999999999) (width 0.25) (layer "F.Cu"))
            (segment (start 218.76 71.29599999999999) (end 219.52599999999998 70.53) (width 0.25) (layer "F.Cu"))
            (segment (start 216.22799999999998 71.29599999999999) (end 218.76 71.29599999999999) (width 0.25) (layer "F.Cu"))
            (segment (start 210.64 69.764) (end 209.874 70.53) (width 0.25) (layer "B.Cu"))
            (segment (start 214.696 69.764) (end 210.64 69.764) (width 0.25) (layer "B.Cu"))
            (segment (start 215.462 70.53) (end 214.696 69.764) (width 0.25) (layer "B.Cu"))
            (segment (start 216.22799999999998 73.836) (end 218.76 73.836) (width 0.25) (layer "F.Cu"))
            (segment (start 215.462 73.07) (end 216.22799999999998 73.836) (width 0.25) (layer "F.Cu"))
            (segment (start 218.76 73.836) (end 219.52599999999998 73.07) (width 0.25) (layer "F.Cu"))
            (segment (start 214.696 72.304) (end 210.64 72.304) (width 0.25) (layer "B.Cu"))
            (segment (start 210.64 72.304) (end 209.874 73.07) (width 0.25) (layer "B.Cu"))
            (segment (start 215.462 73.07) (end 214.696 72.304) (width 0.25) (layer "B.Cu"))
            (segment (start 215.462 75.61) (end 216.22799999999998 76.37599999999999) (width 0.25) (layer "F.Cu"))
            (segment (start 216.22799999999998 76.37599999999999) (end 218.76 76.37599999999999) (width 0.25) (layer "F.Cu"))
            (segment (start 218.76 76.37599999999999) (end 219.52599999999998 75.61) (width 0.25) (layer "F.Cu"))
            (segment (start 210.64 74.844) (end 209.874 75.61) (width 0.25) (layer "B.Cu"))
            (segment (start 214.696 74.844) (end 210.64 74.844) (width 0.25) (layer "B.Cu"))
            (segment (start 215.462 75.61) (end 214.696 74.844) (width 0.25) (layer "B.Cu"))
            (segment (start 218.76 78.916) (end 219.52599999999998 78.14999999999999) (width 0.25) (layer "F.Cu"))
            (segment (start 215.462 78.14999999999999) (end 216.22799999999998 78.916) (width 0.25) (layer "F.Cu"))
            (segment (start 216.22799999999998 78.916) (end 218.76 78.916) (width 0.25) (layer "F.Cu"))
            (segment (start 215.462 78.14999999999999) (end 214.696 77.384) (width 0.25) (layer "B.Cu"))
            (segment (start 210.64 77.384) (end 209.874 78.14999999999999) (width 0.25) (layer "B.Cu"))
            (segment (start 214.696 77.384) (end 210.64 77.384) (width 0.25) (layer "B.Cu"))
            (segment (start 215.462 80.69) (end 216.22799999999998 81.456) (width 0.25) (layer "F.Cu"))
            (segment (start 216.22799999999998 81.456) (end 218.76 81.456) (width 0.25) (layer "F.Cu"))
            (segment (start 218.76 81.456) (end 219.52599999999998 80.69) (width 0.25) (layer "F.Cu"))
            (segment (start 215.462 80.69) (end 214.696 79.92399999999999) (width 0.25) (layer "B.Cu"))
            (segment (start 210.64 79.92399999999999) (end 209.874 80.69) (width 0.25) (layer "B.Cu"))
            (segment (start 214.696 79.92399999999999) (end 210.64 79.92399999999999) (width 0.25) (layer "B.Cu"))
            (segment (start 218.76 83.996) (end 219.52599999999998 83.22999999999999) (width 0.25) (layer "F.Cu"))
            (segment (start 216.22799999999998 83.996) (end 218.76 83.996) (width 0.25) (layer "F.Cu"))
            (segment (start 215.462 83.22999999999999) (end 216.22799999999998 83.996) (width 0.25) (layer "F.Cu"))
            (segment (start 215.462 83.22999999999999) (end 214.696 82.464) (width 0.25) (layer "B.Cu"))
            (segment (start 214.696 82.464) (end 210.64 82.464) (width 0.25) (layer "B.Cu"))
            (segment (start 210.64 82.464) (end 209.874 83.22999999999999) (width 0.25) (layer "B.Cu"))
            (segment (start 216.22799999999998 86.536) (end 218.76 86.536) (width 0.25) (layer "F.Cu"))
            (segment (start 215.462 85.77) (end 216.22799999999998 86.536) (width 0.25) (layer "F.Cu"))
            (segment (start 218.76 86.536) (end 219.52599999999998 85.77) (width 0.25) (layer "F.Cu"))
            (segment (start 215.462 85.77) (end 214.696 85.00399999999999) (width 0.25) (layer "B.Cu"))
            (segment (start 210.64 85.00399999999999) (end 209.874 85.77) (width 0.25) (layer "B.Cu"))
            (segment (start 214.696 85.00399999999999) (end 210.64 85.00399999999999) (width 0.25) (layer "B.Cu"))




            (via (at 215.462 60.37) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 32))
            (via (at 213.938 60.37) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 38))
            (via (at 213.938 57.83) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 37))
            (via (at 215.462 57.83) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 31))
            (via (at 213.938 62.91) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 32))
            (via (at 215.462 62.91) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 33))
            (via (at 213.938 65.45) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 32))
            (via (at 215.462 65.45) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 34))
            (via (at 213.938 67.99) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 39))
            (via (at 215.462 67.99) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 1))
            (via (at 213.938 70.53) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 40))
            (via (at 215.462 70.53) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 5))
            (via (at 213.938 73.07) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 27))
            (via (at 215.462 73.07) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 9))
            (via (at 213.938 75.61) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 28))
            (via (at 215.462 75.61) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 13))
            (via (at 213.938 78.14999999999999) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 29))
            (via (at 215.462 78.14999999999999) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 17))
            (via (at 213.938 80.69) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 30))
            (via (at 215.462 80.69) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 21))
            (via (at 213.938 83.22999999999999) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 41))
            (via (at 215.462 83.22999999999999) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 35))
            (via (at 213.938 85.77) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 42))
            (via (at 215.462 85.77) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 36))
        

        (module lib:OLED_headers (layer F.Cu) (tedit 5E1ADAC2)
        (at 208.66 94.45 90) 

                
        (fp_text reference "OLED1" (at 0 0) (layer F.SilkS) hide (effects (font (size 1.27 1.27) (thickness 0.15))))
        (fp_text value OLED (at 0 -7.3) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (pad 4 thru_hole oval (at 1.6 2.18 360) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
        (net 39 "SDA"))
        (pad 3 thru_hole oval (at 1.6 4.72 360) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
        (net 40 "SCL"))
        (pad 2 thru_hole oval (at 1.6 7.26 360) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
        (net 34 "VCC"))
        (pad 1 thru_hole rect (at 1.6 9.8 360) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
        (net 32 "GND"))
        )
        

    (module kbd:ResetSW (layer F.Cu) (tedit 5B9559E6) (tstamp 61905781)

        (descr "Two pin through hole Tactile Switch, the same as on the Corne")
        (tags "Tactile Switch")

        (at 222.5 92.45 -90)
        
        (fp_text reference "B1" (at 0 2.55) (layer F.SilkS) hide (effects (font (size 1 1) (thickness 0.15))))
        (fp_text value "" (at 0 -2.55) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

        
        (fp_text user RESET (at 0 0 -90) (layer F.SilkS) (effects (font (size 1 1) (thickness 0.15))))
        (fp_text user RESET (at 0.127 0 -90) (layer B.SilkS) (effects (font (size 1 1) (thickness 0.15)) (justify mirror)))

        (fp_line (start 3 1.5) (end 3 1.75) (layer B.SilkS) (width 0.15))
        (fp_line (start 3 1.75) (end -3 1.75) (layer B.SilkS) (width 0.15))
        (fp_line (start -3 1.75) (end -3 1.5) (layer B.SilkS) (width 0.15))
        (fp_line (start -3 -1.5) (end -3 -1.75) (layer B.SilkS) (width 0.15))
        (fp_line (start -3 -1.75) (end 3 -1.75) (layer B.SilkS) (width 0.15))
        (fp_line (start 3 -1.75) (end 3 -1.5) (layer B.SilkS) (width 0.15))
        (fp_line (start -3 1.75) (end 3 1.75) (layer F.SilkS) (width 0.15))
        (fp_line (start 3 1.75) (end 3 1.5) (layer F.SilkS) (width 0.15))
        (fp_line (start -3 1.75) (end -3 1.5) (layer F.SilkS) (width 0.15))
        (fp_line (start -3 -1.75) (end -3 -1.5) (layer F.SilkS) (width 0.15))
        (fp_line (start -3 -1.75) (end 3 -1.75) (layer F.SilkS) (width 0.15))
        (fp_line (start 3 -1.75) (end 3 -1.5) (layer F.SilkS) (width 0.15))

        
        (pad 2 thru_hole circle (at -3.25 0 -90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask F.SilkS) (net 33 "RST"))
        (pad 1 thru_hole circle (at 3.25 0 -90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask F.SilkS) (net 32 "GND"))
    )
    

        
      (module TRRS-PJ-320A-dual (layer F.Cu) (tedit 5970F8E5)

      (at 223.7 102.55 -90)   

      
      (fp_text reference "TRRS1" (at 0 14.2) (layer Dwgs.User) (effects (font (size 1 1) (thickness 0.15))))
      (fp_text value TRRS-PJ-320A-dual (at 0 -5.6) (layer F.Fab) (effects (font (size 1 1) (thickness 0.15))))

      
      (fp_line (start 0.5 -2) (end -5.1 -2) (layer Dwgs.User) (width 0.15))
      (fp_line (start -5.1 0) (end -5.1 -2) (layer Dwgs.User) (width 0.15))
      (fp_line (start 0.5 0) (end 0.5 -2) (layer Dwgs.User) (width 0.15))
      (fp_line (start -5.35 0) (end -5.35 12.1) (layer Dwgs.User) (width 0.15))
      (fp_line (start 0.75 0) (end 0.75 12.1) (layer Dwgs.User) (width 0.15))
      (fp_line (start 0.75 12.1) (end -5.35 12.1) (layer Dwgs.User) (width 0.15))
      (fp_line (start 0.75 0) (end -5.35 0) (layer Dwgs.User) (width 0.15))

      
        
        (pad "" np_thru_hole circle (at -2.3 8.6) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
        (pad "" np_thru_hole circle (at -2.3 1.6) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
      
        
        (pad 1 thru_hole oval (at -4.6 11.3 -90) (size 1.6 2.2) (drill oval 0.9 1.5) (layers *.Cu *.Mask) (net 43 "J1-PadA"))
        (pad 2 thru_hole oval (at 0 10.2 -90) (size 1.6 2.2) (drill oval 0.9 1.5) (layers *.Cu *.Mask) (net 38 "data"))
        (pad 3 thru_hole oval (at 0 6.2 -90) (size 1.6 2.2) (drill oval 0.9 1.5) (layers *.Cu *.Mask) (net 32 "GND"))
        (pad 4 thru_hole oval (at 0 3.2 -90) (size 1.6 2.2) (drill oval 0.9 1.5) (layers *.Cu *.Mask) (net 34 "VCC"))
      )
      
            (gr_line (start 91 109.5) (end 147.22730215593222 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 90.5 109) (end 90.5 53) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 91 52.5) (end 128 52.5) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 147 47.75) (end 129 47.75) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 128.5 48.25) (end 128.5 52) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 166.5 47.25) (end 166.5 45.875) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 166 45.375) (end 148 45.375) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 147.5 45.875) (end 147.5 47.25) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 185.5 49.625) (end 185.5 48.25) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 185 47.75) (end 167 47.75) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 204.5 52) (end 204.5 50.625) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 204 50.125) (end 186 50.125) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 210.3979412988017 137.62313710032112) (end 224.39794129999996 113.3744258) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 194.19299154809863 128.84455526290066) (end 209.71492859880163 137.80614980032107) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 147.6476597559322 109.72926120000002) (end 156.8730776751543 124.05293639037114) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 157.2326620183834 124.27849049566476) (end 194.00376480486958 128.78127505760708) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 224.5 113.43334944776565) (end 224.5 53) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 224 52.5) (end 205 52.5) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_line (start 224.5 113.43334944776565) (end 224.39794129999996 113.3744258) (angle 90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 147.22730215593222 110) (end 147.6476597559322 109.7292612) (angle -57.2157184809877) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 157.2934352751543 123.78219759037117) (end 156.87307767515432 124.05293639037117) (angle -50.23435431888237) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 193.94299154809863 129.27756796290063) (end 194.19299154809863 128.84455526290063) (angle -23.01863594630671) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 209.96492859880166 137.37313710032106) (end 209.71492859880166 137.80614980032107) (angle -89.99999999999889) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 224 53) (end 224.5 53) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 205 52) (end 204.5 52) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 204 50.625) (end 204.5 50.625) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 186 49.625) (end 185.5 49.625) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 185 48.25) (end 185.5 48.25) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 167 47.25) (end 166.5 47.25) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 166 45.875) (end 166.5 45.875) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 148 45.875) (end 148 45.375) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 147 47.25) (end 147 47.75) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 129 48.25) (end 129 47.75) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 128 52) (end 128 52.5) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 91 53) (end 91 52.5) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_arc (start 91 109) (end 90.5 109) (angle -90) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 109.5 71.5) (end 111.55 71.5) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 109.5 90.5) (end 111.55 90.5) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 185.5 67.725) (end 187.55 67.725) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 153 107.65) (end 155.05 107.65) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 199.49776989999998 115.4527878) (end 201.5477699 115.4527878) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 207.31164829999997 100.2187534) (end 208.41164829999997 100.2187534) (layer Edge.Cuts) (width 0.15))
(gr_circle (center 222.12068269999997 108.7687534) (end 223.22068269999997 108.7687534) (layer Edge.Cuts) (width 0.15))
            
)

        