(kicad_pcb (version 20201002) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (aux_axis_origin 148.4 80.2)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )


  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "VCC")

  (module "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu") (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005ebea01d)
    (at 146.3 78.6)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (path "/00000000-0000-0000-0000-00005ebe91ac")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c974f755-f11c-4e72-9337-9b1b03ad46d6)
    )
    (fp_text value "1uF" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2b79ad18-d7d7-43df-ab38-e75b2da12556)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 5db96da7-af8d-43d8-8dc7-a398bfc8659a)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 3076b8ca-409a-4abb-8543-19f45b2d32e7))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp a32b7c78-669e-4058-9e8f-159773d391d1))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 5298dbf1-ff20-463f-b22f-955b234f027b))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 5ee42af7-ef65-46ec-93e1-21c0e6077de0))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 9aaa51e5-eb42-4e37-9164-e5b31a4cd652))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp e610961e-a821-4b86-8c7d-d4cb27796910))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 1ffd0374-60f5-4975-8863-7ed9f29dac0e))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 26a053d6-55aa-4839-adb7-568fd5c066bb))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 8367eaee-e0ca-41eb-bc30-e532a8b59fdd))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp e3a76526-d318-4ed9-8120-844abbdc3456))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)") (tstamp 34fb9d00-02b1-48b3-a790-0112e6a08449))
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (tstamp 0336c0d4-c4f4-4020-8380-287f839c852a))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu") (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005ebea02e)
    (at 146.3 81.55 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005ebe8a2e")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7ef0f81b-f6e6-4f07-b717-38c4b1e50a5e)
    )
    (fp_text value "100" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8cd4eec9-ceb5-4b8f-83f2-9a146ee7ddd5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 93acb41a-3723-4469-9dee-a34acc325774)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 39441d2f-6110-4320-92bb-88f09b0de90b))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp ae28541a-0239-4867-9639-a73e46808278))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 752a50bd-195a-4ad5-acdb-d18c11a301e4))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 757c5363-13ba-436b-9db8-e5dc02596d27))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 91e75b42-fb6a-4a6b-be78-4013b6183b9a))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp c76bc75f-8181-4476-9973-7173e45c68ed))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 337d7915-43e4-4835-8aab-ff527c0de866))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 656d7de6-1e65-4eb7-8002-7e680bef80b9))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp ba9a410d-1c13-461f-b6a8-eeb7c4c46e58))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp fe5b7a7b-9594-494a-8fe7-df5ac5e9fd07))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VCC") (tstamp ee158b8c-0101-4c4c-b5ce-76e87c497fb9))
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)") (tstamp b67e7460-96bc-4aa0-8593-880eb3320d89))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu") (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005ebea03f)
    (at 150.71 78.6 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005ebe8e9e")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9d088aec-c53e-413e-8715-779a6ee7e407)
    )
    (fp_text value "200" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp abf3504c-c638-4bb0-8898-7b38d0241a11)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 730e1bed-bd81-4343-85e9-17d6a47cb046)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 7613df36-4992-4dd5-b97e-1f17e43e73c6))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp b6f74bca-cdeb-4109-905d-6a81777da69b))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 0e6314c1-5679-49cb-898a-296f9477855a))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 434bf54a-a88a-45dc-a569-a0a5b81a7096))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp ea59c7f6-51a1-4630-b89e-075386e527c9))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp ee5f10ba-08e8-4cb5-8185-dae7f54c20a3))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 5c2f40eb-308c-4cc2-9669-44b6645a7910))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 608be37a-af03-4e73-9e8e-c1bb3353eaf4))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp a384a468-0937-4800-9a3b-e63b6186898c))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp dc5732f3-4764-4a19-a8e3-24308ca8b363))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)") (tstamp 55440b89-8f8a-483a-9b2b-9ccc95708f75))
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (tstamp 3d8a4e48-dfd4-4c64-8dd3-885d6a7ed460))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 153 84) (end 153 76) (layer "Edge.Cuts") (width 0.05) (tstamp 00000000-0000-0000-0000-00005ebea29b))
  (gr_line (start 144 76) (end 144 84) (layer "Edge.Cuts") (width 0.05) (tstamp bb3326cd-028c-43fb-af47-5975412a67c7))
  (gr_line (start 153 76) (end 144 76) (layer "Edge.Cuts") (width 0.05) (tstamp d534140b-6f16-4b83-8893-ef4b026f6ec9))
  (gr_line (start 144 84) (end 153 84) (layer "Edge.Cuts") (width 0.05) (tstamp ea655683-6135-4d3f-a322-1186e1a703b2))

  (segment (start 147.2375 78.6) (end 149.7725 78.6) (width 0.25) (layer "F.Cu") (net 1) (tstamp 4ebf58f7-8428-4480-b240-bb7d3c895103))
  (segment (start 150.62249 77.57499) (end 151.161973 78.114473) (width 0.25) (layer "F.Cu") (net 2) (tstamp 4ed009e2-b8f5-47d8-ba45-e73cbf2524c2))
  (segment (start 145.3625 78.6) (end 145.3625 79.3) (width 0.25) (layer "F.Cu") (net 2) (tstamp 5505e502-12b2-42b0-9e88-71997ebbcbde))
  (segment (start 151.161973 78.114473) (end 151.6475 78.6) (width 0.25) (layer "F.Cu") (net 2) (tstamp 5e3899fa-1efc-49c7-bd03-0723e6564f66))
  (segment (start 145.3625 78.6) (end 146.38751 77.57499) (width 0.25) (layer "F.Cu") (net 2) (tstamp 88b2a9f5-ec07-44cc-be7d-6243af8d21a7))
  (segment (start 145.3625 79.3) (end 145.3625 81.55) (width 0.25) (layer "F.Cu") (net 2) (tstamp a49ce2ce-5d29-415b-a41f-07567cbabb0f))
  (segment (start 146.38751 77.57499) (end 150.62249 77.57499) (width 0.25) (layer "F.Cu") (net 2) (tstamp fd90cb38-571b-4f7c-8630-139c123989e3))

)
