(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 148.4 80.2)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "VCC")

  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005ebea01d)
    (at 146.3 78.6)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (path "/00000000-0000-0000-0000-00005ebe91ac")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8174b4de-74b1-48db-ab8e-c8432251095b)
    )
    (fp_text value "1uF" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 704d6d51-bb34-4cbf-83d8-841e208048d8)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 0eaa98f0-9565-4637-ace3-42a5231b07f7)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 0f22151c-f260-4674-b486-4710a2c42a55))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 1831fb37-1c5d-42c4-b898-151be6fca9dc))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 181abe7a-f941-42b6-bd46-aaa3131f90fb))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 9340c285-5767-42d5-8b6d-63fe2a40ddf3))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp c41b3c8b-634e-435a-b582-96b83bbd4032))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp ce83728b-bebd-48c2-8734-b6a50d837931))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 0b21a65d-d20b-411e-920a-75c343ac5136))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 3cd1bda0-18db-417d-b581-a0c50623df68))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp d57dcfee-5058-4fc2-a68b-05f9a48f685b))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp fe8d9267-7834-48d6-a191-c8724b2ee78d))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)") (tstamp a1823eb2-fb0d-4ed8-8b96-04184ac3a9d5))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (tstamp 03c52831-5dc5-43c5-a442-8d23643b46fb))
    (model "${MYVAR}/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005ebea02e)
    (at 146.3 81.55 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005ebe8a2e")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d8603679-3e7b-4337-8dbc-1827f5f54d8a)
    )
    (fp_text value "100" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 30f15357-ce1d-48b9-93dc-7d9b1b2aa048)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 87371631-aa02-498a-998a-09bdb74784c1)
    )
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp a3e4f0ae-9f86-49e9-b386-ed8b42e012fb))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp a690fc6c-55d9-47e6-b533-faa4b67e20f3))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 2e642b3e-a476-4c54-9a52-dcea955640cd))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 5038e144-5119-49db-b6cf-f7c345f1cf03))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 54365317-1355-4216-bb75-829375abc4ec))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp ac264c30-3e9a-4be2-b97a-9949b68bd497))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 5fc27c35-3e1c-4f96-817c-93b5570858a6))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 6c9b793c-e74d-4754-a2c0-901e73b26f1c))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp c144caa5-b0d4-4cef-840a-d4ad178a2102))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp efeac2a2-7682-4dc7-83ee-f6f1b23da506))
    (pad "1" smd roundrect locked (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VCC") (tstamp b1086f75-01ba-4188-8d36-75a9e2828ca9))
    (pad "2" smd roundrect locked (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)") (tstamp 6a45789b-3855-401f-8139-3c734f7f52f9))
    (model "${KIPRJMOD}/../../data/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005ebea03f)
    (at 150.71 78.6 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005ebe8e9e")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e8314017-7be6-4011-9179-37449a29b311)
    )
    (fp_text value "200" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e10b5627-3247-4c86-b9f6-ef474ca11543)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 746ba970-8279-4e7b-aed3-f28687777c21)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 47baf4b1-0938-497d-88f9-671136aa8be7))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp c022004a-c968-410e-b59e-fbab0e561e9d))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 10109f84-4940-47f8-8640-91f185ac9bc1))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 55e740a3-0735-4744-896e-2bf5437093b9))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 71c31975-2c45-4d18-a25a-18e07a55d11e))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp f4f99e3d-7269-4f6a-a759-16ad2a258779))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 4fb02e58-160a-4a39-9f22-d0c75e82ee72))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 77ed3941-d133-4aef-a9af-5a39322d14eb))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp e615f7aa-337e-474d-9615-2ad82b1c44ca))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp ef8fe2ac-6a7f-4682-9418-b801a1b10a3b))
    (pad "1" smd roundrect locked (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)") (tstamp eb667eea-300e-4ca7-8a6f-4b00de80cd45))
    (pad "2" smd roundrect locked (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (tstamp 44d8279a-9cd1-4db6-856f-0363131605fc))
    (model "${KIPRJMOD}/../../data/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 153 84) (end 153 76) (layer "Edge.Cuts") (width 0.05) (tstamp 00000000-0000-0000-0000-00005ebea29b))
  (gr_line (start 144 84) (end 153 84) (layer "Edge.Cuts") (width 0.05) (tstamp 4c8eb964-bdf4-44de-90e9-e2ab82dd5313))
  (gr_line (start 153 76) (end 144 76) (layer "Edge.Cuts") (width 0.05) (tstamp 9bb20359-0f8b-45bc-9d38-6626ed3a939d))
  (gr_line (start 144 76) (end 144 84) (layer "Edge.Cuts") (width 0.05) (tstamp aa14c3bd-4acc-4908-9d28-228585a22a9d))

  (segment (start 147.2375 78.6) (end 149.7725 78.6) (width 0.25) (layer "F.Cu") (net 1) (tstamp 2d210a96-f81f-42a9-8bf4-1b43c11086f3))
  (segment (start 151.161973 78.114473) (end 151.6475 78.6) (width 0.25) (layer "F.Cu") (net 2) (tstamp 666713b0-70f4-42df-8761-f65bc212d03b))
  (segment (start 145.3625 78.6) (end 145.3625 79.3) (width 0.25) (layer "F.Cu") (net 2) (tstamp 6c2e273e-743c-4f1e-a647-4171f8122550))
  (segment (start 145.3625 78.6) (end 146.38751 77.57499) (width 0.25) (layer "F.Cu") (net 2) (tstamp 7aed3a71-054b-4aaa-9c0a-030523c32827))
  (segment (start 150.62249 77.57499) (end 151.161973 78.114473) (width 0.25) (layer "F.Cu") (net 2) (tstamp 7dc880bc-e7eb-4cce-8d8c-0b65a9dd788e))
  (segment (start 146.38751 77.57499) (end 150.62249 77.57499) (width 0.25) (layer "F.Cu") (net 2) (tstamp 9157f4ae-0244-4ff1-9f73-3cb4cbb5f280))
  (segment (start 145.3625 79.3) (end 145.3625 81.55) (width 0.25) (layer "F.Cu") (net 2) (tstamp e857610b-4434-4144-b04e-43c1ebdc5ceb))

)
