(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(J1-Pad1)")

  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 00000000-0000-0000-0000-0000619bcbca)
    (at 138 93)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (path "/00000000-0000-0000-0000-00005f10f92f")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.68) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ef8fe2ac-6a7f-4682-9418-b801a1b10a3b)
    )
    (fp_text value "1nF" (at 0 1.68) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 44d8279a-9cd1-4db6-856f-0363131605fc)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 5038e144-5119-49db-b6cf-f7c345f1cf03)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer "F.SilkS") (width 0.12) (tstamp 1e1b062d-fad0-427c-a622-c5b8a80b5268))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer "F.SilkS") (width 0.12) (tstamp cbdcaa78-3bbc-413f-91bf-2709119373ce))
    (fp_line (start -1.7 0.98) (end -1.7 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp 3b838d52-596d-4e4d-a6ac-e4c8e7621137))
    (fp_line (start 1.7 -0.98) (end 1.7 0.98) (layer "F.CrtYd") (width 0.05) (tstamp 66116376-6967-4178-9f23-a26cdeafc400))
    (fp_line (start -1.7 -0.98) (end 1.7 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp 749dfe75-c0d6-4872-9330-29c5bbcb8ff8))
    (fp_line (start 1.7 0.98) (end -1.7 0.98) (layer "F.CrtYd") (width 0.05) (tstamp eb667eea-300e-4ca7-8a6f-4b00de80cd45))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 2e642b3e-a476-4c54-9a52-dcea955640cd))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 30f15357-ce1d-48b9-93dc-7d9b1b2aa048))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 87371631-aa02-498a-998a-09bdb74784c1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp d8603679-3e7b-4337-8dbc-1827f5f54d8a))
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)") (tstamp ac264c30-3e9a-4be2-b97a-9949b68bd497))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)") (tstamp 54365317-1355-4216-bb75-829375abc4ec))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp 00000000-0000-0000-0000-0000619bcbf6)
    (at 133.4609 93.95672)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (path "/00000000-0000-0000-0000-00005f10e81f")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a44418c-7bb4-4e99-8836-57f153c19721)
    )
    (fp_text value "Molex KK" (at 0 4.87) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0147f16a-c952-4891-8f53-a9fb8cddeb8d)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a05d7640-f2f6-4ba7-8c51-5a4af431fc13)
    )
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 0a3cc030-c9dd-4d74-9d50-715ed2b361a2))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 15875808-74d5-4210-b8ca-aa8fbc04ae21))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 81bbc3ff-3938-49ac-8297-ce2bcc9a42bd))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 8322f275-268c-4e87-a69f-4cfbf05e747f))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp b6270a28-e0d9-4655-a18a-03dbf007b940))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp dd00c2e1-6027-4717-b312-4fab3ee52002))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp 0d0bb7b2-a6e5-46d2-9492-a1aa6e5a7b2f))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp b1169a2d-8998-4b50-a48d-c520bcc1b8e1))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp d1262c4d-2245-4c4f-8f35-7bb32cd9e21e))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp d22e95aa-f3db-4fbc-a331-048a2523233e))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 1860e030-7a36-4298-b7fc-a16d48ab15ba))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 32667662-ae86-4904-b198-3e95f11851bf))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 3dcc657b-55a1-48e0-9667-e01e7b6b08b5))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 67f6e996-3c99-493c-8f6f-e739e2ed5d7a))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp f3490fa5-5a27-423b-af60-53609669542c))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)") (tstamp 13abf99d-5265-4779-8973-e94370fd18ff))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)") (tstamp a7520ad3-0f8b-4788-92d4-8ffb277041e6))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 00000000-0000-0000-0000-0000619bcc07)
    (at 137.9909 96.11672)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f10f746")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1a2f72d1-0b36-4610-afc4-4ad1660d5d3b)
    )
    (fp_text value "1k" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0dcdf1b8-13c6-48b4-bd94-5d26038ff231)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp e877bf4a-4210-4bd3-b7b0-806eb4affc5b)
    )
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "F.SilkS") (width 0.12) (tstamp 13475e15-f37c-4de8-857e-1722b0c39513))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "F.SilkS") (width 0.12) (tstamp 2732632c-4768-42b6-bf7f-14643424019e))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 58dc14f9-c158-4824-a84e-24a6a482a7a4))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp b635b16e-60bb-4b3e-9fc3-47d34eef8381))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp dde3dba8-1b81-466c-93a3-c284ff4da1ef))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp f976e2cc-36f9-4479-a816-2c74d1d5da6f))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 120a7b0f-ddfd-4447-85c1-35665465acdb))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 48f827a8-6e22-4a2e-abdc-c2a03098d883))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 854dd5d4-5fd2-4730-bd49-a9cd8299a065))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 8d55e186-3e11-40e8-a65e-b36a8a00069e))
    (pad "1" smd roundrect locked (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "Net-(C1-Pad1)") (tstamp cef6f603-8a0b-4dd0-af99-ebfbef7d1b4b))
    (pad "2" smd roundrect locked (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 3 "Net-(J1-Pad1)") (tstamp 9c8ccb2a-b1e9-4f2c-94fe-301b5975277e))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp 00000000-0000-0000-0000-0000619bccdc)
    (at 142.80388 96.47174 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (path "/00000000-0000-0000-0000-00005f10e435")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 78cbdd6c-4878-4cc5-9a58-0e506478e37d)
    )
    (fp_text value "Molex KK ñoño" (at 0 4.87) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6e105729-aba0-497c-a99e-c32d2b3ddb6d)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 10109f84-4940-47f8-8640-91f185ac9bc1)
    )
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 3f5fe6b7-98fc-4d3e-9567-f9f7202d1455))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 5cbb5968-dbb5-4b84-864a-ead1cacf75b9))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp afb8e687-4a13-41a1-b8c0-89a749e897fe))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp bb7f0588-d4d8-44bf-9ebf-3c533fe4d6ae))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp da469d11-a8a4-414b-9449-d151eeaf4853))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp f1830a1b-f0cc-47ae-a2c9-679c82032f14))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp 62c076a3-d618-44a2-9042-9a08b3576787))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 983c426c-24e0-4c65-ab69-1f1824adc5c6))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp c1d83899-e380-49f9-a87d-8e78bc089ebf))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp e9bb29b2-2bb9-4ea2-acd9-2bb3ca677a12))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 6a955fc7-39d9-4c75-9a69-676ca8c0b9b2))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 71c31975-2c45-4d18-a25a-18e07a55d11e))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 746ba970-8279-4e7b-aed3-f28687777c21))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp e10b5627-3247-4c86-b9f6-ef474ca11543))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp e8314017-7be6-4011-9179-37449a29b311))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)") (tstamp 55e740a3-0735-4744-896e-2bf5437093b9))
    (pad "2" thru_hole oval locked (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)") (tstamp f4f99e3d-7269-4f6a-a759-16ad2a258779))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 131 100) (end 131 91) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-0000619bcf98))
  (gr_line (start 131 91) (end 146 91) (layer "Edge.Cuts") (width 0.1) (tstamp 5fc27c35-3e1c-4f96-817c-93b5570858a6))
  (gr_line (start 146 100) (end 131 100) (layer "Edge.Cuts") (width 0.1) (tstamp c144caa5-b0d4-4cef-840a-d4ad178a2102))
  (gr_line (start 146 91) (end 146 100) (layer "Edge.Cuts") (width 0.1) (tstamp efeac2a2-7682-4dc7-83ee-f6f1b23da506))

  (segment (start 145 98) (end 145 95) (width 0.25) (layer "B.Cu") (net 1) (tstamp 127679a9-3981-4934-815e-896a4e3ff56e))
  (segment (start 143.93174 93.93174) (end 142.80388 93.93174) (width 0.25) (layer "B.Cu") (net 1) (tstamp 48ab88d7-7084-4d02-b109-3ad55a30bb11))
  (segment (start 133.49672 96.49672) (end 136 99) (width 0.25) (layer "B.Cu") (net 1) (tstamp 6a45789b-3855-401f-8139-3c734f7f52f9))
  (segment (start 133.4609 96.49672) (end 133.49672 96.49672) (width 0.25) (layer "B.Cu") (net 1) (tstamp 6c9b793c-e74d-4754-a2c0-901e73b26f1c))
  (segment (start 144 99) (end 145 98) (width 0.25) (layer "B.Cu") (net 1) (tstamp 716e31c5-485f-40b5-88e3-a75900da9811))
  (segment (start 139.93174 93.93174) (end 139 93) (width 0.25) (layer "B.Cu") (net 1) (tstamp 8174b4de-74b1-48db-ab8e-c8432251095b))
  (segment (start 136 99) (end 144 99) (width 0.25) (layer "B.Cu") (net 1) (tstamp b1086f75-01ba-4188-8d36-75a9e2828ca9))
  (segment (start 145 95) (end 143.93174 93.93174) (width 0.25) (layer "B.Cu") (net 1) (tstamp f71da641-16e6-4257-80c3-0b9d804fee4f))
  (segment (start 142.80388 93.93174) (end 139.93174 93.93174) (width 0.25) (layer "B.Cu") (net 1) (tstamp fd470e95-4861-44fe-b1e4-6d8a7c66e144))
  (segment (start 135.04328 93.95672) (end 136 93) (width 0.25) (layer "B.Cu") (net 2) (tstamp 0eaa98f0-9565-4637-ace3-42a5231b07f7))
  (segment (start 136 93) (end 137 93) (width 0.25) (layer "B.Cu") (net 2) (tstamp 181abe7a-f941-42b6-bd46-aaa3131f90fb))
  (segment (start 133.4609 93.95672) (end 135.04328 93.95672) (width 0.25) (layer "B.Cu") (net 2) (tstamp 704d6d51-bb34-4cbf-83d8-841e208048d8))
  (segment (start 137 93) (end 137 96) (width 0.25) (layer "B.Cu") (net 2) (tstamp ce83728b-bebd-48c2-8734-b6a50d837931))
  (segment (start 139.47174 96.47174) (end 139 96) (width 0.25) (layer "B.Cu") (net 3) (tstamp 9340c285-5767-42d5-8b6d-63fe2a40ddf3))
  (segment (start 142.80388 96.47174) (end 139.47174 96.47174) (width 0.25) (layer "B.Cu") (net 3) (tstamp c41b3c8b-634e-435a-b582-96b83bbd4032))

)
