(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 4.69)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")

  (gr_line (start 78 94) (end 78 34) (layer "F.Cu") (width 1) (tstamp 262f85ee-a49a-4194-bdee-29ac02a484ec))
  (gr_line (start 70 40) (end 130 40) (layer "F.Cu") (width 1) (tstamp 77da69f1-4a7e-4daf-b100-27fb75871e8c))
  (gr_line (start 80 94) (end 80 34) (layer "In1.Cu") (width 1) (tstamp fa1503a0-19c0-4e06-a1de-65c87d9f3046))
  (gr_line (start 70 42) (end 130 42) (layer "In1.Cu") (width 1) (tstamp fb7c97ee-bfba-49df-b0a6-949d8c1dbc80))
  (gr_line (start 82 94) (end 82 34) (layer "In2.Cu") (width 1) (tstamp 09c5b2e9-fadc-49a8-867f-ed662ece0465))
  (gr_line (start 70 44) (end 130 44) (layer "In2.Cu") (width 1) (tstamp ea4e4e6a-929c-474e-821a-a752170b4f9c))
  (gr_line (start 84 94) (end 84 34) (layer "B.Cu") (width 1) (tstamp 54c8435a-0b4b-47ec-b2ba-919fa8bf92bd))
  (gr_line (start 70 46) (end 130 46) (layer "B.Cu") (width 1) (tstamp d312a4d8-3900-420d-83df-acf2d1616827))
  (gr_line (start 70 50) (end 130 50) (layer "B.Adhes") (width 1) (tstamp db8a60a1-6c78-42ba-b45c-08cf72ddf99e))
  (gr_line (start 88 94) (end 88 34) (layer "B.Adhes") (width 1) (tstamp e3da7779-0ea1-46dc-90c1-3da0eae63ac3))
  (gr_line (start 70 48) (end 130 48) (layer "F.Adhes") (width 1) (tstamp 2c93e68b-23e0-4a8f-845c-7911d3abc09e))
  (gr_line (start 86 94) (end 86 34) (layer "F.Adhes") (width 1) (tstamp 959a520e-05e4-488b-a17d-dfb714eea3cc))
  (gr_line (start 70 54) (end 130 54) (layer "B.Paste") (width 1) (tstamp 69029636-79e5-47ae-bb14-9bc5dbdeb2b4))
  (gr_line (start 92 94) (end 92 34) (layer "B.Paste") (width 1) (tstamp b5ffc3b0-893d-4977-bac8-ca0fd10d098d))
  (gr_line (start 90 94) (end 90 34) (layer "F.Paste") (width 1) (tstamp 364ea6d5-81d6-485d-af85-ad66a6d4fe3f))
  (gr_line (start 70 52) (end 130 52) (layer "F.Paste") (width 1) (tstamp 52c6d709-bf2c-4bb8-aab3-486121f784ad))
  (gr_line (start 96 94) (end 96 34) (layer "B.SilkS") (width 1) (tstamp 4c0f28bd-4fdd-4e3f-866b-0af6e20563d6))
  (gr_line (start 70 58) (end 130 58) (layer "B.SilkS") (width 1) (tstamp de4d9514-3cb5-4e56-aa34-9a36cc7ab2fb))
  (gr_line (start 70 56) (end 130 56) (layer "F.SilkS") (width 1) (tstamp 55366e14-cec9-493d-901d-448b04d2f286))
  (gr_line (start 94 94) (end 94 34) (layer "F.SilkS") (width 1) (tstamp ac400113-5b0c-4ba3-90f5-fba5c1ab46ed))
  (gr_line (start 70 62) (end 130 62) (layer "B.Mask") (width 1) (tstamp 004f1cac-5431-476d-8d12-f0d7e1d2971c))
  (gr_line (start 100 94) (end 100 34) (layer "B.Mask") (width 1) (tstamp 61d13227-ea38-4175-a5c0-8f75a3d5765d))
  (gr_line (start 70 60) (end 130 60) (layer "F.Mask") (width 1) (tstamp 5aeb1e78-7ed8-446f-a1fa-e72019642e8e))
  (gr_line (start 98 94) (end 98 34) (layer "F.Mask") (width 1) (tstamp 92927a9e-f25b-41ba-9c93-2d6e3e6c1f89))
  (gr_line (start 70 64) (end 130 64) (layer "Dwgs.User") (width 1) (tstamp c457d6bc-d372-4e5a-9060-512765531115))
  (gr_line (start 102 94) (end 102 34) (layer "Dwgs.User") (width 1) (tstamp ed719640-2001-4a0b-956b-2fc557f849a0))
  (gr_line (start 104 94) (end 104 34) (layer "Cmts.User") (width 1) (tstamp 65648dec-894d-4846-9000-a3f37128d377))
  (gr_line (start 70 66) (end 130 66) (layer "Cmts.User") (width 1) (tstamp 8bcf2b99-1928-47d5-9785-f90fe779323f))
  (gr_line (start 106 94) (end 106 34) (layer "Eco1.User") (width 1) (tstamp 725ddd62-c356-4053-88dd-d8de16f6d111))
  (gr_line (start 70 68) (end 130 68) (layer "Eco1.User") (width 1) (tstamp 883e7763-c7c3-4085-8e36-b949c37033d0))
  (gr_line (start 108 94) (end 108 34) (layer "Eco2.User") (width 1) (tstamp 8d9916ee-e2bd-408c-960d-d9bae62b28e4))
  (gr_line (start 70 70) (end 130 70) (layer "Eco2.User") (width 1) (tstamp c898c915-89f5-4003-9fb8-8b0c3f06dfe7))
  (gr_line (start 110 94) (end 110 34) (layer "Edge.Cuts") (width 1) (tstamp 196afe34-74fd-48ae-9b9f-d7a341cb4cdd))
  (gr_line (start 70 72) (end 130 72) (layer "Edge.Cuts") (width 1) (tstamp 925356e8-9fe3-4fca-8329-eba967a76629))
  (gr_line (start 70 74) (end 130 74) (layer "Margin") (width 1) (tstamp da88cf57-0975-4f67-b828-34f4f4c6151f))
  (gr_line (start 112 94) (end 112 34) (layer "Margin") (width 1) (tstamp e36b28a4-7427-4708-a63e-3fe312e8d49f))
  (gr_line (start 116 94) (end 116 34) (layer "B.CrtYd") (width 1) (tstamp aef028c9-bd4b-4984-aea9-019dcc39d7ec))
  (gr_line (start 70 78) (end 130 78) (layer "B.CrtYd") (width 1) (tstamp f8978d6f-bc80-4d45-99fe-9eda6ceed8ec))
  (gr_line (start 70 76) (end 130 76) (layer "F.CrtYd") (width 1) (tstamp 84164d3c-90bc-45b0-ac63-7f7a93843cb3))
  (gr_line (start 114 94) (end 114 34) (layer "F.CrtYd") (width 1) (tstamp e10a8197-feb1-49a8-8ce1-531c3527f182))
  (gr_line (start 120 94) (end 120 34) (layer "B.Fab") (width 1) (tstamp 2a77a72e-d058-40b9-a6e8-cfe4c97e7ab1))
  (gr_line (start 70 82) (end 130 82) (layer "B.Fab") (width 1) (tstamp 96916265-4653-41c3-9a80-f6775aa2b630))
  (gr_line (start 70 80) (end 130 80) (layer "F.Fab") (width 1) (tstamp 1a253373-7aaa-4800-82a0-f05224ca4a7a))
  (gr_line (start 118 94) (end 118 34) (layer "F.Fab") (width 1) (tstamp c00a6ff3-d367-48aa-9987-c597c23d6ece))
  (gr_line (start 70 84) (end 130 84) (layer "User.1") (width 1) (tstamp 1e5a4a4f-7ec1-4d5e-aab0-77eebafcd5cd))
  (gr_line (start 122 94) (end 122 34) (layer "User.1") (width 1) (tstamp 75e54a73-a71d-4649-833f-7b284b918c88))
  (gr_line (start 124 94) (end 124 34) (layer "User.2") (width 1) (tstamp 63775781-01d0-47bd-b139-79a50fca0217))
  (gr_line (start 70 86) (end 130 86) (layer "User.2") (width 1) (tstamp 7505eede-a417-42c3-88a2-1fe21ee21a2a))
  (gr_text "F.Cu\nIn1.Cu\nIn2.Cu\nB.Cu\nF.Adhes\nB.Adhes\nF.Paste\nB.Paste\nF.SilkS\nB.SilkS\nF.Mask\nB.Mask\nDwgs.User\nCmts.User\nEco1.User\nEco2.User\nEdge.Cuts\nMargin\nF.CrtYd\nB.CrtYd\nF.Fab\nB.Fab\nUser.1\nUser.2" (at 69 63) (layer "F.Cu") (tstamp 82c3fcff-0c4d-46ec-9117-fd4b044c0976)
    (effects (font (size 1.25 1.5) (thickness 0.25)) (justify right))
  )
  (gr_text "F.Cu\nIn1.Cu\nIn2.Cu\nB.Cu\nF.Adhes\nB.Adhes\nF.Paste\nB.Paste\nF.SilkS\nB.SilkS\nF.Mask\nB.Mask\nDwgs.User\nCmts.User\nEco1.User\nEco2.User\nEdge.Cuts\nMargin\nF.CrtYd\nB.CrtYd\nF.Fab\nB.Fab\nUser.1\nUser.2" (at 101 33 90) (layer "F.Cu") (tstamp f231041b-336c-4b9b-9f86-123f9dc12d97)
    (effects (font (size 1.25 1.5) (thickness 0.25)) (justify left))
  )

)
