(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (title_block
    (title "Simple Plotting Test")
    (date "2018-06-04")
    (rev "A")
    (company "KiPlot - KiCad Plotting Driver")
  )

  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")

  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 5B1533F4) (tstamp 00000000-0000-0000-0000-00005b15541f)
    (at 140 100)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP1" (at 0 -2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6de6eb96-2bce-4893-8df8-ee4f11c74ee2)
    )
    (fp_text value "TestPoint2mm" (at 0 2.05) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 41a9120a-c6ae-4f4c-89c9-74577a60e61b)
    )
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6d950297-d87f-4013-828d-d61567be0ff9)
    )
    (fp_line (start -1.2 -1.2) (end 1.2 -1.2) (layer "F.SilkS") (width 0.12) (tstamp 96569f29-d14d-459b-aa18-c71851f86ebd))
    (fp_line (start 1.2 -1.2) (end 1.2 1.2) (layer "F.SilkS") (width 0.12) (tstamp e0b3cf66-8357-4d7c-b7f6-f72b3c01d9a3))
    (fp_line (start 1.2 1.2) (end -1.2 1.2) (layer "F.SilkS") (width 0.12) (tstamp f071f4fd-84af-4ce5-92c3-8cbf0759c557))
    (fp_line (start -1.2 1.2) (end -1.2 -1.2) (layer "F.SilkS") (width 0.12) (tstamp fce549bf-eb06-4c57-9871-f274395a6db4))
    (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 007608dd-c1f2-45c2-badb-3a62f64a38ba))
    (fp_line (start -1.5 -1.5) (end -1.5 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 6b7b21e3-3ef8-47a3-ac37-f233999767d9))
    (fp_line (start 1.5 1.5) (end 1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 89f4a15b-e62b-41db-be77-4222d41d0594))
    (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp d7e8bce2-c343-42c9-b249-7442bfcbfac1))
    (pad "1" thru_hole rect locked (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 59e3f63a-c9de-4e49-b736-b450c077c5ee))
  )

  (gr_line (start 145 95) (end 132 95) (layer "Edge.Cuts") (width 0.2) (tstamp 0e145530-18ad-4043-9162-57ab89376be3))
  (gr_line (start 132 95) (end 132 106) (layer "Edge.Cuts") (width 0.2) (tstamp 0f5b234a-5391-423f-914b-6481e2e4b824))
  (gr_line (start 148 106) (end 148 98) (layer "Edge.Cuts") (width 0.2) (tstamp 2fdbf9a7-eb5f-4089-b5d6-a2ce1a74d77d))
  (gr_arc (start 145 95) (mid 147.12132 95.87868) (end 148 98) (layer "Edge.Cuts") (width 0.2) (tstamp 6fdb63ac-c5a6-4cde-a60f-ceff411b1607))
  (gr_line (start 132 106) (end 148 106) (layer "Edge.Cuts") (width 0.2) (tstamp bf8b6910-62ee-4e86-8c6e-6aaf131bdde2))
  (dimension (type aligned) (layer "Dwgs.User") (tstamp e5864fe6-2a71-47f0-90ce-38c3f8901580)
    (pts (xy 132 106) (xy 148 106))
    (height 3)
    (gr_text "0,6299 in" (at 140 107.2) (layer "Dwgs.User") (tstamp e5864fe6-2a71-47f0-90ce-38c3f8901580)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )

  (segment (start 140 100) (end 143 100) (width 1) (layer "F.Cu") (net 0) (tstamp 2024a043-b527-4a79-8fd0-789dc8affa64))
  (segment (start 134 99) (end 134 101) (width 1) (layer "F.Cu") (net 0) (tstamp ad45ccad-656d-4667-8c74-5c79ecd6675b))
  (segment (start 142 102) (end 143 102) (width 1) (layer "B.Cu") (net 0) (tstamp 11d54499-6257-4e14-b0ac-6c8398bbc4be))
  (segment (start 140 100) (end 142 102) (width 1) (layer "B.Cu") (net 0) (tstamp 38bd6bf7-b2df-46b0-88e4-290d244f92c3))

)
