(kicad_pcb (version 20201002) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )


  (net 0 "")

  (module "Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu") (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005ea76d80)
    (at 105 35 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7accab11-60c9-461f-ba53-a70ef610ef19)
    )
    (fp_text value "R_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (at 0 1.65 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bfb2ae84-71ae-497d-817c-7afccc6c3d10)
    )
    (fp_text user "100" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 3e391892-edcb-4f5c-8776-b26e20029ef6)
    )
    (fp_line (start -0.261252 0.71) (end 0.261252 0.71) (layer "F.SilkS") (width 0.12) (tstamp 3011df62-c0d7-4b9c-b1f9-a9984bc57a14))
    (fp_line (start -0.261252 -0.71) (end 0.261252 -0.71) (layer "F.SilkS") (width 0.12) (tstamp f46daced-b9c6-4d64-a28c-6afb7e2c3065))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 0217af6d-5725-4e07-b2d1-e6f17cf8c636))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 3e9cce14-3415-452e-bdc2-0227361387b6))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 4b0e6714-7a3d-4a9c-8633-296acc4bc88d))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 7cd569c7-a497-43f6-8a18-c63a614332b7))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 2702b853-e972-47a7-ad9a-9798d1c0efbd))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 2ddef00a-9f12-4837-8569-6063e471cad8))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 8023ef0f-6945-46ec-a981-7b131d3d0abe))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 85bb78b4-3e17-45b4-b116-981f52407a88))
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391) (tstamp 9b6853f1-1f2b-46bb-86bb-c96ab23e5fa9))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391) (tstamp 082ba767-9485-4883-93b1-46cd6b032d47))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "Resistor_THT:R_Box_L13.0mm_W4.0mm_P9.00mm" (layer "F.Cu") (tedit 5AE5139B) (tstamp 00000000-0000-0000-0000-00005ea76ec0)
    (at 110 45)
    (descr "Resistor, Box series, Radial, pin pitch=9.00mm, 2W, length*width=13.0*4.0mm^2, http://www.produktinfo.conrad.com/datenblaetter/425000-449999/443860-da-01-de-METALLBAND_WIDERSTAND_0_1_OHM_5W_5Pr.pdf")
    (tags "Resistor Box series Radial pin pitch 9.00mm 2W length 13.0mm width 4.0mm")
    (attr through_hole)
    (fp_text reference "R3" (at 4.5 -3.25) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 60ea5e3e-dd18-4da5-b8f0-939cb41d6498)
    )
    (fp_text value "R_Box_L13.0mm_W4.0mm_P9.00mm" (at 4.5 3.25) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3def6d7e-7290-44d2-8ed9-c2e5c43626ce)
    )
    (fp_text user "300" (at 4.5 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 27407789-cdfc-4f8a-8ac7-06bdef979f56)
    )
    (fp_line (start -2.12 -2.12) (end -2.12 2.12) (layer "F.SilkS") (width 0.12) (tstamp 7af4e766-b871-48ce-8b98-48f12ab55700))
    (fp_line (start 11.12 -2.12) (end 11.12 2.12) (layer "F.SilkS") (width 0.12) (tstamp bff197df-2e9d-4e5b-b02a-6d1d875c548e))
    (fp_line (start -2.12 2.12) (end 11.12 2.12) (layer "F.SilkS") (width 0.12) (tstamp cf4e44be-ae4e-40a9-ad68-f03d79dcb1dd))
    (fp_line (start -2.12 -2.12) (end 11.12 -2.12) (layer "F.SilkS") (width 0.12) (tstamp f4411b38-872b-4492-b9f6-a161361afc62))
    (fp_line (start 11.25 -2.25) (end -2.25 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp 5e6c289d-b3c4-4bbb-80aa-eb9526a12989))
    (fp_line (start 11.25 2.25) (end 11.25 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp 6e5e110d-b885-4f13-9af0-7002489251f2))
    (fp_line (start -2.25 -2.25) (end -2.25 2.25) (layer "F.CrtYd") (width 0.05) (tstamp 77564e42-6b2c-411a-a64c-f03943640b57))
    (fp_line (start -2.25 2.25) (end 11.25 2.25) (layer "F.CrtYd") (width 0.05) (tstamp ca93b3d8-521f-49e8-81e9-b797eabca533))
    (fp_line (start -2 2) (end 11 2) (layer "F.Fab") (width 0.1) (tstamp 69b2f250-7e3c-4177-a6a5-11798c1789fe))
    (fp_line (start -2 -2) (end -2 2) (layer "F.Fab") (width 0.1) (tstamp bab10405-2df6-4f09-a546-81486a8098ef))
    (fp_line (start 11 2) (end 11 -2) (layer "F.Fab") (width 0.1) (tstamp c88e7db9-6e27-4690-a360-aa8a64ff13e1))
    (fp_line (start 11 -2) (end -2 -2) (layer "F.Fab") (width 0.1) (tstamp dcbc4cda-7fe2-47d5-b1dc-59b7e2a8301a))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 785912b7-60c1-43ec-9811-4a74538adb8a))
    (pad "2" thru_hole circle (at 9 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp d69c2026-913a-4a9c-866d-4df3d8ce63a8))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Box_L13.0mm_W4.0mm_P9.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "MountingHole:MountingHole_2.1mm" (layer "F.Cu") (tedit 5B924765) (tstamp 00000000-0000-0000-0000-00005ebe1aa4)
    (at 120 29)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1d2988d6-294f-4e93-b979-f438ff3544cc)
    )
    (fp_text value "MountingHole_2.1mm" (at 0 3.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e014c3c2-85c0-400c-8ee1-749eca4c0d34)
    )
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c994ca02-fbbf-4c56-9a36-6854a0a43ff0)
    )
    (fp_circle (center 0 0) (end 2.1 0) (layer "Cmts.User") (width 0.15) (tstamp 7387fc61-ddba-40f1-bd9e-b6df68988ed3))
    (fp_circle (center 0 0) (end 2.35 0) (layer "F.CrtYd") (width 0.05) (tstamp 0d6b9c1e-4afb-499a-a533-00e027146f71))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask) (tstamp ceb4799f-93d5-4176-a733-69d970a274b6))
  )

  (module "Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "B.Cu") (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005ea76de9)
    (at 110 35 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "R2" (at 0 1.65 -90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e71fc067-1e15-464b-a67c-ed53b03d94de)
    )
    (fp_text value "R_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (at 0 -1.65 -90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 47b7ed7b-6581-4ac7-a0c2-91351ff83e2e)
    )
    (fp_text user "150" (at 0 0 -90) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp c62bf5bc-d850-4481-a9b8-3934e9ff0e51)
    )
    (fp_line (start -0.261252 -0.71) (end 0.261252 -0.71) (layer "B.SilkS") (width 0.12) (tstamp f3ca6d98-c2d2-499c-a2b3-2b3e369f9988))
    (fp_line (start -0.261252 0.71) (end 0.261252 0.71) (layer "B.SilkS") (width 0.12) (tstamp f9e5a22a-6646-4709-b9b7-9673f6fcc184))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95) (layer "B.CrtYd") (width 0.05) (tstamp 067cc84e-2712-40e8-a493-07e950859342))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95) (layer "B.CrtYd") (width 0.05) (tstamp 35b98d65-bd80-4ef9-8e78-54ec2fd1d85a))
    (fp_line (start -1.85 0.95) (end 1.85 0.95) (layer "B.CrtYd") (width 0.05) (tstamp c2821538-1c13-4611-9dba-ef30a5f812b7))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95) (layer "B.CrtYd") (width 0.05) (tstamp eb39ded6-0c38-4927-9aa9-43dba7d17210))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer "B.Fab") (width 0.1) (tstamp 2715ac95-ae1c-47bd-8b6a-bcf194b9cd8d))
    (fp_line (start 1 -0.6) (end -1 -0.6) (layer "B.Fab") (width 0.1) (tstamp 56f71ae4-54d4-4aea-911f-bd9df256d954))
    (fp_line (start -1 -0.6) (end -1 0.6) (layer "B.Fab") (width 0.1) (tstamp 600a7f13-2d22-43ba-84c0-98c3577b6a77))
    (fp_line (start -1 0.6) (end 1 0.6) (layer "B.Fab") (width 0.1) (tstamp 7c8ec9db-6194-410f-91ef-e468f5bdb544))
    (pad "1" smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391) (tstamp d736e075-184f-4366-96db-afeb06451de8))
    (pad "2" smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391) (tstamp 385f301d-d00a-47c6-9ff4-fd5305d883b6))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 100 25) (end 100 50) (layer "Edge.Cuts") (width 0.05) (tstamp 00000000-0000-0000-0000-00005ea7192f))
  (gr_line (start 125 25) (end 125 50) (layer "Edge.Cuts") (width 0.05) (tstamp 00000000-0000-0000-0000-00005ea76efc))
  (gr_line (start 100 25) (end 125 25) (layer "Edge.Cuts") (width 0.05) (tstamp 00000000-0000-0000-0000-00005ea76f1d))
  (gr_line (start 100 50) (end 125 50) (layer "Edge.Cuts") (width 0.05) (tstamp eb88665f-f4a5-4024-9e6d-ee323df0995d))

)
