(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-rc2-76-gb5f63567d)")

  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 4)
    (zones 0)
    (modules 1)
    (nets 1)
  )

  (page A4)
  (title_block
    (title "Simple Plotting Test")
    (date 2018-06-04)
    (rev A)
    (company "KiPlot - KiCad Plotting Driver")
  )

  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5B1533F4) (tstamp 5B15541F)
    (at 140 100)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TestPoint2mm (at 0 2.05) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.5 1.5) (end 1.5 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -1.5) (end -1.5 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.2 1.2) (end -1.2 -1.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 1.2) (end -1.2 1.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 -1.2) (end 1.2 1.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.2 -1.2) (end 1.2 -1.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (dimension 16 (width 0.15) (layer Dwgs.User)
    (gr_text "16,000 mm" (at 140 109.3) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (feature1 (pts (xy 148 106) (xy 148 108.586421)))
    (feature2 (pts (xy 132 106) (xy 132 108.586421)))
    (crossbar (pts (xy 132 108) (xy 148 108)))
    (arrow1a (pts (xy 148 108) (xy 146.873496 108.586421)))
    (arrow1b (pts (xy 148 108) (xy 146.873496 107.413579)))
    (arrow2a (pts (xy 132 108) (xy 133.126504 108.586421)))
    (arrow2b (pts (xy 132 108) (xy 133.126504 107.413579)))
  )
  (gr_arc (start 145 98) (end 148 98) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 145 95) (end 132 95) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 148 106) (end 148 98) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 132 106) (end 148 106) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 132 95) (end 132 106) (layer Edge.Cuts) (width 0.2))

  (segment (start 140 100) (end 143 100) (width 1) (layer F.Cu) (net 0))
  (segment (start 140 100) (end 142 102) (width 1) (layer B.Cu) (net 0))
  (segment (start 142 102) (end 143 102) (width 1) (layer B.Cu) (net 0))
  (segment (start 134 99) (end 134 101) (width 1) (layer F.Cu) (net 0))

)
