(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (title_block
    (comment 2 "The_C2")
  )

  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(R1-Pad2)")
  (net 2 "Net-(R1-Pad1)")
  (net 3 "Net-(R2-Pad2)")
  (net 4 "Net-(R2-Pad1)")
  (net 5 "Net-(R3-Pad2)")
  (net 6 "Net-(R3-Pad1)")
  (net 7 "Net-(R4-Pad2)")
  (net 8 "Net-(R4-Pad1)")
  (net 9 "Net-(R5-Pad2)")
  (net 10 "Net-(R5-Pad1)")
  (net 11 "Net-(R6-Pad2)")
  (net 12 "Net-(R6-Pad1)")
  (net 13 "Net-(R7-Pad2)")
  (net 14 "Net-(R7-Pad1)")
  (net 15 "Net-(R8-Pad2)")
  (net 16 "Net-(R8-Pad1)")
  (net 17 "Net-(R9-Pad2)")
  (net 18 "Net-(R9-Pad1)")
  (net 19 "Net-(R10-Pad2)")
  (net 20 "Net-(R10-Pad1)")
  (net 21 "Net-(R11-Pad2)")
  (net 22 "Net-(R11-Pad1)")
  (net 23 "Net-(R12-Pad2)")
  (net 24 "Net-(R12-Pad1)")
  (net 25 "Net-(R13-Pad2)")
  (net 26 "Net-(R13-Pad1)")
  (net 27 "Net-(R14-Pad2)")
  (net 28 "Net-(R14-Pad1)")
  (net 29 "Net-(R15-Pad2)")
  (net 30 "Net-(R15-Pad1)")
  (net 31 "Net-(R16-Pad2)")
  (net 32 "Net-(R16-Pad1)")
  (net 33 "Net-(R17-Pad2)")
  (net 34 "Net-(R17-Pad1)")
  (net 35 "Net-(R18-Pad2)")
  (net 36 "Net-(R18-Pad1)")
  (net 37 "Net-(R19-Pad2)")
  (net 38 "Net-(R19-Pad1)")
  (net 39 "Net-(R20-Pad2)")
  (net 40 "Net-(R20-Pad1)")

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b1ae)
    (at 127 89.027)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005e6a2873")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b6135480-ace6-42b2-9c47-856ef57cded1)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6d1d60ff-408a-47a7-892f-c5cf9ef6ca75)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp e4aa537c-eb9d-4dbb-ac87-fae46af42391)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 0f31f11f-c374-4640-b9a4-07bbdba8d354))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 998b7fa5-31a5-472e-9572-49d5226d6098))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 7c04618d-9115-4179-b234-a8faf854ea92))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp e4d2f565-25a0-48c6-be59-f4bf31ad2558))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp e502d1d5-04b0-4d4b-b5c3-8c52d09668e7))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp e67b9f8c-019b-4145-98a4-96545f6bb128))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 18b7e157-ae67-48ad-bd7c-9fef6fe45b22))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 5fc9acb6-6dbb-4598-825b-4b9e7c4c67c4))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp a53767ed-bb28-4f90-abe0-e0ea734812a4))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp f9403623-c00c-4b71-bc5c-d763ff009386))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(R1-Pad1)") (tstamp 109caac1-5036-4f23-9a66-f569d871501b))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(R1-Pad2)") (tstamp 19b0959e-a79b-43b2-a5ad-525ced7e9131))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b1bf)
    (at 127 91.977)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005e6a330d")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c24d6ac8-802d-4df3-a210-9cb1f693e865)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 88668202-3f0b-4d07-84d4-dcd790f57272)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 37f31dec-63fc-4634-a141-5dc5d2b60fe4)
    )
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 70fb572d-d5ec-41e7-9482-63d4578b4f47))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp eae0ab9f-65b2-44d3-aba7-873c3227fba7))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 609b9e1b-4e3b-42b7-ac76-a62ec4d0e7c7))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 7afa54c4-2181-41d3-81f7-39efc497ecae))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp b7867831-ef82-4f33-a926-59e5c1c09b91))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp e54e5e19-1deb-49a9-8629-617db8e434c0))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 009a4fb4-fcc0-4623-ae5d-c1bae3219583))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 2dc54bac-8640-4dd7-b8ed-3c7acb01a8ea))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 91c1eb0a-67ae-4ef0-95ce-d060a03a7313))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp cf386a39-fc62-49dd-8ec5-e044f6bd67ce))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(R2-Pad1)") (tstamp 25e5aa8e-2696-44a3-8d3c-c2c53f2923cf))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(R2-Pad2)") (tstamp 6bf05d19-ba3e-4ba6-8a6f-4e0bc45ea3b2))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b1d0)
    (at 131.41 89.027)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005e6a35e1")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cb614b23-9af3-4aec-bed8-c1374e001510)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 20cca02e-4c4d-4961-b6b4-b40a1731b220)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 5487601b-81d3-4c70-8f3d-cf9df9c63302)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 59ec3156-036e-4049-89db-91a9dd07095f))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp d39d813e-3e64-490c-ba5c-a64bb5ad6bd0))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 071522c0-d0ed-49b9-906e-6295f67fb0dc))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 2846428d-39de-4eae-8ce2-64955d56c493))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 4e315e69-0417-463a-8b7f-469a08d1496e))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 6a2b20ae-096c-4d9f-92f8-2087c865914f))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 597a11f2-5d2c-4a65-ac95-38ad106e1367))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 926001fd-2747-4639-8c0f-4fc46ff7218d))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp a29f8df0-3fae-4edf-8d9c-bd5a875b13e3))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp e3fc1e69-a11c-4c84-8952-fefb9372474e))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(R3-Pad1)") (tstamp 9cbf35b8-f4d3-42a3-bb16-04ffd03fd8fd))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(R3-Pad2)") (tstamp 4fa10683-33cd-4dcd-8acc-2415cd63c62a))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b1e1)
    (at 127 94.927)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005e6a37b2")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7b044939-8c4d-444f-b9e0-a15fcdeb5a86)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 576c6616-e95d-4f1e-8ead-dea30fcdc8c2)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 89e83c2e-e90a-4a50-b278-880bac0cfb49)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 5edcefbe-9766-42c8-9529-28d0ec865573))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp ec5c2062-3a41-4636-8803-069e60a1641a))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 22999e73-da32-43a5-9163-4b3a41614f25))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 6e68f0cd-800e-4167-9553-71fc59da1eeb))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 81a15393-727e-448b-a777-b18773023d89))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp a4f86a46-3bc8-4daa-9125-a63f297eb114))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 262f1ea9-0133-4b43-be36-456207ea857c))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 721d1be9-236e-470b-ba69-f1cc6c43faf9))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp a5e521b9-814e-4853-a5ac-f158785c6269))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp c1c799a0-3c93-493a-9ad7-8a0561bc69ee))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(R4-Pad1)") (tstamp 40b14a16-fb82-4b9d-89dd-55cd98abb5cc))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(R4-Pad2)") (tstamp 658dad07-97fd-466c-8b49-21892ac96ea4))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b1f2)
    (at 131.41 91.977)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0f7340")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0e8f7fc0-2ef2-4b90-9c15-8a3a601ee459)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b0906e10-2fbc-4309-a8b4-6fc4cd1a5490)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 0ce8d3ab-2662-4158-8a2a-18b782908fc5)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp c9667181-b3c7-4b01-b8b4-baa29a9aea63))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp ebd06df3-d52b-4cff-99a2-a771df6d3733))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 309b3bff-19c8-41ec-a84d-63399c649f46))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 8c0807a7-765b-4fa5-baaa-e09a2b610e6b))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp bd9595a1-04f3-4fda-8f1b-e65ad874edd3))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp be645d0f-8568-47a0-a152-e3ddd33563eb))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 29195ea4-8218-44a1-b4bf-466bee0082e4))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp cff34251-839c-4da9-a0ad-85d0fc4e32af))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp d0fb0864-e79b-4bdc-8e8e-eed0cabe6d56))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp d5b800ca-1ab6-4b66-b5f7-2dda5658b504))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(R5-Pad1)") (tstamp 173f6f06-e7d0-42ac-ab03-ce6b79b9eeee))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(R5-Pad2)") (tstamp 2e842263-c0ba-46fd-a760-6624d4c78278))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b203)
    (at 135.82 89.027)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0f734b")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 814763c2-92e5-4a2c-941c-9bbd073f6e87)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e65b62be-e01b-4688-a999-1d1be370c4ae)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 82be7aae-5d06-4178-8c3e-98760c41b054)
    )
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 20c315f4-1e4f-49aa-8d61-778a7389df7e))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 7a4ce4b3-518a-4819-b8b2-5127b3347c64))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 27d56953-c620-4d5b-9c1c-e48bc3d9684a))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 7e0a03ae-d054-4f76-a131-5c09b8dc1636))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 9193c41e-d425-447d-b95c-6986d66ea01c))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp d6fb27cf-362d-4568-967c-a5bf49d5931b))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp a6b7df29-bcf8-46a9-b623-7eaac47f5110))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp a9b3f6e4-7a6d-4ae8-ad28-3d8458e0ca1a))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp d9c6d5d2-0b49-49ba-a970-cd2c32f74c54))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp e1535036-5d36-405f-bb86-3819621c4f23))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(R6-Pad1)") (tstamp 6fd4442e-30b3-428b-9306-61418a63d311))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(R6-Pad2)") (tstamp 8d0c1d66-35ef-4a53-a28f-436a11b54f42))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b214)
    (at 127 97.877)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0f7356")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 644ae9fc-3c8e-4089-866e-a12bf371c3e9)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 41acfe41-fac7-432a-a7a3-946566e2d504)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 3a52f112-cb97-43db-aaeb-20afe27664d7)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 7f2301df-e4bc-479e-a681-cc59c9a2dbbb))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp a8447faf-e0a0-4c4a-ae53-4d4b28669151))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 101ef598-601d-400e-9ef6-d655fbb1dbfa))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 6781326c-6e0d-4753-8f28-0f5c687e01f9))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 7f52d787-caa3-4a92-b1b2-19d554dc29a4))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp c8029a4c-945d-42ca-871a-dd73ff50a1a3))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 65134029-dbd2-409a-85a8-13c2a33ff019))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 8087f566-a94d-4bbc-985b-e49ee7762296))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 98c78427-acd5-4f90-9ad6-9f61c4809aec))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp f4eb0267-179f-46c9-b516-9bfb06bac1ba))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R7-Pad1)") (tstamp 5b34a16c-5a14-4291-8242-ea6d6ac54372))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(R7-Pad2)") (tstamp c701ee8e-1214-4781-a973-17bef7b6e3eb))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b225)
    (at 131.41 94.927)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0f7361")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 240e5dac-6242-47a5-bbef-f76d11c715c0)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aa2ea573-3f20-43c1-aa99-1f9c6031a9aa)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp f40d350f-0d3e-4f8a-b004-d950f2f8f1ba)
    )
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 097edb1b-8998-4e70-b670-bba125982348))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 477311b9-8f81-40c8-9c55-fd87e287247a))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 6284122b-79c3-4e04-925e-3d32cc3ec077))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 67763d19-f622-4e1e-81e5-5b24da7c3f99))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 994b6220-4755-4d84-91b3-6122ac1c2c5e))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp ca5a4651-0d1d-441b-b17d-01518ef3b656))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 0e1ed1c5-7428-4dc7-b76e-49b2d5f8177d))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 14c51520-6d91-4098-a59a-5121f2a898f7))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 2d67a417-188f-4014-9282-000265d80009))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 84e5506c-143e-495f-9aa4-d3a71622f213))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(R8-Pad1)") (tstamp 099096e4-8c2a-4d84-a16f-06b4b6330e7a))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(R8-Pad2)") (tstamp a13ab237-8f8d-4e16-8c47-4440653b8534))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b236)
    (at 135.82 91.977)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0f7fe1")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6ec113ca-7d27-4b14-a180-1e5e2fd1c167)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e43dbe34-ed17-4e35-a5c7-2f1679b3c415)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 14769dc5-8525-4984-8b15-a734ee247efa)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 7cee474b-af8f-4832-b07a-c43c1ab0b464))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 853ee787-6e2c-4f32-bc75-6c17337dd3d5))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 275aa44a-b61f-489f-9e2a-819a0fe0d1eb))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 57c0c267-8bf9-4cc7-b734-d71a239ac313))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 5ca4be1c-537e-4a4a-b344-d0c8ffde8546))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 6c67e4f6-9d04-4539-b356-b76e915ce848))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 19c56563-5fe3-442a-885b-418dbc2421eb))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 21ae9c3a-7138-444e-be38-56a4842ab594))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 9cb12cc8-7f1a-4a01-9256-c119f11a8a02))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp c7e7067c-5f5e-48d8-ab59-df26f9b35863))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(R9-Pad1)") (tstamp cfa5c16e-7859-460d-a0b8-cea7d7ea629c))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(R9-Pad2)") (tstamp b447dbb1-d38e-4a15-93cb-12c25382ea53))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b247)
    (at 140.23 89.027)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0f7fec")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b1c649b1-f44d-46c7-9dea-818e75a1b87e)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f3628265-0155-43e2-a467-c40ff783e265)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 6595b9c7-02ee-4647-bde5-6b566e35163e)
    )
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 789ca812-3e0c-4a3f-97bc-a916dd9bce80))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp e4c6fdbb-fdc7-4ad4-a516-240d84cdc120))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp a17904b9-135e-4dae-ae20-401c7787de72))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp cdfb07af-801b-44ba-8c30-d021a6ad3039))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp e6b860cc-cb76-4220-acfb-68f1eb348bfa))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp f202141e-c20d-4cac-b016-06a44f2ecce8))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 16a9ae8c-3ad2-439b-8efe-377c994670c7))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 770ad51a-7219-4633-b24a-bd20feb0a6c5))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp b7199d9b-bebb-4100-9ad3-c2bd31e21d65))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp db36f6e3-e72a-487f-bda9-88cc84536f62))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(R10-Pad1)") (tstamp 5114c7bf-b955-49f3-a0a8-4b954c81bde0))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(R10-Pad2)") (tstamp 182b2d54-931d-49d6-9f39-60a752623e36))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b258)
    (at 131.41 97.877)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0f7ff7")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dde51ae5-b215-445e-92bb-4a12ec410531)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7599133e-c681-4202-85d9-c20dac196c64)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 4fb21471-41be-4be8-9687-66030f97befc)
    )
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 85b7594c-358f-454b-b2ad-dd0b1d67ed76))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp c5eb1e4c-ce83-470e-8f32-e20ff1f886a3))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 01e9b6e7-adf9-4ee7-9447-a588630ee4a2))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 16bd6381-8ac0-4bf2-9dce-ecc20c724b8d))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 4f66b314-0f62-4fb6-8c3c-f9c6a75cd3ec))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp a5cd8da1-8f7f-4f80-bb23-0317de562222))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 0755aee5-bc01-4cb5-b830-583289df50a3))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 4a21e717-d46d-4d9e-8b98-af4ecb02d3ec))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 60dcd1fe-7079-4cb8-b509-04558ccf5097))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp ec31c074-17b2-48e1-ab01-071acad3fa04))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(R11-Pad1)") (tstamp 7d928d56-093a-4ca8-aed1-414b7e703b45))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(R11-Pad2)") (tstamp ca87f11b-5f48-4b57-8535-68d3ec2fe5a9))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b269)
    (at 135.82 94.927)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0f8002")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d3c11c8f-a73d-4211-934b-a6da255728ad)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 639c0e59-e95c-4114-bccd-2e7277505454)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 8ca3e20d-bcc7-4c5e-9deb-562dfed9fecb)
    )
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 13c0ff76-ed71-4cd9-abb0-92c376825d5d))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp a27eb049-c992-4f11-a026-1e6a8d9d0160))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 8412992d-8754-44de-9e08-115cec1a3eff))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp c332fa55-4168-4f55-88a5-f82c7c21040b))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp df32840e-2912-4088-b54c-9a85f64c0265))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp ffd175d1-912a-4224-be1e-a8198680f46b))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 03caada9-9e22-4e2d-9035-b15433dfbb17))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 0ff508fd-18da-4ab7-9844-3c8a28c2587e))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 1f3003e6-dce5-420f-906b-3f1e92b67249))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 378af8b4-af3d-46e7-89ae-deff12ca9067))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(R12-Pad1)") (tstamp b96fe6ac-3535-4455-ab88-ed77f5e46d6e))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(R12-Pad2)") (tstamp 68877d35-b796-44db-9124-b8e744e7412e))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b27a)
    (at 140.23 91.977)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0fa280")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8e06ba1f-e3ba-4eb9-a10e-887dffd566d6)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 40165eda-4ba6-4565-9bb4-b9df6dbb08da)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 7e023245-2c2b-4e2b-bfb9-5d35176e88f2)
    )
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp aca4de92-9c41-4c2b-9afa-540d02dafa1c))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp d7269d2a-b8c0-422d-8f25-f79ea31bf75e))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 1e8701fc-ad24-40ea-846a-e3db538d6077))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 25d545dc-8f50-4573-922c-35ef5a2a3a19))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp c43663ee-9a0d-4f27-a292-89ba89964065))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp c830e3bc-dc64-4f65-8f47-3b106bae2807))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 4780a290-d25c-4459-9579-eba3f7678762))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp babeabf2-f3b0-4ed5-8d9e-0215947e6cf3))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp df68c26a-03b5-4466-aecf-ba34b7dce6b7))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp e8c50f1b-c316-4110-9cce-5c24c65a1eaa))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(R13-Pad1)") (tstamp c25a772d-af9c-4ebc-96f6-0966738c13a8))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(R13-Pad2)") (tstamp d5641ac9-9be7-46bf-90b3-6c83d852b5ba))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b28b)
    (at 144.64 89.027)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0fa28b")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b88717bd-086f-46cd-9d3f-0396009d0996)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 61fe293f-6808-4b7f-9340-9aaac7054a97)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 2f215f15-3d52-4c91-93e6-3ea03a95622f)
    )
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 1d9cdadc-9036-4a95-b6db-fa7b3b74c869))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 6bfe5804-2ef9-4c65-b2a7-f01e4014370a))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 24f7628d-681d-4f0e-8409-40a129e929d9))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 3a7648d8-121a-4921-9b92-9b35b76ce39b))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 3e903008-0276-4a73-8edb-5d9dfde6297c))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 75ffc65c-7132-4411-9f2a-ae0c73d79338))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 0217dfc4-fc13-4699-99ad-d9948522648e))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 8da933a9-35f8-42e6-8504-d1bab7264306))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp bd5408e4-362d-4e43-9d39-78fb99eb52c8))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp c0eca5ed-bc5e-4618-9bcd-80945bea41ed))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(R14-Pad1)") (tstamp 8c6a821f-8e19-48f3-8f44-9b340f7689bc))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(R14-Pad2)") (tstamp 6475547d-3216-45a4-a15c-48314f1dd0f9))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b29c)
    (at 135.82 97.877)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0fa296")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6441b183-b8f2-458f-a23d-60e2b1f66dd6)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 31e08896-1992-4725-96d9-9d2728bca7a3)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp b5352a33-563a-4ffe-a231-2e68fb54afa3)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 5528bcad-2950-4673-90eb-c37e6952c475))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 7edc9030-db7b-43ac-a1b3-b87eeacb4c2d))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 08a7c925-7fae-4530-b0c9-120e185cb318))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 4a4ec8d9-3d72-4952-83d4-808f65849a2b))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp cbd8faed-e1f8-4406-87c8-58b2c504a5d4))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp f2c93195-af12-4d3e-acdf-bdd0ff675c24))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 2d6db888-4e40-41c8-b701-07170fc894bc))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 66043bca-a260-4915-9fce-8a51d324c687))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 7bbf981c-a063-4e30-8911-e4228e1c0743))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 852dabbf-de45-4470-8176-59d37a754407))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(R15-Pad1)") (tstamp 003c2200-0632-4808-a662-8ddd5d30c768))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(R15-Pad2)") (tstamp 240e07e1-770b-4b27-894f-29fd601c924d))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b2ad)
    (at 140.23 94.927)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0fa2a1")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9bb20359-0f8b-45bc-9d38-6626ed3a939d)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2d210a96-f81f-42a9-8bf4-1b43c11086f3)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp e857610b-4434-4144-b04e-43c1ebdc5ceb)
    )
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 1a1ab354-5f85-45f9-938c-9f6c4c8c3ea2))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 7aed3a71-054b-4aaa-9c0a-030523c32827))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 1bf544e3-5940-4576-9291-2464e95c0ee2))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 3aaee4c4-dbf7-49a5-a620-9465d8cc3ae7))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 42713045-fffd-4b2d-ae1e-7232d705fb12))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp c0515cd2-cdaa-467e-8354-0f6eadfa35c9))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 666713b0-70f4-42df-8761-f65bc212d03b))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 6c2e273e-743c-4f1e-a647-4171f8122550))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 7dc880bc-e7eb-4cce-8d8c-0b65a9dd788e))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 9157f4ae-0244-4ff1-9f73-3cb4cbb5f280))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(R16-Pad1)") (tstamp 97fe9c60-586f-4895-8504-4d3729f5f81a))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(R16-Pad2)") (tstamp bdc7face-9f7c-4701-80bb-4cc144448db1))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b2be)
    (at 144.64 91.977)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0fcaa9")
    (attr smd)
    (fp_text reference "R17" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fd470e95-4861-44fe-b1e4-6d8a7c66e144)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8174b4de-74b1-48db-ab8e-c8432251095b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 704d6d51-bb34-4cbf-83d8-841e208048d8)
    )
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 1831fb37-1c5d-42c4-b898-151be6fca9dc))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 9340c285-5767-42d5-8b6d-63fe2a40ddf3))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 0b21a65d-d20b-411e-920a-75c343ac5136))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 0f22151c-f260-4674-b486-4710a2c42a55))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 3cd1bda0-18db-417d-b581-a0c50623df68))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp fe8d9267-7834-48d6-a191-c8724b2ee78d))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 0eaa98f0-9565-4637-ace3-42a5231b07f7))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 181abe7a-f941-42b6-bd46-aaa3131f90fb))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp c41b3c8b-634e-435a-b582-96b83bbd4032))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp ce83728b-bebd-48c2-8734-b6a50d837931))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(R17-Pad1)") (tstamp 03c52831-5dc5-43c5-a442-8d23643b46fb))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(R17-Pad2)") (tstamp d57dcfee-5058-4fc2-a68b-05f9a48f685b))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b2cf)
    (at 140.23 97.877)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0fcab4")
    (attr smd)
    (fp_text reference "R18" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1e1b062d-fad0-427c-a622-c5b8a80b5268)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d8603679-3e7b-4337-8dbc-1827f5f54d8a)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 30f15357-ce1d-48b9-93dc-7d9b1b2aa048)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 54365317-1355-4216-bb75-829375abc4ec))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp a3e4f0ae-9f86-49e9-b386-ed8b42e012fb))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 5fc27c35-3e1c-4f96-817c-93b5570858a6))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp a690fc6c-55d9-47e6-b533-faa4b67e20f3))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp c144caa5-b0d4-4cef-840a-d4ad178a2102))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp efeac2a2-7682-4dc7-83ee-f6f1b23da506))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 2e642b3e-a476-4c54-9a52-dcea955640cd))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 5038e144-5119-49db-b6cf-f7c345f1cf03))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 87371631-aa02-498a-998a-09bdb74784c1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp ac264c30-3e9a-4be2-b97a-9949b68bd497))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(R18-Pad1)") (tstamp 6a45789b-3855-401f-8139-3c734f7f52f9))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(R18-Pad2)") (tstamp 6c9b793c-e74d-4754-a2c0-901e73b26f1c))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b2e0)
    (at 144.64 94.927)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0fcabf")
    (attr smd)
    (fp_text reference "R19" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a955fc7-39d9-4c75-9a69-676ca8c0b9b2)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e8314017-7be6-4011-9179-37449a29b311)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp e10b5627-3247-4c86-b9f6-ef474ca11543)
    )
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp c022004a-c968-410e-b59e-fbab0e561e9d))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp f4f99e3d-7269-4f6a-a759-16ad2a258779))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 47baf4b1-0938-497d-88f9-671136aa8be7))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 4fb02e58-160a-4a39-9f22-d0c75e82ee72))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 77ed3941-d133-4aef-a9af-5a39322d14eb))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp e615f7aa-337e-474d-9615-2ad82b1c44ca))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 10109f84-4940-47f8-8640-91f185ac9bc1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 55e740a3-0735-4744-896e-2bf5437093b9))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 71c31975-2c45-4d18-a25a-18e07a55d11e))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 746ba970-8279-4e7b-aed3-f28687777c21))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(R19-Pad1)") (tstamp 44d8279a-9cd1-4db6-856f-0363131605fc))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(R19-Pad2)") (tstamp ef8fe2ac-6a7f-4682-9418-b801a1b10a3b))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f53b2f1)
    (at 144.64 97.877)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f0fcaca")
    (attr smd)
    (fp_text reference "R20" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a05d7640-f2f6-4ba7-8c51-5a4af431fc13)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 13abf99d-5265-4779-8973-e94370fd18ff)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp a7520ad3-0f8b-4788-92d4-8ffb277041e6)
    )
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 23bb2798-d93a-4696-a962-c305c4298a0c))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 78cbdd6c-4878-4cc5-9a58-0e506478e37d))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 6e105729-aba0-497c-a99e-c32d2b3ddb6d))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 983c426c-24e0-4c65-ab69-1f1824adc5c6))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp c1d83899-e380-49f9-a87d-8e78bc089ebf))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp e9bb29b2-2bb9-4ea2-acd9-2bb3ca677a12))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 46918595-4a45-48e8-84c0-961b4db7f35f))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 94c158d1-8503-4553-b511-bf42f506c2a8))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 9ccf03e8-755a-4cd9-96fc-30e1d08fa253))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp a795f1ba-cdd5-4cc5-9a52-08586e982934))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(R20-Pad1)") (tstamp da469d11-a8a4-414b-9449-d151eeaf4853))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(R20-Pad2)") (tstamp 62c076a3-d618-44a2-9042-9a08b3576787))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/../../data/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 124.46 85.09) (end 124.46 101.6) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-00005f53b433))
  (gr_line (start 124.46 101.6) (end 147.32 101.6) (layer "Edge.Cuts") (width 0.1) (tstamp 0cc45b5b-96b3-4284-9cae-a3a9e324a916))
  (gr_line (start 147.193 85.09) (end 124.46 85.09) (layer "Edge.Cuts") (width 0.1) (tstamp f1447ad6-651c-45be-a2d6-33bddf672c2c))
  (gr_line (start 147.32 101.6) (end 147.193 85.09) (layer "Edge.Cuts") (width 0.1) (tstamp f6c644f4-3036-41a6-9e14-2c08c079c6cd))

)
