(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "GND")
  (net 3 "Net-(C2-Pad1)")

  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0) (tstamp 0bd14c6f-3c3f-4efc-a261-5f4613e96239)
    (at 121 104 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "Archivo: ../Circuit/1_SCH_2_diff_PCBs.kicad_sch")
    (property "Sheetname" "Filter circuit")
    (path "/77d5b6d2-5833-4084-b955-4eb239724e2d/e5e3dd91-4c50-4c56-a840-8fe41b627763")
    (attr through_hole)
    (fp_text reference "C1" (at 1.25 -2.05 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 88dacc8d-a7ca-4c2a-beb9-744d15254d83)
    )
    (fp_text value "100nF" (at 1.25 2.05 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 90f1f628-84ea-43f5-bb3e-ccda863b7d94)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab")
      (effects (font (size 0.6 0.6) (thickness 0.09)))
      (tstamp 0ed2abff-bb01-45c3-9084-5fae61afb694)
    )
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer "F.SilkS") (width 0.12) (tstamp 1b931a0a-edf2-405e-96c8-6cb4e50ffd37))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer "F.SilkS") (width 0.12) (tstamp 4dba0471-72ae-4807-8b8b-0598284717a5))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 1391027a-cabc-44db-a8f2-3f901f7c1215))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 58f1f87c-779b-48e7-943d-ff7116a11710))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 8665f630-ea40-4043-b884-041f62f4134d))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp d034edf2-6503-4dab-9af8-41b3e2e22042))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer "F.Fab") (width 0.1) (tstamp 57b19317-c1f2-4c13-b51f-471afde6803b))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer "F.Fab") (width 0.1) (tstamp 6c8a9400-c64c-4686-a114-8632fee4e10a))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer "F.Fab") (width 0.1) (tstamp 7d673d17-359e-46fc-967f-1e5cdbb49239))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer "F.Fab") (width 0.1) (tstamp 8a37347a-daee-4bb8-9929-12e3fda55388))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pintype "passive") (tstamp a95f43ac-6307-461a-94bf-e8e8bd6a4569))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive") (tstamp 35b8ab2f-48ec-4be0-8b7c-ec4bbcf8e347))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B) (tstamp 2c438cd8-5935-4d8f-8fd9-e408374bcf20)
    (at 145 104 -90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Sheetfile" "Archivo: ../Circuit/1_SCH_2_diff_PCBs.kicad_sch")
    (property "Sheetname" "Filter circuit")
    (path "/77d5b6d2-5833-4084-b955-4eb239724e2d/1a0b04d9-cdf4-4256-b39a-932f9cef60f9")
    (attr through_hole)
    (fp_text reference "J2" (at 1.27 -4.12 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d6473a8d-4571-40f0-89db-9ca51e2b4a54)
    )
    (fp_text value "Out" (at 1.27 4.08 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6220522b-6e3b-4e8d-aa89-8b6e940087c2)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.22 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a46b5a73-47cc-4fa7-a8d8-2306365e8cc3)
    )
    (fp_line (start 3.92 2.99) (end 3.92 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 00667517-a4f6-4c08-8cc1-cc5a6d9e04cb))
    (fp_line (start 1.74 -2.43) (end 3.34 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 025c9da3-7b52-4804-b69f-8a1f6701bf57))
    (fp_line (start 0 1.99) (end 0.25 1.46) (layer "F.SilkS") (width 0.12) (tstamp 09e24dc3-b8d7-44a9-84ee-81d749b46c3a))
    (fp_line (start 3.34 -2.43) (end 3.34 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 0dc5856f-6e28-4cae-94f7-68173520be51))
    (fp_line (start 0 2.99) (end 0 1.99) (layer "F.SilkS") (width 0.12) (tstamp 13520e72-07ec-4567-8199-f81cd825fff4))
    (fp_line (start -0.8 -3.03) (end -0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 2633df2f-8918-424e-8d1e-81b41f484509))
    (fp_line (start 3.92 -3.03) (end -1.38 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 3b69a44e-22f3-4cf1-a5a3-8b013580606a))
    (fp_line (start 2.29 2.99) (end 2.29 1.99) (layer "F.SilkS") (width 0.12) (tstamp 4810a047-234f-491f-9fd3-4f70eca423f6))
    (fp_line (start 0.8 -2.43) (end 0.8 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 4a18fcdf-a616-4194-8ac3-015847ad4ec3))
    (fp_line (start 0.25 2.99) (end 0.25 1.99) (layer "F.SilkS") (width 0.12) (tstamp 607cb585-eacc-475b-a5f8-15abab95a2ce))
    (fp_line (start -1.38 -3.03) (end -1.38 2.99) (layer "F.SilkS") (width 0.12) (tstamp 61e43608-4af3-4b80-82ec-b509f882b2dc))
    (fp_line (start -1.38 2.99) (end 3.92 2.99) (layer "F.SilkS") (width 0.12) (tstamp 653d2557-1965-4ada-80f0-30bc0280d601))
    (fp_line (start 0.25 1.46) (end 2.29 1.46) (layer "F.SilkS") (width 0.12) (tstamp 74234bbd-ddc7-4014-b01a-a4be1c1ca824))
    (fp_line (start 2.54 1.99) (end 2.54 2.99) (layer "F.SilkS") (width 0.12) (tstamp 85590d9f-718b-4774-b42c-a6e2f28eec2a))
    (fp_line (start -0.8 -2.43) (end 0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 907984e0-5997-455e-84f9-fe8737a6ab31))
    (fp_line (start -1.67 -2) (end -1.67 2) (layer "F.SilkS") (width 0.12) (tstamp 9d757430-800d-4163-93d7-70ea356ffe57))
    (fp_line (start 1.74 -3.03) (end 1.74 -2.43) (layer "F.SilkS") (width 0.12) (tstamp abfe29e6-4af2-4918-9fa6-d8015412fffa))
    (fp_line (start 0 1.99) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp c972631c-1c55-4dea-9ddf-13489659ca8a))
    (fp_line (start 2.29 1.46) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp d1e878a6-a85e-4298-8818-df0e4df5994a))
    (fp_line (start -1.77 3.38) (end 4.31 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 438f2092-9ba7-42ae-a9a0-dca1f7f51502))
    (fp_line (start -1.77 -3.42) (end -1.77 3.38) (layer "F.CrtYd") (width 0.05) (tstamp bc897384-e9df-4052-912c-abf2ae5edef1))
    (fp_line (start 4.31 -3.42) (end -1.77 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp cf8815bf-97aa-4c07-b7a0-7b1c64cf42e9))
    (fp_line (start 4.31 3.38) (end 4.31 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp f3e3a73f-a1e5-4b2d-a367-6a4aa1fdd84c))
    (fp_line (start 3.81 -2.92) (end -1.27 -2.92) (layer "F.Fab") (width 0.1) (tstamp 0e1880f8-a0a3-4b3d-8783-91a25850238b))
    (fp_line (start 3.81 2.88) (end 3.81 -2.92) (layer "F.Fab") (width 0.1) (tstamp 4447c868-4127-4f9c-8d13-c440bae8d1a1))
    (fp_line (start -1.27 -0.5) (end -0.562893 0) (layer "F.Fab") (width 0.1) (tstamp 480b08ab-add4-4470-b216-37cf48ccd821))
    (fp_line (start -1.27 -2.92) (end -1.27 2.88) (layer "F.Fab") (width 0.1) (tstamp c0b30ef4-3640-4bd2-881a-2c110ce81cce))
    (fp_line (start -1.27 2.88) (end 3.81 2.88) (layer "F.Fab") (width 0.1) (tstamp c97b7863-8511-4942-9ee9-48df3c2a1a1b))
    (fp_line (start -0.562893 0) (end -1.27 0.5) (layer "F.Fab") (width 0.1) (tstamp fef757a3-fabf-4aa3-bbc7-96824c1132ef))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 3 "Net-(C2-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp b43a2641-40ed-41f4-858f-8c8d38d7ed02))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive") (tstamp 0a5dee59-d8f1-47c7-8d47-43c4d4ef8102))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B) (tstamp 4c86ca82-73e7-400c-9af2-af1348234920)
    (at 114 107 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Sheetfile" "Archivo: ../Circuit/1_SCH_2_diff_PCBs.kicad_sch")
    (property "Sheetname" "Filter circuit")
    (path "/77d5b6d2-5833-4084-b955-4eb239724e2d/c00eaf45-c1bf-4fcf-9758-e056d0bcad77")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -4.12 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 93f4dfba-3e9f-4b51-97c3-71478f23dd5e)
    )
    (fp_text value "In" (at 1.27 4.08 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e5dfd1ef-3ee6-47ca-883d-028ed85b841c)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.22 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19da462b-5fcb-4676-8885-cd83437905a7)
    )
    (fp_line (start 1.74 -2.43) (end 3.34 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 0d6ca354-6422-4b45-840a-0e54e94b382d))
    (fp_line (start 3.34 -2.43) (end 3.34 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 0ee47609-2305-4896-9cd1-a6fa3c090b12))
    (fp_line (start 0.25 2.99) (end 0.25 1.99) (layer "F.SilkS") (width 0.12) (tstamp 2e0696c0-7675-4d48-9cee-4bc80e058eac))
    (fp_line (start 0.25 1.46) (end 2.29 1.46) (layer "F.SilkS") (width 0.12) (tstamp 39b609c9-f9b6-4bd2-a0b4-68c92eb3b351))
    (fp_line (start -1.38 2.99) (end 3.92 2.99) (layer "F.SilkS") (width 0.12) (tstamp 4b192523-d107-4255-ac1c-4f678ad76abc))
    (fp_line (start 1.74 -3.03) (end 1.74 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 5078858e-db5f-4149-a4e6-bff70147a4bd))
    (fp_line (start -0.8 -3.03) (end -0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 55adf4e3-6020-4a7d-a37f-678d7fa379f7))
    (fp_line (start 0 2.99) (end 0 1.99) (layer "F.SilkS") (width 0.12) (tstamp 696cede1-e968-461f-ae76-7edad59b9586))
    (fp_line (start 0 1.99) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp 7ba7fd63-8512-42ba-b583-a862e01804d4))
    (fp_line (start 3.92 2.99) (end 3.92 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 7dedb5d4-28a4-4b64-ba5f-e7588a7cb657))
    (fp_line (start -1.67 -2) (end -1.67 2) (layer "F.SilkS") (width 0.12) (tstamp 8d5a68bc-ebc7-4933-b010-0eebba2129bd))
    (fp_line (start 2.54 1.99) (end 2.54 2.99) (layer "F.SilkS") (width 0.12) (tstamp 9b5144bb-a472-4e1a-b4fe-1962e97efc8c))
    (fp_line (start 0 1.99) (end 0.25 1.46) (layer "F.SilkS") (width 0.12) (tstamp aeb09480-2856-42ae-b201-855143c7ff74))
    (fp_line (start -1.38 -3.03) (end -1.38 2.99) (layer "F.SilkS") (width 0.12) (tstamp b8dba3f6-7e48-4c94-bc80-2357703fa456))
    (fp_line (start 0.8 -2.43) (end 0.8 -3.03) (layer "F.SilkS") (width 0.12) (tstamp c58934c6-9a04-4f82-97e2-108c99a834e0))
    (fp_line (start 2.29 1.46) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp c66569c7-6ffc-4210-ad4a-c6f318b254e4))
    (fp_line (start 3.92 -3.03) (end -1.38 -3.03) (layer "F.SilkS") (width 0.12) (tstamp e708ca9f-8470-4477-a2b5-7403707a00d8))
    (fp_line (start -0.8 -2.43) (end 0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp e9e9b65c-66c2-4233-b166-1d4657909f58))
    (fp_line (start 2.29 2.99) (end 2.29 1.99) (layer "F.SilkS") (width 0.12) (tstamp f1020dc1-dcc5-4400-bce4-7f5a84bb97a3))
    (fp_line (start -1.77 3.38) (end 4.31 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 14434f46-56da-4f4b-a1fc-546ca88d2f92))
    (fp_line (start 4.31 -3.42) (end -1.77 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp b2c96aa7-2ae7-4bbb-a175-fc2ca51617c5))
    (fp_line (start -1.77 -3.42) (end -1.77 3.38) (layer "F.CrtYd") (width 0.05) (tstamp c62c0b17-43a7-4c9c-b606-7db375b2e7cb))
    (fp_line (start 4.31 3.38) (end 4.31 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp cc175f48-6959-4328-80b6-babe14748baf))
    (fp_line (start -0.562893 0) (end -1.27 0.5) (layer "F.Fab") (width 0.1) (tstamp 06b01859-bdc7-4f49-945c-da96c00dff6f))
    (fp_line (start 3.81 2.88) (end 3.81 -2.92) (layer "F.Fab") (width 0.1) (tstamp 17600569-2ed6-405d-9acb-ef78b21e28b8))
    (fp_line (start -1.27 2.88) (end 3.81 2.88) (layer "F.Fab") (width 0.1) (tstamp 1d7949b6-9227-48d4-8f80-97b9fc8141fa))
    (fp_line (start -1.27 -2.92) (end -1.27 2.88) (layer "F.Fab") (width 0.1) (tstamp b2b981c7-2605-47bc-a261-86b0e51df524))
    (fp_line (start 3.81 -2.92) (end -1.27 -2.92) (layer "F.Fab") (width 0.1) (tstamp be695824-2e83-4a03-a25d-72407410ff72))
    (fp_line (start -1.27 -0.5) (end -0.562893 0) (layer "F.Fab") (width 0.1) (tstamp f1857287-b033-4999-b3fb-bcc966f0193b))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp a4b36159-b451-4538-924d-0e2740718222))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 5daa9dd3-44c1-4aae-9544-ab4418adb818))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp 9bdda352-924d-49b6-95aa-675326de7791)
    (at 133 106 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Archivo: ../Circuit/1_SCH_2_diff_PCBs.kicad_sch")
    (property "Sheetname" "Filter circuit")
    (path "/77d5b6d2-5833-4084-b955-4eb239724e2d/5ff51348-3b0c-4051-ac3f-8bbe52a23b46")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -2.37) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7ce280cf-8c94-41a6-ab9c-2517ccfb0c71)
    )
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e52aa082-1872-4bce-8742-b0a87c32518f)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1af447e6-7b2f-4183-b9b0-ee963151ab15)
    )
    (fp_line (start 7.08 1.37) (end 7.08 1.04) (layer "F.SilkS") (width 0.12) (tstamp 12d75bfe-a516-4b83-a151-8f5b17f254ee))
    (fp_line (start 0.54 1.37) (end 7.08 1.37) (layer "F.SilkS") (width 0.12) (tstamp 1f202aff-705b-4eb0-9ce2-c3d28456b93b))
    (fp_line (start 0.54 -1.37) (end 7.08 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 47a4c57d-5e0a-4f17-a4a0-30c0d09c8947))
    (fp_line (start 0.54 1.04) (end 0.54 1.37) (layer "F.SilkS") (width 0.12) (tstamp 4ae5ff02-0dd6-4483-aecf-120f3f7e2fba))
    (fp_line (start 0.54 -1.04) (end 0.54 -1.37) (layer "F.SilkS") (width 0.12) (tstamp e7cd4de3-9fa4-43d4-9c6a-467dd748b7c0))
    (fp_line (start 7.08 -1.37) (end 7.08 -1.04) (layer "F.SilkS") (width 0.12) (tstamp fe17ba14-3c0a-4f05-a203-422d14481be5))
    (fp_line (start 8.67 1.5) (end 8.67 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 318318cd-23ad-4f65-b363-7e05d4e8f676))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 353cf4fb-691f-401e-96ae-51d3345cfda6))
    (fp_line (start -1.05 1.5) (end 8.67 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 3ad98a63-5f21-4250-ae0d-f947137955df))
    (fp_line (start 8.67 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp e6151624-e9da-4f61-a9ae-6d508f77bd34))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer "F.Fab") (width 0.1) (tstamp 30b2f8a2-e55e-487e-b213-26c6c7f0c018))
    (fp_line (start 0 0) (end 0.66 0) (layer "F.Fab") (width 0.1) (tstamp 312fd1d0-b052-4a55-ad0b-110ea836377f))
    (fp_line (start 7.62 0) (end 6.96 0) (layer "F.Fab") (width 0.1) (tstamp 654ca737-c7d1-4d55-82a3-7cb61a71fa28))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer "F.Fab") (width 0.1) (tstamp 8224fa90-e332-4dab-a37c-d5c6dc55bde8))
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer "F.Fab") (width 0.1) (tstamp b0067d5d-bcc9-4261-9510-cf96e9a20c2a))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer "F.Fab") (width 0.1) (tstamp eed007ce-1efc-4801-9c5b-64f2c9a802aa))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pintype "passive") (tstamp 5ff29e5f-dffe-4c85-b692-fcc98737cc57))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pintype "passive") (tstamp 06d6c70e-9d31-489e-b8d0-865d3c321239))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0) (tstamp c76f41ff-f0d9-44cc-ad92-c75f5f0ef9ca)
    (at 137 104 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "Archivo: ../Circuit/1_SCH_2_diff_PCBs.kicad_sch")
    (property "Sheetname" "Filter circuit")
    (path "/77d5b6d2-5833-4084-b955-4eb239724e2d/121f51f7-01c0-4925-9aad-c45a8d3be012")
    (attr through_hole)
    (fp_text reference "C2" (at 1.25 -2.05 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19ec8aeb-ef44-457e-a9f9-a01495a14f96)
    )
    (fp_text value "100nF" (at 1.25 2.05 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bbe86728-e377-4410-80c7-244205872ffd)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab")
      (effects (font (size 0.6 0.6) (thickness 0.09)))
      (tstamp d569b74c-8905-4b07-b48e-1e22f77c9f03)
    )
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer "F.SilkS") (width 0.12) (tstamp 90220b73-179a-4d9d-8e53-a7fc7aa4d590))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer "F.SilkS") (width 0.12) (tstamp be2b0215-3268-4672-bc02-a95e8ccde404))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 33948e30-82aa-4a1c-9471-fc81d7120635))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 3c49cc04-c6a1-4c9e-a6a3-c5ee78a114eb))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp a7a2d0df-0e81-4749-879c-071052a7899e))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer "F.CrtYd") (width 0.05) (tstamp c3192c48-1490-44a5-a4e5-835264acce77))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer "F.Fab") (width 0.1) (tstamp 41eac295-134e-420c-abf6-966fcdee88f4))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer "F.Fab") (width 0.1) (tstamp 6d1e0b11-b0bc-467c-9d16-c3c0e87f421f))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer "F.Fab") (width 0.1) (tstamp 9ee9b2bb-7b47-4607-8cd7-59615ab86c91))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer "F.Fab") (width 0.1) (tstamp c00c8b4b-7daf-4e4a-ad53-9e1ec3b2844c))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pintype "passive") (tstamp 9595ef38-b28c-4a87-aaf1-8084b2aec0c3))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive") (tstamp 87b74f10-9784-4677-8201-4cfa0ed504ab))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_circle (center 130 105) (end 110 110) (layer "Edge.Cuts") (width 0.1) (fill none) (tstamp e462d35a-1b64-4730-8086-92c7107a0baa))

  (segment (start 120.54 104.46) (end 121 104) (width 1) (layer "B.Cu") (net 1) (tstamp 0ce2754e-1fd1-4b5c-b87d-4d58e55e2d02))
  (segment (start 114 104.46) (end 120.54 104.46) (width 1) (layer "B.Cu") (net 1) (tstamp 472c35a5-add2-4522-ade1-587e0d34d6da))
  (segment (start 121 104) (end 123.38 104) (width 1) (layer "B.Cu") (net 1) (tstamp 487f5dc4-9e5c-4c15-a593-729f32fa92a1))
  (segment (start 123.38 104) (end 125.38 106) (width 1) (layer "B.Cu") (net 1) (tstamp 9d3c1405-1198-4b10-8a03-8f6a4294cc89))
  (segment (start 144.96 106.5) (end 145 106.54) (width 0.25) (layer "B.Cu") (net 2) (tstamp 2de69564-895b-40d4-9edc-46b9e4a34510))
  (segment (start 137 106.5) (end 144.96 106.5) (width 1) (layer "B.Cu") (net 2) (tstamp 2e434583-6316-42ac-b917-1b8164f5567d))
  (segment (start 114 107) (end 114.5 106.5) (width 0.25) (layer "B.Cu") (net 2) (tstamp 53752922-57f5-41a3-b38f-848d01e5041c))
  (segment (start 114.5 106.5) (end 121 106.5) (width 1) (layer "B.Cu") (net 2) (tstamp 62bada69-db32-4f82-bb1b-d66298b8fd73))
  (segment (start 121 106.5) (end 124 109) (width 1) (layer "B.Cu") (net 2) (tstamp f56f0793-a432-40c7-a8e2-39ec5b8b1577))
  (arc (start 134 109) (mid 135.75 108.05) (end 137 106.5) (width 1) (layer "B.Cu") (net 2) (tstamp 28a0a968-e154-4150-8e46-2ab9b35a8bc6))
  (arc (start 124 109) (mid 129 110) (end 134 109) (width 1) (layer "B.Cu") (net 2) (tstamp f3daa44c-85f6-41b4-9b72-d16d2e7eba4e))
  (segment (start 133 106) (end 135 104) (width 1) (layer "B.Cu") (net 3) (tstamp 55f4c34f-0871-4c3f-ba66-4f40ad15708d))
  (segment (start 135 104) (end 136 104) (width 1) (layer "B.Cu") (net 3) (tstamp 934c9b71-7393-4342-a6ad-81b3c67039a0))
  (segment (start 136 104) (end 137 104) (width 0.25) (layer "B.Cu") (net 3) (tstamp 98e3ff23-5637-4255-a8b3-f1c1996ccbf1))
  (segment (start 136 104) (end 145 104) (width 1) (layer "B.Cu") (net 3) (tstamp a8ce6898-5db4-453a-b657-a905fb9eaf4f))

)
