(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal "GND.Cu")
    (2 "In2.Cu" signal "Signal1.Cu")
    (3 "In3.Cu" signal "Signal2.Cu")
    (4 "In4.Cu" signal "Power.Cu")
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "unconnected-(C1-Pad1)")
  (net 2 "unconnected-(C1-Pad2)")
  (net 3 "unconnected-(C2-Pad1)")
  (net 4 "unconnected-(C2-Pad2)")
  (net 5 "unconnected-(C3-Pad1)")
  (net 6 "unconnected-(C3-Pad2)")
  (net 7 "unconnected-(C4-Pad1)")
  (net 8 "unconnected-(C4-Pad2)")
  (net 9 "unconnected-(R1-Pad1)")
  (net 10 "unconnected-(R1-Pad2)")
  (net 11 "unconnected-(R2-Pad1)")
  (net 12 "unconnected-(R2-Pad2)")
  (net 13 "unconnected-(R3-Pad1)")
  (net 14 "unconnected-(R3-Pad2)")
  (net 15 "unconnected-(R4-Pad1)")
  (net 16 "unconnected-(R4-Pad2)")
  (net 17 "unconnected-(R5-Pad1)")
  (net 18 "unconnected-(R5-Pad2)")
  (net 19 "unconnected-(R6-Pad1)")
  (net 20 "unconnected-(R6-Pad2)")
  (net 21 "unconnected-(R7-Pad1)")
  (net 22 "unconnected-(R7-Pad2)")
  (net 23 "unconnected-(R8-Pad1)")
  (net 24 "unconnected-(R8-Pad2)")
  (net 25 "unconnected-(R9-Pad1)")
  (net 26 "unconnected-(R9-Pad2)")
  (net 27 "unconnected-(R10-Pad1)")
  (net 28 "unconnected-(R10-Pad2)")

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 10c6ccde-e3f7-488e-93a4-a587e57b1e59)
    (at 122.94 73.55)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005e6a39eb")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp adfd1820-34f1-4c10-adb8-0face24c5834)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7e264f41-c112-4a39-8312-31cbfcef6632)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 09344646-ade6-4057-9273-bf72ab8b0cd1)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "F.SilkS") (width 0.12) (tstamp 1d1d74df-c84e-4e5f-b691-a458fb119f89))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "F.SilkS") (width 0.12) (tstamp f0a80b54-cc08-47d9-a6a5-69eddf0e8d9a))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 109c05a6-ec7e-4943-8ea1-e434d69772cb))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 3711cbd4-4966-46f8-abbc-5fcf8331d66c))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 6138546e-9c69-42b2-b417-8b2d867889bc))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp ec126fd4-b87a-4363-a654-d406af6823c7))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 005b2eb8-f0ea-413e-a5fa-9c392cf04a7f))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 2dec1402-5383-4c5e-b5a0-abbe74c1544d))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 541eaa70-75ee-46e7-8933-735deaad5ae6))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 9e62fef3-8c7e-4a86-afaa-014b0688b11c))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 17 "unconnected-(R5-Pad1)") (pintype "passive") (tstamp 06d294a9-d73e-4aa2-bb05-5c4b6f6c1452))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 18 "unconnected-(R5-Pad2)") (pintype "passive") (tstamp 0162c89f-4eb0-4150-b703-f80f9f60a402))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 5eb27656-4bf4-4d8c-920a-845a766dfd14)
    (at 127.35 70.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Config" "DNF")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005e6a3ca0")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d0f41196-cdf4-44f2-911f-7dab20a2c688)
    )
    (fp_text value "4K7" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2d6d1bb6-f7d2-4033-972c-2bae1080d303)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 4e7280b8-b008-4500-8ae6-a10bf8a97f58)
    )
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "F.SilkS") (width 0.12) (tstamp c070a764-8cb6-47e9-a672-55f5b881f5eb))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "F.SilkS") (width 0.12) (tstamp f8bf75cb-fdc6-4396-94d2-401af63a86b7))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 09e1ad3a-2668-44da-ba03-f2d133f36750))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 3d6ba4e4-745a-41f5-856f-6d967695ff58))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp d6381922-6645-40b3-b5db-65aa97f8f0bb))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp fc0dc778-5b23-48b9-82ce-48001cedeaa8))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 24bc74b9-d56e-4671-9517-30a6106f284b))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 3ce7458f-c8d0-4503-ac54-6d26e6262b26))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 5e842b06-4232-45e3-9fc5-af3cee7c6481))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 8aa7b8d6-4a88-450a-88bd-1d4f020b5d93))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 19 "unconnected-(R6-Pad1)") (pintype "passive") (tstamp 057dc35f-2259-4112-a9f0-d90f464e61ee))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 20 "unconnected-(R6-Pad2)") (pintype "passive") (tstamp 91fdc5db-b93e-4eac-a908-8419870167ea))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 65f337f4-f719-4c3c-b4fd-ef2dc452ed8d)
    (at 127.35 73.55)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005e6a4181")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b4799665-eed2-4adf-8458-08294aff8a9e)
    )
    (fp_text value "4.7K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f821e04a-7412-470f-ad5a-b4b4fb104a84)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 1db7fabc-7408-4509-97fb-3273b614afb6)
    )
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "F.SilkS") (width 0.12) (tstamp 22b5fdff-08b7-4c5c-bf7f-222e593b0de7))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "F.SilkS") (width 0.12) (tstamp f87d979c-8260-460d-b847-6674eafd9114))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 053a5b56-aa01-4c1b-b28f-119e050fb49d))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp a3b6e705-5ed7-43ab-bd62-ba96e88a8b91))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp dcea6f8a-fb9e-44d0-8d06-485c2991c21f))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp ee7dbb20-dbd4-48eb-bdce-e54a03f5501e))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 2e90688a-4c99-46d9-936e-b914a99b3021))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 670c45af-dc7f-478e-aa8e-525b1052bc2e))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 8df9353b-f8d5-410b-866a-18db5bb96724))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp d5270f20-2ff6-405a-87c8-fe80e24d5d25))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 23 "unconnected-(R8-Pad1)") (pintype "passive") (tstamp a9ae9e73-fc2c-4597-ad62-d2ad9081c41d))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 24 "unconnected-(R8-Pad2)") (pintype "passive") (tstamp 327918aa-781d-4712-936f-f4ca46870e5d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 697e1d3f-68aa-458c-aa42-f1a27950ece4)
    (at 122.94 70.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005e6a35e1")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 50cdc6ba-e1b2-43cd-97fe-aa0d14435450)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 591df35c-9d8d-4839-8f1a-0bbda813f214)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp f59d1e73-baa7-4ddc-a96e-9b7f4064eadb)
    )
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "F.SilkS") (width 0.12) (tstamp 0d74315e-9c10-4e33-afda-5b525a25ec59))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "F.SilkS") (width 0.12) (tstamp b2f633a1-2463-455b-bbe1-784d84774cc3))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 1e3c08b4-1d2e-45a3-a17d-6d8af630ba3d))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 2df8254c-0627-424d-a757-678d0eee3398))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 78975baa-7517-48f5-8204-eb9689a16187))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp f1952d85-22b7-4c70-b85d-402cbfa5c974))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 44504073-3e68-4ed0-918e-292b89104cf3))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 46056e19-edad-4066-a055-d2fca2945f9b))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp b76ca284-109f-40a1-a86b-380bd51c3509))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp c3f2b2a7-2397-486b-aa1c-a3c879e3d1c0))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 13 "unconnected-(R3-Pad1)") (pintype "passive") (tstamp 5ad6aceb-308a-43dc-878d-aade01de2242))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 14 "unconnected-(R3-Pad2)") (pintype "passive") (tstamp f78a287d-a79f-4c5b-aefc-7f099c1b945e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 73e5ca63-baa7-4c0b-af4a-a7086e7ca678)
    (at 125.6 81.93)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005e6a62cc")
    (attr smd exclude_from_pos_files)
    (fp_text reference "C1" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 68ef850a-5737-4335-a688-4149f31c1b00)
    )
    (fp_text value "10nF" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 38d66b48-6d8f-40c7-839b-7e0ba4bc63f4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 99bbc07a-7a17-4bb1-9ce8-c823850febe7)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 1ed3625d-0a48-4c2a-be8d-069437a5e9d1))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "F.SilkS") (width 0.12) (tstamp e021e73a-a5f1-4dcd-9154-0d17b91210c5))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 4415afb8-d918-4139-9117-42cf6d0d5890))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 4cc6f6dd-d8fa-4c56-b9c0-1e4f0d8f9059))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 83f47374-0b5f-46c7-ae4c-c15c22ad4be4))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp f6437080-4555-4795-a6a2-5fc6131616f1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 697874f1-84c5-4d09-a9dd-c781222108e1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 6d0e4f1b-053f-4421-a725-6374cb8820ea))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp cb4a53b9-d006-4289-b21c-38e35c902ef8))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp eabac3d1-ebe2-4753-b0e2-faad04baa0c3))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "unconnected-(C1-Pad1)") (pintype "passive") (tstamp 9765e3ab-4c6d-45a5-9ba1-e209c0cc912f))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "unconnected-(C1-Pad2)") (pintype "passive") (tstamp 759041bf-17d3-44db-97c3-099f7db57bd9))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 7c3fa7de-7cec-475c-b3c4-b8b3a4fd6a43)
    (at 140.09 75.02)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Config" "DNC")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005e6a3f38")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a8958f10-bee0-4128-912a-b58828d001a7)
    )
    (fp_text value "4700" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5101158f-f5e3-487b-9767-2c236120275c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp a240124a-df70-4557-994e-55c6b254e8c6)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "F.SilkS") (width 0.12) (tstamp 18b35024-1661-4424-8ef7-b52cb6d4bfbb))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "F.SilkS") (width 0.12) (tstamp 8c3050f6-ae89-4ca1-8603-4dcea001387c))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 0731aab1-5059-40df-b09e-eaec16eaa6b6))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 3cef635d-6a3b-4fae-9244-4978ba24a800))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp dd2a502c-2fa2-494e-8085-ce272cf48c12))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp f782ca6e-6d7e-492a-8bd4-84f34dfd9d24))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 17acc6c2-5c91-4710-b48f-2b307e435d22))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 1aa47be2-38dd-48d9-8eda-0e26f57e29a5))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 6931e30e-7490-46e5-bf0e-f3c9e35dea4a))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 7eca0036-aab5-42a7-8138-067a77a7543d))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 21 "unconnected-(R7-Pad1)") (pintype "passive") (tstamp ff6e10ae-361c-4a53-ab9d-2528c5e60826))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 22 "unconnected-(R7-Pad2)") (pintype "passive") (tstamp 7a791a71-b88d-4bb6-a775-6e5e56948996))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 904674d0-912e-46a4-b0a8-1c2bf5731712)
    (at 132.69 87.07)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (path "/00000000-0000-0000-0000-00005e6a6a34")
    (attr smd exclude_from_bom)
    (fp_text reference "C3" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2f155aa0-0eda-497e-b5ba-ec85057d28d5)
    )
    (fp_text value "0.01uF" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c5a076b7-3542-4981-be3f-ddf8bfdfcddb)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp c79488ec-dfa0-4a22-93a6-d42edbcfa103)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "F.SilkS") (width 0.12) (tstamp 7e6e6836-6d74-49c2-b5d3-ae1c370d68b0))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 98fe983c-20d8-46f6-af01-566fb3bddca1))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 2ad331c0-ce55-4c67-b196-5a1b5592c3ce))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 53064894-7b0a-4187-81fc-ad26341ac676))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 743843e8-8548-449b-8b29-67c42b0bf2f0))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer "F.CrtYd") (width 0.05) (tstamp ee33e7da-35d1-4105-80d4-9b95e472604c))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 83001755-e596-42b8-882f-40dfde6e40de))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 84a85adb-9567-4551-8772-df5204d55283))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp a9c002ee-1978-4853-8135-c6e6b360db8e))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp f557d1b3-7f5e-493e-8427-39ed94940559))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "unconnected-(C3-Pad1)") (pintype "passive") (tstamp 87bb00bf-f022-4efe-8541-4712f87119cd))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "unconnected-(C3-Pad2)") (pintype "passive") (tstamp 5f61a445-4f2b-4a8f-a486-e49700d1a002))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp b10f2fbe-42b4-4acb-975b-4b3992e082fd)
    (at 112.17 71.49)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005e6a330d")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b6c737dd-fe54-4245-bfed-6925e0649bbe)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 87d9e290-abd3-4efd-90d8-7b3a632a2598)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 44bf2782-f880-43bd-8bdd-1e09ab31ff85)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "F.SilkS") (width 0.12) (tstamp 63985a3f-7206-453a-85c4-f7397c382c34))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "F.SilkS") (width 0.12) (tstamp 64cbf894-a296-43b2-9979-344f0777161e))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 3338d3cc-b03d-4567-a65d-7ee7494ccd28))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 5116d564-80fa-4de2-ad1e-6b5ce859bcb3))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 9a9d18fb-3f6b-4c05-8bb7-615c061b528a))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp d169fed8-51a7-4a06-870d-270b27d81369))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 3d02cf97-e78e-41bb-86a1-1ffaf0dbbbad))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 5a86518d-45d1-4c41-a964-5443c0b7889c))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 72770055-0f56-44d4-9a2b-038d5c77bc5a))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp a19cf67a-b7ff-4f23-9cca-6ef2ec3fd2ba))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 11 "unconnected-(R2-Pad1)") (pintype "passive") (tstamp b7c74ff7-cfbf-4321-ba4e-5d0b4a38de5b))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 12 "unconnected-(R2-Pad2)") (pintype "passive") (tstamp ae940271-f3db-4a2a-bb61-c1e9f7aede71))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp bb06a184-2900-4d34-8d2a-0700e8826e20)
    (at 125.47 86.79)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005e6a6854")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 05c0c31d-b1e3-459f-885a-890ae7c48287)
    )
    (fp_text value "10n" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d0a58aee-4b15-4462-8943-ac86d44e815a)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp f34ed1a6-1588-41e1-a568-2463bc3dcfb5)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "F.SilkS") (width 0.12) (tstamp 7f3a7701-a530-4e0a-b8a9-d43c8b4c090d))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "F.SilkS") (width 0.12) (tstamp a43c8e04-34eb-4aed-ae42-37add43164f6))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 43d6aab9-189f-4811-bddb-bbf6077ac91d))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 9838b40a-1f7c-4684-be46-526f2dae915e))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer "F.CrtYd") (width 0.05) (tstamp ef3a6dde-464a-4bd2-bf9a-96ca48c37c3e))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer "F.CrtYd") (width 0.05) (tstamp f69337fd-860d-488e-a5d5-c945a1204b07))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 6fe527be-253c-4832-b65a-0cd9fdda627b))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 86dcfb90-395f-4188-8f45-7b0814e1e0f2))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 9c780c38-90ba-42a1-812a-932119a675a3))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp c8805354-85be-48f8-bcdf-6bb5f6213e84))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "unconnected-(C2-Pad1)") (pintype "passive") (tstamp c9750c8a-ac89-4e8f-9795-c8e2c7330487))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "unconnected-(C2-Pad2)") (pintype "passive") (tstamp cbf5b3ca-010e-4457-9a87-9ebafd707ee6))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp bcf70ad8-b2cf-4659-9dba-ae981c57fc30)
    (at 131.56 70.38)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005e6a491a")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8ba72740-29c2-4d82-bcfb-8609ab90364d)
    )
    (fp_text value "4K7" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5a7fb40a-5104-4f05-9030-8ee92a95c313)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp dd6b32d5-c842-4a9e-b760-6f3d44fd2bd4)
    )
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 8a9920da-d431-4082-9098-5b5f43c871a4))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225) (layer "F.SilkS") (width 0.12) (tstamp ed036bb4-c036-407c-9c7d-fa17ca0ab6a9))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 0da3f196-0029-4742-87c5-92022ac64634))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 4f543056-350f-4c97-8941-03485df811b2))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp ad8367e5-bafc-4de1-b13c-65f791276d04))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp f0272e95-8ce4-45c0-9a6a-6f2126dc2505))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 1a8697ec-a798-49d3-832e-07ebd7cab4c6))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 8a40723d-f4a6-4b47-82dd-60ae6a486698))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp a4e97c6d-ef1f-46ca-8bdc-2dda559ca229))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp d1307e1c-b67a-41bc-b9ad-571789c0d30c))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "unconnected-(R10-Pad1)") (pintype "passive") (tstamp 6c75c6cf-6da5-451f-8c75-2d5c594d85c2))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "unconnected-(R10-Pad2)") (pintype "passive") (tstamp 6a31403f-9c0b-41a1-a5ca-947e88e1cdab))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp bdaf95c6-eb65-4fb0-93d0-a7f5ac5d630b)
    (at 118.53 70.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005e6a2873")
    (attr smd exclude_from_pos_files)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7b7a031d-d8b7-4e41-afa1-18b0d6307e7d)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a40c626-0eab-43ce-87a9-b06fcf718ec6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 371bbd2c-bf48-455f-bff6-f71ec82c8aef)
    )
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "F.SilkS") (width 0.12) (tstamp 767d0f12-eb08-4fb1-954b-70d4d072a5e9))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "F.SilkS") (width 0.12) (tstamp e40dee47-c286-45ab-8b1b-c5b7262ae503))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 53670963-fac9-41a1-b24d-4218f9d06244))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 91efe98a-1972-4da9-bc8a-ac3948582357))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp c57f0f4f-2588-498f-85e8-1ed9bdfaf77a))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp d7470248-38e8-43a0-a442-0b87ea60add7))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 304b0812-c95d-4f4d-a890-34002d5174c1))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 33f7da41-8a63-4245-9ce3-ba1b0af1a23e))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp c0bab759-ed78-47c1-ab5e-87bb99a1b665))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp dbdcb7a1-b665-4aca-aa8d-76bd49d18430))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "unconnected-(R1-Pad1)") (pintype "passive") (tstamp 6470018d-22bd-48a4-b671-45989b34e2da))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 10 "unconnected-(R1-Pad2)") (pintype "passive") (tstamp 4908086b-f6b0-46b3-9074-fb30a2d46b93))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp ca09d825-ef11-4bdd-b071-10473f4cad52)
    (at 113.27 81.76)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (path "/00000000-0000-0000-0000-00005e6a448b")
    (attr smd exclude_from_bom)
    (fp_text reference "R9" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fa5e215c-4f80-43c2-a296-ce6af82d0e86)
    )
    (fp_text value "4K7" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 65c9635c-ebf0-4b25-b675-22d555a271e6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp d5a41b86-267f-4aaa-96ef-2e00e726d324)
    )
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 07eeabce-07bd-430f-b026-8c4468b4df80))
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp c057768d-471e-4f4c-96e8-a2267c972d46))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 5e4e1bbd-5ec9-4716-a897-d412477b1dbf))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 621f6561-16bd-407c-b8a0-dc8d42e65d21))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 87863e30-acd7-424e-8151-3f2ac6f5c0a7))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 94e4f8d9-8142-416f-b6f2-9d2466a98cfa))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 753ffd4d-b055-48a8-aba4-807a3773251a))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 80e8d936-1f70-4e1b-b180-a3d5ce3c7cf5))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp a90c1cc4-e3f9-4206-ae2e-84f7ab934c13))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp f7352de3-43f3-41b4-b514-24244232f623))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "unconnected-(R9-Pad1)") (pintype "passive") (tstamp c78cc41c-3674-443b-a37b-d317452eea4e))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "unconnected-(R9-Pad2)") (pintype "passive") (tstamp b9608f84-4100-4c25-b2b1-7205de528c4a))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp cddcf2f4-0a8b-415a-ab7a-e65a49927e0a)
    (at 111.98 76.35)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005e6a37b2")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 65380499-c54a-4e19-a0f7-e08e104b7f89)
    )
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e9fb5b74-ab26-4fcd-8605-593d3ae31836)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp a55bbdbe-4549-4f15-8ac0-febab1ef0cdc)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "F.SilkS") (width 0.12) (tstamp 2d1c6138-9bb8-4ce1-8681-bc7f97022cd8))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "F.SilkS") (width 0.12) (tstamp 3a99b559-7a6f-432f-97b3-00ef913ada08))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 637ecfdc-cedf-46aa-a068-61b67a3c3700))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 9f8b21f5-bf90-4b74-9c63-16470aaf00d9))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp db6424b0-5307-49d7-98bc-6641f74db1ea))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp ddac947e-aae0-4fc9-a680-835548f88888))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 804255f2-0981-41be-b7f8-4a5138adfcba))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 85f1f330-8a78-4196-825c-7bd06e4a54c0))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp c030cfef-76a9-48af-8c38-353a57ab85ba))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp c5c2e585-49ec-4342-b519-00f90c54fc53))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 15 "unconnected-(R4-Pad1)") (pintype "passive") (tstamp d0737d11-4d80-4ae7-91da-b297ebcf0619))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 16 "unconnected-(R4-Pad2)") (pintype "passive") (tstamp 0f6f5b96-267e-4849-a7b7-5f9a7e0df777))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp d37aabb7-0c1a-4aca-860a-fbb49a798ba7)
    (at 132.63 82.37)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "kibom-test-marked.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005e6a6cb6")
    (attr smd exclude_from_bom)
    (fp_text reference "C4" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 96ba7f7f-70c4-406f-949f-396905a89bf4)
    )
    (fp_text value "0.01uf" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c88db542-712d-4dca-9936-ffc02a194b77)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp e9356123-baac-455a-8bc3-af9a59d705da)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "F.SilkS") (width 0.12) (tstamp 37e3f524-5be8-4f36-a5fb-f926e3253087))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 3e977e59-1705-440c-a289-9f1e1dbbc39f))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 42771a07-a490-4cab-b5fd-51970a638ce3))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 53d71433-b3d2-48b5-9d32-51a089bb9d9f))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 71a77cb3-93d7-4ed5-b68f-3aff618fe5ae))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp f1136c3c-bc48-4d62-9100-e5b97a67e83c))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 0d8ab1ca-6397-4a56-8d2e-4c68a9c99f8c))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 606d46c0-3674-4655-8ddd-918ad21a6c1d))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 6aa00581-de10-4fca-a54c-44a7a001aa9a))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 7948bc9f-9ac0-441c-b281-96028ad389d5))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "unconnected-(C4-Pad1)") (pintype "passive") (tstamp 28301ee6-d562-476e-bf02-3f119f590a1d))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "unconnected-(C4-Pad2)") (pintype "passive") (tstamp 92bd1ef9-24b4-4d51-890f-3193c3157591))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

)
