(kicad_pcb (version 20171130) (host pcbnew 5.1.6+dfsg1-1)

  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 44)
    (zones 0)
    (modules 4)
    (nets 4)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (1 GND.Cu signal)
    (2 Signal1.Cu signal)
    (3 Signal2.Cu signal)
    (4 Power.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 /Power/VCC)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Power/VCC)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
  )

  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE) (tstamp 5CA72801)
    (at 164.775001 80.505001 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /5CA71704/5CA745A6)
    (attr smd)
    (fp_text reference C1 (at 0 -1.17 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 0 1.17 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.93 0.47) (end -0.93 0.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.93 -0.47) (end 0.93 0.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.93 -0.47) (end 0.93 -0.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.93 0.47) (end -0.93 -0.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.04)))
    )
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /Power/VCC))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KIPRJMOD}/3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE) (tstamp 5CA72810)
    (at 170.18 80.020001 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /5CA75BC1/5CA76352)
    (attr smd)
    (fp_text reference C2 (at 0 -1.17 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 0 1.17 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.93 0.47) (end -0.93 -0.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.93 -0.47) (end 0.93 -0.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.93 -0.47) (end 0.93 0.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.93 0.47) (end -0.93 0.47) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.04)))
    )
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KIPRJMOD}/3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_JWPF_B02B-JWPF-SK-R_1x02_P2.00mm_Vertical (layer F.Cu) (tedit 5B772B89) (tstamp 5CA7282D)
    (at 154.94 80.01)
    (descr "JST JWPF series connector, B02B-JWPF-SK-R (http://www.jst-mfg.com/product/pdf/eng/eJWPF1.pdf), generated with kicad-footprint-generator")
    (tags "connector JST JWPF side entry")
    (path /5CA71704/5CA714F2)
    (fp_text reference P1 (at -1.35 -3.7) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X02 (at -1.35 5.7) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 -1.15) (end -0.375 -1.9) (layer F.Fab) (width 0.1))
    (fp_line (start 0.375 -1.9) (end 0 -1.15) (layer F.Fab) (width 0.1))
    (fp_line (start -0.375 -1.9) (end 0.375 -1.9) (layer F.Fab) (width 0.1))
    (fp_line (start -5.75 -2.85) (end -4.25 -2.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.75 -1.35) (end -5.75 -2.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.81 -1.61) (end 2.81 3.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.51 4.61) (end 1.81 4.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.51 -2.61) (end -5.51 4.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.61) (end -5.51 -2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.7 -1.5) (end 2.7 3.5) (layer F.Fab) (width 0.1))
    (fp_line (start -5.4 4.5) (end 1.7 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -5.4 -2.5) (end -5.4 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -2.5) (end -5.4 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.2 -3) (end -5.9 -3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.2 5) (end 3.2 -3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.9 5) (end 3.2 5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.9 -3) (end -5.9 5) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 1.7 -1.5) (end 1.7 -2.5) (angle 90) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.7 3.5) (end 2.7 3.5) (angle 90) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.81 -1.61) (end 1.81 -2.61) (angle 90) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.81 3.61) (end 2.81 3.61) (angle 90) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at -4.7 1 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole roundrect (at 0 0) (size 2 1.3) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.192308)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2) (size 2 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Power/VCC))
    (pad "" np_thru_hole circle (at -1.5 4.05) (size 1.15 1.15) (drill 1.15) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/3D/B02B-JWPF-SK-R.step
      (offset (xyz -3.2 -4.5 -8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD) (tstamp 5CA7283C)
    (at 167.64 83.82)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (path /5CA75BC1/5CA75C86)
    (attr smd)
    (fp_text reference R1 (at 0 -1.17) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.17) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.93 0.47) (end -0.93 0.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.93 -0.47) (end 0.93 0.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.93 -0.47) (end 0.93 -0.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.93 0.47) (end -0.93 -0.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.04)))
    )
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /Power/VCC))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KIPRJMOD}/3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text "Text in Cmts.User" (at 149 93) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "Text in Dwgs.User" (at 149 68) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_line (start 187.96 69.85) (end 142.24 69.85) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 187.96 91.44) (end 187.96 69.85) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 142.24 91.44) (end 187.96 91.44) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 142.24 69.85) (end 142.24 91.44) (layer Edge.Cuts) (width 0.12))

  (segment (start 160 73) (end 180 73) (width 0.25) (layer GND.Cu) (net 2))
  (segment (start 180 73) (end 180 88) (width 0.25) (layer GND.Cu) (net 2))
  (segment (start 180 88) (end 160 88) (width 0.25) (layer Signal1.Cu) (net 1))
  (segment (start 161 87) (end 179 87) (width 0.25) (layer Signal2.Cu) (net 2))
  (segment (start 179 87) (end 179 74) (width 0.25) (layer Signal2.Cu) (net 2))
  (segment (start 161 74) (end 179 74) (width 0.25) (layer Power.Cu) (net 1))
  (segment (start 179 74) (end 160.995 74) (width 0.25) (layer Signal2.Cu) (net 2))
  (segment (start 160.995 74) (end 161 74.005) (width 0.25) (layer Signal2.Cu) (net 2))
  (segment (start 180 88) (end 160.009 88) (width 0.25) (layer GND.Cu) (net 2))
  (segment (start 160.009 88) (end 160 87.991) (width 0.25) (layer GND.Cu) (net 2))
  (segment (start 167.155 83.37) (end 165.1 81.315) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 167.155 83.82) (end 167.155 83.37) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 165.1 81.315) (end 164.775001 80.990001) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 164.775001 80.990001) (end 157.769999 80.990001) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 156.75 82.01) (end 154.94 82.01) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 157.769999 80.990001) (end 156.75 82.01) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 159.9226 82.01) (end 160 82.0874) (width 0.25) (layer Signal1.Cu) (net 1))
  (segment (start 154.94 82.01) (end 159.9226 82.01) (width 0.25) (layer Signal1.Cu) (net 1))
  (segment (start 160 82.0874) (end 160 73) (width 0.25) (layer Signal1.Cu) (net 1))
  (segment (start 160 88) (end 160 82.0874) (width 0.25) (layer Signal1.Cu) (net 1))
  (segment (start 180 88) (end 180 73.0152) (width 0.25) (layer Signal1.Cu) (net 1))
  (segment (start 179.9848 73) (end 160 73) (width 0.25) (layer Signal1.Cu) (net 1))
  (segment (start 180 73.0152) (end 179.9848 73) (width 0.25) (layer Signal1.Cu) (net 1))
  (segment (start 160.9786 82.01) (end 161 82.0314) (width 0.25) (layer Power.Cu) (net 1))
  (segment (start 154.94 82.01) (end 160.9786 82.01) (width 0.25) (layer Power.Cu) (net 1))
  (segment (start 161 82.0314) (end 161 87) (width 0.25) (layer Power.Cu) (net 1))
  (segment (start 161 74) (end 161 82.0314) (width 0.25) (layer Power.Cu) (net 1))
  (segment (start 161 87) (end 178.9888 87) (width 0.25) (layer Power.Cu) (net 1))
  (segment (start 179 86.9888) (end 179 74) (width 0.25) (layer Power.Cu) (net 1))
  (segment (start 178.9888 87) (end 179 86.9888) (width 0.25) (layer Power.Cu) (net 1))
  (segment (start 164.765 80.01) (end 164.775001 80.020001) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 154.94 80.01) (end 164.765 80.01) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 165.260001 79.535001) (end 170.18 79.535001) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 164.775001 80.020001) (end 165.260001 79.535001) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 154.9708 79.9792) (end 154.94 80.01) (width 0.25) (layer GND.Cu) (net 2))
  (segment (start 160 79.9792) (end 154.9708 79.9792) (width 0.25) (layer GND.Cu) (net 2))
  (segment (start 160 87.991) (end 160 79.9792) (width 0.25) (layer GND.Cu) (net 2))
  (segment (start 160 79.9792) (end 160 73) (width 0.25) (layer GND.Cu) (net 2))
  (segment (start 160.9852 80.01) (end 161 80.0248) (width 0.25) (layer Signal2.Cu) (net 2))
  (segment (start 154.94 80.01) (end 160.9852 80.01) (width 0.25) (layer Signal2.Cu) (net 2))
  (segment (start 161 80.0248) (end 161 87) (width 0.25) (layer Signal2.Cu) (net 2))
  (segment (start 161 74.005) (end 161 80.0248) (width 0.25) (layer Signal2.Cu) (net 2))
  (segment (start 170.18 81.765) (end 168.125 83.82) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 170.18 80.505001) (end 170.18 81.765) (width 0.25) (layer F.Cu) (net 3))

)
