(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (title_block
    (title "Filter A + B")
  )

  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin -116.5 -78.5)
    (grid_origin -116.5 -78.5)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Board_0-Net-(C3-Pad1)")
  (net 2 "Board_0-Net-(C3-Pad2)")
  (net 3 "Board_0-Net-(C4-Pad2)")
  (net 4 "Board_0-Net-(J3-Pad2)")

  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B) (tstamp 0387508d-75b4-4ac3-b140-5dc963bac983)
    (at 47 19 -90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Sheetfile" "Archivo: KiKit_1.kicad_sch")
    (property "Sheetname" "")
    (path "/481f07fd-30d9-4dbd-89ce-664c027703b8")
    (attr through_hole)
    (fp_text reference "J4" (at 1.27 -4.12 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f94d6ed1-deae-449f-83a7-867b09f109a1)
    )
    (fp_text value "OUT" (at 1.27 4.08 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 596c1697-7593-48b0-8e3c-279aef167710)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.22 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f965e49c-6bbd-4dcc-9abc-07d092a87bb7)
    )
    (fp_line (start 2.54 1.99) (end 2.54 2.99) (layer "F.SilkS") (width 0.12) (tstamp 051bf5ce-a679-4cf6-8dfe-908d3b0b52be))
    (fp_line (start 0 1.99) (end 0.25 1.46) (layer "F.SilkS") (width 0.12) (tstamp 0e321b66-0192-4402-8455-0d1a8c9f71a6))
    (fp_line (start 0.8 -2.43) (end 0.8 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 18e928c9-5b85-424d-ab78-e21399ec1413))
    (fp_line (start 3.92 2.99) (end 3.92 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 1c04578f-d1d8-4fad-8df6-e10db47b74ce))
    (fp_line (start -1.38 -3.03) (end -1.38 2.99) (layer "F.SilkS") (width 0.12) (tstamp 1f52da53-8659-4522-abee-5dea38c98e39))
    (fp_line (start 0 2.99) (end 0 1.99) (layer "F.SilkS") (width 0.12) (tstamp 2307f317-8382-4810-8e7e-3bb399e7dbfb))
    (fp_line (start -0.8 -2.43) (end 0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 4a751e82-a693-46bf-9cf2-6db13833a7d0))
    (fp_line (start 3.92 -3.03) (end -1.38 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 56366d14-05de-42ee-835b-51708c2c1c89))
    (fp_line (start -1.67 -2) (end -1.67 2) (layer "F.SilkS") (width 0.12) (tstamp 5f9f9e96-b983-49b5-b621-4a43659f78bc))
    (fp_line (start 0.25 2.99) (end 0.25 1.99) (layer "F.SilkS") (width 0.12) (tstamp 6d5e4c63-db61-4927-a637-fab1dd53c9c0))
    (fp_line (start 3.34 -2.43) (end 3.34 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 71437d2d-f8a8-4a1d-ada9-0cedeefd0646))
    (fp_line (start -0.8 -3.03) (end -0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 8510e7db-c516-4758-928c-cc9ca08fbc64))
    (fp_line (start 0 1.99) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp 8fcfc105-6b64-419f-8f47-14820a15429b))
    (fp_line (start 0.25 1.46) (end 2.29 1.46) (layer "F.SilkS") (width 0.12) (tstamp 971ed272-e3c7-490e-9684-1b590c9fece3))
    (fp_line (start 2.29 2.99) (end 2.29 1.99) (layer "F.SilkS") (width 0.12) (tstamp a8855859-6bfc-4f4d-baa2-ae9773a7cc3d))
    (fp_line (start 1.74 -3.03) (end 1.74 -2.43) (layer "F.SilkS") (width 0.12) (tstamp bbd44b86-6a45-45a4-9b50-ec044e7f0ec6))
    (fp_line (start 2.29 1.46) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp c61120ef-b6d7-40bc-b181-572f634857af))
    (fp_line (start 1.74 -2.43) (end 3.34 -2.43) (layer "F.SilkS") (width 0.12) (tstamp d3df24c5-5eb3-4f9f-8f44-09573d670085))
    (fp_line (start -1.38 2.99) (end 3.92 2.99) (layer "F.SilkS") (width 0.12) (tstamp ff8fa6b5-9703-4af4-b1b3-1af66897b49a))
    (fp_line (start -1.77 -3.42) (end -1.77 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 11701b81-8f62-402a-a03d-2a1bb6eb26aa))
    (fp_line (start -1.77 3.38) (end 4.31 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 2371ced2-334e-414f-9cce-8c41fdc915e7))
    (fp_line (start 4.31 -3.42) (end -1.77 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp 67cea9c5-e2b7-40b2-8271-ee4f31bf8084))
    (fp_line (start 4.31 3.38) (end 4.31 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp 6bf4b3fc-7a7d-4f4c-acce-67652b891a02))
    (fp_line (start 3.81 -2.92) (end -1.27 -2.92) (layer "F.Fab") (width 0.1) (tstamp 08ac69bf-56ed-4a70-83a8-4ec3a2fcc572))
    (fp_line (start -1.27 -2.92) (end -1.27 2.88) (layer "F.Fab") (width 0.1) (tstamp 27863d4f-654c-4623-bd16-19efb1c8a7b0))
    (fp_line (start -0.562893 0) (end -1.27 0.5) (layer "F.Fab") (width 0.1) (tstamp 58fcc653-5730-4aa9-8076-19ea6680cc04))
    (fp_line (start 3.81 2.88) (end 3.81 -2.92) (layer "F.Fab") (width 0.1) (tstamp 63bbbbc8-d6d0-4dc1-9cfb-472128b87fa6))
    (fp_line (start -1.27 -0.5) (end -0.562893 0) (layer "F.Fab") (width 0.1) (tstamp d57a6031-e186-4a15-912b-f4bdf8e7236d))
    (fp_line (start -1.27 2.88) (end 3.81 2.88) (layer "F.Fab") (width 0.1) (tstamp dd2bd571-c02f-45f2-b159-28f11921b1fb))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 3 "Board_0-Net-(C4-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp cb98ad3c-5b78-465a-a094-22e5f5cc5fae))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 4 "Board_0-Net-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp c2f38838-42cd-4aac-b74c-657612448cd4))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp 42df2089-29bc-4e47-a7ae-895bf0597e44)
    (at 33 24.81 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Archivo: KiKit_1.kicad_sch")
    (property "Sheetname" "")
    (path "/ae25c042-bdd9-416c-bac6-25fce33a9083")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 -2.37 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 00e2f1a7-6b4f-46cb-9575-cc1561856d0f)
    )
    (fp_text value "1k" (at 3.81 2.37 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 522babba-7b1c-4c85-9281-2da54f5af050)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8fb9c67d-5166-46f4-9b80-a3ced1d44404)
    )
    (fp_line (start 7.08 1.37) (end 7.08 1.04) (layer "F.SilkS") (width 0.12) (tstamp 1212309a-1231-48d9-97f6-a53b56c5eee0))
    (fp_line (start 7.08 -1.37) (end 7.08 -1.04) (layer "F.SilkS") (width 0.12) (tstamp 168baa62-b624-4e55-95c6-3fa1450c9e5c))
    (fp_line (start 0.54 -1.37) (end 7.08 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 7a6e3285-57da-41b1-a8b3-f3bbd9be1172))
    (fp_line (start 0.54 1.37) (end 7.08 1.37) (layer "F.SilkS") (width 0.12) (tstamp 86eb5627-44b1-4a1a-bd44-ecf17ec0beb1))
    (fp_line (start 0.54 1.04) (end 0.54 1.37) (layer "F.SilkS") (width 0.12) (tstamp 9682c005-fa1a-4dad-a6d4-f9490cc41f06))
    (fp_line (start 0.54 -1.04) (end 0.54 -1.37) (layer "F.SilkS") (width 0.12) (tstamp ebbc4f7d-e87e-4a34-ad98-cef13005a632))
    (fp_line (start -1.05 1.5) (end 8.67 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 169e5810-87ef-4224-a3da-5b749a148105))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 64db6733-ec01-4524-bc55-d9e5db81f01f))
    (fp_line (start 8.67 1.5) (end 8.67 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 7885b48f-4e4c-48b4-b7f5-8fdec8ccf6cc))
    (fp_line (start 8.67 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp fa4ebc11-6c0e-4113-a006-f2cfdf8ca090))
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer "F.Fab") (width 0.1) (tstamp 380e9128-6097-430e-8628-01b7ac1d1e35))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer "F.Fab") (width 0.1) (tstamp 4893fbca-896d-4325-8eed-683d95380d88))
    (fp_line (start 0 0) (end 0.66 0) (layer "F.Fab") (width 0.1) (tstamp 770abee5-20bf-4deb-ab02-856acd8e9a27))
    (fp_line (start 7.62 0) (end 6.96 0) (layer "F.Fab") (width 0.1) (tstamp 98d60533-d8cd-4fae-848e-824e401e7429))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer "F.Fab") (width 0.1) (tstamp ad141bde-7303-4687-870c-5ba8afab9962))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer "F.Fab") (width 0.1) (tstamp ec29c9af-aef8-4035-b231-6a36ab084a6d))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Board_0-Net-(C3-Pad2)") (pintype "passive") (tstamp 6ce483cc-bc8e-4d21-9b28-eaef48a8d2ef))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Board_0-Net-(J3-Pad2)") (pintype "passive") (tstamp a082d7c3-ad45-4cc2-9007-843a8befd9ad))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0) (tstamp 44c4799a-8fae-4d4c-8c03-53f50abace18)
    (at 24.51 24.13)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "Archivo: KiKit_1.kicad_sch")
    (property "Sheetname" "")
    (path "/643cab15-ddb9-4df5-9f54-72397af6f983")
    (attr through_hole)
    (fp_text reference "C3" (at 2.5 -2.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6e3aac14-8829-4f61-b239-07c5ce95617b)
    )
    (fp_text value "100nF" (at 2.5 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a6e3f8af-0a2e-4ae1-907b-4be4784595b1)
    )
    (fp_text user "${REFERENCE}" (at 2.5 0 unlocked) (layer "F.Fab")
      (effects (font (size 0.94 0.94) (thickness 0.141)))
      (tstamp 897db3d7-fbb0-4f3f-8e12-64b043d491d0)
    )
    (fp_line (start 0.03 -1.37) (end 4.97 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 10480df7-8abe-4603-8df9-39e22d82289d))
    (fp_line (start 0.03 1.37) (end 4.97 1.37) (layer "F.SilkS") (width 0.12) (tstamp 4b163042-73b9-4322-b2ac-4766f1fb300e))
    (fp_line (start 4.97 1.055) (end 4.97 1.37) (layer "F.SilkS") (width 0.12) (tstamp 71c1c453-2a50-45f2-aa3e-fb2c8a1ec99f))
    (fp_line (start 0.03 1.055) (end 0.03 1.37) (layer "F.SilkS") (width 0.12) (tstamp 80e2c9b7-f4e5-4bcc-a013-874ee3196d2b))
    (fp_line (start 0.03 -1.37) (end 0.03 -1.055) (layer "F.SilkS") (width 0.12) (tstamp 9de91c8d-9c36-4a12-9430-2aa95df9c1d9))
    (fp_line (start 4.97 -1.37) (end 4.97 -1.055) (layer "F.SilkS") (width 0.12) (tstamp dbdb11aa-a95b-4252-ba32-822f9535b31a))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 26948c3a-eeee-4b59-98c2-f85707fc68e5))
    (fp_line (start 6.05 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 2b4f0ecc-d482-4219-8137-c465640d5a04))
    (fp_line (start 6.05 1.5) (end 6.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 4ffd165e-9b2e-491c-9946-f89e223f046f))
    (fp_line (start -1.05 1.5) (end 6.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp ea1dd464-a4f5-4b08-b0ec-7989293b3efb))
    (fp_line (start 4.85 1.25) (end 4.85 -1.25) (layer "F.Fab") (width 0.1) (tstamp 32a7c98e-3f20-44c0-a8b8-fd93da7078a7))
    (fp_line (start 0.15 1.25) (end 4.85 1.25) (layer "F.Fab") (width 0.1) (tstamp 5f4bbf40-3a25-4e2e-bed5-35a7aa6c0dc5))
    (fp_line (start 4.85 -1.25) (end 0.15 -1.25) (layer "F.Fab") (width 0.1) (tstamp 90fd7331-31ae-495e-8a03-cc12e32dd2b0))
    (fp_line (start 0.15 -1.25) (end 0.15 1.25) (layer "F.Fab") (width 0.1) (tstamp 9acfc5fc-08cc-428b-b397-1e1e6e464ca3))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Board_0-Net-(C3-Pad1)") (pintype "passive") (tstamp 4970fbd2-5b8a-40c7-b5b5-c7512f512514))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Board_0-Net-(C3-Pad2)") (pintype "passive") (tstamp b21a383c-4e61-4b72-a854-7c83c2ebe804))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0) (tstamp c610db1c-af5e-4a3a-9493-e572fea7893e)
    (at 36.5 24)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "Archivo: KiKit_1.kicad_sch")
    (property "Sheetname" "")
    (path "/49119734-b70f-4139-b2b7-2613438adf86")
    (attr through_hole)
    (fp_text reference "C4" (at 2.5 -2.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dfa6be1b-836f-4f41-94eb-0c8118c9b93a)
    )
    (fp_text value "100nF" (at 2.5 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a7aeb592-5b0b-4d83-9df9-6763707452be)
    )
    (fp_text user "${REFERENCE}" (at 2.5 0 unlocked) (layer "F.Fab")
      (effects (font (size 0.94 0.94) (thickness 0.141)))
      (tstamp b07146c2-4d24-4014-9f11-106f2070be10)
    )
    (fp_line (start 0.03 1.055) (end 0.03 1.37) (layer "F.SilkS") (width 0.12) (tstamp 195fa925-0c4d-4ec4-b1cb-6983a8141dc0))
    (fp_line (start 0.03 -1.37) (end 0.03 -1.055) (layer "F.SilkS") (width 0.12) (tstamp 659fe1d6-9272-484f-8498-773a91f68237))
    (fp_line (start 0.03 -1.37) (end 4.97 -1.37) (layer "F.SilkS") (width 0.12) (tstamp abccc7de-b472-4931-ae55-ac4acf598ccb))
    (fp_line (start 4.97 -1.37) (end 4.97 -1.055) (layer "F.SilkS") (width 0.12) (tstamp b49325ad-0d28-4f64-be2e-6fcbcff8bbdf))
    (fp_line (start 4.97 1.055) (end 4.97 1.37) (layer "F.SilkS") (width 0.12) (tstamp bdfcc65f-f83e-4a4e-9853-ddac665baad1))
    (fp_line (start 0.03 1.37) (end 4.97 1.37) (layer "F.SilkS") (width 0.12) (tstamp f82af252-73ab-4929-85fc-acdbce81e4bc))
    (fp_line (start 6.05 1.5) (end 6.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 634b48c1-4033-4a45-a9d9-e93373b4e925))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 6a37230f-9eff-4b67-a16e-300f20bb3ffe))
    (fp_line (start -1.05 1.5) (end 6.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp a71c44f8-bf70-4d84-ab5b-ad0036030479))
    (fp_line (start 6.05 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp f7860890-eb4c-4c03-8187-55b2e50d9e5f))
    (fp_line (start 4.85 1.25) (end 4.85 -1.25) (layer "F.Fab") (width 0.1) (tstamp 1d02419d-45be-45ab-9df8-604adca7e6ef))
    (fp_line (start 0.15 -1.25) (end 0.15 1.25) (layer "F.Fab") (width 0.1) (tstamp 6fa42747-3fe8-4e82-9b98-63137dfabeee))
    (fp_line (start 0.15 1.25) (end 4.85 1.25) (layer "F.Fab") (width 0.1) (tstamp a1215b5f-a62a-4af4-b15c-c63c4be273f0))
    (fp_line (start 4.85 -1.25) (end 0.15 -1.25) (layer "F.Fab") (width 0.1) (tstamp b742bbbb-baf7-4201-9248-65f6e737675b))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Board_0-Net-(C3-Pad2)") (pintype "passive") (tstamp 238d6fc7-9ae2-4615-9494-5b5287cec11f))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Board_0-Net-(C4-Pad2)") (pintype "passive") (tstamp 2b71a92d-38f6-423c-906b-8f6e7400da37))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "kikit:Board" (layer "F.Cu")
    (tedit 605A21C1) (tstamp de6748bd-ece6-4164-8a1b-cb6d909f3f86)
    (at 19 15)
    (descr "Mark board for extraction")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "B" (at -4.5 -5 unlocked) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 6d45fc2a-6eec-407b-aa4f-0b09c0840d57)
    )
    (fp_text value "Board" (at -7.25 -5 unlocked) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a87fcda9-2ef7-4596-8228-c2cc37789e07)
    )
    (fp_line (start 0 0) (end 0.5 -1) (layer "Dwgs.User") (width 0.2) (tstamp 0e5cf2fb-8f19-4e7b-98b5-6db41c9c20f7))
    (fp_line (start 0 0) (end -1.25 -4) (layer "Dwgs.User") (width 0.2) (tstamp 380423ea-74b2-4251-abe8-2482c3d2cd03))
    (fp_line (start 0 0) (end -1 -0.5) (layer "Dwgs.User") (width 0.2) (tstamp 968a00f8-54b6-413c-82e8-5f5b3954f91e))
    (fp_line (start -1.25 -4) (end -9.25 -4) (layer "Dwgs.User") (width 0.2) (tstamp e37d8e66-3371-4d67-8631-a8fc408e06c5))
  )

  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B) (tstamp fc18f0e2-e9f8-4661-851b-fd3dc170c344)
    (at 20 21.73 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Sheetfile" "Archivo: KiKit_1.kicad_sch")
    (property "Sheetname" "")
    (path "/f0bb987b-65e8-4f4d-a7e6-23c362322cf7")
    (attr through_hole)
    (fp_text reference "J3" (at 1.27 -4.12 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 52440a78-31d4-4ae6-b13a-edbb611f2970)
    )
    (fp_text value "IN" (at 1.27 4.08 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 54e3d1e7-4bd6-4244-b381-441e1fcc1eb2)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.22 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f419f4c7-c195-43d8-97ed-d904267cfe45)
    )
    (fp_line (start 0.25 2.99) (end 0.25 1.99) (layer "F.SilkS") (width 0.12) (tstamp 3ead9bd5-9080-4979-8ed6-4dc9d045a2b3))
    (fp_line (start 3.92 -3.03) (end -1.38 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 4b25dd63-790f-4bbf-8577-286f10d97fa0))
    (fp_line (start -1.38 -3.03) (end -1.38 2.99) (layer "F.SilkS") (width 0.12) (tstamp 4ebfd1a1-e307-4b65-a0a2-9061d9715f3c))
    (fp_line (start -1.67 -2) (end -1.67 2) (layer "F.SilkS") (width 0.12) (tstamp 52a9b95e-04a0-4e55-a530-25c7e3e87cc0))
    (fp_line (start -0.8 -3.03) (end -0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 54200570-383a-4d41-8f4f-fec6a9ddd01e))
    (fp_line (start 0 1.99) (end 0.25 1.46) (layer "F.SilkS") (width 0.12) (tstamp 5fc50222-fdff-43d1-a25c-d56068ff3bfb))
    (fp_line (start 1.74 -2.43) (end 3.34 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 6386665a-42b8-4d68-9874-c5495ed494fd))
    (fp_line (start 1.74 -3.03) (end 1.74 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 679b2cb6-4666-4d08-97cf-2bcf64757c73))
    (fp_line (start 3.92 2.99) (end 3.92 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 705c30ec-91dc-4181-800e-ec618671d948))
    (fp_line (start -0.8 -2.43) (end 0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 730731d2-45a0-44f2-9cdf-aefc3d70a83f))
    (fp_line (start 2.54 1.99) (end 2.54 2.99) (layer "F.SilkS") (width 0.12) (tstamp 76eb7253-1dc8-4893-a34c-27b786d55454))
    (fp_line (start 0.25 1.46) (end 2.29 1.46) (layer "F.SilkS") (width 0.12) (tstamp 795bc052-b8db-404f-bae5-83e364ecf0b2))
    (fp_line (start -1.38 2.99) (end 3.92 2.99) (layer "F.SilkS") (width 0.12) (tstamp 8173d75e-778a-4fcb-8da2-21da0205ecb3))
    (fp_line (start 0 1.99) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp aed57207-e4c8-4cbd-92cc-f37b7aeacab9))
    (fp_line (start 2.29 2.99) (end 2.29 1.99) (layer "F.SilkS") (width 0.12) (tstamp b9a50f58-af35-4810-a646-8837d64301af))
    (fp_line (start 2.29 1.46) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp c3f17ac5-9809-41c5-ad35-0a623eb743ab))
    (fp_line (start 3.34 -2.43) (end 3.34 -3.03) (layer "F.SilkS") (width 0.12) (tstamp cd3e216e-9d24-4d38-8e50-9fc65631b79f))
    (fp_line (start 0 2.99) (end 0 1.99) (layer "F.SilkS") (width 0.12) (tstamp d3460405-c9f7-462c-ab26-913a8eca2076))
    (fp_line (start 0.8 -2.43) (end 0.8 -3.03) (layer "F.SilkS") (width 0.12) (tstamp db7dd1df-ed64-464c-b79b-02330c283e2f))
    (fp_line (start -1.77 -3.42) (end -1.77 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 402c2815-d288-44d1-b704-b2a720c7c9a2))
    (fp_line (start 4.31 -3.42) (end -1.77 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp 832c75a3-773d-4d4f-bd23-54c6efd3f9b5))
    (fp_line (start -1.77 3.38) (end 4.31 3.38) (layer "F.CrtYd") (width 0.05) (tstamp dc52e2d8-bb85-41ca-9b20-51eab62611d0))
    (fp_line (start 4.31 3.38) (end 4.31 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp ee0364eb-0166-4e65-8e05-05d829560f6d))
    (fp_line (start -1.27 -2.92) (end -1.27 2.88) (layer "F.Fab") (width 0.1) (tstamp 004d6870-27ad-4e51-8256-acf56f2ca977))
    (fp_line (start -1.27 2.88) (end 3.81 2.88) (layer "F.Fab") (width 0.1) (tstamp 23c8a3ec-b833-478c-9fdc-a42f87a0ee4b))
    (fp_line (start -0.562893 0) (end -1.27 0.5) (layer "F.Fab") (width 0.1) (tstamp 342eda15-df27-4e9c-ba35-4a4cde049b6b))
    (fp_line (start -1.27 -0.5) (end -0.562893 0) (layer "F.Fab") (width 0.1) (tstamp 8124bf28-742f-4e1b-91bb-1428f4500bb3))
    (fp_line (start 3.81 -2.92) (end -1.27 -2.92) (layer "F.Fab") (width 0.1) (tstamp ddad3a7e-1d97-459a-b89e-00e30de59dc7))
    (fp_line (start 3.81 2.88) (end 3.81 -2.92) (layer "F.Fab") (width 0.1) (tstamp ee1a7733-adc6-432b-8885-e2ca572195b7))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 1 "Board_0-Net-(C3-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 0dd76e4f-2110-41c4-8f74-839cf216708a))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 4 "Board_0-Net-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp a8ef4667-f888-4d31-91a2-4133abf8d31f))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 52 28) (end 15 28) (layer "Edge.Cuts") (width 0.1) (tstamp 242d8508-bd99-4a04-b1b5-a2b64803c1c7))
  (gr_line (start 15 28) (end 15 15) (layer "Edge.Cuts") (width 0.1) (tstamp 44c27041-2c48-4b7e-80af-f40e359f4f2d))
  (gr_line (start 52 15) (end 52 28) (layer "Edge.Cuts") (width 0.1) (tstamp 477df641-9cdb-4957-8ea5-1a0e3f7fce10))
  (gr_line (start 15 15) (end 52 15) (layer "Edge.Cuts") (width 0.1) (tstamp 693eb750-4e73-43a0-b852-249e04112acd))
  (gr_line (start 15 15) (end 15 15) (layer "Edge.Cuts") (width 0.1) (tstamp c6cf92c4-a949-41c3-9245-50f213adc0f4))

  (segment (start 21.73 21.73) (end 20.51 21.73) (width 1) (layer "B.Cu") (net 1) (tstamp ca534d1a-002a-4fd8-a7db-7ec927813814))
  (segment (start 23 23) (end 21.73 21.73) (width 1) (layer "B.Cu") (net 1) (tstamp d807f9ad-cd8f-46b0-b007-b552c796bbfc))
  (segment (start 24.51 24.13) (end 23.38 23) (width 1) (layer "B.Cu") (net 1) (tstamp eaf2f989-3dc6-4784-8aa1-50e0470c6043))
  (segment (start 23.38 23) (end 23 23) (width 1) (layer "B.Cu") (net 1) (tstamp f90c7589-3253-416c-9ed9-25f8840d1dba))
  (segment (start 33.81 24) (end 33 24.81) (width 1) (layer "B.Cu") (net 2) (tstamp 1c3591c5-e06f-43f3-807c-a1e368c30801))
  (segment (start 32.19 24) (end 32 24) (width 1) (layer "B.Cu") (net 2) (tstamp 674e43e8-a0e7-40c7-910a-0ef3ae1ef906))
  (segment (start 32 24) (end 31.87 24.13) (width 1) (layer "B.Cu") (net 2) (tstamp 699a6d5a-afea-4639-ba9f-f7a7bec79e59))
  (segment (start 36.5 24) (end 33.81 24) (width 1) (layer "B.Cu") (net 2) (tstamp 9c5cd7c4-5298-4669-85d8-dd0d724cc78a))
  (segment (start 33 24.81) (end 32.19 24) (width 1) (layer "B.Cu") (net 2) (tstamp caab5f66-beb9-4e6b-aa7d-a0bfef75989c))
  (segment (start 31.87 24.13) (end 29.51 24.13) (width 1) (layer "B.Cu") (net 2) (tstamp cd560a9f-d291-40a7-bb34-bd58f3be76f9))
  (segment (start 48 19) (end 50 21) (width 1) (layer "B.Cu") (net 3) (tstamp 0dd3a0b5-625b-4357-a225-43814eb776c7))
  (segment (start 47 19) (end 48 19) (width 1) (layer "B.Cu") (net 3) (tstamp 2f24fe54-69dd-4ce4-a8fd-c424310bc116))
  (segment (start 50 23) (end 49 24) (width 1) (layer "B.Cu") (net 3) (tstamp 3309f6cd-2e5e-499e-8e9b-d75140104081))
  (segment (start 50 21) (end 50 23) (width 1) (layer "B.Cu") (net 3) (tstamp 704619be-e4d4-435d-a175-44876fbe3d59))
  (segment (start 49 24) (end 41.5 24) (width 1) (layer "B.Cu") (net 3) (tstamp a1098a99-8a6e-4818-babb-e7df6153457c))
  (segment (start 43.54 21.54) (end 47 21.54) (width 1) (layer "B.Cu") (net 4) (tstamp 127403ec-2d5d-454e-b833-e91f194153a9))
  (segment (start 20.51 19.19) (end 20.51 18.49) (width 1) (layer "B.Cu") (net 4) (tstamp 2dc31c1a-c0ee-4003-af49-7beb27659e52))
  (segment (start 33 17.19) (end 39.19 17.19) (width 1) (layer "B.Cu") (net 4) (tstamp 60fc9ec3-ab18-4426-9179-1c5db5353731))
  (segment (start 21 18) (end 22.19 17.19) (width 1) (layer "B.Cu") (net 4) (tstamp 8960c90c-7784-476d-abfb-59017e046fb7))
  (segment (start 39.19 17.19) (end 43.54 21.54) (width 1) (layer "B.Cu") (net 4) (tstamp be4305f3-82c0-4e59-9916-31624c86e2d2))
  (segment (start 22.19 17.19) (end 33 17.19) (width 1) (layer "B.Cu") (net 4) (tstamp c911b882-dd33-4f7a-b035-f74ad2684acb))
  (segment (start 20.51 18.49) (end 21 18) (width 1) (layer "B.Cu") (net 4) (tstamp e203bcad-8fb2-4d64-b631-c2e8932f6536))

)
