(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin 97.0026 97.0026)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")

  (footprint "Package_DFN_QFN:QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm" (layer "B.Cu")
    (tedit 5DC5F6A3) (tstamp 00000000-0000-0000-0000-0000601b53a7)
    (at 100 100)
    (descr "QFN, 12 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_12_%2005-08-1855.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference "U1" (at 0 2.82) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 842e430f-0c35-45f3-a0b5-95ae7b7ae388)
    )
    (fp_text value "QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm" (at 0 -2.82) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 51c4dc0a-5b9f-4edf-a83f-4a12881e42ef)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.75 0.75) (thickness 0.11)) (justify mirror))
      (tstamp a03e565f-d8cd-4032-aae3-b7327d4143dd)
    )
    (fp_line (start 0.885 1.61) (end 1.61 1.61) (layer "B.SilkS") (width 0.12) (tstamp 03d88a85-11fd-47aa-954c-c318bb15294a))
    (fp_line (start -0.885 -1.61) (end -1.61 -1.61) (layer "B.SilkS") (width 0.12) (tstamp 0dcdf1b8-13c6-48b4-bd94-5d26038ff231))
    (fp_line (start 1.61 1.61) (end 1.61 0.885) (layer "B.SilkS") (width 0.12) (tstamp 1a2f72d1-0b36-4610-afc4-4ad1660d5d3b))
    (fp_line (start 0.885 -1.61) (end 1.61 -1.61) (layer "B.SilkS") (width 0.12) (tstamp 58dc14f9-c158-4824-a84e-24a6a482a7a4))
    (fp_line (start -0.885 1.61) (end -1.61 1.61) (layer "B.SilkS") (width 0.12) (tstamp b635b16e-60bb-4b3e-9fc3-47d34eef8381))
    (fp_line (start -1.61 -1.61) (end -1.61 -0.885) (layer "B.SilkS") (width 0.12) (tstamp dde3dba8-1b81-466c-93a3-c284ff4da1ef))
    (fp_line (start 1.61 -1.61) (end 1.61 -0.885) (layer "B.SilkS") (width 0.12) (tstamp f976e2cc-36f9-4479-a816-2c74d1d5da6f))
    (fp_line (start -2.12 2.12) (end -2.12 -2.12) (layer "B.CrtYd") (width 0.05) (tstamp 48f827a8-6e22-4a2e-abdc-c2a03098d883))
    (fp_line (start 2.12 2.12) (end -2.12 2.12) (layer "B.CrtYd") (width 0.05) (tstamp 9c8ccb2a-b1e9-4f2c-94fe-301b5975277e))
    (fp_line (start 2.12 -2.12) (end 2.12 2.12) (layer "B.CrtYd") (width 0.05) (tstamp cef6f603-8a0b-4dd0-af99-ebfbef7d1b4b))
    (fp_line (start -2.12 -2.12) (end 2.12 -2.12) (layer "B.CrtYd") (width 0.05) (tstamp e877bf4a-4210-4bd3-b7b0-806eb4affc5b))
    (fp_line (start -1.5 -1.5) (end -1.5 0.75) (layer "B.Fab") (width 0.1) (tstamp 120a7b0f-ddfd-4447-85c1-35665465acdb))
    (fp_line (start -0.75 1.5) (end 1.5 1.5) (layer "B.Fab") (width 0.1) (tstamp 13475e15-f37c-4de8-857e-1722b0c39513))
    (fp_line (start 1.5 1.5) (end 1.5 -1.5) (layer "B.Fab") (width 0.1) (tstamp 2732632c-4768-42b6-bf7f-14643424019e))
    (fp_line (start 1.5 -1.5) (end -1.5 -1.5) (layer "B.Fab") (width 0.1) (tstamp 854dd5d4-5fd2-4730-bd49-a9cd8299a065))
    (fp_line (start -1.5 0.75) (end -0.75 1.5) (layer "B.Fab") (width 0.1) (tstamp 8d55e186-3e11-40e8-a65e-b36a8a00069e))
    (pad "" smd roundrect locked (at -0.41 -0.41) (size 0.67 0.67) (layers "B.Paste") (roundrect_rratio 0.25) (tstamp 4e3d7c0d-12e3-42f2-b944-e4bcdbbcac2a))
    (pad "" smd roundrect locked (at 0.41 -0.41) (size 0.67 0.67) (layers "B.Paste") (roundrect_rratio 0.25) (tstamp 5b2b5c7d-f943-4634-9f0a-e9561705c49d))
    (pad "" smd roundrect locked (at -0.41 0.41) (size 0.67 0.67) (layers "B.Paste") (roundrect_rratio 0.25) (tstamp aa02e544-13f5-4cf8-a5f4-3e6cda006090))
    (pad "" smd roundrect locked (at 0.41 0.41) (size 0.67 0.67) (layers "B.Paste") (roundrect_rratio 0.25) (tstamp c70d9ef3-bfeb-47e0-a1e1-9aeba3da7864))
    (pad "1" smd roundrect locked (at -1.4625 0.5) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp f3490fa5-5a27-423b-af60-53609669542c))
    (pad "2" smd roundrect locked (at -1.4625 0) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp b6270a28-e0d9-4655-a18a-03dbf007b940))
    (pad "3" smd roundrect locked (at -1.4625 -0.5) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp 8322f275-268c-4e87-a69f-4cfbf05e747f))
    (pad "4" smd roundrect locked (at -0.5 -1.4625) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp 0a3cc030-c9dd-4d74-9d50-715ed2b361a2))
    (pad "5" smd roundrect locked (at 0 -1.4625) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp dd00c2e1-6027-4717-b312-4fab3ee52002))
    (pad "6" smd roundrect locked (at 0.5 -1.4625) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp 15875808-74d5-4210-b8ca-aa8fbc04ae21))
    (pad "7" smd roundrect locked (at 1.4625 -0.5) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp 81bbc3ff-3938-49ac-8297-ce2bcc9a42bd))
    (pad "8" smd roundrect locked (at 1.4625 0) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp b1169a2d-8998-4b50-a48d-c520bcc1b8e1))
    (pad "9" smd roundrect locked (at 1.4625 0.5) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp 0d0bb7b2-a6e5-46d2-9492-a1aa6e5a7b2f))
    (pad "10" smd roundrect locked (at 0.5 1.4625) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp d22e95aa-f3db-4fbc-a331-048a2523233e))
    (pad "11" smd roundrect locked (at 0 1.4625) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp d1262c4d-2245-4c4f-8f35-7bb32cd9e21e))
    (pad "12" smd roundrect locked (at -0.5 1.4625) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25) (tstamp 0147f16a-c952-4891-8f53-a9fb8cddeb8d))
    (pad "13" smd rect locked (at 0 0) (size 1.65 1.65) (layers "B.Cu" "B.Mask") (tstamp 6a44418c-7bb4-4e99-8836-57f153c19721))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

)
