PCB Specifications:
Size:

- 59.69x48.26 mm

Class: 6D

Track width: ≥ 0.15 mm

Insulation distance: ≥ 0.15 mm

Minimum drill size: ≥ 0.35 mm (finished metalized hole: 0.25 mm)

Minimum slot width: ≥ 0.6 mm

Ring collar: ≥ 0.08 mm


Materials:

- FR4, 1.6 mm
- ENIG
- 4 layers
- 35 µm copper thickness

Solder mask:

- TOP / BOTTOM
- Top: Blue / Bottom: Red

Marking:

- TOP / BOTTOM screen printing
- Silk: White

Other markings:

- ROHS / UL / Date - Yes if available
