(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (title_block
    (title "Filter B")
  )

  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(C101-Pad2)")
  (net 2 "/IN")
  (net 3 "/OUT")
  (net 4 "GND2")

  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B) (tstamp 073e10a8-d821-4d90-9930-676820b40a37)
    (at 138 93 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Sheetfile" "Filter_B.kicad_sch")
    (property "Sheetname" "")
    (path "/f51d6c49-aefa-468a-b9a5-ecbf3acdcf27")
    (attr through_hole)
    (fp_text reference "J101" (at 1.27 -4.12 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 48a17d53-4952-4d79-8e4d-50e0be9135cb)
    )
    (fp_text value "IN" (at 1.27 4.08 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8d8dac3a-afe2-43a5-ae30-cb31f62aa7f4)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.22 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b0e68a2a-da9f-4cc7-a703-854231d0221e)
    )
    (fp_line (start 3.92 -3.03) (end -1.38 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 16986895-5470-493c-b749-9c8aa3b8a5d5))
    (fp_line (start -0.8 -2.43) (end 0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 293e6381-9d7e-4cc4-83c6-75d6d352578d))
    (fp_line (start 0.8 -2.43) (end 0.8 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 43cd6088-ebcd-410c-9e43-0901a11042b2))
    (fp_line (start -1.38 -3.03) (end -1.38 2.99) (layer "F.SilkS") (width 0.12) (tstamp 70f066fe-e711-4716-a04f-1e34f0207131))
    (fp_line (start -1.38 2.99) (end 3.92 2.99) (layer "F.SilkS") (width 0.12) (tstamp 758736e6-d195-4589-8332-021a0d81651e))
    (fp_line (start -1.67 -2) (end -1.67 2) (layer "F.SilkS") (width 0.12) (tstamp 9a8530de-1563-47cf-a985-f515dbc56943))
    (fp_line (start 0 2.99) (end 0 1.99) (layer "F.SilkS") (width 0.12) (tstamp 9c117ccb-c841-4fc4-a22c-41defcf2ff67))
    (fp_line (start -0.8 -3.03) (end -0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp a0bcb5fd-c30a-483d-ad43-1c04fa42cf17))
    (fp_line (start 2.29 1.46) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp a2efdcbd-e89e-4beb-a2a3-34ec1a04d064))
    (fp_line (start 0.25 1.46) (end 2.29 1.46) (layer "F.SilkS") (width 0.12) (tstamp a302bb28-82a5-4f7a-8d4e-1cf743e3ec49))
    (fp_line (start 0 1.99) (end 0.25 1.46) (layer "F.SilkS") (width 0.12) (tstamp a668b88a-38d0-47e1-a764-e7f7935c8310))
    (fp_line (start 1.74 -3.03) (end 1.74 -2.43) (layer "F.SilkS") (width 0.12) (tstamp b32f3208-c08b-41dd-8710-80e8b83fce77))
    (fp_line (start 3.92 2.99) (end 3.92 -3.03) (layer "F.SilkS") (width 0.12) (tstamp ba47282b-c2f1-464f-8471-41d4dd26ed21))
    (fp_line (start 2.29 2.99) (end 2.29 1.99) (layer "F.SilkS") (width 0.12) (tstamp dca44611-9bc8-4329-981b-98e08f98edce))
    (fp_line (start 0 1.99) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp e17931b2-a8eb-427f-8519-60bf90645538))
    (fp_line (start 2.54 1.99) (end 2.54 2.99) (layer "F.SilkS") (width 0.12) (tstamp e49e87b4-84fd-4315-b18c-f94cf0141e28))
    (fp_line (start 1.74 -2.43) (end 3.34 -2.43) (layer "F.SilkS") (width 0.12) (tstamp e619811e-8bf6-43e4-b97a-40c146e6f147))
    (fp_line (start 0.25 2.99) (end 0.25 1.99) (layer "F.SilkS") (width 0.12) (tstamp f1b1f716-504f-4f9e-8039-e1469ddacd10))
    (fp_line (start 3.34 -2.43) (end 3.34 -3.03) (layer "F.SilkS") (width 0.12) (tstamp f4a50bd3-19ee-4e34-b36f-c1126fa63387))
    (fp_line (start 4.31 -3.42) (end -1.77 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp 25f79c1e-1387-4f26-a890-8fd7121efd3a))
    (fp_line (start -1.77 3.38) (end 4.31 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 54439a1d-9640-41ae-ba16-33b3dfbae319))
    (fp_line (start 4.31 3.38) (end 4.31 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp c6160866-084b-446f-9988-bd60d738a456))
    (fp_line (start -1.77 -3.42) (end -1.77 3.38) (layer "F.CrtYd") (width 0.05) (tstamp ddc3a62e-814e-45b4-ba37-1bc4013ca8a3))
    (fp_line (start -0.562893 0) (end -1.27 0.5) (layer "F.Fab") (width 0.1) (tstamp 147c0377-b56d-4184-8c4f-059c4d13a7f5))
    (fp_line (start 3.81 -2.92) (end -1.27 -2.92) (layer "F.Fab") (width 0.1) (tstamp 32230b5f-37c0-4e9a-9254-23d1df42b681))
    (fp_line (start -1.27 -2.92) (end -1.27 2.88) (layer "F.Fab") (width 0.1) (tstamp 4266af23-90dc-4f71-8984-caf364e9645f))
    (fp_line (start -1.27 2.88) (end 3.81 2.88) (layer "F.Fab") (width 0.1) (tstamp 92674be5-53b9-43b7-b6c1-42ee8ad5bfce))
    (fp_line (start -1.27 -0.5) (end -0.562893 0) (layer "F.Fab") (width 0.1) (tstamp 964ac08c-5e15-429c-a797-0e9466ef0a89))
    (fp_line (start 3.81 2.88) (end 3.81 -2.92) (layer "F.Fab") (width 0.1) (tstamp d5f75420-31c2-45d3-be9d-d974313dbb9c))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 2 "/IN") (pinfunction "Pin_1") (pintype "passive") (tstamp bed590b5-864c-45bf-b1e9-38b8b973db09))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 4 "GND2") (pinfunction "Pin_2") (pintype "passive") (tstamp d88ba291-3cf0-4464-8b8b-0189d2d857a5))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B) (tstamp 62432fc6-42d3-493e-80b9-24924be4c8bb)
    (at 163 90.46 -90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Sheetfile" "Filter_B.kicad_sch")
    (property "Sheetname" "")
    (path "/e7925c32-55ee-4423-ae0f-a190596cc514")
    (attr through_hole)
    (fp_text reference "J102" (at 1.27 -4.12 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 90336f57-0af8-423c-b84e-56c87274880e)
    )
    (fp_text value "OUT" (at 1.27 4.08 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 47517af5-4b8b-406d-a8ba-3c23aa8315be)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.22 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a3a5729-a3b8-4590-9b11-2dddef4f7bd3)
    )
    (fp_line (start 2.29 2.99) (end 2.29 1.99) (layer "F.SilkS") (width 0.12) (tstamp 0a155d10-6369-4fad-8481-1095aa1175e0))
    (fp_line (start -0.8 -3.03) (end -0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 1050265d-94da-436e-85d0-ccf58c1a0d83))
    (fp_line (start 1.74 -2.43) (end 3.34 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 18653ad4-adeb-44bb-90c1-7df473de6459))
    (fp_line (start 2.29 1.46) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp 26d3f367-32b5-4f5a-a06e-069ec7bf9efa))
    (fp_line (start 0.25 1.46) (end 2.29 1.46) (layer "F.SilkS") (width 0.12) (tstamp 2b23affa-a84d-4ddf-bba7-c10b953cf2d5))
    (fp_line (start 3.92 2.99) (end 3.92 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 2ed09c2c-9cdc-4594-bcee-817ca06c450d))
    (fp_line (start 0.25 2.99) (end 0.25 1.99) (layer "F.SilkS") (width 0.12) (tstamp 55ec6921-0351-4dca-b7b9-0a6babaa1b49))
    (fp_line (start 1.74 -3.03) (end 1.74 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 5e27dcb4-cf1b-4751-9f96-896f49cea80d))
    (fp_line (start 0.8 -2.43) (end 0.8 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 67941cd8-f979-47bc-8e98-880aa5c841aa))
    (fp_line (start 0 2.99) (end 0 1.99) (layer "F.SilkS") (width 0.12) (tstamp 7661d1e5-c789-470e-96c2-2b9437f643e3))
    (fp_line (start 3.92 -3.03) (end -1.38 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 83b8fb0e-a8c9-443e-b68d-037fe92f7696))
    (fp_line (start -0.8 -2.43) (end 0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 94f0f247-7c79-4d46-9fb9-5d90ecbcea00))
    (fp_line (start -1.38 -3.03) (end -1.38 2.99) (layer "F.SilkS") (width 0.12) (tstamp a3bdb23f-eb40-4ff0-a982-fc37ac1fe93e))
    (fp_line (start 2.54 1.99) (end 2.54 2.99) (layer "F.SilkS") (width 0.12) (tstamp a8a7e931-6835-4217-9e55-4e746f35c325))
    (fp_line (start -1.38 2.99) (end 3.92 2.99) (layer "F.SilkS") (width 0.12) (tstamp b226c0bd-624c-4649-bfd0-2d83c5522b64))
    (fp_line (start 3.34 -2.43) (end 3.34 -3.03) (layer "F.SilkS") (width 0.12) (tstamp d9d66db1-e8af-441c-a49f-a5a804bb20ef))
    (fp_line (start -1.67 -2) (end -1.67 2) (layer "F.SilkS") (width 0.12) (tstamp e08cb9eb-ec1a-41b5-abe2-5430207681a8))
    (fp_line (start 0 1.99) (end 0.25 1.46) (layer "F.SilkS") (width 0.12) (tstamp e4e6e9a6-1006-40f8-b6ec-4d8449b638e8))
    (fp_line (start 0 1.99) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp f9cd1f78-ddbc-4ffa-a748-b42f31df1a1a))
    (fp_line (start -1.77 -3.42) (end -1.77 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 467aa28d-59dd-42ba-9014-80a7c789df35))
    (fp_line (start 4.31 3.38) (end 4.31 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp 556da290-4a46-417f-a336-bbfc91f835d6))
    (fp_line (start -1.77 3.38) (end 4.31 3.38) (layer "F.CrtYd") (width 0.05) (tstamp b2ad64b3-bc79-4193-91b0-2aa6df48ae43))
    (fp_line (start 4.31 -3.42) (end -1.77 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp ec7948f8-2269-41d6-9fe1-5aef69119ad9))
    (fp_line (start 3.81 -2.92) (end -1.27 -2.92) (layer "F.Fab") (width 0.1) (tstamp 26fb1c92-68fd-4211-9452-b267c1235944))
    (fp_line (start -0.562893 0) (end -1.27 0.5) (layer "F.Fab") (width 0.1) (tstamp 28cfbbe0-a93f-4c8c-ad45-69363eceaed7))
    (fp_line (start -1.27 -2.92) (end -1.27 2.88) (layer "F.Fab") (width 0.1) (tstamp 9f848461-aa46-4380-9760-fa676c8f9e6d))
    (fp_line (start -1.27 2.88) (end 3.81 2.88) (layer "F.Fab") (width 0.1) (tstamp d0c7c944-49d6-4a04-a4d7-6f089ac9ffdf))
    (fp_line (start -1.27 -0.5) (end -0.562893 0) (layer "F.Fab") (width 0.1) (tstamp dd0b5065-e316-4458-8690-e3be23790d56))
    (fp_line (start 3.81 2.88) (end 3.81 -2.92) (layer "F.Fab") (width 0.1) (tstamp ff84434b-bd04-4385-951c-da75ca411c48))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 3 "/OUT") (pinfunction "Pin_1") (pintype "passive") (tstamp 0bc46d4c-a2d2-4239-b55a-b0a09867c5cc))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 4 "GND2") (pinfunction "Pin_2") (pintype "passive") (tstamp 40bd4fcd-2b4d-4de4-808c-8678ad544fa4))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0) (tstamp cd08b253-0f11-4514-b16f-dd1dee81f79d)
    (at 152 93)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "Filter_B.kicad_sch")
    (property "Sheetname" "")
    (path "/d0a907f2-ec04-492b-ab07-69facca32dd1")
    (attr through_hole)
    (fp_text reference "C102" (at 2.5 3) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 57569598-69c1-45e5-98bf-2a0ff2ab886b)
    )
    (fp_text value "100nF" (at 2.5 2.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 75d6ca52-8403-4966-bc8e-8b78949ada22)
    )
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab")
      (effects (font (size 0.94 0.94) (thickness 0.141)))
      (tstamp b4500a13-f636-40d2-a73b-69c39ed0adb7)
    )
    (fp_line (start 0.03 1.37) (end 4.97 1.37) (layer "F.SilkS") (width 0.12) (tstamp 3ac54696-77e0-4f16-9cd1-b8c4f2da14e8))
    (fp_line (start 4.97 -1.37) (end 4.97 -1.055) (layer "F.SilkS") (width 0.12) (tstamp 45a25ed4-3f85-4f8d-b6b6-ad6ad77a9f93))
    (fp_line (start 4.97 1.055) (end 4.97 1.37) (layer "F.SilkS") (width 0.12) (tstamp 509079dd-4f21-4260-9f51-cf7e23ab435c))
    (fp_line (start 0.03 1.055) (end 0.03 1.37) (layer "F.SilkS") (width 0.12) (tstamp a6863c1a-6875-4595-9bfe-bfb2121bb1a1))
    (fp_line (start 0.03 -1.37) (end 0.03 -1.055) (layer "F.SilkS") (width 0.12) (tstamp a940f583-4de0-4bd3-b46d-f7dd5b3a1152))
    (fp_line (start 0.03 -1.37) (end 4.97 -1.37) (layer "F.SilkS") (width 0.12) (tstamp ba5bf8b1-1387-469c-9055-005337032420))
    (fp_line (start -1.05 1.5) (end 6.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 785d3d42-cf19-414a-bc35-30d8a25ff31e))
    (fp_line (start 6.05 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 93b18b95-9fdb-45ff-b1c9-f90a31d41892))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp a6e6dfcf-5a22-4603-91ad-b3a8d4072e8d))
    (fp_line (start 6.05 1.5) (end 6.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp f9de89be-1984-4a59-9377-7314374e8312))
    (fp_line (start 4.85 -1.25) (end 0.15 -1.25) (layer "F.Fab") (width 0.1) (tstamp 80d19f72-8e84-4d78-9440-8193771caf0a))
    (fp_line (start 0.15 1.25) (end 4.85 1.25) (layer "F.Fab") (width 0.1) (tstamp 891c2812-2267-44ad-a55b-fb70924aa8e1))
    (fp_line (start 0.15 -1.25) (end 0.15 1.25) (layer "F.Fab") (width 0.1) (tstamp b0ff6081-c19e-4355-a239-733427026436))
    (fp_line (start 4.85 1.25) (end 4.85 -1.25) (layer "F.Fab") (width 0.1) (tstamp b3385ee3-f23c-4b88-8b2d-b691fcfe3e5c))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C101-Pad2)") (pintype "passive") (tstamp ccd424a1-6d7b-43d6-af11-e3558ab6ecb3))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/OUT") (pintype "passive") (tstamp ce492725-dd23-482d-9858-c229f83f7d84))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0) (tstamp d08af1d0-9976-4ed7-85f1-409c61faec36)
    (at 143.5 93)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "Filter_B.kicad_sch")
    (property "Sheetname" "")
    (path "/6130db05-4ed3-49ab-9e3e-6bd0ead0578b")
    (attr through_hole)
    (fp_text reference "C101" (at 2.5 3) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 943b8e83-adab-41cd-b1fa-c3e8739927b3)
    )
    (fp_text value "100nF" (at 2.5 2.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 77b32a4c-9e82-4e8f-8290-39ba636bd41f)
    )
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab")
      (effects (font (size 0.94 0.94) (thickness 0.141)))
      (tstamp 33bc9d5c-1f65-4720-9277-a64515030b84)
    )
    (fp_line (start 0.03 1.055) (end 0.03 1.37) (layer "F.SilkS") (width 0.12) (tstamp 00a5a59a-e103-4622-b57c-8bc1b6796542))
    (fp_line (start 0.03 -1.37) (end 0.03 -1.055) (layer "F.SilkS") (width 0.12) (tstamp 1bc6c7d8-53ba-45a3-b737-47891ec876c7))
    (fp_line (start 4.97 1.055) (end 4.97 1.37) (layer "F.SilkS") (width 0.12) (tstamp 1fb9361f-f089-4021-a51b-6de3bfe77495))
    (fp_line (start 4.97 -1.37) (end 4.97 -1.055) (layer "F.SilkS") (width 0.12) (tstamp 3037c175-787d-4555-9259-791cc91ee150))
    (fp_line (start 0.03 1.37) (end 4.97 1.37) (layer "F.SilkS") (width 0.12) (tstamp 3796276b-dbd7-4815-a164-fbfd9ed9767f))
    (fp_line (start 0.03 -1.37) (end 4.97 -1.37) (layer "F.SilkS") (width 0.12) (tstamp aea88120-f971-4cc5-bee0-9a8c87e99e3f))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 235e8aac-a99d-4e0e-b33b-996127e65b5f))
    (fp_line (start -1.05 1.5) (end 6.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 9afa8d36-0edd-4d17-a2bd-40b40a460475))
    (fp_line (start 6.05 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp b44c75ab-aac4-40de-b61e-d763709eaa54))
    (fp_line (start 6.05 1.5) (end 6.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp bc79b705-a6d1-4191-a810-8080b7d75138))
    (fp_line (start 4.85 1.25) (end 4.85 -1.25) (layer "F.Fab") (width 0.1) (tstamp 02363f18-cd61-468b-9ad6-c28b0fc65788))
    (fp_line (start 0.15 1.25) (end 4.85 1.25) (layer "F.Fab") (width 0.1) (tstamp 0bc553b8-4580-4b9c-b8a8-b547a3428c54))
    (fp_line (start 4.85 -1.25) (end 0.15 -1.25) (layer "F.Fab") (width 0.1) (tstamp 15740665-cc21-4f80-a071-5e557993ac91))
    (fp_line (start 0.15 -1.25) (end 0.15 1.25) (layer "F.Fab") (width 0.1) (tstamp 41a55b37-9247-404a-a2f3-45a6fac2ad71))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/IN") (pintype "passive") (tstamp 0b8053b9-3a44-455c-ad04-91a2c1559f87))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C101-Pad2)") (pintype "passive") (tstamp 05106bb8-b251-4aab-a7de-76056a7e817d))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp f87e002d-c217-4696-b5ab-bab74bd5c42d)
    (at 146 89.95)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Filter_B.kicad_sch")
    (property "Sheetname" "")
    (path "/56f140e5-f5a6-453d-90e1-453a9c49ca4b")
    (attr through_hole)
    (fp_text reference "R101" (at 3.81 -2.37) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8af97727-9461-4ec5-b717-244a0b0eeccb)
    )
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7e5dab4e-5e4b-470b-89da-4a4f717b87ed)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5b3e4343-a0c9-453a-9a55-ac0f619b79f4)
    )
    (fp_line (start 0.54 1.04) (end 0.54 1.37) (layer "F.SilkS") (width 0.12) (tstamp 3c33e7da-4da3-4318-8de9-5078e4abd1c4))
    (fp_line (start 0.54 -1.37) (end 7.08 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 50a7b0e5-07f6-4b0a-88ee-5f91dde90242))
    (fp_line (start 7.08 1.37) (end 7.08 1.04) (layer "F.SilkS") (width 0.12) (tstamp 8118fb0c-0349-4a3b-b34c-3e9aa9fc7eae))
    (fp_line (start 0.54 1.37) (end 7.08 1.37) (layer "F.SilkS") (width 0.12) (tstamp 8960c712-4b95-46b9-b9c9-b54e85b739a0))
    (fp_line (start 7.08 -1.37) (end 7.08 -1.04) (layer "F.SilkS") (width 0.12) (tstamp d700cb96-b522-45d0-8074-386b170e07c4))
    (fp_line (start 0.54 -1.04) (end 0.54 -1.37) (layer "F.SilkS") (width 0.12) (tstamp de80cd7f-9e71-4942-a7b0-835c70222530))
    (fp_line (start 8.67 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 3fbd0ef4-8125-456b-bd59-c9d0405c273e))
    (fp_line (start -1.05 1.5) (end 8.67 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 836932cf-ab46-4b02-8f9c-37e391a351cf))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 9fc37066-1b4b-48ac-bee7-ba0dd70dbe40))
    (fp_line (start 8.67 1.5) (end 8.67 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp be8131ed-0ed6-4746-b707-e0eb51c441aa))
    (fp_line (start 0 0) (end 0.66 0) (layer "F.Fab") (width 0.1) (tstamp 0d77522d-a5fc-4c96-ada2-ee2e68fc47f8))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer "F.Fab") (width 0.1) (tstamp 199cb229-0839-4072-82f6-1b8986fe8981))
    (fp_line (start 7.62 0) (end 6.96 0) (layer "F.Fab") (width 0.1) (tstamp bc2711a2-cad5-4785-aefc-d9a6b8d7d952))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer "F.Fab") (width 0.1) (tstamp ce5646ee-180b-42ba-9661-21512b8041e5))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer "F.Fab") (width 0.1) (tstamp cfd1c5ec-cb17-432b-b998-f74c7826a714))
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer "F.Fab") (width 0.1) (tstamp d90968a5-450f-4c50-b06e-7087bb1e7361))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C101-Pad2)") (pintype "passive") (tstamp 040e718a-dc50-4b33-8d18-7c354e96e396))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND2") (pintype "passive") (tstamp b41d7902-891f-46d9-8154-7ef78fe1e1c9))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 168 97) (end 133 86) (layer "Edge.Cuts") (width 0.1) (fill none) (tstamp c6f284c9-9ab3-4ffa-9817-8aae3c3549b0))

  (segment (start 148.5 93) (end 148.5 92.45) (width 1) (layer "B.Cu") (net 1) (tstamp 0e40a12a-83a0-42c3-a0e2-854c3f580fab))
  (segment (start 148.5 93) (end 152 93) (width 1) (layer "B.Cu") (net 1) (tstamp 2df7330d-7f7a-44c3-8753-d363166256e5))
  (segment (start 148.5 92.45) (end 146 89.95) (width 1) (layer "B.Cu") (net 1) (tstamp 7ae7d3fb-c683-4ba8-bd9c-b94104ed84e1))
  (segment (start 138 93) (end 143.5 93) (width 1) (layer "B.Cu") (net 2) (tstamp 4ced6e96-fc5b-4e55-9d2b-7f0d6a7b70f9))
  (segment (start 157 93) (end 160 90) (width 1) (layer "B.Cu") (net 3) (tstamp 32639dd2-d6fe-4484-b76e-b09d127b69b8))
  (segment (start 160 90) (end 162.54 90) (width 1) (layer "B.Cu") (net 3) (tstamp a9f85686-f6bb-4eb8-8fcc-034b32ef9ad0))
  (segment (start 162.54 90) (end 163 90.46) (width 1) (layer "B.Cu") (net 3) (tstamp ab932622-293c-4c6a-a613-202f3fbfad91))
  (segment (start 155.57 88) (end 166 88) (width 1) (layer "B.Cu") (net 4) (tstamp 4c133e97-8b98-4717-b406-b9a29e1a0449))
  (segment (start 166 93) (end 163 93) (width 1) (layer "B.Cu") (net 4) (tstamp 5a344d0e-248c-4d80-8fe3-aea7db708afc))
  (segment (start 167 92) (end 166 93) (width 1) (layer "B.Cu") (net 4) (tstamp 5a349e33-f25d-4bf0-ae52-43d2c6fc3704))
  (segment (start 152.12 88.45) (end 153.62 89.95) (width 1) (layer "B.Cu") (net 4) (tstamp 72943a86-7124-4cea-bf9e-3cbfc0e1651b))
  (segment (start 138 90.46) (end 140.01 88.45) (width 1) (layer "B.Cu") (net 4) (tstamp 8aecfdbb-f2c0-43d9-a7d1-c151c82cf6bc))
  (segment (start 166 88) (end 167 89) (width 1) (layer "B.Cu") (net 4) (tstamp bebbf8bd-0669-42d6-b1ec-fd570313ff2c))
  (segment (start 140.01 88.45) (end 152.12 88.45) (width 1) (layer "B.Cu") (net 4) (tstamp cf7d3835-f1ab-4307-82ec-b5060cf83566))
  (segment (start 167 89) (end 167 92) (width 1) (layer "B.Cu") (net 4) (tstamp d0a28112-a48a-4978-b0a7-70fdc621d4b9))
  (segment (start 153.62 89.95) (end 155.57 88) (width 1) (layer "B.Cu") (net 4) (tstamp e1571ccc-32a0-482b-8aee-5612d41f3b9d))

)
