(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal "El1")
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005ea76d80)
    (at 105 35 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0b21a65d-d20b-411e-920a-75c343ac5136)
    )
    (fp_text value "R_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (at 0 1.65 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3cd1bda0-18db-417d-b581-a0c50623df68)
    )
    (fp_text user "100" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 6c2e273e-743c-4f1e-a647-4171f8122550)
    )
    (fp_line (start -0.261252 0.71) (end 0.261252 0.71) (layer "F.SilkS") (width 0.12) (tstamp 4c8eb964-bdf4-44de-90e9-e2ab82dd5313))
    (fp_line (start -0.261252 -0.71) (end 0.261252 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 94a873dc-af67-4ef9-8159-1f7c93eeb3d7))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 2d210a96-f81f-42a9-8bf4-1b43c11086f3))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 9bb20359-0f8b-45bc-9d38-6626ed3a939d))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp aa14c3bd-4acc-4908-9d28-228585a22a9d))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer "F.CrtYd") (width 0.05) (tstamp e857610b-4434-4144-b04e-43c1ebdc5ceb))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 03c52831-5dc5-43c5-a442-8d23643b46fb))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 29e78086-2175-405e-9ba3-c48766d2f50c))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp a1823eb2-fb0d-4ed8-8b96-04184ac3a9d5))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp d57dcfee-5058-4fc2-a68b-05f9a48f685b))
    (pad "1" smd roundrect locked (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391) (tstamp 7dc880bc-e7eb-4cce-8d8c-0b65a9dd788e))
    (pad "2" smd roundrect locked (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391) (tstamp 666713b0-70f4-42df-8761-f65bc212d03b))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Box_L13.0mm_W4.0mm_P9.00mm" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp 00000000-0000-0000-0000-00005ea76ec0)
    (at 110 45)
    (descr "Resistor, Box series, Radial, pin pitch=9.00mm, 2W, length*width=13.0*4.0mm^2, http://www.produktinfo.conrad.com/datenblaetter/425000-449999/443860-da-01-de-METALLBAND_WIDERSTAND_0_1_OHM_5W_5Pr.pdf")
    (tags "Resistor Box series Radial pin pitch 9.00mm 2W length 13.0mm width 4.0mm")
    (attr through_hole)
    (fp_text reference "R3" (at 4.5 -3.25) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 47baf4b1-0938-497d-88f9-671136aa8be7)
    )
    (fp_text value "R_Box_L13.0mm_W4.0mm_P9.00mm" (at 4.5 3.25) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 77ed3941-d133-4aef-a9af-5a39322d14eb)
    )
    (fp_text user "300" (at 4.5 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 87371631-aa02-498a-998a-09bdb74784c1)
    )
    (fp_line (start 11.12 -2.12) (end 11.12 2.12) (layer "F.SilkS") (width 0.12) (tstamp 3b838d52-596d-4e4d-a6ac-e4c8e7621137))
    (fp_line (start -2.12 2.12) (end 11.12 2.12) (layer "F.SilkS") (width 0.12) (tstamp 66116376-6967-4178-9f23-a26cdeafc400))
    (fp_line (start -2.12 -2.12) (end -2.12 2.12) (layer "F.SilkS") (width 0.12) (tstamp 749dfe75-c0d6-4872-9330-29c5bbcb8ff8))
    (fp_line (start -2.12 -2.12) (end 11.12 -2.12) (layer "F.SilkS") (width 0.12) (tstamp eb667eea-300e-4ca7-8a6f-4b00de80cd45))
    (fp_line (start -2.25 2.25) (end 11.25 2.25) (layer "F.CrtYd") (width 0.05) (tstamp 1e1b062d-fad0-427c-a622-c5b8a80b5268))
    (fp_line (start 11.25 -2.25) (end -2.25 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp 30f15357-ce1d-48b9-93dc-7d9b1b2aa048))
    (fp_line (start -2.25 -2.25) (end -2.25 2.25) (layer "F.CrtYd") (width 0.05) (tstamp cbdcaa78-3bbc-413f-91bf-2709119373ce))
    (fp_line (start 11.25 2.25) (end 11.25 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp d8603679-3e7b-4337-8dbc-1827f5f54d8a))
    (fp_line (start 11 -2) (end -2 -2) (layer "F.Fab") (width 0.1) (tstamp 44d8279a-9cd1-4db6-856f-0363131605fc))
    (fp_line (start -2 2) (end 11 2) (layer "F.Fab") (width 0.1) (tstamp 4fb02e58-160a-4a39-9f22-d0c75e82ee72))
    (fp_line (start -2 -2) (end -2 2) (layer "F.Fab") (width 0.1) (tstamp e615f7aa-337e-474d-9615-2ad82b1c44ca))
    (fp_line (start 11 2) (end 11 -2) (layer "F.Fab") (width 0.1) (tstamp ef8fe2ac-6a7f-4682-9418-b801a1b10a3b))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 5038e144-5119-49db-b6cf-f7c345f1cf03))
    (pad "2" thru_hole circle locked (at 9 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 2e642b3e-a476-4c54-9a52-dcea955640cd))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Box_L13.0mm_W4.0mm_P9.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_2.1mm" (layer "F.Cu")
    (tedit 5B924765) (tstamp 00000000-0000-0000-0000-00005ebe1aa4)
    (at 120 29)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bb7f0588-d4d8-44bf-9ebf-3c533fe4d6ae)
    )
    (fp_text value "MountingHole_2.1mm" (at 0 3.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f1830a1b-f0cc-47ae-a2c9-679c82032f14)
    )
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e10b5627-3247-4c86-b9f6-ef474ca11543)
    )
    (fp_circle (center 0 0) (end 2.1 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 6a955fc7-39d9-4c75-9a69-676ca8c0b9b2))
    (fp_circle (center 0 0) (end 2.35 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp e8314017-7be6-4011-9179-37449a29b311))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask) (tstamp 746ba970-8279-4e7b-aed3-f28687777c21))
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005ea76de9)
    (at 110 35 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "R2" (at 0 1.65 -90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp efeac2a2-7682-4dc7-83ee-f6f1b23da506)
    )
    (fp_text value "R_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (at 0 -1.65 -90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5fc27c35-3e1c-4f96-817c-93b5570858a6)
    )
    (fp_text user "150" (at 0 0 -90) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 0eaa98f0-9565-4637-ace3-42a5231b07f7)
    )
    (fp_line (start -0.261252 0.71) (end 0.261252 0.71) (layer "B.SilkS") (width 0.12) (tstamp 127679a9-3981-4934-815e-896a4e3ff56e))
    (fp_line (start -0.261252 -0.71) (end 0.261252 -0.71) (layer "B.SilkS") (width 0.12) (tstamp 48ab88d7-7084-4d02-b109-3ad55a30bb11))
    (fp_line (start 1.85 -0.95) (end -1.85 -0.95) (layer "B.CrtYd") (width 0.05) (tstamp 704d6d51-bb34-4cbf-83d8-841e208048d8))
    (fp_line (start 1.85 0.95) (end 1.85 -0.95) (layer "B.CrtYd") (width 0.05) (tstamp 8174b4de-74b1-48db-ab8e-c8432251095b))
    (fp_line (start -1.85 -0.95) (end -1.85 0.95) (layer "B.CrtYd") (width 0.05) (tstamp f71da641-16e6-4257-80c3-0b9d804fee4f))
    (fp_line (start -1.85 0.95) (end 1.85 0.95) (layer "B.CrtYd") (width 0.05) (tstamp fd470e95-4861-44fe-b1e4-6d8a7c66e144))
    (fp_line (start -1 0.6) (end 1 0.6) (layer "B.Fab") (width 0.1) (tstamp 6a45789b-3855-401f-8139-3c734f7f52f9))
    (fp_line (start -1 -0.6) (end -1 0.6) (layer "B.Fab") (width 0.1) (tstamp 6c9b793c-e74d-4754-a2c0-901e73b26f1c))
    (fp_line (start 1 -0.6) (end -1 -0.6) (layer "B.Fab") (width 0.1) (tstamp 716e31c5-485f-40b5-88e3-a75900da9811))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer "B.Fab") (width 0.1) (tstamp b1086f75-01ba-4188-8d36-75a9e2828ca9))
    (pad "1" smd roundrect locked (at -1.025 0 270) (size 1.15 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391) (tstamp ce83728b-bebd-48c2-8734-b6a50d837931))
    (pad "2" smd roundrect locked (at 1.025 0 270) (size 1.15 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391) (tstamp 181abe7a-f941-42b6-bd46-aaa3131f90fb))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 100 25) (end 100 50) (layer "Edge.Cuts") (width 0.05) (tstamp 00000000-0000-0000-0000-00005ea7192f))
  (gr_line (start 125 25) (end 125 50) (layer "Edge.Cuts") (width 0.05) (tstamp 00000000-0000-0000-0000-00005ea76efc))
  (gr_line (start 100 25) (end 125 25) (layer "Edge.Cuts") (width 0.05) (tstamp 00000000-0000-0000-0000-00005ea76f1d))
  (gr_line (start 100 50) (end 125 50) (layer "Edge.Cuts") (width 0.05) (tstamp 1a1ab354-5f85-45f9-938c-9f6c4c8c3ea2))

  (via (at 117 34) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (free) (net 0) (tstamp 240c10af-51b5-420e-a6f4-a2c8f5db1db5))
  (via blind (at 119.25 37.75) (size 0.8) (drill 0.4) (layers "F.Cu" "In1.Cu") (net 0) (tstamp 97fe9c60-586f-4895-8504-4d3729f5f81a))
  (via blind (at 117.5 36.25) (size 0.8) (drill 0.4) (layers "F.Cu" "In2.Cu") (net 0) (tstamp bdc7face-9f7c-4701-80bb-4cc144448db1))
  (via blind (at 120.75 36.25) (size 0.8) (drill 0.4) (layers "In1.Cu" "In2.Cu") (net 0) (tstamp 922058ca-d09a-45fd-8394-05f3e2c1e03a))
  (via blind (at 119.25 34.5) (size 0.8) (drill 0.4) (layers "In2.Cu" "B.Cu") (net 0) (tstamp 0f54db53-a272-4955-88fb-d7ab00657bb0))

)
