(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "GND")
  (net 3 "Net-(C2-Pad1)")

  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0) (tstamp 41b35754-3436-421e-8e97-e439c06d466b)
    (at 113 80 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "Archivo: ../Circuit/1_SCH_2_diff_PCBs.kicad_sch")
    (property "Sheetname" "Rectangular PCB")
    (path "/7492e407-3dca-4dd2-a436-008a743b6181/e5e3dd91-4c50-4c56-a840-8fe41b627763")
    (attr through_hole)
    (fp_text reference "C1" (at 1.25 -2.05 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 08c2dbd0-b20e-427f-850b-d26a49b96708)
    )
    (fp_text value "100nF" (at 1.25 2.05 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a452f3a2-f96f-4470-8848-1fbb42e4b3a3)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab")
      (effects (font (size 0.6 0.6) (thickness 0.09)))
      (tstamp 19b8e498-5d0e-4185-af39-4badca486632)
    )
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer "F.SilkS") (width 0.12) (tstamp 5e2ece88-568e-458b-b8ea-c07133f1d4d7))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer "F.SilkS") (width 0.12) (tstamp e72ecbaf-f274-436e-8498-7c0370d8c755))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 854cf4b1-450e-45e1-b2c2-daad992d9bfd))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer "F.CrtYd") (width 0.05) (tstamp aa59dec6-193f-43d6-a3bc-26f86b40af91))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp b3b5d975-52e6-4d3d-8614-20e148fd5f81))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer "F.CrtYd") (width 0.05) (tstamp ee5a509b-aea9-45a8-9432-271fceb31f27))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer "F.Fab") (width 0.1) (tstamp 07c61673-831d-483b-b26b-6247848aef5d))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer "F.Fab") (width 0.1) (tstamp 1edac835-60bc-4270-ac43-b3b888cfc25e))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer "F.Fab") (width 0.1) (tstamp 44ff8250-4314-44fe-93a1-895b162917f0))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer "F.Fab") (width 0.1) (tstamp ca5c034e-b7ca-48af-8aa9-33bcf68a1c75))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pintype "passive") (tstamp 5964a391-922f-4450-ab49-1332821c5fac))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive") (tstamp 4b530baa-390d-495f-bba2-ace611285a6c))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B) (tstamp 765f88e2-9221-4279-9adb-a8c1e33eaf45)
    (at 96 77 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Sheetfile" "Archivo: ../Circuit/1_SCH_2_diff_PCBs.kicad_sch")
    (property "Sheetname" "Rectangular PCB")
    (path "/7492e407-3dca-4dd2-a436-008a743b6181/c00eaf45-c1bf-4fcf-9758-e056d0bcad77")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -4.12 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 369fe5a5-80ed-4666-8851-628dc866367c)
    )
    (fp_text value "In" (at 1.27 4.08 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 419bd830-2094-4a1d-a157-ca846131a85a)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.22 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 585c473b-2c2e-4069-ad4f-5e7a3a9533c7)
    )
    (fp_line (start 0.8 -2.43) (end 0.8 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 03b2c50b-4587-427d-823c-66dd59a4998a))
    (fp_line (start 3.92 -3.03) (end -1.38 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 0ba7f1a4-e81b-4204-a2c1-8fe18263fe33))
    (fp_line (start 2.29 1.46) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp 11441018-0b85-4a0a-b8f5-1e4680b2e76c))
    (fp_line (start 1.74 -3.03) (end 1.74 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 1a9a1135-815f-479b-a062-a15198173e77))
    (fp_line (start 0 2.99) (end 0 1.99) (layer "F.SilkS") (width 0.12) (tstamp 2640073f-096f-4560-a244-23a6d6d01fc4))
    (fp_line (start 2.29 2.99) (end 2.29 1.99) (layer "F.SilkS") (width 0.12) (tstamp 3199a94f-c425-4237-8048-9b4939015bbf))
    (fp_line (start 3.92 2.99) (end 3.92 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 3e139896-9f62-4f03-afb9-9a25ca972489))
    (fp_line (start 1.74 -2.43) (end 3.34 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 59991c57-c699-422c-af72-d4455bc0ed97))
    (fp_line (start 0.25 1.46) (end 2.29 1.46) (layer "F.SilkS") (width 0.12) (tstamp 5b64d5a7-6395-40e9-8d6f-61e419a6b5ee))
    (fp_line (start -0.8 -2.43) (end 0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 773ed370-ffa6-4d1e-abe3-ce7a4de62d50))
    (fp_line (start 3.34 -2.43) (end 3.34 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 893441ca-ddad-4a92-898d-8339b8374b70))
    (fp_line (start -1.38 -3.03) (end -1.38 2.99) (layer "F.SilkS") (width 0.12) (tstamp 98b90646-16c0-40ef-900f-08ef6eddff07))
    (fp_line (start -1.38 2.99) (end 3.92 2.99) (layer "F.SilkS") (width 0.12) (tstamp b02dd231-7812-4695-b5dd-6ccfd8cb6136))
    (fp_line (start 0 1.99) (end 0.25 1.46) (layer "F.SilkS") (width 0.12) (tstamp bd6ea34a-e849-4db6-a213-5c746730001f))
    (fp_line (start 0.25 2.99) (end 0.25 1.99) (layer "F.SilkS") (width 0.12) (tstamp c37068b5-87ee-4d97-8c78-b7cc7c255d7b))
    (fp_line (start -1.67 -2) (end -1.67 2) (layer "F.SilkS") (width 0.12) (tstamp ed810b7e-9704-4dea-a51b-84114a32ba7e))
    (fp_line (start 0 1.99) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp f1422576-1cd7-4452-a36c-2bcbbc13e7fc))
    (fp_line (start -0.8 -3.03) (end -0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp f3628542-e328-44d0-9671-ad87db5bc469))
    (fp_line (start 2.54 1.99) (end 2.54 2.99) (layer "F.SilkS") (width 0.12) (tstamp f98bffdc-bcb7-4516-aaa0-50d1305e8434))
    (fp_line (start -1.77 -3.42) (end -1.77 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 5183f7dd-bdf2-46c2-a8d3-70e6b3cdd9a7))
    (fp_line (start -1.77 3.38) (end 4.31 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 915b6630-c87d-4d52-8fd8-9604dfd32c2f))
    (fp_line (start 4.31 3.38) (end 4.31 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp 99ef533a-3872-43ed-a171-bfc73ba567df))
    (fp_line (start 4.31 -3.42) (end -1.77 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp efd43026-649f-4b9c-b927-37de9cdd270e))
    (fp_line (start -1.27 2.88) (end 3.81 2.88) (layer "F.Fab") (width 0.1) (tstamp 38ac4a04-ac19-4eb0-8a1c-af95fa1afec0))
    (fp_line (start 3.81 2.88) (end 3.81 -2.92) (layer "F.Fab") (width 0.1) (tstamp 449ba773-a017-4509-8e15-48a80c141315))
    (fp_line (start 3.81 -2.92) (end -1.27 -2.92) (layer "F.Fab") (width 0.1) (tstamp 5d65aab4-09f9-448f-8648-2d28191a5f61))
    (fp_line (start -1.27 -2.92) (end -1.27 2.88) (layer "F.Fab") (width 0.1) (tstamp c9a602ea-e148-4ace-83a7-f619846c0ba4))
    (fp_line (start -1.27 -0.5) (end -0.562893 0) (layer "F.Fab") (width 0.1) (tstamp d3406c10-29ee-4e2d-8a74-a2701dbeff69))
    (fp_line (start -0.562893 0) (end -1.27 0.5) (layer "F.Fab") (width 0.1) (tstamp e6ac6504-0a44-49b4-923b-5b563d70a982))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp ef5447f3-ea75-481c-bfb2-14230a7e69f3))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 629f23d7-4a2f-4aa4-91c4-83bee755387a))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B) (tstamp c5d62daa-1d12-476a-a0af-75d2259e9021)
    (at 121 75 -90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Sheetfile" "Archivo: ../Circuit/1_SCH_2_diff_PCBs.kicad_sch")
    (property "Sheetname" "Rectangular PCB")
    (path "/7492e407-3dca-4dd2-a436-008a743b6181/1a0b04d9-cdf4-4256-b39a-932f9cef60f9")
    (attr through_hole)
    (fp_text reference "J2" (at 1.27 -4.12 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 52da7d98-bd6e-49f1-9e88-a9232fadd658)
    )
    (fp_text value "Out" (at 1.27 4.08 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 74ea6877-6d94-497c-87cd-775580ade2e9)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.22 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 60c41d8f-7c0e-4c90-a416-8dc05de6c4e4)
    )
    (fp_line (start 0.25 2.99) (end 0.25 1.99) (layer "F.SilkS") (width 0.12) (tstamp 0f54df95-66b9-4ab1-8217-548cb250bfde))
    (fp_line (start 2.54 1.99) (end 2.54 2.99) (layer "F.SilkS") (width 0.12) (tstamp 153e5de4-68c4-442d-8dd7-0303d93239aa))
    (fp_line (start 0.8 -2.43) (end 0.8 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 15853617-a054-46ba-968a-220ce947c78e))
    (fp_line (start 3.34 -2.43) (end 3.34 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 28837c69-511c-4905-8e35-bf45480d1e0c))
    (fp_line (start -1.38 2.99) (end 3.92 2.99) (layer "F.SilkS") (width 0.12) (tstamp 465b1804-a776-4901-bf4d-5f0b995530c6))
    (fp_line (start 1.74 -2.43) (end 3.34 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 482edf92-fd8d-4e97-a3ac-9a4511280f0c))
    (fp_line (start -1.67 -2) (end -1.67 2) (layer "F.SilkS") (width 0.12) (tstamp 55442735-18e5-4b64-9fa6-4c6888bd5e36))
    (fp_line (start 2.29 2.99) (end 2.29 1.99) (layer "F.SilkS") (width 0.12) (tstamp 5f87f70a-d3a6-4252-9d7c-599c17a7082b))
    (fp_line (start 2.29 1.46) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp 6b9da7af-f3af-40ab-b5db-ede099d88c87))
    (fp_line (start 0 1.99) (end 0.25 1.46) (layer "F.SilkS") (width 0.12) (tstamp 8ddc6c2a-f0ea-434a-9936-3e33f852b1b0))
    (fp_line (start 0 2.99) (end 0 1.99) (layer "F.SilkS") (width 0.12) (tstamp 97bc9146-8384-42e6-860b-9e26c847f5a1))
    (fp_line (start 0 1.99) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp 97dbd656-533d-4304-9c53-b7e7dbaf4f65))
    (fp_line (start 3.92 -3.03) (end -1.38 -3.03) (layer "F.SilkS") (width 0.12) (tstamp a5b1834f-93c3-4ed3-bddf-de3f5898c645))
    (fp_line (start 0.25 1.46) (end 2.29 1.46) (layer "F.SilkS") (width 0.12) (tstamp af523ed7-0a17-4527-a4c7-0bf7cebbebd1))
    (fp_line (start -0.8 -3.03) (end -0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp c4a7ff55-45b3-4c06-884c-e9a276f0dc21))
    (fp_line (start -0.8 -2.43) (end 0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp ce831e63-1c43-42ca-9310-693bcaa4b7dd))
    (fp_line (start -1.38 -3.03) (end -1.38 2.99) (layer "F.SilkS") (width 0.12) (tstamp d2a174f8-1e84-451a-b002-41ea0a981c09))
    (fp_line (start 3.92 2.99) (end 3.92 -3.03) (layer "F.SilkS") (width 0.12) (tstamp d3d6100b-00d2-4e0f-abb1-cd1985b1c5a0))
    (fp_line (start 1.74 -3.03) (end 1.74 -2.43) (layer "F.SilkS") (width 0.12) (tstamp f3534492-4903-4cf3-80c4-1a48570c6522))
    (fp_line (start -1.77 3.38) (end 4.31 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 0403ff10-5feb-4c9a-aaee-5e25ab331d06))
    (fp_line (start 4.31 3.38) (end 4.31 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp 54428092-56e2-4b01-926d-a185cdbfc805))
    (fp_line (start -1.77 -3.42) (end -1.77 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 7dac2776-4934-408f-a4ea-e959502716b0))
    (fp_line (start 4.31 -3.42) (end -1.77 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp bee7296f-4e3f-4bd0-8c87-c65a7108f4ff))
    (fp_line (start 3.81 2.88) (end 3.81 -2.92) (layer "F.Fab") (width 0.1) (tstamp 05e34374-ee99-4321-b4bb-c067d042ce23))
    (fp_line (start -0.562893 0) (end -1.27 0.5) (layer "F.Fab") (width 0.1) (tstamp 0c007eb5-a8f8-463e-b463-2cb5ec34c39a))
    (fp_line (start 3.81 -2.92) (end -1.27 -2.92) (layer "F.Fab") (width 0.1) (tstamp 58c0941a-de12-48b5-82db-1812584eb921))
    (fp_line (start -1.27 2.88) (end 3.81 2.88) (layer "F.Fab") (width 0.1) (tstamp 69b6fb7c-59f0-4c1e-806c-5db257536a17))
    (fp_line (start -1.27 -0.5) (end -0.562893 0) (layer "F.Fab") (width 0.1) (tstamp 9c671494-55c6-482d-bf48-bd2a49fdffe4))
    (fp_line (start -1.27 -2.92) (end -1.27 2.88) (layer "F.Fab") (width 0.1) (tstamp a20c2208-5d1e-4a91-bd7a-8a1b28613d25))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 3 "Net-(C2-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp c5da4566-0495-4b35-8b20-376a196c2b0b))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive") (tstamp 7395030b-ef32-4b91-8ce8-82b0e2c1e089))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0) (tstamp ec5754c9-7c4d-41c1-91e6-ccfe035e3755)
    (at 103 72 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "Archivo: ../Circuit/1_SCH_2_diff_PCBs.kicad_sch")
    (property "Sheetname" "Rectangular PCB")
    (path "/7492e407-3dca-4dd2-a436-008a743b6181/121f51f7-01c0-4925-9aad-c45a8d3be012")
    (attr through_hole)
    (fp_text reference "C2" (at 1.25 -2.05 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 91e67699-8aac-48b7-872a-1e94332e143d)
    )
    (fp_text value "100nF" (at 1.25 2.05 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9fa42677-7ea1-480b-aa90-f1ad247d14e8)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab")
      (effects (font (size 0.6 0.6) (thickness 0.09)))
      (tstamp 08b2da83-fea3-45a4-a42e-ac94e8f74846)
    )
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer "F.SilkS") (width 0.12) (tstamp 52e0075a-e6d7-4ed5-a59f-6eb8cb01f259))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer "F.SilkS") (width 0.12) (tstamp a26b42c2-05e7-4d06-8117-583ec7b95499))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 02c95094-6885-4a9e-b407-b86150ed7e6c))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 04cb84f5-3a63-4423-a08e-b95c74eb3b1f))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 2ba6d4a2-952f-4fae-b7a0-5c5dc0cacf14))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 81b2763e-6ea0-4486-9764-f501155f2028))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer "F.Fab") (width 0.1) (tstamp 5742d35b-37a1-4086-a71f-470af97fe952))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer "F.Fab") (width 0.1) (tstamp 935e7ceb-6af4-44a3-a233-3ac43ebde1af))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer "F.Fab") (width 0.1) (tstamp aecdb3aa-7aca-41bc-a341-5bf55f707c69))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer "F.Fab") (width 0.1) (tstamp e8a52d9f-2b4c-43da-9469-59fb3e8eaa05))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pintype "passive") (tstamp aa7a3ce3-726c-4230-9fe5-5448984ac7ab))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive") (tstamp c95b9382-9c81-4675-a4fd-7527fecad7bb))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp f728367f-d1db-4f86-af45-3bc3b2ae3a0d)
    (at 108 72.19 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Archivo: ../Circuit/1_SCH_2_diff_PCBs.kicad_sch")
    (property "Sheetname" "Rectangular PCB")
    (path "/7492e407-3dca-4dd2-a436-008a743b6181/5ff51348-3b0c-4051-ac3f-8bbe52a23b46")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -2.37 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b37f84d7-6c8e-45d8-bff1-946d7e5214b9)
    )
    (fp_text value "1k" (at 3.81 2.37 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a502f24-5e5d-4b4f-b3a2-aceb9f9df836)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a6cbac0b-4533-4500-85ec-ae558c5366d3)
    )
    (fp_line (start 0.54 -1.37) (end 7.08 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 36d19a18-a019-4448-8e9c-9167af791abd))
    (fp_line (start 0.54 1.37) (end 7.08 1.37) (layer "F.SilkS") (width 0.12) (tstamp 71800483-b3c2-4cd3-954f-8a3045c395d2))
    (fp_line (start 7.08 -1.37) (end 7.08 -1.04) (layer "F.SilkS") (width 0.12) (tstamp 83077f1e-8491-4c4f-abb4-72742728df54))
    (fp_line (start 7.08 1.37) (end 7.08 1.04) (layer "F.SilkS") (width 0.12) (tstamp aaf1b9db-e6dd-4034-9028-2f2a305599bc))
    (fp_line (start 0.54 -1.04) (end 0.54 -1.37) (layer "F.SilkS") (width 0.12) (tstamp b0166c5f-0d97-4dfe-b3a5-52b0ac042004))
    (fp_line (start 0.54 1.04) (end 0.54 1.37) (layer "F.SilkS") (width 0.12) (tstamp fd6fd013-462b-4729-84ba-b9287fd06e54))
    (fp_line (start 8.67 1.5) (end 8.67 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp c5f43f8f-2f77-4db0-bf7c-19dd9b415422))
    (fp_line (start -1.05 1.5) (end 8.67 1.5) (layer "F.CrtYd") (width 0.05) (tstamp cfe5f03d-ad17-45b7-a291-e4a7b300220a))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp db7202ba-8089-4c93-802a-f3c559a29e38))
    (fp_line (start 8.67 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp e2e25113-d526-4fa3-ab69-f059c3fd688e))
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer "F.Fab") (width 0.1) (tstamp 5cecc5f1-0f10-400c-8369-80c905f6372f))
    (fp_line (start 7.62 0) (end 6.96 0) (layer "F.Fab") (width 0.1) (tstamp 7b378867-2328-4453-940f-c16f050b2f3d))
    (fp_line (start 0 0) (end 0.66 0) (layer "F.Fab") (width 0.1) (tstamp 88ede3ad-82c5-45ea-a847-a9cca9b593b4))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer "F.Fab") (width 0.1) (tstamp a1d0722a-c2b2-4dae-9b3d-0c27ea6af527))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer "F.Fab") (width 0.1) (tstamp c57cb1c8-a50d-4c62-a67f-294dc04b4b27))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer "F.Fab") (width 0.1) (tstamp f9afe1a9-3470-447a-864b-43c4a60bc3d6))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pintype "passive") (tstamp 7113b6a2-6e2f-4aff-8dcb-a918da60d100))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pintype "passive") (tstamp ed50c35f-ece0-4c86-a4e1-7b16b3100d46))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 90 70) (end 127 82) (layer "Edge.Cuts") (width 0.1) (fill none) (tstamp ec14ee5a-801c-4365-a5d0-240d306c7603))

  (segment (start 96 74.46) (end 94.58 75.88) (width 1) (layer "B.Cu") (net 1) (tstamp 01743757-5c41-4baf-a345-c7bdc7f731f6))
  (segment (start 94.58 78.58) (end 95.81 79.81) (width 1) (layer "B.Cu") (net 1) (tstamp 9af469f9-0452-4755-bd29-34123bb2ee27))
  (segment (start 108 79.81) (end 112.81 79.81) (width 1) (layer "B.Cu") (net 1) (tstamp 9caa0b96-8dfa-4c2a-8304-e998fd63a128))
  (segment (start 94.58 75.88) (end 94.58 78.58) (width 1) (layer "B.Cu") (net 1) (tstamp b6be5042-4447-4c9b-80b1-240574cb0955))
  (segment (start 112.81 79.81) (end 113 80) (width 0.25) (layer "B.Cu") (net 1) (tstamp ddb1e783-67ef-44d4-bf58-4e5d55c79923))
  (segment (start 95.81 79.81) (end 108 79.81) (width 1) (layer "B.Cu") (net 1) (tstamp ff2893c5-7e63-4c60-9851-199d2c7c5ca2))
  (segment (start 110 74.5) (end 113 77.5) (width 1) (layer "B.Cu") (net 2) (tstamp 75063c2c-e531-404a-bc31-23a74138de09))
  (segment (start 100.5 77) (end 103 74.5) (width 1) (layer "B.Cu") (net 2) (tstamp 91f0706e-ee29-4fba-8648-26333e449672))
  (segment (start 103 74.5) (end 110 74.5) (width 1) (layer "B.Cu") (net 2) (tstamp c1445ad8-2505-4469-b4f6-e8e54a058685))
  (segment (start 113 77.5) (end 120.96 77.5) (width 1) (layer "B.Cu") (net 2) (tstamp d2e305f2-a168-4a93-b266-e256385a831d))
  (segment (start 120.96 77.5) (end 121 77.54) (width 0.25) (layer "B.Cu") (net 2) (tstamp e7cdf359-c91d-4419-98a6-4e34872b550c))
  (segment (start 96 77) (end 100.5 77) (width 1) (layer "B.Cu") (net 2) (tstamp e7e28fe2-ae42-48f2-9a95-e90c06575187))
  (segment (start 103 72) (end 107.81 72) (width 1) (layer "B.Cu") (net 3) (tstamp 35f76f3a-96c6-44d9-a166-031d75cad7ea))
  (segment (start 108 72.19) (end 118.19 72.19) (width 1) (layer "B.Cu") (net 3) (tstamp 40bff48e-b9a3-40f8-8893-e772009fbd60))
  (segment (start 118.19 72.19) (end 121 75) (width 1) (layer "B.Cu") (net 3) (tstamp c3023bf0-4124-49c5-aba6-17451a9d5538))
  (segment (start 107.81 72) (end 108 72.19) (width 0.25) (layer "B.Cu") (net 3) (tstamp c9c50760-e71f-4863-ae39-e2dfacebb335))

)
