(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (title_block
    (title "Filter A + B")
  )

  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin -119.5 -79)
    (grid_origin -119.5 -79)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Board_0-Net-(C1-Pad1)")
  (net 2 "Board_0-Net-(C2-Pad1)")
  (net 3 "Board_0-Net-(J1-Pad2)")

  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B) (tstamp 47635cfa-6076-40c4-8899-161b5df14b79)
    (at 20 20.54 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Sheetfile" "Archivo: KiKit_1.kicad_sch")
    (property "Sheetname" "")
    (path "/c2e186cd-5f00-475d-b708-2a8e8b8453a6")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -4.12 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4d26bc9d-35ed-4434-8497-e0b6b2543cfc)
    )
    (fp_text value "In" (at 1.27 4.08 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3ca5da9a-b675-4bb4-91ad-c8085ca13c5a)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.22 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ad144da7-03b3-433c-a6f8-cc6de8b40a3c)
    )
    (fp_line (start -1.38 -3.03) (end -1.38 2.99) (layer "F.SilkS") (width 0.12) (tstamp 04ed3202-291b-473d-a34e-07725d73eb31))
    (fp_line (start -0.8 -2.43) (end 0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 208f9250-0554-4e28-9bd0-8daeb5ff2ac4))
    (fp_line (start 0.25 2.99) (end 0.25 1.99) (layer "F.SilkS") (width 0.12) (tstamp 3ddf72f8-106d-42df-9e6f-1db51463bf64))
    (fp_line (start 0.25 1.46) (end 2.29 1.46) (layer "F.SilkS") (width 0.12) (tstamp 50556d84-73c9-4daf-b187-c20ff01f0ad8))
    (fp_line (start 0.8 -2.43) (end 0.8 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 53dd8d1f-bbc8-4634-9446-895566e78cc3))
    (fp_line (start 3.92 2.99) (end 3.92 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 5523e69d-fd9d-4150-be8c-cadc13a08028))
    (fp_line (start 0 1.99) (end 0.25 1.46) (layer "F.SilkS") (width 0.12) (tstamp 67571fa3-44d8-4b37-8e0c-aba768334821))
    (fp_line (start 2.54 1.99) (end 2.54 2.99) (layer "F.SilkS") (width 0.12) (tstamp 689933d9-8217-4b94-a287-dfb25d14bc30))
    (fp_line (start -1.38 2.99) (end 3.92 2.99) (layer "F.SilkS") (width 0.12) (tstamp 6a6ef22e-752d-47e9-8d91-ec32349d3a9d))
    (fp_line (start 0 2.99) (end 0 1.99) (layer "F.SilkS") (width 0.12) (tstamp 71a70de4-134f-4164-b061-761a44eddf25))
    (fp_line (start -0.8 -3.03) (end -0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 9bfe899b-3764-4111-b467-0e920b8308c1))
    (fp_line (start 3.34 -2.43) (end 3.34 -3.03) (layer "F.SilkS") (width 0.12) (tstamp a3e01c14-07e5-498f-8ecb-4061989a0b7f))
    (fp_line (start 1.74 -3.03) (end 1.74 -2.43) (layer "F.SilkS") (width 0.12) (tstamp a4b12d00-7373-43d2-92cc-62c9b4ce8fed))
    (fp_line (start 2.29 1.46) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp aad2056b-1df0-49f6-a71b-9a195e6e3d58))
    (fp_line (start 0 1.99) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp b636bf64-1121-4285-81f9-daa96d6d74e5))
    (fp_line (start 3.92 -3.03) (end -1.38 -3.03) (layer "F.SilkS") (width 0.12) (tstamp bd926564-e549-42cd-b2f1-dcc3afa5eb58))
    (fp_line (start -1.67 -2) (end -1.67 2) (layer "F.SilkS") (width 0.12) (tstamp cef66ca2-8791-46ce-9c8d-5bba69777e2f))
    (fp_line (start 1.74 -2.43) (end 3.34 -2.43) (layer "F.SilkS") (width 0.12) (tstamp e223325d-6924-4336-8802-3cea2a5577b0))
    (fp_line (start 2.29 2.99) (end 2.29 1.99) (layer "F.SilkS") (width 0.12) (tstamp f6143f84-c2d0-4736-b008-e384e82ac8e0))
    (fp_line (start 4.31 3.38) (end 4.31 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp 00138e3b-fdcf-46b0-8b0f-dc80bc463731))
    (fp_line (start 4.31 -3.42) (end -1.77 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp 3ec9a330-72af-42c9-bd8f-cae812fe3b10))
    (fp_line (start -1.77 3.38) (end 4.31 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 99ad30c7-b0d7-47b7-ac9a-df5acdfab9a9))
    (fp_line (start -1.77 -3.42) (end -1.77 3.38) (layer "F.CrtYd") (width 0.05) (tstamp fecf7588-5455-4b24-94ef-1810f8e9eb64))
    (fp_line (start -1.27 2.88) (end 3.81 2.88) (layer "F.Fab") (width 0.1) (tstamp 1233cc5f-2281-4d59-ac74-b98e9fbdbbd9))
    (fp_line (start -1.27 -2.92) (end -1.27 2.88) (layer "F.Fab") (width 0.1) (tstamp 9c022f8d-69ea-4bc6-be0e-6f542179fdac))
    (fp_line (start -1.27 -0.5) (end -0.562893 0) (layer "F.Fab") (width 0.1) (tstamp d04cabc1-0420-414f-a375-c9489fbb70cd))
    (fp_line (start 3.81 -2.92) (end -1.27 -2.92) (layer "F.Fab") (width 0.1) (tstamp e65ab8ad-5e3c-459b-b8b0-9c0db703d94f))
    (fp_line (start 3.81 2.88) (end 3.81 -2.92) (layer "F.Fab") (width 0.1) (tstamp ecefc270-8be9-4f3c-81fa-ebbb22e0702a))
    (fp_line (start -0.562893 0) (end -1.27 0.5) (layer "F.Fab") (width 0.1) (tstamp ef1f70be-d126-4ad1-ba2c-54eda65a92fc))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 1 "Board_0-Net-(C1-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp c8c55f89-e4dc-4d49-90ce-c174d3eb342c))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 3 "Board_0-Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp b97c00b8-2110-4032-b964-dba24013fd07))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B) (tstamp 4d69c3f1-8468-4248-aa57-8829874afdbb)
    (at 41 18 -90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Sheetfile" "Archivo: KiKit_1.kicad_sch")
    (property "Sheetname" "")
    (path "/f72353ed-bcd3-4a4b-8876-c4bbda278908")
    (attr through_hole)
    (fp_text reference "J2" (at 1.27 -4.12 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1a1e9ce1-352e-410c-99db-a920cbd931a5)
    )
    (fp_text value "Out" (at 1.27 4.08 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 092c671e-e4e2-4e86-8804-05b1b7104de3)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.22 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b7413663-7e9a-4603-a969-830b3498315d)
    )
    (fp_line (start 0.8 -2.43) (end 0.8 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 1539aa7f-3be9-46a3-b870-0cb7fa99889c))
    (fp_line (start -1.67 -2) (end -1.67 2) (layer "F.SilkS") (width 0.12) (tstamp 2827edae-4833-4b67-842b-169e7db8cd41))
    (fp_line (start 3.92 2.99) (end 3.92 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 43ab4c06-aee1-4818-a557-1ed688f375b5))
    (fp_line (start -0.8 -3.03) (end -0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 54b30116-98f1-4950-80ea-de6beb711bc1))
    (fp_line (start 0.25 1.46) (end 2.29 1.46) (layer "F.SilkS") (width 0.12) (tstamp 564c3759-eb3b-4d2f-b206-48d21a1e8bf2))
    (fp_line (start -0.8 -2.43) (end 0.8 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 613c08c5-30e3-443e-a451-b1694d0452f8))
    (fp_line (start 3.92 -3.03) (end -1.38 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 7b12c631-83bf-43dc-9f6a-3d9d6feaf1ec))
    (fp_line (start 0 2.99) (end 0 1.99) (layer "F.SilkS") (width 0.12) (tstamp 7d69e6b5-385f-4f88-9f8a-e08e356ab1b4))
    (fp_line (start 1.74 -2.43) (end 3.34 -2.43) (layer "F.SilkS") (width 0.12) (tstamp 817c76c2-a946-417c-a60d-46fe7ac2c7ab))
    (fp_line (start 0.25 2.99) (end 0.25 1.99) (layer "F.SilkS") (width 0.12) (tstamp 82f6f992-de86-4d42-9860-cedf41fd750b))
    (fp_line (start -1.38 2.99) (end 3.92 2.99) (layer "F.SilkS") (width 0.12) (tstamp 91849060-0ab6-4cfa-9fae-72bbca42a913))
    (fp_line (start 0 1.99) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp 92126db9-219b-4284-bdae-51e4043a6581))
    (fp_line (start 3.34 -2.43) (end 3.34 -3.03) (layer "F.SilkS") (width 0.12) (tstamp 95fbd477-88ec-4f1b-aa75-f7870564eecc))
    (fp_line (start 2.29 2.99) (end 2.29 1.99) (layer "F.SilkS") (width 0.12) (tstamp a3a165ce-64a0-453f-8e93-2899b9ae435f))
    (fp_line (start 0 1.99) (end 0.25 1.46) (layer "F.SilkS") (width 0.12) (tstamp a8222bd5-bd2d-4fda-b693-a375bfd3b06e))
    (fp_line (start 2.54 1.99) (end 2.54 2.99) (layer "F.SilkS") (width 0.12) (tstamp b6bbb375-694c-45ad-ac59-e54539bb98c6))
    (fp_line (start -1.38 -3.03) (end -1.38 2.99) (layer "F.SilkS") (width 0.12) (tstamp d4a17956-159d-44eb-a532-84c6237b3c19))
    (fp_line (start 1.74 -3.03) (end 1.74 -2.43) (layer "F.SilkS") (width 0.12) (tstamp dde96444-ce61-492d-827c-ff8240956a21))
    (fp_line (start 2.29 1.46) (end 2.54 1.99) (layer "F.SilkS") (width 0.12) (tstamp fce3ffcd-2f07-4dba-9702-cc50b67537ff))
    (fp_line (start -1.77 3.38) (end 4.31 3.38) (layer "F.CrtYd") (width 0.05) (tstamp 3e829f57-f498-42c2-957b-9374c8c4da79))
    (fp_line (start 4.31 3.38) (end 4.31 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp 66d38760-f894-4808-be5e-b57f7486c9b9))
    (fp_line (start -1.77 -3.42) (end -1.77 3.38) (layer "F.CrtYd") (width 0.05) (tstamp baf3910f-6a4f-4c1c-a939-ae43a1889a77))
    (fp_line (start 4.31 -3.42) (end -1.77 -3.42) (layer "F.CrtYd") (width 0.05) (tstamp bf0dee9c-28bf-46a9-8610-9db026946d4a))
    (fp_line (start 3.81 2.88) (end 3.81 -2.92) (layer "F.Fab") (width 0.1) (tstamp 2b7f326d-07bf-410c-8a9b-3f2c5dc2840d))
    (fp_line (start -0.562893 0) (end -1.27 0.5) (layer "F.Fab") (width 0.1) (tstamp 3233dea3-60aa-4445-b9c6-3d54986d12f6))
    (fp_line (start -1.27 -0.5) (end -0.562893 0) (layer "F.Fab") (width 0.1) (tstamp 51b20dbf-ba42-4da8-838a-a08ae05c740f))
    (fp_line (start 3.81 -2.92) (end -1.27 -2.92) (layer "F.Fab") (width 0.1) (tstamp 570a92de-6e2c-4f77-bc7f-4f165e4eca3b))
    (fp_line (start -1.27 -2.92) (end -1.27 2.88) (layer "F.Fab") (width 0.1) (tstamp 9808fbbd-60ee-43c9-8a29-d40c73629a69))
    (fp_line (start -1.27 2.88) (end 3.81 2.88) (layer "F.Fab") (width 0.1) (tstamp d8d14388-29ee-4737-9fdb-9612d119059c))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 2 "Board_0-Net-(C2-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 0301957f-a5c3-4680-8e32-b2d7fc0287c4))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 3 "Board_0-Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 3618b6f6-bd67-4bb8-a36d-a0fcab5a3500))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0) (tstamp 4eb2f71f-cf08-46bf-b3de-feff2910ed0c)
    (at 27 20 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "Archivo: KiKit_1.kicad_sch")
    (property "Sheetname" "")
    (path "/3634c702-8296-4ef0-8f77-04464227b915")
    (attr through_hole)
    (fp_text reference "C1" (at 1.25 -2.05 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b685df6d-a9e0-41de-999b-5eb425025f32)
    )
    (fp_text value "100nF" (at 1.25 2.05 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3c16e475-cb56-493c-8cfc-7e038daa37de)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0 90 unlocked) (layer "F.Fab")
      (effects (font (size 0.6 0.6) (thickness 0.09)))
      (tstamp ef66ab28-e9fb-4f1b-8426-d36178807862)
    )
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer "F.SilkS") (width 0.12) (tstamp 21e07d6a-5a5d-4766-841f-d76b991823dd))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer "F.SilkS") (width 0.12) (tstamp db5d1923-aa96-4404-be4e-6482a914832a))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 198c9958-ab22-488d-8e20-1fc3504eb61c))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 43292f07-3ceb-4ebb-a5ae-979b6c5282c7))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 98a8e285-18f2-4dde-baf3-c6d3dd11bc28))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer "F.CrtYd") (width 0.05) (tstamp cc5ebda1-e52d-4749-86b3-103fe6e666f7))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer "F.Fab") (width 0.1) (tstamp 114da3cb-8026-472d-ad34-ee0d727b5744))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer "F.Fab") (width 0.1) (tstamp 1b9fc078-961e-4878-b140-b759e7dec7db))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer "F.Fab") (width 0.1) (tstamp 808906da-064a-464c-9804-b4684dab3c23))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer "F.Fab") (width 0.1) (tstamp 8b71f22a-6b80-45aa-9c13-fb03656da0b9))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Board_0-Net-(C1-Pad1)") (pintype "passive") (tstamp 90ef5626-824c-4c46-bf95-0d6135bf241b))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Board_0-Net-(J1-Pad2)") (pintype "passive") (tstamp 8c6c7100-9f44-4769-966c-2ec5719cad2d))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp 52f08ed2-c2f9-45cb-b3b9-e3971e2f9690)
    (at 34.81 23 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Archivo: KiKit_1.kicad_sch")
    (property "Sheetname" "")
    (path "/a8e1595e-8e57-4f44-b5b4-2356cc29a7ad")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -2.37 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bdf97616-ce49-4530-9ce6-3c943a1f0b41)
    )
    (fp_text value "1k" (at 3.81 2.37 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp afb57c8c-17da-48f6-b717-0d255a1057a8)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6c6dc259-c8a1-4664-9b3e-154ecb0d15ce)
    )
    (fp_line (start 0.54 1.04) (end 0.54 1.37) (layer "F.SilkS") (width 0.12) (tstamp 406a6dba-163c-4697-95f0-f340522abf32))
    (fp_line (start 7.08 1.37) (end 7.08 1.04) (layer "F.SilkS") (width 0.12) (tstamp 55e27df3-8d6e-455e-aa99-0b856007ec47))
    (fp_line (start 0.54 -1.04) (end 0.54 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 70fd0532-ac49-4cfd-a2fb-f2a2ea734f16))
    (fp_line (start 0.54 -1.37) (end 7.08 -1.37) (layer "F.SilkS") (width 0.12) (tstamp baba97e1-afdb-4c25-8746-317643d6e78c))
    (fp_line (start 0.54 1.37) (end 7.08 1.37) (layer "F.SilkS") (width 0.12) (tstamp d23ad130-d3d5-48e5-a665-e87b96ac66fe))
    (fp_line (start 7.08 -1.37) (end 7.08 -1.04) (layer "F.SilkS") (width 0.12) (tstamp dc249a13-71dc-4c87-be0a-0e08854dd401))
    (fp_line (start 8.67 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 1fc08c9b-4b18-4b1d-8d58-aa7ea633c285))
    (fp_line (start -1.05 1.5) (end 8.67 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 312733b3-05c6-4756-be76-4c2ff2c03afe))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp eecd2656-b4b6-4b88-9070-ca070b5e940d))
    (fp_line (start 8.67 1.5) (end 8.67 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp f55aca44-d6f0-4961-af54-0a58b20fa22e))
    (fp_line (start 7.62 0) (end 6.96 0) (layer "F.Fab") (width 0.1) (tstamp 00abad24-66fd-40be-8464-655d35b48ab9))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer "F.Fab") (width 0.1) (tstamp 054ce88e-950a-4c1e-a698-1e6b1d6503a3))
    (fp_line (start 0 0) (end 0.66 0) (layer "F.Fab") (width 0.1) (tstamp 55fbc245-6ef9-400c-94bc-2bf836dc252c))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer "F.Fab") (width 0.1) (tstamp f3a59614-e4e1-4d92-804b-8faf53e6816f))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer "F.Fab") (width 0.1) (tstamp f513a173-92fc-4728-b424-4440077991ad))
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer "F.Fab") (width 0.1) (tstamp fa531b58-b230-49cd-b40d-89e994bafdd1))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Board_0-Net-(C2-Pad1)") (pintype "passive") (tstamp 80676ef3-485c-4078-adeb-1394a24f090f))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Board_0-Net-(C1-Pad1)") (pintype "passive") (tstamp 6f5609c4-d796-4049-ad95-c60d17d6d1f9))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0) (tstamp 79ac32ba-f7fe-48d8-9d0e-29f24b449ec1)
    (at 33 20 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "Archivo: KiKit_1.kicad_sch")
    (property "Sheetname" "")
    (path "/6262c752-74d0-4165-861d-2dcda33232e2")
    (attr through_hole)
    (fp_text reference "C2" (at 1.25 -2.05 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 750d3836-cd27-4015-acba-6baa8da62303)
    )
    (fp_text value "100nF" (at 1.25 2.05 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c1f3041c-14dc-4db6-851c-2ac3f8a3d26e)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0 90 unlocked) (layer "F.Fab")
      (effects (font (size 0.6 0.6) (thickness 0.09)))
      (tstamp eff3fa20-4732-4f52-94ac-43b02f1f5f08)
    )
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer "F.SilkS") (width 0.12) (tstamp 10588173-01ef-4810-9608-f51a5fc50970))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer "F.SilkS") (width 0.12) (tstamp eae31f77-0d39-4e73-b7a7-2f5858c411f0))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 4a3a7421-f73f-45fc-8f05-2dc8f76506ab))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 8ac0940d-6f41-4a53-b49f-d999c207d4b6))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 9e606054-df7a-43a4-ac55-3615feb1e6ad))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp c3e5a672-85c8-4e64-8713-8f84653cde28))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer "F.Fab") (width 0.1) (tstamp 0e483243-7e06-4e97-b1f1-6a43c5526b8a))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer "F.Fab") (width 0.1) (tstamp 356dd584-92ab-4d4a-a58c-7fc07db689bd))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer "F.Fab") (width 0.1) (tstamp 8525f3d8-991c-405c-9837-e15f4dae2a5b))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer "F.Fab") (width 0.1) (tstamp f6ab1a73-a5ce-4e7d-a6eb-0a1fa98626a1))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Board_0-Net-(C2-Pad1)") (pintype "passive") (tstamp 57e961f9-6bb5-4f87-b0ab-3769d1b89b74))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Board_0-Net-(J1-Pad2)") (pintype "passive") (tstamp ffe390db-b991-4a14-b681-26baa75adac4))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "kikit:Board" (layer "F.Cu")
    (tedit 605A21C1) (tstamp 8f9ebc34-cd2c-4beb-9224-d717c6f740ae)
    (at 17 15)
    (descr "Mark board for extraction")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "A" (at -4.5 -5 unlocked) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp a3901e1c-ebb3-4351-8695-180e6b5551e2)
    )
    (fp_text value "Board" (at -7.25 -5 unlocked) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ec00096b-a30d-4a7a-bb6a-f01ecfe7a4d8)
    )
    (fp_line (start 0 0) (end -1 -0.5) (layer "Dwgs.User") (width 0.2) (tstamp b9194ef7-9227-49da-af5c-cce5a0830ea6))
    (fp_line (start 0 0) (end 0.5 -1) (layer "Dwgs.User") (width 0.2) (tstamp c323caa6-7c3d-4602-bf04-f02651cc41f9))
    (fp_line (start 0 0) (end -1.25 -4) (layer "Dwgs.User") (width 0.2) (tstamp ce5a56d3-62b0-4772-990b-193093386c66))
    (fp_line (start -1.25 -4) (end -9.25 -4) (layer "Dwgs.User") (width 0.2) (tstamp f16f09f0-fb0e-4ddb-886c-94eda75179b4))
  )

  (gr_line (start 46 27) (end 46 27) (layer "Edge.Cuts") (width 0.1) (tstamp 3a4c9b05-be7c-441e-a1e7-27536ac7c4cd))
  (gr_line (start 46 15) (end 46 27) (layer "Edge.Cuts") (width 0.1) (tstamp 6199bd18-68ee-4bbb-9dd1-35eabf9c7252))
  (gr_line (start 15 27) (end 15 15) (layer "Edge.Cuts") (width 0.1) (tstamp 6f9542d3-7ff8-48e7-b205-3c5d4dc754c3))
  (gr_line (start 46 27) (end 15 27) (layer "Edge.Cuts") (width 0.1) (tstamp b888b6b1-4b55-4191-97a2-1551820f43fb))
  (gr_line (start 15 15) (end 46 15) (layer "Edge.Cuts") (width 0.1) (tstamp c3118582-37f9-495c-a6fa-7c5282d045f3))

  (segment (start 27 20) (end 27 22.81) (width 1) (layer "B.Cu") (net 1) (tstamp 9b6a36d9-dd8e-4478-89cf-964f37b93660))
  (segment (start 20 20.54) (end 26.46 20.54) (width 1) (layer "B.Cu") (net 1) (tstamp 9e6d15ea-d008-4661-90d7-974aec9c396e))
  (segment (start 27 22.81) (end 27.19 23) (width 1) (layer "B.Cu") (net 1) (tstamp dd998522-dea9-4881-af68-ddeb80b3613d))
  (segment (start 26.46 20.54) (end 27 20) (width 1) (layer "B.Cu") (net 1) (tstamp e9c38959-2717-4617-acf8-fda460ed143f))
  (segment (start 33 21.19) (end 34.81 23) (width 1) (layer "B.Cu") (net 2) (tstamp 052026d3-bd65-42b2-8964-99b45c0ef169))
  (segment (start 44 20) (end 44 23) (width 1) (layer "B.Cu") (net 2) (tstamp 0f034afe-b6d9-42af-b21d-8e367bb50d50))
  (segment (start 33 20) (end 33 21.19) (width 1) (layer "B.Cu") (net 2) (tstamp 35257455-01bf-416a-8ffe-64dfcbe7fe82))
  (segment (start 35.81 24) (end 34.81 23) (width 1) (layer "B.Cu") (net 2) (tstamp 5cc8036a-db11-40f7-9729-9cdeec67aeb3))
  (segment (start 44 23) (end 43 24) (width 1) (layer "B.Cu") (net 2) (tstamp 8b63ea97-60ab-4abe-9d50-4408d7513bb5))
  (segment (start 43 24) (end 35.81 24) (width 1) (layer "B.Cu") (net 2) (tstamp 8d7b4a04-917a-487f-9982-b0abe702e891))
  (segment (start 42 18) (end 44 20) (width 1) (layer "B.Cu") (net 2) (tstamp 9f1aeff3-816d-4c13-accc-bf43d27fd49c))
  (segment (start 41 18) (end 42 18) (width 1) (layer "B.Cu") (net 2) (tstamp d3d66d15-1ac1-4ca6-afa7-62054b3ec444))
  (segment (start 35.5 17.5) (end 39 21) (width 1) (layer "B.Cu") (net 3) (tstamp 10903efb-53fd-4bd4-a42f-8b0d6e1f0da8))
  (segment (start 40.54 21) (end 41 20.54) (width 1) (layer "B.Cu") (net 3) (tstamp 7d862bd9-e231-49e8-b62a-2a4d5ece8efb))
  (segment (start 39 21) (end 40.54 21) (width 1) (layer "B.Cu") (net 3) (tstamp 81f29d2e-db72-494a-bd02-3cda6ae0c87a))
  (segment (start 20 18) (end 26.5 18) (width 1) (layer "B.Cu") (net 3) (tstamp 930a57af-1631-4a83-8804-2f0e9083354c))
  (segment (start 26.5 18) (end 27 17.5) (width 1) (layer "B.Cu") (net 3) (tstamp 9647f75d-8102-459c-b62e-984391193472))
  (segment (start 33 17.5) (end 35.5 17.5) (width 1) (layer "B.Cu") (net 3) (tstamp a94a0d2a-25ca-4b92-83a4-64fdd23dd24d))
  (segment (start 27 17.5) (end 33 17.5) (width 1) (layer "B.Cu") (net 3) (tstamp f2023103-9ede-41b1-9491-88a09f45e81f))

)
