(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin 139.89 89.63)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(R1-Pad2)")
  (net 6 "Net-(R1-Pad1)")
  (net 7 "Net-(R2-Pad2)")
  (net 8 "Net-(R2-Pad1)")

  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f496a58)
    (at 137.16 87.63)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (path "/00000000-0000-0000-0000-00005f43bec2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "C1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5fc27c35-3e1c-4f96-817c-93b5570858a6)
    )
    (fp_text value "1nF" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6c9b793c-e74d-4754-a2c0-901e73b26f1c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp ce83728b-bebd-48c2-8734-b6a50d837931)
    )
    (fp_circle (center 0 0) (end 0.4 0) (layer "F.Adhes") (width 0.1) (fill none) (tstamp 6a45789b-3855-401f-8139-3c734f7f52f9))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp f71da641-16e6-4257-80c3-0b9d804fee4f))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp fd470e95-4861-44fe-b1e4-6d8a7c66e144))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 127679a9-3981-4934-815e-896a4e3ff56e))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 48ab88d7-7084-4d02-b109-3ad55a30bb11))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 716e31c5-485f-40b5-88e3-a75900da9811))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp b1086f75-01ba-4188-8d36-75a9e2828ca9))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 0eaa98f0-9565-4637-ace3-42a5231b07f7))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 181abe7a-f941-42b6-bd46-aaa3131f90fb))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 704d6d51-bb34-4cbf-83d8-841e208048d8))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 8174b4de-74b1-48db-ab8e-c8432251095b))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)") (tstamp 9340c285-5767-42d5-8b6d-63fe2a40ddf3))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)") (tstamp c41b3c8b-634e-435a-b582-96b83bbd4032))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f496a8b)
    (at 141.57 90.58)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f43d4bb")
    (attr through_hole)
    (fp_text reference "R2" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 81bbc3ff-3938-49ac-8297-ce2bcc9a42bd)
    )
    (fp_text value "1000" (at 1.178 2.13) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 15875808-74d5-4210-b8ca-aa8fbc04ae21)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp a7520ad3-0f8b-4788-92d4-8ffb277041e6)
    )
    (fp_circle (center 0 0) (end 0.4 0) (layer "F.Adhes") (width 0.1) (fill none) (tstamp dd00c2e1-6027-4717-b312-4fab3ee52002))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 1860e030-7a36-4298-b7fc-a16d48ab15ba))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 3dcc657b-55a1-48e0-9667-e01e7b6b08b5))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 0a3cc030-c9dd-4d74-9d50-715ed2b361a2))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 8322f275-268c-4e87-a69f-4cfbf05e747f))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp b6270a28-e0d9-4655-a18a-03dbf007b940))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp f3490fa5-5a27-423b-af60-53609669542c))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 13abf99d-5265-4779-8973-e94370fd18ff))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 32667662-ae86-4904-b198-3e95f11851bf))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 67f6e996-3c99-493c-8f6f-e739e2ed5d7a))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp a05d7640-f2f6-4ba7-8c51-5a4af431fc13))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(R2-Pad1)") (tstamp 46918595-4a45-48e8-84c0-961b4db7f35f))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(R2-Pad2)") (tstamp a795f1ba-cdd5-4cc5-9a52-08586e982934))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f503c2a)
    (at 141.57 87.63)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f43d144")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 983c426c-24e0-4c65-ab69-1f1824adc5c6)
    )
    (fp_text value "1k" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c1d83899-e380-49f9-a87d-8e78bc089ebf)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 746ba970-8279-4e7b-aed3-f28687777c21)
    )
    (fp_circle (center 0 0) (end 0.4 0) (layer "F.Adhes") (width 0.1) (fill none) (tstamp e9bb29b2-2bb9-4ea2-acd9-2bb3ca677a12))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 3f5fe6b7-98fc-4d3e-9567-f9f7202d1455))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp bb7f0588-d4d8-44bf-9ebf-3c533fe4d6ae))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 5cbb5968-dbb5-4b84-864a-ead1cacf75b9))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 62c076a3-d618-44a2-9042-9a08b3576787))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp afb8e687-4a13-41a1-b8c0-89a749e897fe))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp da469d11-a8a4-414b-9449-d151eeaf4853))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 6a955fc7-39d9-4c75-9a69-676ca8c0b9b2))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp e10b5627-3247-4c86-b9f6-ef474ca11543))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp e8314017-7be6-4011-9179-37449a29b311))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp f1830a1b-f0cc-47ae-a2c9-679c82032f14))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(R1-Pad1)") (tstamp 10109f84-4940-47f8-8640-91f185ac9bc1))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(R1-Pad2)") (tstamp 71c31975-2c45-4d18-a25a-18e07a55d11e))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f503c4a)
    (at 148.555 89.154)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f43d144")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b635b16e-60bb-4b3e-9fc3-47d34eef8381)
    )
    (fp_text value "1k" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 13475e15-f37c-4de8-857e-1722b0c39513)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 4e3d7c0d-12e3-42f2-b944-e4bcdbbcac2a)
    )
    (fp_circle (center 0 0) (end 0.4 0) (layer "F.Adhes") (width 0.1) (fill none) (tstamp 2732632c-4768-42b6-bf7f-14643424019e))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp cef6f603-8a0b-4dd0-af99-ebfbef7d1b4b))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp e877bf4a-4210-4bd3-b7b0-806eb4affc5b))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 120a7b0f-ddfd-4447-85c1-35665465acdb))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 48f827a8-6e22-4a2e-abdc-c2a03098d883))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 854dd5d4-5fd2-4730-bd49-a9cd8299a065))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 8d55e186-3e11-40e8-a65e-b36a8a00069e))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 5b2b5c7d-f943-4634-9f0a-e9561705c49d))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 9c8ccb2a-b1e9-4f2c-94fe-301b5975277e))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp a03e565f-d8cd-4032-aae3-b7327d4143dd))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp c70d9ef3-bfeb-47e0-a1e1-9aeba3da7864))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp aa02e544-13f5-4cf8-a5f4-3e6cda006090))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6a44418c-7bb4-4e99-8836-57f153c19721))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f496a69)
    (at 137.16 90.58)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (path "/00000000-0000-0000-0000-00005f43ce1c")
    (attr through_hole)
    (fp_text reference "C2" (at 0 1.65) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e615f7aa-337e-474d-9615-2ad82b1c44ca)
    )
    (fp_text value "1000 pF" (at -0.508 -2.13) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4fb02e58-160a-4a39-9f22-d0c75e82ee72)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 2e642b3e-a476-4c54-9a52-dcea955640cd)
    )
    (fp_circle (center 0 0) (end 0.4 0) (layer "B.Adhes") (width 0.1) (fill none) (tstamp ef8fe2ac-6a7f-4682-9418-b801a1b10a3b))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "B.SilkS") (width 0.12) (tstamp 3b838d52-596d-4e4d-a6ac-e4c8e7621137))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "B.SilkS") (width 0.12) (tstamp cbdcaa78-3bbc-413f-91bf-2709119373ce))
    (fp_line (start 1.68 -0.95) (end -1.68 -0.95) (layer "B.CrtYd") (width 0.05) (tstamp 44d8279a-9cd1-4db6-856f-0363131605fc))
    (fp_line (start -1.68 0.95) (end 1.68 0.95) (layer "B.CrtYd") (width 0.05) (tstamp 66116376-6967-4178-9f23-a26cdeafc400))
    (fp_line (start -1.68 -0.95) (end -1.68 0.95) (layer "B.CrtYd") (width 0.05) (tstamp 749dfe75-c0d6-4872-9330-29c5bbcb8ff8))
    (fp_line (start 1.68 0.95) (end 1.68 -0.95) (layer "B.CrtYd") (width 0.05) (tstamp eb667eea-300e-4ca7-8a6f-4b00de80cd45))
    (fp_line (start 1 -0.6) (end -1 -0.6) (layer "B.Fab") (width 0.1) (tstamp 1e1b062d-fad0-427c-a622-c5b8a80b5268))
    (fp_line (start -1 0.6) (end 1 0.6) (layer "B.Fab") (width 0.1) (tstamp 30f15357-ce1d-48b9-93dc-7d9b1b2aa048))
    (fp_line (start -1 -0.6) (end -1 0.6) (layer "B.Fab") (width 0.1) (tstamp 87371631-aa02-498a-998a-09bdb74784c1))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer "B.Fab") (width 0.1) (tstamp d8603679-3e7b-4337-8dbc-1827f5f54d8a))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)") (tstamp ac264c30-3e9a-4be2-b97a-9949b68bd497))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad2)") (tstamp 5038e144-5119-49db-b6cf-f7c345f1cf03))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 133.35 83.82) (end 133.35 93.98) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-00005f496acc))
  (gr_line (start 146.05 83.82) (end 133.35 83.82) (layer "Edge.Cuts") (width 0.1) (tstamp 0b21a65d-d20b-411e-920a-75c343ac5136))
  (gr_line (start 146.05 93.98) (end 146.05 83.82) (layer "Edge.Cuts") (width 0.1) (tstamp 3cd1bda0-18db-417d-b581-a0c50623df68))
  (gr_line (start 133.35 93.98) (end 146.05 93.98) (layer "Edge.Cuts") (width 0.1) (tstamp d57dcfee-5058-4fc2-a68b-05f9a48f685b))
  (gr_text "Bogus component.\nNot in schematic." (at 161.163 89.281) (layer "Cmts.User") (tstamp 1831fb37-1c5d-42c4-b898-151be6fca9dc)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )

)
