(kicad_pcb (version 20171130) (host pcbnew 5.1.9-73d0e3b20d~88~ubuntu21.04.1)

  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 0)
    (zones 0)
    (modules 1)
    (nets 1)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 97.0026 97.0026)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (module Package_DFN_QFN:QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm (layer B.Cu) (tedit 5DC5F6A3) (tstamp 601B53A7)
    (at 100 100)
    (descr "QFN, 12 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_12_%2005-08-1855.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U1 (at 0 2.82) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm (at 0 -2.82) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.885 1.61) (end 1.61 1.61) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.61 1.61) (end 1.61 0.885) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.885 -1.61) (end -1.61 -1.61) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.61 -1.61) (end -1.61 -0.885) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.885 -1.61) (end 1.61 -1.61) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.61 -1.61) (end 1.61 -0.885) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.885 1.61) (end -1.61 1.61) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.75 1.5) (end 1.5 1.5) (layer B.Fab) (width 0.1))
    (fp_line (start 1.5 1.5) (end 1.5 -1.5) (layer B.Fab) (width 0.1))
    (fp_line (start 1.5 -1.5) (end -1.5 -1.5) (layer B.Fab) (width 0.1))
    (fp_line (start -1.5 -1.5) (end -1.5 0.75) (layer B.Fab) (width 0.1))
    (fp_line (start -1.5 0.75) (end -0.75 1.5) (layer B.Fab) (width 0.1))
    (fp_line (start -2.12 2.12) (end -2.12 -2.12) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.12 -2.12) (end 2.12 -2.12) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.12 -2.12) (end 2.12 2.12) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.12 2.12) (end -2.12 2.12) (layer B.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 0.75 0.75) (thickness 0.11)) (justify mirror))
    )
    (pad "" smd roundrect (at 0.41 -0.41) (size 0.67 0.67) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.41 0.41) (size 0.67 0.67) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.41 -0.41) (size 0.67 0.67) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.41 0.41) (size 0.67 0.67) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 13 smd rect (at 0 0) (size 1.65 1.65) (layers B.Cu B.Mask))
    (pad 12 smd roundrect (at -0.5 1.4625) (size 0.25 0.825) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 11 smd roundrect (at 0 1.4625) (size 0.25 0.825) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 0.5 1.4625) (size 0.25 0.825) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at 1.4625 0.5) (size 0.825 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at 1.4625 0) (size 0.825 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 1.4625 -0.5) (size 0.825 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at 0.5 -1.4625) (size 0.25 0.825) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at 0 -1.4625) (size 0.25 0.825) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -0.5 -1.4625) (size 0.25 0.825) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -1.4625 -0.5) (size 0.825 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -1.4625 0) (size 0.825 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -1.4625 0.5) (size 0.825 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

)
