(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 4.69)
  )

  (paper "User" 431.8 279.4)
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")

  (footprint "Audio_Module:Reverb_BTDR-1H" (layer "F.Cu")
    (tedit 5F6F0B02) (tstamp bffa9999-0aad-445d-aed6-786119adfaf0)
    (at 142.24 81.28)
    (descr "Digital Reverberation Unit, http://www.belton.co.kr/inc/downfile.php?seq=17&file=pdf (footprint from http://www.uk-electronic.de/PDF/BTDR-1.pdf)")
    (tags "audio belton reverb")
    (attr through_hole)
    (fp_text reference "REF**" (at -3.5 -36) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp acecc061-90e9-488f-9e86-434d2e5e59c2)
    )
    (fp_text value "Reverb_BTDR-1H" (at 29 6) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 597dc5a5-9dcd-461c-9152-2d3c585f01ae)
    )
    (fp_text user "${REFERENCE}" (at 29 -15.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 73faa932-eb21-4bb4-a852-85bfc8e9d620)
    )
    (fp_line (start -6.38 4) (end 61.62 4) (layer "Edge.Cuts") (width 0.1) (tstamp 6278d65c-6156-44e1-be78-132aabccd777))
    (fp_line (start 61.62 -35) (end 61.62 -23) (layer "Edge.Cuts") (width 0.1) (tstamp 796c8096-b86e-4481-a5de-80504a659038))
    (fp_line (start -6.38 -23) (end -6.38 -35) (layer "Edge.Cuts") (width 0.1) (tstamp 7fe4937f-3e23-4030-8cb4-6f5d54ca1e0e))
    (fp_line (start -6.38 -35) (end 61.62 -35) (layer "Edge.Cuts") (width 0.1) (tstamp 9d02d43c-99e4-41b3-9b88-526d30f0b848))
    (fp_line (start -6.38 -8) (end -6.38 4) (layer "Edge.Cuts") (width 0.1) (tstamp ad07676c-6647-4754-be00-b8c5a14f297d))
    (fp_line (start 61.62 -8) (end 61.62 4) (layer "Edge.Cuts") (width 0.1) (tstamp ebcc77a7-6f5a-40d6-93ef-ba0fc620df4d))
    (fp_arc (start 64.62 -20) (mid 69.12 -15.5) (end 64.62 -11) (layer "Edge.Cuts") (width 0.1) (tstamp 1dc77144-0e99-4294-980b-82c2bcd9c278))
    (fp_arc (start -9.38 -11) (mid -7.25868 -10.12132) (end -6.38 -8) (layer "Edge.Cuts") (width 0.1) (tstamp 8d59061d-b86f-4b66-b027-59bbb9d96890))
    (fp_arc (start -6.38 -23) (mid -7.25868 -20.87868) (end -9.38 -20) (layer "Edge.Cuts") (width 0.1) (tstamp 8e64f078-4077-40b3-9715-e2e0068b6a0d))
    (fp_arc (start 64.62 -20) (mid 62.49868 -20.87868) (end 61.62 -23) (layer "Edge.Cuts") (width 0.1) (tstamp c06e0f71-190c-49f1-8fd3-1d0e15812cca))
    (fp_arc (start -9.38 -11) (mid -13.88 -15.5) (end -9.38 -20) (layer "Edge.Cuts") (width 0.1) (tstamp dff555d5-9f8d-4d6d-ab80-c061eb72a829))
    (fp_arc (start 61.62 -8) (mid 62.49868 -10.12132) (end 64.62 -11) (layer "Edge.Cuts") (width 0.1) (tstamp e7c418bd-59e9-40db-8d6e-3d8f56ac1547))
    (pad "" np_thru_hole circle (at -9.38 -15.5) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask) (tstamp 349b2b90-e8d5-4661-9ea3-e808a3cafb04))
    (pad "" np_thru_hole circle (at 64.62 -15.5) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask) (tstamp e336a07c-cbe8-49f4-b6e7-316722520680))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask "Edge.Cuts") (tstamp ae6ec705-a29a-4441-b705-653f844a5005))
    (pad "2" thru_hole circle (at 2.54 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 98cd6edd-9087-4718-ab27-d0ea9b4d1b74))
    (pad "3" thru_hole circle (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp e5c6953b-cccb-4e65-afc1-7bacc1581173))
    (pad "4" thru_hole circle (at 7.62 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 5b98611e-f230-43eb-99f6-8c300a56921d))
    (pad "5" thru_hole circle (at 50.62 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp ac1ddec3-f63c-41f7-b711-69dcd26edfea))
    (pad "6" thru_hole circle (at 53.16 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 3896d12f-4204-4775-a917-0f598d9d1e0b))
    (pad "7" thru_hole circle (at 55.7 0) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp c952264d-af42-4abc-b795-5343c9dab05d))
    (model "${KICAD6_3DMODEL_DIR}/Audio_Module.3dshapes/Reverb_BTDR-1H.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (via blind (at 159.225 59.7) (size 2) (drill 1) (layers "In1.Cu" "B.Cu") (free) (net 0) (tstamp 87d63687-7b19-4a89-aa5a-e093ef7dbdb2))

)
