(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin 139.89 89.63)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (property "text" "Test")

  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(R1-Pad2)")
  (net 6 "Net-(R1-Pad1)")
  (net 7 "Net-(R2-Pad2)")
  (net 8 "Net-(R2-Pad1)")

  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f496a58)
    (at 137.16 87.63)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (path "/00000000-0000-0000-0000-00005f43bec2")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a17658ae-6bb1-4adb-b6b3-ef4c836b3104)
    )
    (fp_text value "1nF" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7a3ff137-c90e-4755-bfaa-61ac4559c1c4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 610d3dab-96f1-467e-a8bb-982e1a5e28b3)
    )
    (fp_circle (center 0 0) (end 0.4 0) (layer "F.Adhes") (width 0.1) (fill none) (tstamp b95c9af6-d571-4ff7-aa89-c20d6a5096f9))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 535fb667-3ef5-4c7d-8b0e-f211f4b2598f))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 877d03b3-2e6b-4283-8774-f9a3972e5d1b))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 179b1cfd-2c85-4f43-a5f6-868ca3ed1710))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 68d5b6f4-dbf5-4aa8-9240-b1053c3090c9))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 7b599469-c7d3-440a-82c3-3fb41a9ddc82))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp f815ff74-24a8-400f-8ca4-b5af8d9ae8aa))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 09f8738f-4304-4557-bcc0-63f51e2bb272))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 53842113-2eed-4e07-83f9-cf62ab0b8b6b))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 6052d8c7-51a2-4347-a770-b463e8004a6a))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp ffd4eef0-200f-473f-98ef-875ae2710211))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)") (tstamp 0396208e-a401-46d6-a9d6-4fc5f29a991e))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)") (tstamp c0e176e6-2b65-4e42-ab43-deafd4b2725e))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f496a69)
    (at 137.16 90.58)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (path "/00000000-0000-0000-0000-00005f43ce1c")
    (attr through_hole)
    (fp_text reference "C2" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4de8c707-0d2d-4070-9fe2-95aba800da97)
    )
    (fp_text value "1000 pF" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1aadc258-dafc-428e-a9e1-059c1ee3bc24)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 210883df-9124-4ab7-9e4d-1d5de0e14436)
    )
    (fp_circle (center 0 0) (end 0.4 0) (layer "F.Adhes") (width 0.1) (fill none) (tstamp 565df081-bb0e-4272-889c-8883a6cf574f))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp b38aac83-d426-48eb-8136-075909ca0d4a))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp f39138bd-8e9c-4749-b1f6-ad562a76c547))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 446b00b9-49fb-4d19-99d8-f7dfbf5ba90e))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 8cd966ec-936a-4a2a-97a1-c162eb60f3e5))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp c3bee8b2-8413-4ed0-8a3c-b25a7b938428))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp cfca8046-57f9-4bad-b147-0e4cb641e71b))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 55b19cfa-b606-4080-b04d-dd557256f1ba))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 72ae4549-fa18-4dbf-93bb-1305330c71a6))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 7fc277fd-f98e-4d8c-95fe-9dde488db0c6))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp ff6fa4d8-6d22-441b-96c5-4b33ac32fe1e))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)") (tstamp bb444f3e-7d1f-4c82-8eb7-24fddaab885c))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad2)") (tstamp 378300c0-8cef-4c8a-8338-6f66311fc3c2))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f496a8b)
    (at 141.57 90.58)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f43d4bb")
    (attr through_hole)
    (fp_text reference "R2" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a16bb11f-1ae1-452b-ab06-c0c0c5550581)
    )
    (fp_text value "1000" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8d62e4b1-2b78-479f-8bd0-b822c934ecc5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp e7acb238-433c-4d0c-9ac5-aada44ae87c6)
    )
    (fp_circle (center 0 0) (end 0.4 0) (layer "F.Adhes") (width 0.1) (fill none) (tstamp 5e9a445e-d281-40e5-aa88-5a4ca0015602))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 2f751c07-db61-4fb2-a551-ac48ab965e3e))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 77b6adbd-4ea1-4b55-ac32-3d73199bfa37))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 1c18e8fe-20b5-44a9-abff-9239aded7a2a))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 321cd77f-700d-4ffc-989c-fc5e37251c36))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp bcb3d769-6147-42c5-ad88-f725f9c8e563))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp ff0028a2-d2a5-403f-bb0c-e9daef57d7dd))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp 10ce8a66-bf48-418c-bc77-95fd17a79c81))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp a40020d7-ffd1-4386-b107-b0101c1b0ce5))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp c22ae2e3-a19d-4183-bd18-87d52e335b80))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp df843824-3ab8-4db7-a313-5cb6e638d41e))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(R2-Pad1)") (tstamp d82b2b32-b91d-4cb1-86e2-007ccd994e78))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(R2-Pad2)") (tstamp ba5049a8-ad9a-49c4-997a-84e5c7fdd3d9))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f503c2a)
    (at 141.57 87.63)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f43d144")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b6a444b7-f4ce-419c-89ef-2cfd5db7a945)
    )
    (fp_text value "1k" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 855c640f-0598-43af-83dd-404d817a88f8)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 6d891518-8781-400e-8095-ad01983a9315)
    )
    (fp_circle (center 0 0) (end 0.4 0) (layer "F.Adhes") (width 0.1) (fill none) (tstamp b6bf2be9-d47d-4982-baf3-f6485d5fc2fa))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 3f82faa0-e76b-430f-9a3e-124be5e074a2))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 47987321-48a0-4e03-bdbc-dad9ea6b9662))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 2320c397-f9b3-417f-93bc-7684581ff540))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 76d0d3ec-964c-4d0d-9433-cb608686da84))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp b02a9d87-40a3-4d0f-ba46-740e56a66166))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp eff8f9e3-70f6-43f8-b054-b752e97ce246))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp 010c6a20-5856-4bad-b771-0fe13323a108))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 5d794526-beca-4e0a-b441-f09f1366536c))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp a32c49f6-0990-4f13-ad49-4db52adad6aa))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp b953df13-a55a-4953-a0fa-5fdc226f66e6))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(R1-Pad1)") (tstamp 3fbca69d-47ae-4671-b766-56ad2b10b635))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(R1-Pad2)") (tstamp 364ef61c-3c7f-49af-92ac-c9cb1c72df90))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B) (tstamp 00000000-0000-0000-0000-00005f503c4a)
    (at 148.555 89.154)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00005f43d144")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1ebe2927-938f-48bf-a28f-b1341cb4eb92)
    )
    (fp_text value "1k" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6639c313-6496-4cf4-b2f1-d7ac22590bf8)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 760a8cec-d133-4ac1-9b68-2a482625bd1f)
    )
    (fp_circle (center 0 0) (end 0.4 0) (layer "F.Adhes") (width 0.1) (fill none) (tstamp e5b325c5-598d-4f6b-a413-d3a79eb95cbb))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer "F.SilkS") (width 0.12) (tstamp 02c4cbf5-9900-4c08-981d-8f9deb435440))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer "F.SilkS") (width 0.12) (tstamp 35b37184-c1db-4605-9bcd-675b2c4b2158))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 2ad9142c-8923-4abd-b90a-c8ae2f7c9d80))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 885792c5-6361-4eb1-8fbb-77d0c940bafc))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp ab11510d-aa5c-41d7-a0b9-335045f11724))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp e1cd1c41-7c11-498a-9141-5d74c0f912c2))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer "F.Fab") (width 0.1) (tstamp 3e58ad13-421d-4712-a3a6-baa45f7a50d9))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer "F.Fab") (width 0.1) (tstamp c9abcf12-7a33-4d52-8f7f-751243a70726))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer "F.Fab") (width 0.1) (tstamp d540225e-b626-44df-a06e-d1355b1826a9))
    (fp_line (start 1 0.6) (end -1 0.6) (layer "F.Fab") (width 0.1) (tstamp d7ea9ea0-5b1e-4200-8463-6407ba1b21a5))
    (pad "1" smd roundrect locked (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(R1-Pad1)") (tstamp 7c75769f-18a4-4d0c-9703-f047e8f5ab1d))
    (pad "2" smd roundrect locked (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(R1-Pad2)") (tstamp 2b8f6242-95b2-4ff4-8124-8f1c2a171f0a))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Fiducial:Fiducial_0.5mm_Mask1mm" (layer "F.Cu")
    (tedit 5C18CB26) (tstamp 00000000-0000-0000-0000-00005f57ee4f)
    (at 139.6746 82.9564)
    (descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
    (tags "fiducial")
    (path "/00000000-0000-0000-0000-00005f57eddb")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "FID1" (at 0 -1.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7b643210-edc8-42fc-ae01-131c3f64b382)
    )
    (fp_text value "Fiducial" (at 0 1.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0efa37b2-af85-4c04-a3a9-67fbb3deae71)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.04)))
      (tstamp af5353c5-81fd-4093-969d-2b7178673638)
    )
    (fp_circle (center 0 0) (end 0.75 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp bd1aa9f8-fd9c-4c73-ad79-67b18a6317f1))
    (fp_circle (center 0 0) (end 0.5 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp b2736e48-774d-475e-b008-2b03645f9be3))
    (pad "" smd circle locked (at 0 0) (size 0.5 0.5) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.25) (clearance 0.25) (tstamp 1dde19d5-99c8-4d8b-8f79-2b55c7e0cf67))
  )

  (gr_line (start 133.35 80.4) (end 133.35 93.98) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-00005f496acc))
  (gr_line (start 146.05 80.4) (end 133.35 80.4) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-00005f57eeaf))
  (gr_line (start 146.05 93.98) (end 146.05 80.4) (layer "Edge.Cuts") (width 0.1) (tstamp 123e2e63-e5a2-438b-a092-e86abe433be1))
  (gr_line (start 133.35 93.98) (end 146.05 93.98) (layer "Edge.Cuts") (width 0.1) (tstamp db70ada3-b7ba-4225-9c00-3f7474e61b64))
  (gr_text "${text}" (at 139 92.5) (layer "F.SilkS") (tstamp b873bc5d-a9af-4bd9-afcb-87ce4d417120)
    (effects (font (size 1 1.5) (thickness 0.25)))
  )
  (gr_text "Bogus component.\nNot in schematic." (at 161.163 89.281) (layer "Cmts.User") (tstamp 5f5ef4dd-f4ae-40a8-adf2-0ac2296d03fa)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )

  (segment (start 145 82) (end 145 92) (width 0.25) (layer "F.Cu") (net 0) (tstamp 86f6faec-7eee-404c-a73a-2ae625f33d8c))
  (segment (start 145 92) (end 144 92) (width 0.25) (layer "F.Cu") (net 0) (tstamp 90337a8b-a8c5-48e1-ad0f-b0e67716fe3c))
  (segment (start 144 92) (end 144 82) (width 0.25) (layer "F.Cu") (net 0) (tstamp d3db736b-0e33-4126-b950-5488923df40e))
  (segment (start 144 82) (end 145 82) (width 0.25) (layer "F.Cu") (net 0) (tstamp eb83440d-aa8b-4a1e-9e93-00cf0de78de9))

)
