(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C3-Pad1)")
  (net 7 "Net-(C4-Pad2)")
  (net 8 "Net-(C4-Pad1)")
  (net 9 "Net-(R1-Pad2)")
  (net 10 "Net-(R1-Pad1)")
  (net 11 "Net-(R2-Pad2)")
  (net 12 "Net-(R2-Pad1)")
  (net 13 "Net-(R3-Pad2)")
  (net 14 "Net-(R3-Pad1)")
  (net 15 "Net-(R4-Pad2)")
  (net 16 "Net-(R4-Pad1)")

  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 00000000-0000-0000-0000-00006223ab1c)
    (at 128.25 93 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (path "/00000000-0000-0000-0000-00006223ba95")
    (attr smd)
    (fp_text reference "C1" (at -1 -1.68 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 48ab88d7-7084-4d02-b109-3ad55a30bb11)
    )
    (fp_text value "1u" (at 0 1.68 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f71da641-16e6-4257-80c3-0b9d804fee4f)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp fd470e95-4861-44fe-b1e4-6d8a7c66e144)
    )
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer "F.SilkS") (width 0.12) (tstamp c41b3c8b-634e-435a-b582-96b83bbd4032))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer "F.SilkS") (width 0.12) (tstamp ce83728b-bebd-48c2-8734-b6a50d837931))
    (fp_line (start 1.7 -0.98) (end 1.7 0.98) (layer "F.CrtYd") (width 0.05) (tstamp 0f22151c-f260-4674-b486-4710a2c42a55))
    (fp_line (start -1.7 -0.98) (end 1.7 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp 1831fb37-1c5d-42c4-b898-151be6fca9dc))
    (fp_line (start -1.7 0.98) (end -1.7 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp 9340c285-5767-42d5-8b6d-63fe2a40ddf3))
    (fp_line (start 1.7 0.98) (end -1.7 0.98) (layer "F.CrtYd") (width 0.05) (tstamp fe8d9267-7834-48d6-a191-c8724b2ee78d))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 0eaa98f0-9565-4637-ace3-42a5231b07f7))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 181abe7a-f941-42b6-bd46-aaa3131f90fb))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 704d6d51-bb34-4cbf-83d8-841e208048d8))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 8174b4de-74b1-48db-ab8e-c8432251095b))
    (pad "1" smd roundrect locked (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)") (tstamp 3cd1bda0-18db-417d-b581-a0c50623df68))
    (pad "2" smd roundrect locked (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)") (tstamp 0b21a65d-d20b-411e-920a-75c343ac5136))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metrico.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 00000000-0000-0000-0000-00006223ab2d)
    (at 133 93.25 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (path "/00000000-0000-0000-0000-00006223bc65")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.68 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3b838d52-596d-4e4d-a6ac-e4c8e7621137)
    )
    (fp_text value "2u" (at 0 1.68 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cbdcaa78-3bbc-413f-91bf-2709119373ce)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 1e1b062d-fad0-427c-a622-c5b8a80b5268)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer "F.SilkS") (width 0.12) (tstamp 5038e144-5119-49db-b6cf-f7c345f1cf03))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer "F.SilkS") (width 0.12) (tstamp ac264c30-3e9a-4be2-b97a-9949b68bd497))
    (fp_line (start -1.7 0.98) (end -1.7 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp 54365317-1355-4216-bb75-829375abc4ec))
    (fp_line (start -1.7 -0.98) (end 1.7 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp a3e4f0ae-9f86-49e9-b386-ed8b42e012fb))
    (fp_line (start 1.7 -0.98) (end 1.7 0.98) (layer "F.CrtYd") (width 0.05) (tstamp a690fc6c-55d9-47e6-b533-faa4b67e20f3))
    (fp_line (start 1.7 0.98) (end -1.7 0.98) (layer "F.CrtYd") (width 0.05) (tstamp c144caa5-b0d4-4cef-840a-d4ad178a2102))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 2e642b3e-a476-4c54-9a52-dcea955640cd))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 30f15357-ce1d-48b9-93dc-7d9b1b2aa048))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 87371631-aa02-498a-998a-09bdb74784c1))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp d8603679-3e7b-4337-8dbc-1827f5f54d8a))
    (pad "1" smd roundrect locked (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)") (tstamp 5fc27c35-3e1c-4f96-817c-93b5570858a6))
    (pad "2" smd roundrect locked (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad2)") (tstamp efeac2a2-7682-4dc7-83ee-f6f1b23da506))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 00000000-0000-0000-0000-00006223ab60)
    (at 128.25 99)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00006223a923")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a03e565f-d8cd-4032-aae3-b7327d4143dd)
    )
    (fp_text value "1" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5b2b5c7d-f943-4634-9f0a-e9561705c49d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp c70d9ef3-bfeb-47e0-a1e1-9aeba3da7864)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "F.SilkS") (width 0.12) (tstamp d1262c4d-2245-4c4f-8f35-7bb32cd9e21e))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "F.SilkS") (width 0.12) (tstamp d22e95aa-f3db-4fbc-a331-048a2523233e))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 0d0bb7b2-a6e5-46d2-9492-a1aa6e5a7b2f))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 15875808-74d5-4210-b8ca-aa8fbc04ae21))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 81bbc3ff-3938-49ac-8297-ce2bcc9a42bd))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp b1169a2d-8998-4b50-a48d-c520bcc1b8e1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 0147f16a-c952-4891-8f53-a9fb8cddeb8d))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 4e3d7c0d-12e3-42f2-b944-e4bcdbbcac2a))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 6a44418c-7bb4-4e99-8836-57f153c19721))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp aa02e544-13f5-4cf8-a5f4-3e6cda006090))
    (pad "1" smd roundrect locked (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 10 "Net-(R1-Pad1)") (tstamp 0a3cc030-c9dd-4d74-9d50-715ed2b361a2))
    (pad "2" smd roundrect locked (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "Net-(R1-Pad2)") (tstamp dd00c2e1-6027-4717-b312-4fab3ee52002))
    (model "ALIAS1:test.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 00000000-0000-0000-0000-00006223ab71)
    (at 133 98.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00006223adf1")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b3d08afa-f296-4e3b-8825-73b6331d35bf)
    )
    (fp_text value "2" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 98e81e80-1f85-4152-be3f-99785ea97751)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 842e430f-0c35-45f3-a0b5-95ae7b7ae388)
    )
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "F.SilkS") (width 0.12) (tstamp 58dc14f9-c158-4824-a84e-24a6a482a7a4))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "F.SilkS") (width 0.12) (tstamp dde3dba8-1b81-466c-93a3-c284ff4da1ef))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 13475e15-f37c-4de8-857e-1722b0c39513))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 2732632c-4768-42b6-bf7f-14643424019e))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp b635b16e-60bb-4b3e-9fc3-47d34eef8381))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp f976e2cc-36f9-4479-a816-2c74d1d5da6f))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 03d88a85-11fd-47aa-954c-c318bb15294a))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 0dcdf1b8-13c6-48b4-bd94-5d26038ff231))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 1a2f72d1-0b36-4610-afc4-4ad1660d5d3b))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 51c4dc0a-5b9f-4edf-a83f-4a12881e42ef))
    (pad "1" smd roundrect locked (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 12 "Net-(R2-Pad1)") (tstamp 120a7b0f-ddfd-4447-85c1-35665465acdb))
    (pad "2" smd roundrect locked (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 11 "Net-(R2-Pad2)") (tstamp 854dd5d4-5fd2-4730-bd49-a9cd8299a065))
    (model "ALIAS2:test.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 00000000-0000-0000-0000-00006223ab3e)
    (at 128.25 93.25 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (path "/00000000-0000-0000-0000-00006223c1b3")
    (attr smd)
    (fp_text reference "C3" (at 0 1.68 -90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bb7f0588-d4d8-44bf-9ebf-3c533fe4d6ae)
    )
    (fp_text value "3u" (at 0 -1.68 -90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f1830a1b-f0cc-47ae-a2c9-679c82032f14)
    )
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 6a955fc7-39d9-4c75-9a69-676ca8c0b9b2)
    )
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer "B.SilkS") (width 0.12) (tstamp 10109f84-4940-47f8-8640-91f185ac9bc1))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer "B.SilkS") (width 0.12) (tstamp 55e740a3-0735-4744-896e-2bf5437093b9))
    (fp_line (start 1.7 0.98) (end 1.7 -0.98) (layer "B.CrtYd") (width 0.05) (tstamp 47baf4b1-0938-497d-88f9-671136aa8be7))
    (fp_line (start 1.7 -0.98) (end -1.7 -0.98) (layer "B.CrtYd") (width 0.05) (tstamp 77ed3941-d133-4aef-a9af-5a39322d14eb))
    (fp_line (start -1.7 0.98) (end 1.7 0.98) (layer "B.CrtYd") (width 0.05) (tstamp c022004a-c968-410e-b59e-fbab0e561e9d))
    (fp_line (start -1.7 -0.98) (end -1.7 0.98) (layer "B.CrtYd") (width 0.05) (tstamp f4f99e3d-7269-4f6a-a759-16ad2a258779))
    (fp_line (start 1 -0.625) (end -1 -0.625) (layer "B.Fab") (width 0.1) (tstamp 71c31975-2c45-4d18-a25a-18e07a55d11e))
    (fp_line (start 1 0.625) (end 1 -0.625) (layer "B.Fab") (width 0.1) (tstamp 746ba970-8279-4e7b-aed3-f28687777c21))
    (fp_line (start -1 0.625) (end 1 0.625) (layer "B.Fab") (width 0.1) (tstamp e10b5627-3247-4c86-b9f6-ef474ca11543))
    (fp_line (start -1 -0.625) (end -1 0.625) (layer "B.Fab") (width 0.1) (tstamp e8314017-7be6-4011-9179-37449a29b311))
    (pad "1" smd roundrect locked (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C3-Pad1)") (tstamp 4fb02e58-160a-4a39-9f22-d0c75e82ee72))
    (pad "2" smd roundrect locked (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C3-Pad2)") (tstamp e615f7aa-337e-474d-9615-2ad82b1c44ca))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 00000000-0000-0000-0000-00006223ab4f)
    (at 127.75 99 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (path "/00000000-0000-0000-0000-00006223c217")
    (attr smd)
    (fp_text reference "C4" (at 0 1.68 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 67f6e996-3c99-493c-8f6f-e739e2ed5d7a)
    )
    (fp_text value "4u" (at 0 -1.68 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 32667662-ae86-4904-b198-3e95f11851bf)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp a05d7640-f2f6-4ba7-8c51-5a4af431fc13)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer "B.SilkS") (width 0.12) (tstamp 94c158d1-8503-4553-b511-bf42f506c2a8))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer "B.SilkS") (width 0.12) (tstamp 9ccf03e8-755a-4cd9-96fc-30e1d08fa253))
    (fp_line (start -1.7 -0.98) (end -1.7 0.98) (layer "B.CrtYd") (width 0.05) (tstamp 23bb2798-d93a-4696-a962-c305c4298a0c))
    (fp_line (start 1.7 0.98) (end 1.7 -0.98) (layer "B.CrtYd") (width 0.05) (tstamp 6e105729-aba0-497c-a99e-c32d2b3ddb6d))
    (fp_line (start -1.7 0.98) (end 1.7 0.98) (layer "B.CrtYd") (width 0.05) (tstamp 78cbdd6c-4878-4cc5-9a58-0e506478e37d))
    (fp_line (start 1.7 -0.98) (end -1.7 -0.98) (layer "B.CrtYd") (width 0.05) (tstamp 983c426c-24e0-4c65-ab69-1f1824adc5c6))
    (fp_line (start -1 -0.625) (end -1 0.625) (layer "B.Fab") (width 0.1) (tstamp 13abf99d-5265-4779-8973-e94370fd18ff))
    (fp_line (start 1 -0.625) (end -1 -0.625) (layer "B.Fab") (width 0.1) (tstamp 46918595-4a45-48e8-84c0-961b4db7f35f))
    (fp_line (start -1 0.625) (end 1 0.625) (layer "B.Fab") (width 0.1) (tstamp a7520ad3-0f8b-4788-92d4-8ffb277041e6))
    (fp_line (start 1 0.625) (end 1 -0.625) (layer "B.Fab") (width 0.1) (tstamp a795f1ba-cdd5-4cc5-9a52-08586e982934))
    (pad "1" smd roundrect locked (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C4-Pad1)") (tstamp e9bb29b2-2bb9-4ea2-acd9-2bb3ca677a12))
    (pad "2" smd roundrect locked (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C4-Pad2)") (tstamp c1d83899-e380-49f9-a87d-8e78bc089ebf))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 00000000-0000-0000-0000-00006223ab82)
    (at 133 93.75)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00006223b0e5")
    (attr smd)
    (fp_text reference "R3" (at -0.5 1.65) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp afd3dbad-e7a8-4e4c-b77c-4065a69aefa2)
    )
    (fp_text value "3" (at 0 -1.65) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1b54105e-6590-4d26-a763-ecfcf81eedc4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 0f41a909-27c4-4be2-9d5e-9ae2108c8ff5)
    )
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "B.SilkS") (width 0.12) (tstamp dabe541b-b164-4180-97a4-5ca761b86800))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "B.SilkS") (width 0.12) (tstamp e12e827e-36be-4503-8eef-6fc7e8bc5d49))
    (fp_line (start 1.68 -0.95) (end -1.68 -0.95) (layer "B.CrtYd") (width 0.05) (tstamp 0088d107-13d8-496c-8da6-7bbeb9d096b0))
    (fp_line (start -1.68 0.95) (end 1.68 0.95) (layer "B.CrtYd") (width 0.05) (tstamp 417f13e4-c121-485a-a6b5-8b55e70350b8))
    (fp_line (start -1.68 -0.95) (end -1.68 0.95) (layer "B.CrtYd") (width 0.05) (tstamp 9dab0cb7-2557-4419-963b-5ae736517f62))
    (fp_line (start 1.68 0.95) (end 1.68 -0.95) (layer "B.CrtYd") (width 0.05) (tstamp c201e1b2-fc01-4110-bdaa-a33290468c83))
    (fp_line (start -1 0.625) (end 1 0.625) (layer "B.Fab") (width 0.1) (tstamp 35354519-a28c-40c4-befd-0943e98dea53))
    (fp_line (start 1 0.625) (end 1 -0.625) (layer "B.Fab") (width 0.1) (tstamp 38f2d955-ea7a-4a21-aba6-02ae23f1bd4a))
    (fp_line (start -1 -0.625) (end -1 0.625) (layer "B.Fab") (width 0.1) (tstamp 632acde9-b7fd-4f04-8cb4-d2cbb06b3595))
    (fp_line (start 1 -0.625) (end -1 -0.625) (layer "B.Fab") (width 0.1) (tstamp 6b25f522-8e2d-4cd8-9d5d-a2b80f60133b))
    (pad "1" smd roundrect locked (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(R3-Pad1)") (tstamp 68e09be7-3bbc-4443-a838-209ce20b2bef))
    (pad "2" smd roundrect locked (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 13 "Net-(R3-Pad2)") (tstamp 6a780180-586a-4241-a52d-dc7a5ffcc966))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 00000000-0000-0000-0000-00006223ab93)
    (at 133 98.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (path "/00000000-0000-0000-0000-00006223b0ef")
    (attr smd)
    (fp_text reference "R4" (at 0 1.65) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9702d639-3b1f-4825-8985-b32b9008503d)
    )
    (fp_text value "4" (at 0 -1.65) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0d35483a-0b12-46cc-b9f2-896fd6831779)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 4e66a44f-7fa6-4e16-bf9b-62ec864301a5)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "B.SilkS") (width 0.12) (tstamp a9ec539a-d80d-40cc-803c-12b6adefe42a))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "B.SilkS") (width 0.12) (tstamp ef1b4b98-541b-4673-a04f-2043250fc40a))
    (fp_line (start -1.68 0.95) (end 1.68 0.95) (layer "B.CrtYd") (width 0.05) (tstamp 2bf3f24b-fd30-41a7-a274-9b519491916b))
    (fp_line (start 1.68 0.95) (end 1.68 -0.95) (layer "B.CrtYd") (width 0.05) (tstamp 4831966c-bb32-4bc8-a400-0382a02ffa1c))
    (fp_line (start -1.68 -0.95) (end -1.68 0.95) (layer "B.CrtYd") (width 0.05) (tstamp c264c438-a475-4ad4-9915-0f1e6ecf3053))
    (fp_line (start 1.68 -0.95) (end -1.68 -0.95) (layer "B.CrtYd") (width 0.05) (tstamp e25ce415-914a-48fe-bf09-324317917b2e))
    (fp_line (start 1 -0.625) (end -1 -0.625) (layer "B.Fab") (width 0.1) (tstamp 34871042-9d5c-4e29-abdd-a168368c3c22))
    (fp_line (start -1 -0.625) (end -1 0.625) (layer "B.Fab") (width 0.1) (tstamp 4412226e-d975-40a2-921f-502ff4129a95))
    (fp_line (start 1 0.625) (end 1 -0.625) (layer "B.Fab") (width 0.1) (tstamp 53c85970-3e21-4fae-a84f-721cfc0513b5))
    (fp_line (start -1 0.625) (end 1 0.625) (layer "B.Fab") (width 0.1) (tstamp 7447a6e7-8205-46ba-afca-d0fa8f90c95a))
    (pad "1" smd roundrect locked (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 16 "Net-(R4-Pad1)") (tstamp 9762c9ed-64d8-4f3e-baf6-f6ba6effc919))
    (pad "2" smd roundrect locked (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 15 "Net-(R4-Pad2)") (tstamp 4d4b0fcd-2c79-4fc3-b5fa-7a0741601344))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 125 102) (end 125 91) (layer "Edge.Cuts") (width 0.05) (tstamp 00000000-0000-0000-0000-00006223ae41))
  (gr_line (start 136 91) (end 136 102) (layer "Edge.Cuts") (width 0.05) (tstamp 29e78086-2175-405e-9ba3-c48766d2f50c))
  (gr_line (start 125 91) (end 136 91) (layer "Edge.Cuts") (width 0.05) (tstamp 94a873dc-af67-4ef9-8159-1f7c93eeb3d7))
  (gr_line (start 136 102) (end 125 102) (layer "Edge.Cuts") (width 0.05) (tstamp a1823eb2-fb0d-4ed8-8b96-04184ac3a9d5))

)
