(kicad_pcb (version 20171130) (host pcbnew 5.1.9-73d0e3b20d~88~ubuntu20.04.1)

  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 0)
    (zones 0)
    (modules 3)
    (nets 1)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (module kikit:Board (layer F.Cu) (tedit 605A1488) (tstamp 605A707C)
    (at 185 90)
    (descr "Mark board for extraction")
    (fp_text reference B3 (at -4.5 -5) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    )
    (fp_text value Board (at -7.25 -5) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 0) (end -1.25 -4) (layer Dwgs.User) (width 0.2))
    (fp_line (start -1.25 -4) (end -9.25 -4) (layer Dwgs.User) (width 0.2))
    (fp_line (start 0 0) (end 0.5 -1) (layer Dwgs.User) (width 0.2))
    (fp_line (start 0 0) (end -1 -0.5) (layer Dwgs.User) (width 0.2))
  )

  (module kikit:Board (layer F.Cu) (tedit 605A1488) (tstamp 605A706E)
    (at 135 90)
    (descr "Mark board for extraction")
    (fp_text reference B2 (at -4.5 -5) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    )
    (fp_text value Board (at -7.25 -5) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 0) (end -1 -0.5) (layer Dwgs.User) (width 0.2))
    (fp_line (start 0 0) (end 0.5 -1) (layer Dwgs.User) (width 0.2))
    (fp_line (start -1.25 -4) (end -9.25 -4) (layer Dwgs.User) (width 0.2))
    (fp_line (start 0 0) (end -1.25 -4) (layer Dwgs.User) (width 0.2))
  )

  (module kikit:Board (layer F.Cu) (tedit 605A1488) (tstamp 605A7057)
    (at 100 90)
    (descr "Mark board for extraction")
    (fp_text reference B1 (at -4.5 -5) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    )
    (fp_text value Board (at -7.25 -5) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 0) (end -1.25 -4) (layer Dwgs.User) (width 0.2))
    (fp_line (start -1.25 -4) (end -9.25 -4) (layer Dwgs.User) (width 0.2))
    (fp_line (start 0 0) (end 0.5 -1) (layer Dwgs.User) (width 0.2))
    (fp_line (start 0 0) (end -1 -0.5) (layer Dwgs.User) (width 0.2))
  )

  (gr_text C (at 185 100) (layer F.SilkS) (tstamp 605A709F)
    (effects (font (size 5 5) (thickness 1)))
  )
  (gr_text B (at 145 100) (layer F.SilkS) (tstamp 605A709D)
    (effects (font (size 5 5) (thickness 1)))
  )
  (gr_text A (at 100 100) (layer F.SilkS)
    (effects (font (size 5 5) (thickness 1)))
  )
  (gr_line (start 200 100) (end 190 100) (layer Edge.Cuts) (width 0.2) (tstamp 605A142A))
  (gr_line (start 200 105) (end 200 100) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 190 105) (end 200 105) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 190 100) (end 190 105) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 210 90) (end 180 90) (layer Edge.Cuts) (width 0.2) (tstamp 605A1425))
  (gr_line (start 210 110) (end 210 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 180 110) (end 210 110) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 180 90) (end 180 110) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 150 110) (end 135 110) (layer Edge.Cuts) (width 0.2) (tstamp 605A1415))
  (gr_line (start 150 100) (end 150 110) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 160 100) (end 150 100) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 160 90) (end 160 100) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 135 90) (end 160 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 135 110) (end 135 90) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 100 100) (end 110 100) (layer Edge.Cuts) (width 0.2))

)
