/*
 * Copyright (c) 2022 The ZMK Contributors
 *
 * SPDX-License-Identifier: MIT
 */

#include <behaviors.dtsi>
#include <dt-bindings/zmk/keys.h>
#include <dt-bindings/zmk/backlight.h>
#include <dt-bindings/zmk/bt.h>
#include <dt-bindings/zmk/ext_power.h>
#include <dt-bindings/zmk/outputs.h>
#include <dt-bindings/zmk/rgb.h>

// Uncomment the following lines if using the "Direct Wire" jumper to switch the matrix to a direct wire.

// / {
//     chosen {
//         zmk,physical-layout = &direct_physical_layout;
//     };
// };

/ {

    keymap {
        compatible = "zmk,keymap";

        default_layer {
            bindings = <
                &kp A &bl BL_TOG
                &rgb_ug RGB_EFF &bt BT_CLR

                &kp C &kp D
                &kp E &kp F
           >;

           sensor-bindings = <&inc_dec_kp C_VOL_UP C_VOL_DN &inc_dec_kp PG_UP PG_DN>;
        };
    };
};
