/*
 * Copyright (c) 2021 The ZMK Contributors
 * SPDX-License-Identifier: MIT
 */

/dts-v1/;
#include <nordic/nrf52840_qiaa.dtsi>

#include <dt-bindings/zmk/matrix_transform.h>

/ {
    chosen {
        zmk,kscan = &kscan0;
        zmk,matrix-transform = &default_transform;
        zephyr,code-partition = &code_partition;
        zephyr,sram = &sram0;
        zephyr,flash = &flash0;
    };

    default_transform: keymap_transform_0 {
        compatible = "zmk,matrix-transform";
        columns = <14>;
        rows = <6>;
        map = <
            RC(0,0) RC(0,1) RC(0,2) RC(0,3) RC(0,4)                                                                    RC(0,9) RC(0,10) RC(0,11) RC(0,12) RC(0,13)
            RC(1,0) RC(1,1) RC(1,2) RC(1,3) RC(1,4) RC(1,5)                                                    RC(1,8) RC(1,9) RC(1,10) RC(1,11) RC(1,12) RC(1,13)
            RC(2,0) RC(2,1) RC(2,2) RC(2,3) RC(2,4) RC(2,5)                                                    RC(2,8) RC(2,9) RC(2,10) RC(2,11) RC(2,12) RC(2,13)
            RC(3,0) RC(3,1) RC(3,2) RC(3,3) RC(3,4) RC(3,5)                                                    RC(3,8) RC(3,9) RC(3,10) RC(3,11) RC(3,12) RC(3,13)
            RC(4,0) RC(4,1) RC(4,2) RC(4,3) RC(4,4) RC(4,5) RC(0,6) RC(1,6) RC(2,6)   RC(2,7) RC(1,7)  RC(0,7) RC(4,8) RC(4,9) RC(4,10) RC(4,11) RC(4,12) RC(4,13)
            RC(5,0) RC(5,1) RC(5,2) RC(5,3) RC(5,4)         RC(3,6) RC(4,6) RC(5,6)   RC(5,7) RC(4,7)  RC(3,7)         RC(5,9) RC(5,10) RC(5,11) RC(5,12) RC(5,13)
        >;
    };

    kscan0: kscan {
        compatible = "zmk,kscan-gpio-matrix";
        wakeup-source;

        diode-direction = "col2row";
        debounce-press-ms = <4>;
        debounce-release-ms = <20>;
    };

};

&adc {
    status = "okay";
};

&gpiote {
    status = "okay";
};

&gpio0 {
    status = "okay";
};

&gpio1 {
    status = "okay";
};

zephyr_udc0: &usbd {
    status = "okay";
};

&flash0 {
    /*
     * For more information, see:
     * http://docs.zephyrproject.org/latest/devices/dts/flash_partitions.html
     */
    partitions {
        compatible = "fixed-partitions";
        #address-cells = <1>;
        #size-cells = <1>;

        sd_partition: partition@0 {
            reg = <0x00000000 0x00026000>;
        };
        code_partition: partition@26000 {
            reg = <0x00026000 0x000c6000>;
        };

        /*
         * The flash starting at 0x000ec000 and ending at
         * 0x000f3fff is reserved for use by the application.
         */

        /*
         * Storage partition will be used by FCB/LittleFS/NVS
         * if enabled.
         */
        storage_partition: partition@ec000 {
            reg = <0x000ec000 0x00008000>;
        };

        boot_partition: partition@f4000 {
            reg = <0x000f4000 0x0000c000>;
        };
    };
};
