/*
 * Copyright (c) 2020 The ZMK Contributors
 *
 * SPDX-License-Identifier: MIT
 */

#include <dt-bindings/zmk/matrix_transform.h>

/ {
    chosen {
        zmk,kscan = &kscan0;

        zmk,matrix-transform = &default_transform;
    };

    /*
     * This transform correspondsto the 60% left without macro keypad and 65% right, even this
     * combination of PCBs can have keys in different locations based on configuration.
     */
    default_transform: keymap_transform_0 {
        compatible = "zmk,matrix-transform";
        columns = <15>;
        rows = <6>;
        map = <
RC(0,0) RC(0,1) RC(0,2) RC(0,3) RC(0,4) RC(0,5) RC(0,6)   /**/ RC(0,7) RC(0,8) RC(0,9) RC(0,10) RC(0,11) RC(0,12)   RC(0,14)     RC(5,13)
RC(1,0)     RC(1,1) RC(1,2) RC(1,3) RC(1,4) RC(1,5)       /**/RC(1,7) RC(1,8) RC(1,9) RC(1,10) RC(1,11) RC(1,12) RC(1,13)   RC(1,14)  RC(5,14)
RC(2,0)       RC(2,1) RC(2,2) RC(2,3) RC(2,4) RC(2,5)     /**/ RC(2,7) RC(2,8) RC(2,9) RC(2,10) RC(2,11) RC(2,12)     RC(2,14)       RC(2,13)
RC(3,0)          RC(3,2) RC(3,3) RC(3,4) RC(3,5) RC(3,6)  /**/   RC(3,7) RC(3,8) RC(3,9) RC(3,10) RC(3,12)     RC(3,13)     RC(3,14) RC(3,11)
RC(4,0)  RC(4,1)  RC(4,2)         RC(4,4)         RC(4,6) /**/   RC(4,7)                 RC(4,10) RC(4,11) RC(4,12) RC(4,13) RC(4,14) RC(4,9)
        >;
    };
};
