(kicad_sch (version 20200828) (generator eeschema)

  (page 1 1)

  (paper "A4")

  (title_block
    (title "KiBom Test Schematic")
    (date "2020-03-12")
    (rev "A")
    (company "https://github.com/SchrodingersGat/KiBom")
  )

  (lib_symbols
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Value" "C" (id 1) (at 0.635 -2.54 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (stroke (width 0.508)) (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (stroke (width 0.508)) (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "R" (id 1) (at 0 0 90)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at -1.778 0 90)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Resistor" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (stroke (width 0.254)) (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Mechanical:Fiducial" (in_bom yes) (on_board yes)
      (property "Reference" "FID" (id 0) (at 0 5.08 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "Fiducial" (id 1) (at 0 3.175 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "fiducial marker" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Fiducial Marker" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Fiducial*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Fiducial_0_1"
        (circle (center 0 0) (radius 1.27) (stroke (width 0.508)) (fill (type background)))
      )
    )
  )


  (text "This schematic serves as a test-file for the KiBot export script.\nHere we implement the IBoM variants style."
    (at 12.7 19.05 0)
    (effects (font (size 2.0066 2.0066)) (justify left bottom))
  )
  (text "The test tests the following \nvariants matrix:\n        production   test   default\nC1                     X\nC2          X          X\nR1          X          X       X\nR2          X                  X\n\nproduction: blacklist T2\ntest: blacklist T1\ndefault: whitelist T1,default \n         blacklist T2,T3"
    (at 151.13 81.28 0)
    (effects (font (size 2.9972 2.9972)) (justify left bottom))
  )

  (symbol (lib_id "Mechanical:Fiducial") (at 44.45 57.15 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid "00000000-0000-0000-0000-00005f57eddb")
    (property "Reference" "FID1" (id 0) (at 46.609 55.9816 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "Fiducial" (id 1) (at 46.609 58.293 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Fiducial:Fiducial_0.5mm_Mask1mm" (id 2) (at 44.45 57.15 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 44.45 57.15 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )

  (symbol (lib_id "Device:R") (at 53.34 43.18 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid "00000000-0000-0000-0000-00005f43d144")
    (property "Reference" "R1" (id 0) (at 55.118 42.0116 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "1k" (id 1) (at 55.118 44.323 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 51.562 43.18 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 53.34 43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Config" "default" (id 4) (at 53.34 43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )

  (symbol (lib_id "Device:R") (at 63.5 43.18 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid "00000000-0000-0000-0000-00005f43d4bb")
    (property "Reference" "R2" (id 0) (at 65.278 42.0116 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "1000" (id 1) (at 65.278 44.323 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 61.722 43.18 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 63.5 43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Config" "T1" (id 4) (at 63.5 43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )

  (symbol (lib_id "Device:C") (at 25.4 43.18 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid "00000000-0000-0000-0000-00005f43bec2")
    (property "Reference" "C1" (id 0) (at 28.321 42.0116 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "1nF" (id 1) (at 28.321 44.323 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 26.3652 46.99 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 25.4 43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Config" "T2" (id 4) (at 25.4 43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )

  (symbol (lib_id "Device:C") (at 36.83 43.18 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid "00000000-0000-0000-0000-00005f43ce1c")
    (property "Reference" "C2" (id 0) (at 39.751 42.0116 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "1000 pF" (id 1) (at 39.751 44.323 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 37.7952 46.99 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 36.83 43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Config" "T3" (id 4) (at 36.83 43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )

  (symbol_instances
    (path "/00000000-0000-0000-0000-00005f43bec2"
      (reference "C1") (unit 1) (value "1nF") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path "/00000000-0000-0000-0000-00005f43ce1c"
      (reference "C2") (unit 1) (value "1000 pF") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path "/00000000-0000-0000-0000-00005f57eddb"
      (reference "FID1") (unit 1) (value "Fiducial") (footprint "Fiducial:Fiducial_0.5mm_Mask1mm")
    )
    (path "/00000000-0000-0000-0000-00005f43d144"
      (reference "R1") (unit 1) (value "1k") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path "/00000000-0000-0000-0000-00005f43d4bb"
      (reference "R2") (unit 1) (value "1000") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
  )
)
