(kicad_sch (version 20211123) (generator eeschema)

  (uuid e6521bef-4109-48f7-8b88-4121b0468927)

  (paper "A4")

  (title_block
    (title "KiCost subparts test")
    (date "2021-03-16")
    (rev "r1")
    (company "KiBot")
  )

  (lib_symbols
    (symbol "Connector_Generic:Conn_01x06" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 7.62 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "Conn_01x06" (id 1) (at 0 -10.16 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "connector" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Conn_01x06_1_1"
        (rectangle (start -1.27 -7.493) (end 0 -7.747)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start -1.27 6.35) (end 1.27 -8.89)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_2" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_3" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_4" (effects (font (size 1.27 1.27))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_5" (effects (font (size 1.27 1.27))))
          (number "5" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "Pin_6" (effects (font (size 1.27 1.27))))
          (number "6" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Device:Q_NPN_BCE" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.27 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Value" "Q_NPN_BCE" (id 1) (at 5.08 -1.27 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Footprint" "" (id 2) (at 5.08 2.54 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "transistor NPN" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "NPN transistor, base/collector/emitter" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Q_NPN_BCE_0_1"
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (stroke (width 0.508) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.778)
            (xy 1.778 -1.27)
            (xy 2.286 -2.286)
            (xy 1.27 -1.778)
            (xy 1.27 -1.778)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "Q_NPN_BCE_1_1"
        (pin input line (at -5.08 0 0) (length 5.715)
          (name "B" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "R" (id 1) (at 0 0 90)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at -1.778 0 90)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Resistor" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Mechanical:Heatsink" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "HS" (id 0) (at 0 5.08 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "Heatsink" (id 1) (at 0 -1.27 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0.3048 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0.3048 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "thermal heat temperature" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Heatsink" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Heatsink_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Heatsink_0_1"
        (polyline
          (pts
            (xy -0.3302 1.27)
            (xy -0.9652 1.27)
            (xy -0.9652 3.81)
            (xy -1.6002 3.81)
            (xy -1.6002 1.27)
            (xy -2.2352 1.27)
            (xy -2.2352 3.81)
            (xy -2.8702 3.81)
            (xy -2.8702 0)
            (xy -0.9652 0)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.3302 1.27)
            (xy -0.3302 3.81)
            (xy 0.3048 3.81)
            (xy 0.3048 1.27)
            (xy 0.9398 1.27)
            (xy 0.9398 3.81)
            (xy 1.5748 3.81)
            (xy 1.5748 1.27)
            (xy 2.2098 1.27)
            (xy 2.2098 3.81)
            (xy 2.8448 3.81)
            (xy 2.8448 0)
            (xy -0.9652 0)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
    )
  )


  (text "A Transistor and its heatsink\nOnly one goes to the PCB"
    (at 91.44 27.94 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 04f5865e-f449-4408-a0c8-771cccfcb129)
  )
  (text "Equivalent to ->" (at 67.31 39.37 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 0c30a4be-5679-499f-8c5b-5f3024f9d6cf)
  )
  (text "A simple resistor, \nbut multiplied by 4/5" (at 93.345 100.965 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 35354519-a28c-40c4-befd-0943e98dea53)
  )
  (text "A male header\nBut we want to include the female, the pins and the two\nsensors wired to the female."
    (at 22.86 60.96 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 5740c959-93d8-47fd-8f68-62f0109e753d)
  )
  (text "KiCost subparts" (at 14.605 20.955 0)
    (effects (font (size 5.08 5.08) (thickness 1.016) bold) (justify left bottom))
    (uuid 6199bec7-e7eb-4ae0-b9ec-c563e157d635)
  )
  (text "A simple resistor, \nbut multiplied by 5\nWe add: R4 no mult \n      and R5 no manf#\nTotal: 7"
    (at 93.345 62.865 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 7447a6e7-8205-46ba-afca-d0fa8f90c95a)
  )
  (text "A simple resistor, \nbut multiplied by 4.5" (at 93.345 81.915 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 9762c9ed-64d8-4f3e-baf6-f6ba6effc919)
  )

  (symbol (lib_id "Mechanical:Heatsink") (at 95.25 33.655 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00006063ab02)
    (property "Reference" "HS1" (id 0) (at 98.8314 29.4386 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "322400B00000G" (id 1) (at 98.8314 31.75 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 95.5548 33.655 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 95.5548 33.655 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf" "Aavid" (id 4) (at 95.25 33.655 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf#" "322400B00000G" (id 5) (at 98.8314 34.0614 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "digikey#" "HS100-ND" (id 6) (at 95.25 33.655 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Description" "HEAT SINK TO-18 1W BLK" (id 7) (at 95.25 33.655 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )

  (symbol (lib_id "Device:Q_NPN_BCE") (at 95.25 39.37 90) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00006063d25d)
    (property "Reference" "Q2" (id 0) (at 100.33 41.275 90))
    (property "Value" "2N2222A" (id 1) (at 102.87 43.815 90))
    (property "Footprint" "Package_TO_SOT_THT:TO-18-3" (id 2) (at 92.71 34.29 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 95.25 39.37 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf" "Central Semiconductor Corp" (id 4) (at 95.25 39.37 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf#" "2N2222A PBFREE" (id 5) (at 106.68 45.72 90))
    (property "Description" "TRANS NPN 40V 0.8A TO-18" (id 6) (at 95.25 39.37 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "digikey#" "1514-2N2222APBFREE-ND" (id 7) (at 95.25 39.37 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 6d3de064-0d13-4601-bce6-b355f2b62ba4))
    (pin "2" (uuid cc634f93-a623-42a2-9e47-0450d1d64f3b))
    (pin "3" (uuid ac4937af-2dda-4425-ac86-d4a17930e7f6))
  )

  (symbol (lib_id "Device:Q_NPN_BCE") (at 27.305 33.02 90) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-000060640f08)
    (property "Reference" "Q1" (id 0) (at 32.385 34.925 90))
    (property "Value" "2N2222A" (id 1) (at 34.925 37.465 90))
    (property "Footprint" "Package_TO_SOT_THT:TO-18-3" (id 2) (at 24.765 27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 27.305 33.02 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf" "Central Semiconductor Corp; Aavid" (id 4) (at 27.305 33.02 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf#" "2N2222A PBFREE; 322400B00000G" (id 5) (at 47.625 39.37 90))
    (property "Description" "TRANS NPN 40V 0.8A TO-18 + Heatsink" (id 6) (at 27.305 33.02 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "digikey#" "1514-2N2222APBFREE-ND; HS100-ND" (id 7) (at 27.305 33.02 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Value_Subparts" "2N2222A;322400B00000G" (id 8) (at -5.715 31.115 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 10139ec9-5972-4c3e-9672-4814ee8cc191))
    (pin "2" (uuid 2ed4d635-58a6-4d95-937a-a13d12eab682))
    (pin "3" (uuid 326eb9fa-9c8a-446f-9184-a16e6e7cb861))
  )

  (symbol (lib_id "Connector_Generic:Conn_01x06") (at 29.21 66.04 90) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-000060649b1f)
    (property "Reference" "J1" (id 0) (at 39.0652 66.9544 90)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "Conn_01x06" (id 1) (at 39.0652 69.2658 90)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (id 2) (at 29.21 66.04 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 29.21 66.04 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf" "Molex; Molex; Molex; LEM; LEM" (id 4) (at 29.21 66.04 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf#" "0022232061;0022012067; 6: 08-50-0114;  LA 55-P; lv 25-P" (id 5) (at 29.21 66.04 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "digikey#" "WM4204-ND; WM2015-ND; WM1114-ND; 398-1010-ND; 398-1019-ND" (id 6) (at 29.21 66.04 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Description" "CONN HEADER VERT 6POS 2.54MM; CONN HOUSING 6POS .100 W/RAMP; CONN 22-30AWG CRIMP TIN; SENSOR CURRENT HALL 50A AC/DC; TRANSDUCR VOLTAG CLOSE LOOP 10MA" (id 7) (at 29.21 66.04 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Value_Subparts" "Male_01x06;Female_01x06;Crimp_Pin;LA 55-P;LV 25-P" (id 8) (at 29.21 66.04 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid ba7dc470-e81e-48f8-b801-e3ad56903912))
    (pin "2" (uuid 6a4427bb-8402-4948-a241-18d89788209f))
    (pin "3" (uuid 0e3b31cf-0b07-47e0-92f2-166ac60927c5))
    (pin "4" (uuid e0257b22-e037-406a-bb51-11222be4b5ca))
    (pin "5" (uuid f67d6d8f-e55a-4ea8-9f4b-740c3756ce78))
    (pin "6" (uuid 14d48dbc-3c08-4fcf-8db7-077f8ae6191c))
  )

  (symbol (lib_id "Device:R") (at 95.25 67.31 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00006064c12f)
    (property "Reference" "R1" (id 0) (at 97.028 66.1416 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "0" (id 1) (at 97.028 68.453 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 93.472 67.31 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 95.25 67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf" "Bourns" (id 4) (at 95.25 67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf#" "CR0603-J/-000ELF:5" (id 5) (at 95.25 67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "digikey#" "CR0603-J/-000ELFCT-ND:  5" (id 6) (at 95.25 67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Description" "RES SMD 0 OHM JUMPER 1/8W 0603" (id 7) (at 95.25 67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 6dbc895c-1dd3-4e7d-b81b-ca254a096bab))
    (pin "2" (uuid 558a8b89-a06b-4db7-ba1e-2d751631ce5b))
  )

  (symbol (lib_id "Device:R") (at 95.25 86.36 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00006064ca86)
    (property "Reference" "R2" (id 0) (at 97.028 85.1916 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "100" (id 1) (at 97.028 87.503 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 93.472 86.36 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 95.25 86.36 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf" "Bourns" (id 4) (at 95.25 86.36 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf#" "CR0603-JW-101ELF   :   4.5" (id 5) (at 95.25 86.36 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "digikey#" "CR0603-JW-101ELFCT-ND   :4.5" (id 6) (at 95.25 86.36 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Description" "RES SMD 100 OHM 5% 1/10W 0603" (id 7) (at 95.25 86.36 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 1c9b334a-7672-4385-8ac7-d9b02e3281f4))
    (pin "2" (uuid a1573dc7-79bf-4f43-8435-ce6e930d0540))
  )

  (symbol (lib_id "Device:R") (at 95.25 105.41 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00006064d8d1)
    (property "Reference" "R3" (id 0) (at 97.028 104.2416 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "100k" (id 1) (at 97.028 106.553 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 93.472 105.41 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 95.25 105.41 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf" "Bourns" (id 4) (at 95.25 105.41 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf#" "4/5 : CR0603-JW-104ELF  " (id 5) (at 95.25 105.41 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "digikey#" "  4/5  :   CR0603-JW-104ELFCT-ND" (id 6) (at 95.25 105.41 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Description" "RES SMD 100K OHM 5% 1/10W 0603" (id 7) (at 95.25 105.41 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 537a62b7-ff88-435f-aaf6-1e0429e84e7c))
    (pin "2" (uuid 512fd277-9de7-454a-b3d9-ab06f52cae1a))
  )

  (symbol (lib_id "Device:R") (at 107.95 67.31 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00006064ef62)
    (property "Reference" "R4" (id 0) (at 109.728 66.1416 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "0" (id 1) (at 109.728 68.453 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 106.172 67.31 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 107.95 67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf" "Bourns" (id 4) (at 107.95 67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "manf#" "CR0603-J/-000ELF" (id 5) (at 107.95 67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "digikey#" "CR0603-J/-000ELFCT-ND" (id 6) (at 107.95 67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Description" "RES SMD 0 OHM JUMPER 1/8W 0603" (id 7) (at 107.95 67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 363660d1-fcfe-4523-bd03-465f5f34f254))
    (pin "2" (uuid e9c40bb3-be70-4a91-ac6a-6ecc9e9df269))
  )

  (symbol (lib_id "Device:R") (at 114.3 67.31 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00006064f812)
    (property "Reference" "R5" (id 0) (at 116.078 66.1416 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "0" (id 1) (at 116.078 68.453 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 112.522 67.31 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 114.3 67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Description" "RES SMD 0 OHM JUMPER 1/8W 0603" (id 4) (at 114.3 67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid c767df34-174c-4650-b7c3-54d87eeafd3c))
    (pin "2" (uuid 1a9ee27d-22cb-44eb-bb67-3f13b74866fa))
  )

  (sheet_instances
    (path "/" (page "1"))
  )

  (symbol_instances
    (path "/00000000-0000-0000-0000-00006063ab02"
      (reference "HS1") (unit 1) (value "322400B00000G") (footprint "")
    )
    (path "/00000000-0000-0000-0000-000060649b1f"
      (reference "J1") (unit 1) (value "Conn_01x06") (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical")
    )
    (path "/00000000-0000-0000-0000-000060640f08"
      (reference "Q1") (unit 1) (value "2N2222A") (footprint "Package_TO_SOT_THT:TO-18-3")
    )
    (path "/00000000-0000-0000-0000-00006063d25d"
      (reference "Q2") (unit 1) (value "2N2222A") (footprint "Package_TO_SOT_THT:TO-18-3")
    )
    (path "/00000000-0000-0000-0000-00006064c12f"
      (reference "R1") (unit 1) (value "0") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00006064ca86"
      (reference "R2") (unit 1) (value "100") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00006064d8d1"
      (reference "R3") (unit 1) (value "100k") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00006064ef62"
      (reference "R4") (unit 1) (value "0") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00006064f812"
      (reference "R5") (unit 1) (value "0") (footprint "")
    )
  )
)
