(kicad_sch (version 20211123) (generator eeschema)

  (uuid e6521bef-4109-48f7-8b88-4121b0468927)

  (paper "A4")

  (title_block
    (title "KiBom Test Schematic")
    (date "2020-03-12")
    (rev "A")
    (company "https://github.com/SchrodingersGat/KiBom")
  )

  (lib_symbols
    (symbol "Connector:TestPoint" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 6.858 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "TestPoint" (id 1) (at 0 5.08 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 5.08 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 5.08 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "test point" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "TestPoint_0_1"
        (circle (center 0 3.302) (radius 0.762)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "TestPoint_1_1"
        (pin passive line (at 0 0 90) (length 2.54)
          (name "1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Connector:TestPoint_2Pole" (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 1.524 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "TestPoint_2Pole" (id 1) (at 0 -1.778 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "point tp" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "2-polar test point" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "TestPoint_2Pole_0_1"
        (circle (center -1.778 0) (radius 0.762)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (circle (center 1.778 0) (radius 0.762)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Connector:TestPoint_Alt" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 6.858 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "TestPoint_Alt" (id 1) (at 0 5.08 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 5.08 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 5.08 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "test point (alternative shape)" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "TestPoint_Alt_0_1"
        (polyline
          (pts
            (xy 0 2.54)
            (xy -0.762 3.302)
            (xy 0 4.064)
            (xy 0.762 3.302)
            (xy 0 2.54)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "TestPoint_Alt_1_1"
        (pin passive line (at 0 0 90) (length 2.54)
          (name "1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Connector:TestPoint_Flag" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 3.429 1.778 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "TestPoint_Flag" (id 1) (at 3.302 4.191 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 5.08 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 5.08 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "test point (alternative flag-style design)" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "TestPoint_Flag_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0.889 0.889)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start 0.889 2.794) (end 5.842 0.889)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
      (symbol "TestPoint_Flag_1_1"
        (pin passive line (at 0 0 90) (length 0)
          (name "1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Connector:TestPoint_Probe" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 1.651 5.842 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "TestPoint_Probe" (id 1) (at 1.651 4.064 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 5.08 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 5.08 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "test point (alternative probe-style design)" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "TestPoint_Probe_0_1"
        (polyline
          (pts
            (xy 1.27 0.762)
            (xy 0 0)
            (xy 0.762 1.27)
            (xy 1.27 0.762)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 1.397 0.635)
            (xy 0.635 1.397)
            (xy 2.413 3.175)
            (xy 3.175 2.413)
            (xy 1.397 0.635)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
      (symbol "TestPoint_Probe_1_1"
        (pin passive line (at 0 0 90) (length 0)
          (name "1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Connector:TestPoint_Small" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 3.81 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "TestPoint_Small" (id 1) (at 0 2.032 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 5.08 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 5.08 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "test point" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "TestPoint_Small_0_1"
        (circle (center 0 0) (radius 0.508)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "TestPoint_Small_1_1"
        (pin passive line (at 0 0 90) (length 0)
          (name "1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Value" "C" (id 1) (at 0.635 -2.54 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (stroke (width 0.508) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (stroke (width 0.508) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "R" (id 1) (at 0 0 90)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at -1.778 0 90)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Resistor" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Jumper:SolderJumper_2_Bridged" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at 0 2.032 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "SolderJumper_2_Bridged" (id 1) (at 0 -2.54 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "solder jumper SPST" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Solder Jumper, 2-pole, closed/bridged" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "SolderJumper*Bridged*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "SolderJumper_2_Bridged_0_1"
        (rectangle (start -0.508 0.508) (end 0.508 -0.508)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (arc (start -0.254 1.016) (mid -1.27 0) (end -0.254 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start -0.254 1.016) (mid -1.27 0) (end -0.254 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -0.254 1.016)
            (xy -0.254 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 1.016)
            (xy 0.254 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0.254 -1.016) (mid 1.27 0) (end 0.254 1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0.254 -1.016) (mid 1.27 0) (end 0.254 1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
      )
      (symbol "SolderJumper_2_Bridged_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "B" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Jumper:SolderJumper_2_Open" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at 0 2.032 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "SolderJumper_2_Open" (id 1) (at 0 -2.54 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "solder jumper SPST" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Solder Jumper, 2-pole, open" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "SolderJumper*Open*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "SolderJumper_2_Open_0_1"
        (arc (start -0.254 1.016) (mid -1.27 0) (end -0.254 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start -0.254 1.016) (mid -1.27 0) (end -0.254 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -0.254 1.016)
            (xy -0.254 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 1.016)
            (xy 0.254 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0.254 -1.016) (mid 1.27 0) (end 0.254 1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0.254 -1.016) (mid 1.27 0) (end 0.254 1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
      )
      (symbol "SolderJumper_2_Open_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "B" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Jumper:SolderJumper_3_Bridged12" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at -2.54 -2.54 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "SolderJumper_3_Bridged12" (id 1) (at 0 2.794 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "Solder Jumper SPDT" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "3-pole Solder Jumper, pins 1+2 closed/bridged" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "SolderJumper*Bridged12*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "SolderJumper_3_Bridged12_0_1"
        (rectangle (start -1.016 0.508) (end -0.508 -0.508)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (arc (start -1.016 1.016) (mid -2.032 0) (end -1.016 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start -1.016 1.016) (mid -2.032 0) (end -1.016 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (rectangle (start -0.508 1.016) (end 0.508 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -2.032 0)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 1.016)
            (xy -1.016 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 1.016)
            (xy 1.016 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 2.032 0)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 1.016 -1.016) (mid 2.032 0) (end 1.016 1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 1.016 -1.016) (mid 2.032 0) (end 1.016 1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
      )
      (symbol "SolderJumper_3_Bridged12_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at 0 -3.81 90) (length 2.54)
          (name "C" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Jumper:SolderJumper_3_Bridged123" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at -2.54 -2.54 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "SolderJumper_3_Bridged123" (id 1) (at 0 2.794 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "Solder Jumper SPDT" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Solder Jumper, 3-pole, pins 1+2+3 closed/bridged" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "SolderJumper*Bridged123*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "SolderJumper_3_Bridged123_0_1"
        (rectangle (start -1.016 0.508) (end -0.508 -0.508)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (arc (start -1.016 1.016) (mid -2.032 0) (end -1.016 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start -1.016 1.016) (mid -2.032 0) (end -1.016 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (rectangle (start -0.508 1.016) (end 0.508 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -2.032 0)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 1.016)
            (xy -1.016 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 1.016)
            (xy 1.016 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 2.032 0)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start 0.508 0.508) (end 1.016 -0.508)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (arc (start 1.016 -1.016) (mid 2.032 0) (end 1.016 1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 1.016 -1.016) (mid 2.032 0) (end 1.016 1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
      )
      (symbol "SolderJumper_3_Bridged123_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at 0 -3.81 90) (length 2.54)
          (name "C" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Jumper:SolderJumper_3_Open" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at -2.54 -2.54 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "SolderJumper_3_Open" (id 1) (at 0 2.794 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "Solder Jumper SPDT" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Solder Jumper, 3-pole, open" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "SolderJumper*Open*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "SolderJumper_3_Open_0_1"
        (arc (start -1.016 1.016) (mid -2.032 0) (end -1.016 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start -1.016 1.016) (mid -2.032 0) (end -1.016 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (rectangle (start -0.508 1.016) (end 0.508 -1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -2.032 0)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 1.016)
            (xy -1.016 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 1.016)
            (xy 1.016 -1.016)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 2.032 0)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 1.016 -1.016) (mid 2.032 0) (end 1.016 1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 1.016 -1.016) (mid 2.032 0) (end 1.016 1.016)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
      )
      (symbol "SolderJumper_3_Open_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at 0 -3.81 90) (length 2.54)
          (name "C" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Mechanical:Fiducial" (in_bom yes) (on_board yes)
      (property "Reference" "FID" (id 0) (at 0 5.08 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "Fiducial" (id 1) (at 0 3.175 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "fiducial marker" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Fiducial Marker" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Fiducial*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Fiducial_0_1"
        (circle (center 0 0) (radius 1.27)
          (stroke (width 0.508) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
    )
    (symbol "Mechanical:Heatsink" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "HS" (id 0) (at 0 5.08 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "Heatsink" (id 1) (at 0 -1.27 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0.3048 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0.3048 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "thermal heat temperature" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Heatsink" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Heatsink_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Heatsink_0_1"
        (polyline
          (pts
            (xy -0.3302 1.27)
            (xy -0.9652 1.27)
            (xy -0.9652 3.81)
            (xy -1.6002 3.81)
            (xy -1.6002 1.27)
            (xy -2.2352 1.27)
            (xy -2.2352 3.81)
            (xy -2.8702 3.81)
            (xy -2.8702 0)
            (xy -0.9652 0)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.3302 1.27)
            (xy -0.3302 3.81)
            (xy 0.3048 3.81)
            (xy 0.3048 1.27)
            (xy 0.9398 1.27)
            (xy 0.9398 3.81)
            (xy 1.5748 3.81)
            (xy 1.5748 1.27)
            (xy 2.2098 1.27)
            (xy 2.2098 3.81)
            (xy 2.8448 3.81)
            (xy 2.8448 0)
            (xy -0.9652 0)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
    )
    (symbol "Mechanical:MountingHole" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "H" (id 0) (at 0 5.08 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "MountingHole" (id 1) (at 0 3.175 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "mounting hole" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Mounting Hole without connection" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "MountingHole*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "MountingHole_0_1"
        (circle (center 0 0) (radius 1.27)
          (stroke (width 1.27) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
    )
    (symbol "Mechanical:MountingHole_Pad" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "H" (id 0) (at 0 6.35 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "MountingHole_Pad" (id 1) (at 0 4.445 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "mounting hole" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Mounting Hole with connection" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "MountingHole*Pad*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "MountingHole_Pad_0_1"
        (circle (center 0 1.27) (radius 1.27)
          (stroke (width 1.27) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "MountingHole_Pad_1_1"
        (pin input line (at 0 -2.54 90) (length 2.54)
          (name "1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
      )
    )
  )


  (text "3 x 4K7 resistors in 0603 package" (at 88.9 92.71 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 4412226e-d975-40a2-921f-502ff4129a95)
  )
  (text "This schematic serves as a test-file for the KiBom export script.\n\nAfter making a change to the schematic, remember to re-export the BOM to generate the intermediate .xml file\n\n(The testing framework cannot perform the netlist-export step!)"
    (at 13.97 24.13 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 7447a6e7-8205-46ba-afca-d0fa8f90c95a)
  )
  (text "3 x 4K7 resistors in 0805 package\nNote: Values are identical even if specified differently"
    (at 88.9 80.01 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 7e08f2a4-63d6-468b-bd8b-ec607077e023)
  )
  (text "5 x 10K resistors in 0805 package" (at 88.9 64.77 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 7f3eb118-a20c-4239-b800-c9211c66847d)
  )

  (symbol (lib_id "Device:R") (at 55.88 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a2873)
    (property "Reference" "R1" (id 0) (at 57.912 64.77 90))
    (property "Value" "10K" (id 1) (at 55.88 64.77 90))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 54.102 64.77 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 55.88 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tolerance" "5%" (id 4) (at 55.88 64.77 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 33068017-4804-4e39-bfa3-a6b963d602cc))
    (pin "2" (uuid dd23fb13-35cc-46df-916c-53464d31a148))
  )

  (symbol (lib_id "Device:R") (at 63.5 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a330d)
    (property "Reference" "R2" (id 0) (at 65.532 64.77 90))
    (property "Value" "10K" (id 1) (at 63.5 64.77 90))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 61.722 64.77 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 63.5 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tolerance" "10%" (id 4) (at 63.5 64.77 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid aad88d8c-d4fa-438f-a307-1c35c698a358))
    (pin "2" (uuid 5eee4b87-4429-4601-ac19-62db1bf881ea))
  )

  (symbol (lib_id "Device:R") (at 69.85 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a35e1)
    (property "Reference" "R3" (id 0) (at 71.882 64.77 90))
    (property "Value" "10K" (id 1) (at 69.85 64.77 90))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 68.072 64.77 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 69.85 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 8b275ec8-4d81-4865-aa95-7f7c7bb593a3))
    (pin "2" (uuid 5ae40ad6-1046-4090-b144-f4578be03bdc))
  )

  (symbol (lib_id "Device:R") (at 76.2 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a37b2)
    (property "Reference" "R4" (id 0) (at 78.232 64.77 90))
    (property "Value" "10K" (id 1) (at 76.2 64.77 90))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 74.422 64.77 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 76.2 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 5be48e87-cbbe-4535-994d-7af4d609224b))
    (pin "2" (uuid 162b5d3a-0dcc-4218-a7e1-bdcf1300f666))
  )

  (symbol (lib_id "Device:R") (at 82.55 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a39eb)
    (property "Reference" "R5" (id 0) (at 84.582 64.77 90))
    (property "Value" "10K" (id 1) (at 82.55 64.77 90))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 80.772 64.77 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 82.55 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 4850ce4c-0ffb-47c3-9b8c-34450b163c84))
    (pin "2" (uuid bcbb007a-82ae-4624-9376-66fd3004ff1c))
  )

  (symbol (lib_id "Device:R") (at 55.88 78.74 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a3ca0)
    (property "Reference" "R6" (id 0) (at 57.912 78.74 90))
    (property "Value" "4K7" (id 1) (at 55.88 78.74 90))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 54.102 78.74 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 55.88 78.74 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Config" "DNF" (id 4) (at 55.88 78.74 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid e4d167bf-df98-43bf-8b7b-545fc523dbf2))
    (pin "2" (uuid ee87b791-7bf6-4294-bf5f-21508e7078b8))
  )

  (symbol (lib_id "Device:R") (at 63.5 78.74 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a3f38)
    (property "Reference" "R7" (id 0) (at 65.532 78.74 90))
    (property "Value" "4700" (id 1) (at 63.5 78.74 90))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 61.722 78.74 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 63.5 78.74 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Config" "DNC" (id 4) (at 63.5 78.74 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 8881639b-8c4a-4aa2-aaf4-0f49bc2cff73))
    (pin "2" (uuid d3e27832-4c96-4087-8a3b-bb6f81aca8f1))
  )

  (symbol (lib_id "Device:R") (at 69.85 78.74 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a4181)
    (property "Reference" "R8" (id 0) (at 71.882 78.74 90))
    (property "Value" "4.7K" (id 1) (at 69.85 78.74 90))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 68.072 78.74 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 69.85 78.74 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid a66112cd-2eb5-4744-80fb-e2d33c5f5277))
    (pin "2" (uuid 9f5e063c-15fd-4b1b-9ac7-139401f906c9))
  )

  (symbol (lib_id "Device:R") (at 55.88 92.71 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a448b)
    (property "Reference" "R9" (id 0) (at 57.912 92.71 90))
    (property "Value" "4K7" (id 1) (at 55.88 92.71 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 54.102 92.71 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 55.88 92.71 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 4d11d16f-8509-4406-b816-a96c0c352516))
    (pin "2" (uuid 9f095dd4-7522-4f5e-8dbd-36a8a511cb15))
  )

  (symbol (lib_id "Device:R") (at 63.5 92.71 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a491a)
    (property "Reference" "R10" (id 0) (at 65.532 92.71 90))
    (property "Value" "4K7" (id 1) (at 63.5 92.71 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 61.722 92.71 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 63.5 92.71 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 3065493e-deea-45cd-94dc-4af67b0ce02a))
    (pin "2" (uuid 8ce6f495-1529-4aea-a8f2-bce549a4d19e))
  )

  (symbol (lib_id "Device:C") (at 168.91 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a62cc)
    (property "Reference" "C1" (id 0) (at 169.545 62.23 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "10nF" (id 1) (at 169.545 67.31 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 169.8752 68.58 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 168.91 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 5470a9c9-b552-443a-9cde-c1b1d8fa895b))
    (pin "2" (uuid 135c29c7-66f3-4799-9d85-30447f5c0522))
  )

  (symbol (lib_id "Device:C") (at 179.07 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a6854)
    (property "Reference" "C2" (id 0) (at 179.705 62.23 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "10n" (id 1) (at 179.705 67.31 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 180.0352 68.58 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 179.07 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 31a4ed14-aeae-4da4-9fa2-e96896dedc51))
    (pin "2" (uuid 8624136f-a780-493a-ae6d-ed2b94288860))
  )

  (symbol (lib_id "Device:C") (at 189.23 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a6a34)
    (property "Reference" "C3" (id 0) (at 189.865 62.23 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "0.01uF" (id 1) (at 189.865 67.31 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 190.1952 68.58 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 189.23 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 5edf7739-53e3-4a4d-b7c7-a479e09b3119))
    (pin "2" (uuid 068418de-6b06-46f8-a42a-f6e7af9942f0))
  )

  (symbol (lib_id "Device:C") (at 200.66 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005e6a6cb6)
    (property "Reference" "C4" (id 0) (at 201.295 62.23 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "0.01uf" (id 1) (at 201.295 67.31 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 201.6252 68.58 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 200.66 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid c3bda053-a317-478b-9661-cf51e69da846))
    (pin "2" (uuid 39b9d340-a88f-43ab-b665-8c0d0b261be6))
  )

  (symbol (lib_id "Connector:TestPoint") (at 57.15 115.57 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f32ef71)
    (property "Reference" "P1" (id 0) (at 58.6232 112.5728 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TestPoint" (id 1) (at 58.6232 114.8842 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 62.23 115.57 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 62.23 115.57 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 6914ffbd-64da-428e-9832-d92ed02f44a6))
  )

  (symbol (lib_id "Mechanical:Fiducial") (at 57.15 123.19 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f32f77f)
    (property "Reference" "FID1" (id 0) (at 59.309 122.0216 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "Fiducial" (id 1) (at 59.309 124.333 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 57.15 123.19 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 57.15 123.19 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )

  (symbol (lib_id "Mechanical:MountingHole") (at 54.61 133.35 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f32fc3f)
    (property "Reference" "H1" (id 0) (at 57.15 132.1816 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MountingHole" (id 1) (at 57.15 134.493 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 54.61 133.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 54.61 133.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )

  (symbol (lib_id "Mechanical:MountingHole_Pad") (at 78.74 134.62 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f3304c4)
    (property "Reference" "H3" (id 0) (at 81.28 133.3754 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MountingHole_Pad" (id 1) (at 81.28 135.6868 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 78.74 134.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 78.74 134.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 4eb429c7-4fab-4fba-b290-f2bf48616d50))
  )

  (symbol (lib_id "Jumper:SolderJumper_2_Bridged") (at 85.09 113.03 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f3315cc)
    (property "Reference" "JP2" (id 0) (at 85.09 107.823 0))
    (property "Value" "SolderJumper_2_Bridged" (id 1) (at 85.09 110.1344 0))
    (property "Footprint" "" (id 2) (at 85.09 113.03 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 85.09 113.03 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid b3720aa0-3a9f-43ce-995b-08150aa0e4dd))
    (pin "2" (uuid ba99016a-752a-4802-9e11-b31d8c68f6ab))
  )

  (symbol (lib_id "Jumper:SolderJumper_2_Open") (at 85.09 123.19 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f33205b)
    (property "Reference" "JP3" (id 0) (at 85.09 117.983 0))
    (property "Value" "SolderJumper_2_Open" (id 1) (at 85.09 120.2944 0))
    (property "Footprint" "" (id 2) (at 85.09 123.19 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 85.09 123.19 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 30a6b211-0dc3-4f51-bcb7-52fe848ee97e))
    (pin "2" (uuid c0a65da3-beb8-4138-941f-bdc7366559f8))
  )

  (symbol (lib_id "Jumper:SolderJumper_3_Bridged12") (at 111.76 113.03 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f332e98)
    (property "Reference" "JP4" (id 0) (at 111.76 107.823 0))
    (property "Value" "SolderJumper_3_Bridged12" (id 1) (at 111.76 110.1344 0))
    (property "Footprint" "" (id 2) (at 111.76 113.03 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 111.76 113.03 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 20a29213-67f4-49db-b6f8-4f44dd17ae6d))
    (pin "2" (uuid c1560820-3c1b-4ced-ad8a-1e62ae54f3bf))
    (pin "3" (uuid b57d2ad2-879c-4417-bb2d-e54271dcd2a1))
  )

  (symbol (lib_id "Jumper:SolderJumper_3_Bridged123") (at 111.76 125.73 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f333ee0)
    (property "Reference" "JP5" (id 0) (at 111.76 120.523 0))
    (property "Value" "SolderJumper_3_Bridged123" (id 1) (at 111.76 122.8344 0))
    (property "Footprint" "" (id 2) (at 111.76 125.73 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 111.76 125.73 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid b0813dc4-dc82-49ff-81b0-cb5e56980f48))
    (pin "2" (uuid 44ad8cf6-8dd2-4e85-8ec1-ce89487221ca))
    (pin "3" (uuid 9ae74a5a-35b8-41d1-b0bc-b0c268d80282))
  )

  (symbol (lib_id "Jumper:SolderJumper_3_Open") (at 111.76 138.43 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f334fb5)
    (property "Reference" "JP6" (id 0) (at 111.76 133.223 0))
    (property "Value" "SolderJumper_3_Open" (id 1) (at 111.76 135.5344 0))
    (property "Footprint" "" (id 2) (at 111.76 138.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 111.76 138.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 57ae5647-0796-4ac6-bcfb-5c6815dbd65b))
    (pin "2" (uuid 95fc8353-65f9-4e47-8dc2-21e6681cd87d))
    (pin "3" (uuid 5e63b868-252d-4750-aa33-b9a59444f4ac))
  )

  (symbol (lib_id "Connector:TestPoint_2Pole") (at 139.7 113.03 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f33653c)
    (property "Reference" "P4" (id 0) (at 139.7 108.077 0))
    (property "Value" "TestPoint_2Pole" (id 1) (at 139.7 110.3884 0))
    (property "Footprint" "" (id 2) (at 139.7 113.03 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 139.7 113.03 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 50de7d87-b6d1-4ebd-b0f1-749a3f12ea8f))
    (pin "2" (uuid ffd3e603-745e-42af-959a-7e50314e66ea))
  )

  (symbol (lib_id "Connector:TestPoint_Alt") (at 139.7 120.65 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f336fc3)
    (property "Reference" "P5" (id 0) (at 141.1732 117.6528 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TestPoint_Alt" (id 1) (at 141.1732 119.9642 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 144.78 120.65 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 144.78 120.65 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 5536665c-f95e-4936-acb8-df6d0c3c8ee9))
  )

  (symbol (lib_id "Connector:TestPoint_Flag") (at 138.43 127 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f33770d)
    (property "Reference" "P2" (id 0) (at 145.034 124.6124 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TestPoint_Flag" (id 1) (at 145.034 126.9238 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 143.51 127 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 143.51 127 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid d4655a23-c468-4a8b-99e6-64b8fe288202))
  )

  (symbol (lib_id "Connector:TestPoint_Small") (at 138.43 133.35 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f337fd0)
    (property "Reference" "P3" (id 0) (at 139.6492 132.1816 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TestPoint_Small" (id 1) (at 139.6492 134.493 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 143.51 133.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 143.51 133.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 38983155-b87a-497c-9b83-4071135b9376))
  )

  (symbol (lib_id "Connector:TestPoint_Probe") (at 139.7 142.24 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f33872c)
    (property "Reference" "P6" (id 0) (at 143.5862 139.6746 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TestPoint_Probe" (id 1) (at 143.5862 141.986 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 144.78 142.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 144.78 142.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 0036210c-00f4-4166-b741-600551aa9068))
  )

  (symbol (lib_id "Mechanical:MountingHole") (at 55.88 147.32 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f338f80)
    (property "Reference" "H2" (id 0) (at 58.42 146.1516 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "2mm" (id 1) (at 58.42 148.463 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 55.88 147.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 55.88 147.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )

  (symbol (lib_id "Jumper:SolderJumper_3_Open") (at 77.47 147.32 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f33938a)
    (property "Reference" "JP1" (id 0) (at 77.47 142.113 0))
    (property "Value" "Select" (id 1) (at 77.47 144.4244 0))
    (property "Footprint" "" (id 2) (at 77.47 147.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 77.47 147.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid ef739c4f-87e5-4e81-b796-4843e8c1db8a))
    (pin "2" (uuid 6a6f11e3-ebb1-4b21-8d4a-25853bcf4a7a))
    (pin "3" (uuid bedf389a-7ee8-4bb5-a9cc-9e9bab4f29ac))
  )

  (symbol (lib_id "Mechanical:Fiducial") (at 92.71 148.59 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f339b4f)
    (property "Reference" "X1" (id 0) (at 94.869 147.4216 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "Mark" (id 1) (at 94.869 149.733 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Fiducial:Fiducial_1mm_Mask2mm" (id 2) (at 92.71 148.59 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 92.71 148.59 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )

  (symbol (lib_id "Mechanical:Heatsink") (at 111.76 149.86 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f33aa80)
    (property "Reference" "TP1" (id 0) (at 115.3668 146.7866 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "Heatsink" (id 1) (at 115.3668 149.098 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 112.0648 149.86 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 112.0648 149.86 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )

  (sheet_instances
    (path "/" (page "1"))
  )

  (symbol_instances
    (path "/00000000-0000-0000-0000-00005e6a62cc"
      (reference "C1") (unit 1) (value "10nF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path "/00000000-0000-0000-0000-00005e6a6854"
      (reference "C2") (unit 1) (value "10n") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path "/00000000-0000-0000-0000-00005e6a6a34"
      (reference "C3") (unit 1) (value "0.01uF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path "/00000000-0000-0000-0000-00005e6a6cb6"
      (reference "C4") (unit 1) (value "0.01uf") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path "/00000000-0000-0000-0000-00005f32f77f"
      (reference "FID1") (unit 1) (value "Fiducial") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f32fc3f"
      (reference "H1") (unit 1) (value "MountingHole") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f338f80"
      (reference "H2") (unit 1) (value "2mm") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f3304c4"
      (reference "H3") (unit 1) (value "MountingHole_Pad") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f33938a"
      (reference "JP1") (unit 1) (value "Select") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f3315cc"
      (reference "JP2") (unit 1) (value "SolderJumper_2_Bridged") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f33205b"
      (reference "JP3") (unit 1) (value "SolderJumper_2_Open") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f332e98"
      (reference "JP4") (unit 1) (value "SolderJumper_3_Bridged12") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f333ee0"
      (reference "JP5") (unit 1) (value "SolderJumper_3_Bridged123") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f334fb5"
      (reference "JP6") (unit 1) (value "SolderJumper_3_Open") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f32ef71"
      (reference "P1") (unit 1) (value "TestPoint") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f33770d"
      (reference "P2") (unit 1) (value "TestPoint_Flag") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f337fd0"
      (reference "P3") (unit 1) (value "TestPoint_Small") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f33653c"
      (reference "P4") (unit 1) (value "TestPoint_2Pole") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f336fc3"
      (reference "P5") (unit 1) (value "TestPoint_Alt") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f33872c"
      (reference "P6") (unit 1) (value "TestPoint_Probe") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005e6a2873"
      (reference "R1") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path "/00000000-0000-0000-0000-00005e6a330d"
      (reference "R2") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path "/00000000-0000-0000-0000-00005e6a35e1"
      (reference "R3") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path "/00000000-0000-0000-0000-00005e6a37b2"
      (reference "R4") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path "/00000000-0000-0000-0000-00005e6a39eb"
      (reference "R5") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path "/00000000-0000-0000-0000-00005e6a3ca0"
      (reference "R6") (unit 1) (value "4K7") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path "/00000000-0000-0000-0000-00005e6a3f38"
      (reference "R7") (unit 1) (value "4700") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path "/00000000-0000-0000-0000-00005e6a4181"
      (reference "R8") (unit 1) (value "4.7K") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path "/00000000-0000-0000-0000-00005e6a448b"
      (reference "R9") (unit 1) (value "4K7") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path "/00000000-0000-0000-0000-00005e6a491a"
      (reference "R10") (unit 1) (value "4K7") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path "/00000000-0000-0000-0000-00005f33aa80"
      (reference "TP1") (unit 1) (value "Heatsink") (footprint "")
    )
    (path "/00000000-0000-0000-0000-00005f339b4f"
      (reference "X1") (unit 1) (value "Mark") (footprint "Fiducial:Fiducial_1mm_Mask2mm")
    )
  )
)
