(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")

  (footprint "kikit:Board" (layer "F.Cu")
    (tedit 605A1488) (tstamp 00000000-0000-0000-0000-0000605a7057)
    (at 100 90)
    (descr "Mark board for extraction")
    (attr through_hole)
    (fp_text reference "B1" (at -4.5 -5) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp cc934527-b84e-4ca1-ad52-399f8e7bf3df)
    )
    (fp_text value "Board" (at -7.25 -5) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 43c89b73-cf56-4390-ad99-0ff92ac35d30)
    )
    (fp_line (start 0 0) (end 0.5 -1) (layer "Dwgs.User") (width 0.2) (tstamp 2d675f93-d44f-485c-8207-150c12492452))
    (fp_line (start 0 0) (end -1.25 -4) (layer "Dwgs.User") (width 0.2) (tstamp 87358536-a504-44ce-8c66-b8b876d8894f))
    (fp_line (start -1.25 -4) (end -9.25 -4) (layer "Dwgs.User") (width 0.2) (tstamp 982364b6-bcbd-41ff-a125-84aef9991943))
    (fp_line (start 0 0) (end -1 -0.5) (layer "Dwgs.User") (width 0.2) (tstamp dd80f3b3-31f9-4741-adf5-c81fa1f4c68b))
  )

  (footprint "kikit:Board" (layer "F.Cu")
    (tedit 605A1488) (tstamp 00000000-0000-0000-0000-0000605a706e)
    (at 135 90)
    (descr "Mark board for extraction")
    (attr through_hole)
    (fp_text reference "B2" (at -4.5 -5) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 5c8f7927-58c0-47ef-854e-3dd8cc0bf312)
    )
    (fp_text value "Board" (at -7.25 -5) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bb77f266-f95c-4d63-b73d-9eb5f6c9f1bc)
    )
    (fp_line (start 0 0) (end -1 -0.5) (layer "Dwgs.User") (width 0.2) (tstamp 17e1baca-0f8f-4171-b616-6601bb7efd5b))
    (fp_line (start -1.25 -4) (end -9.25 -4) (layer "Dwgs.User") (width 0.2) (tstamp 2cc0aca6-d467-4eed-bd95-c60b0cdb0ccc))
    (fp_line (start 0 0) (end 0.5 -1) (layer "Dwgs.User") (width 0.2) (tstamp 3605dbc5-2619-4e06-bf86-49f1c1817220))
    (fp_line (start 0 0) (end -1.25 -4) (layer "Dwgs.User") (width 0.2) (tstamp 500b75b0-5ef8-4f0f-8bab-ed9123c39485))
  )

  (footprint "kikit:Board" (layer "F.Cu")
    (tedit 605A1488) (tstamp 00000000-0000-0000-0000-0000605a707c)
    (at 185 90)
    (descr "Mark board for extraction")
    (attr through_hole)
    (fp_text reference "B3" (at -4.5 -5) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 01bee0de-da40-4390-898d-9738e5a86bcc)
    )
    (fp_text value "Board" (at -7.25 -5) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3f2b141b-7bc9-4979-84f7-000f6c66c53b)
    )
    (fp_line (start 0 0) (end 0.5 -1) (layer "Dwgs.User") (width 0.2) (tstamp 0ef8c6c7-83b7-4ec8-8948-2e70fa334d77))
    (fp_line (start -1.25 -4) (end -9.25 -4) (layer "Dwgs.User") (width 0.2) (tstamp 181c6f00-96c3-4bb7-ba16-c3fde41797ab))
    (fp_line (start 0 0) (end -1.25 -4) (layer "Dwgs.User") (width 0.2) (tstamp 5e41870a-537a-491e-a56f-ec6759e82e36))
    (fp_line (start 0 0) (end -1 -0.5) (layer "Dwgs.User") (width 0.2) (tstamp f1ebaa83-56da-4499-929a-773021ade5b3))
  )

  (gr_line (start 150 110) (end 135 110) (layer "Edge.Cuts") (width 0.2) (tstamp 00000000-0000-0000-0000-0000605a1415))
  (gr_line (start 210 90) (end 180 90) (layer "Edge.Cuts") (width 0.2) (tstamp 00000000-0000-0000-0000-0000605a1425))
  (gr_line (start 200 100) (end 190 100) (layer "Edge.Cuts") (width 0.2) (tstamp 00000000-0000-0000-0000-0000605a142a))
  (gr_line (start 160 100) (end 150 100) (layer "Edge.Cuts") (width 0.2) (tstamp 51ee268f-1cdb-4d7d-9c21-906f097e0468))
  (gr_line (start 180 90) (end 180 110) (layer "Edge.Cuts") (width 0.2) (tstamp 64c01c4a-0872-44ed-b267-b18d90185def))
  (gr_line (start 210 110) (end 210 90) (layer "Edge.Cuts") (width 0.2) (tstamp 7197a3a4-13b0-4964-97bb-d3c67b25d3cc))
  (gr_line (start 160 90) (end 160 100) (layer "Edge.Cuts") (width 0.2) (tstamp 993fe7e0-bb83-477b-b768-ddb19b694f3e))
  (gr_line (start 135 90) (end 160 90) (layer "Edge.Cuts") (width 0.2) (tstamp a3e28d38-69cd-42a1-b425-f1a15302e858))
  (gr_line (start 180 110) (end 210 110) (layer "Edge.Cuts") (width 0.2) (tstamp afbb53e6-3063-40ce-bb83-3604be396e1d))
  (gr_line (start 190 105) (end 200 105) (layer "Edge.Cuts") (width 0.2) (tstamp c0684255-d65e-4027-adfe-519b7fcde519))
  (gr_line (start 135 110) (end 135 90) (layer "Edge.Cuts") (width 0.2) (tstamp c30d7998-579c-409d-b75a-00fa9f4eed59))
  (gr_circle (center 100 100) (end 110 100) (layer "Edge.Cuts") (width 0.2) (fill none) (tstamp c817e371-265a-41a5-8be4-97a10008c2fc))
  (gr_line (start 150 100) (end 150 110) (layer "Edge.Cuts") (width 0.2) (tstamp d2bf3808-d0b7-47de-a1f9-f2e94b771c7b))
  (gr_line (start 190 100) (end 190 105) (layer "Edge.Cuts") (width 0.2) (tstamp da6b8bc6-f48f-49c2-9e3e-3bb909ccfe9a))
  (gr_line (start 200 105) (end 200 100) (layer "Edge.Cuts") (width 0.2) (tstamp e6c0520a-00d5-4fde-85e1-681298498d17))
  (gr_text "B" (at 145 100) (layer "F.SilkS") (tstamp 00000000-0000-0000-0000-0000605a709d)
    (effects (font (size 5 5) (thickness 1)))
  )
  (gr_text "C" (at 185 100) (layer "F.SilkS") (tstamp 00000000-0000-0000-0000-0000605a709f)
    (effects (font (size 5 5) (thickness 1)))
  )
  (gr_text "A" (at 100 100) (layer "F.SilkS") (tstamp eb565a94-7da3-44d3-82d1-76c30d6f561a)
    (effects (font (size 5 5) (thickness 1)))
  )

)
