(kicad_sch (version 20211123) (generator eeschema)

  (uuid e6521bef-4109-48f7-8b88-4121b0468927)

  (paper "A4")

  (lib_symbols
    (symbol "RF:AX5043" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -8.89 21.59 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "AX5043" (id 1) (at 8.89 21.59 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm" (id 2) (at 53.34 36.83 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "https://www.onsemi.com/pub/Collateral/AX5043-D.PDF" (id 3) (at 34.29 34.29 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "RF, tranceiver" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Advanced High Performance ASK and FSK Narrow-band Transceiver for 27 - 1050 MHz Range" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "QFN?28*5x5mm*P0.5mm*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "AX5043_1_0"
        (rectangle (start -10.16 -20.32) (end 10.16 20.32)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
      (symbol "AX5043_1_1"
        (pin power_out line (at 2.54 22.86 270) (length 2.54)
          (name "VDD_ANA" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -12.7 -15.24 0) (length 2.54)
          (name "L1" (effects (font (size 1.27 1.27))))
          (number "10" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 12.7 -15.24 180) (length 2.54)
          (name "DATA" (effects (font (size 1.27 1.27))))
          (number "11" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 12.7 -12.7 180) (length 2.54)
          (name "DCLK" (effects (font (size 1.27 1.27))))
          (number "12" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 12.7 -10.16 180) (length 2.54)
          (name "SYSCLK" (effects (font (size 1.27 1.27))))
          (number "13" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -12.7 -5.08 0) (length 2.54)
          (name "SEL" (effects (font (size 1.27 1.27))))
          (number "14" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -12.7 2.54 0) (length 2.54)
          (name "CLK" (effects (font (size 1.27 1.27))))
          (number "15" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at -12.7 0 0) (length 2.54)
          (name "MISO" (effects (font (size 1.27 1.27))))
          (number "16" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -12.7 -2.54 0) (length 2.54)
          (name "MOSI" (effects (font (size 1.27 1.27))))
          (number "17" (effects (font (size 1.27 1.27))))
        )
        (pin no_connect line (at -2.54 -20.32 90) (length 2.54) hide
          (name "NC" (effects (font (size 1.27 1.27))))
          (number "18" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at 12.7 5.08 180) (length 2.54)
          (name "IRQ" (effects (font (size 1.27 1.27))))
          (number "19" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at 0 -22.86 90) (length 2.54)
          (name "GND" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 12.7 7.62 180) (length 2.54)
          (name "PWRAMP" (effects (font (size 1.27 1.27))))
          (number "20" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 12.7 10.16 180) (length 2.54)
          (name "ANTSEL" (effects (font (size 1.27 1.27))))
          (number "21" (effects (font (size 1.27 1.27))))
        )
        (pin no_connect line (at 2.54 -20.32 90) (length 2.54) hide
          (name "NC" (effects (font (size 1.27 1.27))))
          (number "22" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at 0 22.86 270) (length 2.54)
          (name "VDD_IO" (effects (font (size 1.27 1.27))))
          (number "23" (effects (font (size 1.27 1.27))))
        )
        (pin no_connect line (at -5.08 -20.32 90) (length 2.54) hide
          (name "NC" (effects (font (size 1.27 1.27))))
          (number "24" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -12.7 10.16 0) (length 2.54)
          (name "GPADC1" (effects (font (size 1.27 1.27))))
          (number "25" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -12.7 7.62 0) (length 2.54)
          (name "GPADC2" (effects (font (size 1.27 1.27))))
          (number "26" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -12.7 17.78 0) (length 2.54)
          (name "CLK16N" (effects (font (size 1.27 1.27))))
          (number "27" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -12.7 15.24 0) (length 2.54)
          (name "CLK16P" (effects (font (size 1.27 1.27))))
          (number "28" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -22.86 90) (length 2.54) hide
          (name "GND" (effects (font (size 1.27 1.27))))
          (number "29" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
          (name "ANTP" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
          (name "ANTN" (effects (font (size 1.27 1.27))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at 12.7 0 180) (length 2.54)
          (name "ANTP1" (effects (font (size 1.27 1.27))))
          (number "5" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -22.86 90) (length 2.54) hide
          (name "GND" (effects (font (size 1.27 1.27))))
          (number "6" (effects (font (size 1.27 1.27))))
        )
        (pin power_out line (at 5.08 22.86 270) (length 2.54)
          (name "VDD_ANA" (effects (font (size 1.27 1.27))))
          (number "7" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -12.7 -10.16 0) (length 2.54)
          (name "FILT" (effects (font (size 1.27 1.27))))
          (number "8" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -12.7 -12.7 0) (length 2.54)
          (name "L2" (effects (font (size 1.27 1.27))))
          (number "9" (effects (font (size 1.27 1.27))))
        )
      )
    )
  )


  (symbol (lib_id "RF:AX5043") (at 99.06 85.09 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-00005f9852ab)
    (property "Reference" "U1" (id 0) (at 99.06 110.2106 0))
    (property "Value" "AX5043" (id 1) (at 99.06 112.522 0))
    (property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm" (id 2) (at 152.4 48.26 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/AX5043-D.PDF" (id 3) (at 133.35 50.8 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Config" "DNF" (id 4) (at 99.06 85.09 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid c8a7af6e-c432-4fa3-91ee-c8bf0c5a9ebe))
    (pin "10" (uuid 91fe070a-a49b-4bc5-805a-42f23e10d114))
    (pin "11" (uuid 501880c3-8633-456f-9add-0e8fa1932ba6))
    (pin "12" (uuid c454102f-dc92-4550-9492-797fc8e6b49c))
    (pin "13" (uuid 7a879184-fad8-4feb-afb5-86fe8d34f1f7))
    (pin "14" (uuid 528fd7da-c9a6-40ae-9f1a-60f6a7f4d534))
    (pin "15" (uuid e413cfad-d7bd-41ab-b8dd-4b67484671a6))
    (pin "16" (uuid 18ca5aef-6a2c-41ac-9e7f-bf7acb716e53))
    (pin "17" (uuid f9b1563b-384a-447c-9f47-736504e995c8))
    (pin "18" (uuid 03f57fb4-32a3-4bc6-85b9-fd8ece4a9592))
    (pin "19" (uuid b78cb2c1-ae4b-4d9b-acd8-d7fe342342f2))
    (pin "2" (uuid 90e761f6-1432-4f73-ad28-fa8869b7ec31))
    (pin "20" (uuid 4431c0f6-83ea-4eee-95a8-991da2f03ccd))
    (pin "21" (uuid 24b72b0d-63b8-4e06-89d0-e94dcf39a600))
    (pin "22" (uuid a6738794-75ae-48a6-8949-ed8717400d71))
    (pin "23" (uuid d692b5e6-71b2-4fa6-bc83-618add8d8fef))
    (pin "24" (uuid 1e48966e-d29d-4521-8939-ec8ac570431d))
    (pin "25" (uuid 07d160b6-23e1-4aa0-95cb-440482e6fc15))
    (pin "26" (uuid a62609cd-29b7-4918-b97d-7b2404ba61cf))
    (pin "27" (uuid 844d7d7a-b386-45a8-aaf6-bf41bbcb43b5))
    (pin "28" (uuid ebca7c5e-ae52-43e5-ac6c-69a96a9a5b24))
    (pin "29" (uuid a07b6b2b-7179-4297-b163-5e47ffbe76d3))
    (pin "3" (uuid d1a9be32-38ba-44e6-bc35-f031541ab1fe))
    (pin "4" (uuid 6ac3ab53-7523-4805-bfd2-5de19dff127e))
    (pin "5" (uuid a8219a78-6b33-4efa-a789-6a67ce8f7a50))
    (pin "6" (uuid 2a1de22d-6451-488d-af77-0bf8841bd695))
    (pin "7" (uuid f3044f68-903d-4063-b253-30d8e3a83eae))
    (pin "8" (uuid 05f2859d-2820-4e84-b395-696011feb13b))
    (pin "9" (uuid a8fb8ee0-623f-4870-a716-ecc88f37ef9a))
  )

  (sheet_instances
    (path "/" (page "1"))
  )

  (symbol_instances
    (path "/00000000-0000-0000-0000-00005f9852ab"
      (reference "U1") (unit 1) (value "AX5043") (footprint "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm")
    )
  )
)
