(kicad_sch (version 20211123) (generator eeschema)

  (uuid e6521bef-4109-48f7-8b88-4121b0468927)

  (paper "A4")

  (lib_symbols
    (symbol "Comparator:LTC6752xUD-3" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 3.81 -5.08 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Value" "LTC6752xUD-3" (id 1) (at 3.81 -7.62 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Footprint" "Package_DFN_QFN:QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm" (id 2) (at 0 -16.51 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6752fc.pdf" (id 3) (at -2.54 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "single comparator high speed cmos" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Single 280Mhz 2.9ns Comparator, Rail-to-Rail Inputs, CMOS Output, QFN-12" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "LTC6752xUD-3_0_1"
        (polyline
          (pts
            (xy 5.08 3.81)
            (xy 5.08 0)
            (xy -5.08 5.08)
            (xy -5.08 -5.08)
            (xy 5.08 0)
            (xy 5.08 -3.81)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
      (symbol "LTC6752xUD-3_1_1"
        (pin power_in line (at 0 7.62 270) (length 5.08)
          (name "VDD" (effects (font (size 0.762 0.762))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at 7.62 -2.54 180) (length 2.54)
          (name "~{Q}" (effects (font (size 1.27 1.27))))
          (number "10" (effects (font (size 1.27 1.27))))
        )
        (pin no_connect line (at 5.08 0 180) (length 2.54) hide
          (name "NC" (effects (font (size 1.27 1.27))))
          (number "11" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at 7.62 2.54 180) (length 2.54)
          (name "Q" (effects (font (size 1.27 1.27))))
          (number "12" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -2.54 -7.62 90) (length 3.81) hide
          (name "VEE" (effects (font (size 1.016 1.016))))
          (number "13" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at -2.54 7.62 270) (length 3.81)
          (name "VCC" (effects (font (size 1.016 1.016))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at -2.54 -7.62 90) (length 3.81)
          (name "VEE" (effects (font (size 1.016 1.016))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+" (effects (font (size 1.016 1.016))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
        (pin no_connect line (at -5.08 0 0) (length 2.54) hide
          (name "NC" (effects (font (size 1.27 1.27))))
          (number "5" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-" (effects (font (size 1.016 1.016))))
          (number "6" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at 2.54 7.62 270) (length 6.35)
          (name "~{SHDN}" (effects (font (size 0.508 0.508))))
          (number "7" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at 0 -7.62 90) (length 5.08)
          (name "~{LE}" (effects (font (size 0.635 0.635))))
          (number "8" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -2.54 -7.62 90) (length 3.81) hide
          (name "VEE" (effects (font (size 1.016 1.016))))
          (number "9" (effects (font (size 1.27 1.27))))
        )
      )
    )
  )


  (symbol (lib_id "Comparator:LTC6752xUD-3") (at 104.775 85.725 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 00000000-0000-0000-0000-0000601afefd)
    (property "Reference" "U1" (id 0) (at 113.5126 84.5566 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "LTC6752xUD-3" (id 1) (at 113.5126 86.868 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm" (id 2) (at 104.775 102.235 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6752fc.pdf" (id 3) (at 102.235 85.725 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 4d4fecdd-be4a-47e9-9085-2268d5852d8f))
    (pin "10" (uuid 8458d41c-5d62-455d-b6e1-9f718c0faac9))
    (pin "11" (uuid 8de2d84c-ff45-4d4f-bc49-c166f6ae6b91))
    (pin "12" (uuid 935057d5-6882-4c15-9a35-54677912ba12))
    (pin "13" (uuid e091e263-c616-48ef-a460-465c70218987))
    (pin "2" (uuid 71c6e723-673c-45a9-a0e4-9742220c52a3))
    (pin "3" (uuid b4833916-7a3e-4498-86fb-ec6d13262ffe))
    (pin "4" (uuid cc48dd41-7768-48d3-b096-2c4cc2126c9d))
    (pin "5" (uuid 4185c36c-c66e-4dbd-be5d-841e551f4885))
    (pin "6" (uuid a8b4bc7e-da32-4fb8-b71a-d7b47c6f741f))
    (pin "7" (uuid 0fd35a3e-b394-4aae-875a-fac843f9cbb7))
    (pin "8" (uuid c088f712-1abe-4cac-9a8b-d564931395aa))
    (pin "9" (uuid ea6fde00-59dc-4a79-a647-7e38199fae0e))
  )

  (sheet_instances
    (path "/" (page "1"))
  )

  (symbol_instances
    (path "/00000000-0000-0000-0000-0000601afefd"
      (reference "U1") (unit 1) (value "LTC6752xUD-3") (footprint "Package_DFN_QFN:QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm")
    )
  )
)
